(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 38)
    (no_connects 0)
    (area 141.924999 93.924999 158.075001 115.075001)
    (thickness 1.6)
    (drawings 19)
    (tracks 204)
    (zones 0)
    (modules 4)
    (nets 29)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad2)")
  (net 2 "Net-(J1-Pad4)")
  (net 3 "Net-(J1-Pad6)")
  (net 4 "Net-(J1-Pad8)")
  (net 5 "Net-(J1-Pad10)")
  (net 6 "Net-(J1-Pad12)")
  (net 7 "Net-(J1-Pad14)")
  (net 8 "Net-(J1-Pad16)")
  (net 9 "Net-(J1-Pad18)")
  (net 10 "Net-(J1-Pad20)")
  (net 11 "Net-(J1-Pad25)")
  (net 12 "Net-(J1-Pad26)")
  (net 13 "Net-(J1-Pad27)")
  (net 14 "Net-(J1-Pad28)")
  (net 15 /1)
  (net 16 /2)
  (net 17 /3)
  (net 18 /4)
  (net 19 /5)
  (net 20 /6)
  (net 21 /7)
  (net 22 /8)
  (net 23 /9)
  (net 24 /10)
  (net 25 /14)
  (net 26 /11)
  (net 27 /13)
  (net 28 /12)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /1)
    (add_net /10)
    (add_net /11)
    (add_net /12)
    (add_net /13)
    (add_net /14)
    (add_net /2)
    (add_net /3)
    (add_net /4)
    (add_net /5)
    (add_net /6)
    (add_net /7)
    (add_net /8)
    (add_net /9)
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad12)")
    (add_net "Net-(J1-Pad14)")
    (add_net "Net-(J1-Pad16)")
    (add_net "Net-(J1-Pad18)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad20)")
    (add_net "Net-(J1-Pad25)")
    (add_net "Net-(J1-Pad26)")
    (add_net "Net-(J1-Pad27)")
    (add_net "Net-(J1-Pad28)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad8)")
  )
  (module Pin_Headers:Pin_Header_Straight_1x14_Pitch1.00mm_SMD_Pin1Left (layer B.Cu) (tedit 5D2E38D3)
    (at 154 105 270)
    (descr "surface-mounted straight pin header, 1x14, 1.00mm pitch, single row, style 1 (pin 1 left)")
    (tags "Surface mounted pin header SMD 1x14 1.00mm single row style1 pin1 left")
    (attr smd)
    (fp_text reference J4 (at 0 8.06 270) (layer B.SilkS) hide)
    (fp_text value CONN_01X14 (at 0.5 -3.5 270) (layer B.Fab))
    (pad 15 smd rect (at 4.25 -2.5 270) (size 0.4 0.8) (layers B.Cu B.Paste B.Mask))
    (pad 15 smd rect (at -4.25 -2.5 270) (size 0.4 0.8) (layers B.Cu B.Paste B.Mask))
    (pad 14 smd rect (at 3.25 0 270) (size 0.3 0.8) (layers B.Cu B.Paste B.Mask)
      (net 25 /14))
    (pad 13 smd rect (at 2.75 0 270) (size 0.3 0.8) (layers B.Cu B.Paste B.Mask)
      (net 27 /13))
    (pad 12 smd rect (at 2.25 0 270) (size 0.3 0.8) (layers B.Cu B.Paste B.Mask)
      (net 28 /12))
    (pad 11 smd rect (at 1.75 0 270) (size 0.3 0.8) (layers B.Cu B.Paste B.Mask)
      (net 26 /11))
    (pad 10 smd rect (at 1.25 0 270) (size 0.3 0.8) (layers B.Cu B.Paste B.Mask)
      (net 24 /10))
    (pad 9 smd rect (at 0.75 0 270) (size 0.3 0.8) (layers B.Cu B.Paste B.Mask)
      (net 23 /9))
    (pad 8 smd rect (at 0.25 0 270) (size 0.3 0.8) (layers B.Cu B.Paste B.Mask)
      (net 22 /8))
    (pad 7 smd rect (at -0.25 0 270) (size 0.3 0.8) (layers B.Cu B.Paste B.Mask)
      (net 21 /7))
    (pad 6 smd rect (at -0.75 0 270) (size 0.3 0.8) (layers B.Cu B.Paste B.Mask)
      (net 20 /6))
    (pad 5 smd rect (at -1.25 0 270) (size 0.3 0.8) (layers B.Cu B.Paste B.Mask)
      (net 19 /5))
    (pad 4 smd rect (at -1.75 0 270) (size 0.3 0.8) (layers B.Cu B.Paste B.Mask)
      (net 18 /4))
    (pad 3 smd rect (at -2.25 0 270) (size 0.3 0.8) (layers B.Cu B.Paste B.Mask)
      (net 17 /3))
    (pad 2 smd rect (at -2.75 0 270) (size 0.3 0.8) (layers B.Cu B.Paste B.Mask)
      (net 16 /2))
    (pad 1 smd rect (at -3.25 0 270) (size 0.3 0.8) (layers B.Cu B.Paste B.Mask)
      (net 15 /1))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x14_Pitch1.00mm_SMD_Pin1Left.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x12_Pitch1.27mm (layer F.Cu) (tedit 5D2E032B)
    (at 157 96 270)
    (descr "Through hole straight pin header, 1x12, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x12 1.27mm single row")
    (fp_text reference J2 (at 0 -1.695 270) (layer F.SilkS) hide)
    (fp_text value CONN_01X12 (at 0 15.665 270) (layer F.Fab))
    (fp_text user %R (at 0 6.985 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 15 /1))
    (pad 2 thru_hole oval (at 0 1.27 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 16 /2))
    (pad 3 thru_hole oval (at 0 2.54 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 17 /3))
    (pad 4 thru_hole oval (at 0 3.81 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 18 /4))
    (pad 5 thru_hole oval (at 0 5.08 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 19 /5))
    (pad 6 thru_hole oval (at 0 6.35 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 20 /6))
    (pad 7 thru_hole oval (at 0 7.62 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 21 /7))
    (pad 8 thru_hole oval (at 0 8.89 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 22 /8))
    (pad 9 thru_hole oval (at 0 10.16 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 23 /9))
    (pad 10 thru_hole oval (at 0 11.43 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 24 /10))
    (pad 11 thru_hole oval (at 0 12.7 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 26 /11))
    (pad 12 thru_hole oval (at 0 13.97 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 28 /12))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x12_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x12_Pitch1.27mm (layer F.Cu) (tedit 5D2E0302)
    (at 157 113.25 270)
    (descr "Through hole straight pin header, 1x12, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x12 1.27mm single row")
    (fp_text reference J3 (at 0 -1.695 270) (layer F.SilkS) hide)
    (fp_text value CONN_01X12 (at 0 15.665 270) (layer F.Fab))
    (fp_text user %R (at 0 6.985 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad2)"))
    (pad 2 thru_hole oval (at 0 1.27 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad4)"))
    (pad 3 thru_hole oval (at 0 2.54 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad6)"))
    (pad 4 thru_hole oval (at 0 3.81 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad8)"))
    (pad 5 thru_hole oval (at 0 5.08 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad10)"))
    (pad 6 thru_hole oval (at 0 6.35 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad12)"))
    (pad 7 thru_hole oval (at 0 7.62 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad14)"))
    (pad 8 thru_hole oval (at 0 8.89 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad16)"))
    (pad 9 thru_hole oval (at 0 10.16 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad18)"))
    (pad 10 thru_hole oval (at 0 11.43 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad20)"))
    (pad 11 thru_hole oval (at 0 12.7 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 25 /14))
    (pad 12 thru_hole oval (at 0 13.97 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 27 /13))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x12_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module AXT624124:AXT624124 (layer F.Cu) (tedit 5D2DFC31)
    (at 150 105 90)
    (descr AXT624124)
    (tags Connector)
    (attr smd)
    (fp_text reference J1 (at 0 0 90) (layer F.SilkS))
    (fp_text value AXT624124 (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.2 1.225 90) (size 0.23 0.75) (layers F.Cu F.Paste F.Mask)
      (net 15 /1))
    (pad 2 smd rect (at -2.2 -1.225 90) (size 0.23 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J1-Pad2)"))
    (pad 3 smd rect (at -1.8 1.225 90) (size 0.23 0.75) (layers F.Cu F.Paste F.Mask)
      (net 16 /2))
    (pad 4 smd rect (at -1.8 -1.225 90) (size 0.23 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad4)"))
    (pad 5 smd rect (at -1.4 1.225 90) (size 0.23 0.75) (layers F.Cu F.Paste F.Mask)
      (net 17 /3))
    (pad 6 smd rect (at -1.4 -1.225 90) (size 0.23 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad6)"))
    (pad 7 smd rect (at -1 1.225 90) (size 0.23 0.75) (layers F.Cu F.Paste F.Mask)
      (net 18 /4))
    (pad 8 smd rect (at -1 -1.225 90) (size 0.23 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-Pad8)"))
    (pad 9 smd rect (at -0.6 1.225 90) (size 0.23 0.75) (layers F.Cu F.Paste F.Mask)
      (net 19 /5))
    (pad 10 smd rect (at -0.6 -1.225 90) (size 0.23 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J1-Pad10)"))
    (pad 11 smd rect (at -0.2 1.225 90) (size 0.23 0.75) (layers F.Cu F.Paste F.Mask)
      (net 20 /6))
    (pad 12 smd rect (at -0.2 -1.225 90) (size 0.23 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J1-Pad12)"))
    (pad 13 smd rect (at 0.2 1.225 90) (size 0.23 0.75) (layers F.Cu F.Paste F.Mask)
      (net 21 /7))
    (pad 14 smd rect (at 0.2 -1.225 90) (size 0.23 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J1-Pad14)"))
    (pad 15 smd rect (at 0.6 1.225 90) (size 0.23 0.75) (layers F.Cu F.Paste F.Mask)
      (net 22 /8))
    (pad 16 smd rect (at 0.6 -1.225 90) (size 0.23 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J1-Pad16)"))
    (pad 17 smd rect (at 1 1.225 90) (size 0.23 0.75) (layers F.Cu F.Paste F.Mask)
      (net 23 /9))
    (pad 18 smd rect (at 1 -1.225 90) (size 0.23 0.75) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J1-Pad18)"))
    (pad 19 smd rect (at 1.4 1.225 90) (size 0.23 0.75) (layers F.Cu F.Paste F.Mask)
      (net 24 /10))
    (pad 20 smd rect (at 1.4 -1.225 90) (size 0.23 0.75) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J1-Pad20)"))
    (pad 21 smd rect (at 1.8 1.225 90) (size 0.23 0.75) (layers F.Cu F.Paste F.Mask)
      (net 26 /11))
    (pad 22 smd rect (at 1.8 -1.225 90) (size 0.23 0.75) (layers F.Cu F.Paste F.Mask)
      (net 25 /14))
    (pad 23 smd rect (at 2.2 1.225 90) (size 0.23 0.75) (layers F.Cu F.Paste F.Mask)
      (net 28 /12))
    (pad 24 smd rect (at 2.2 -1.225 90) (size 0.23 0.75) (layers F.Cu F.Paste F.Mask)
      (net 27 /13))
    (pad 25 smd rect (at -3 -0.703 90) (size 0.45 0.655) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J1-Pad25)"))
    (pad 26 smd rect (at -3 0.703 90) (size 0.45 0.655) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(J1-Pad26)"))
    (pad 27 smd rect (at 3 0.703 90) (size 0.45 0.655) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(J1-Pad27)"))
    (pad 28 smd rect (at 3 -0.703 90) (size 0.45 0.655) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(J1-Pad28)"))
  )
  (gr_text "H047-5004\nTester" (at 147.32 103.505) (layer B.SilkS))
  (gr_text "14\n13" (at 143.75 111.25 270) (layer B.SilkS))
  (gr_text AYF531465T (at 150.5 110.25) (layer B.SilkS))
  (gr_text "1\n2\n3\n4\n5\n6\n7\n8\n9\n10\n11\n12" (at 150.25 97.5 270) (layer B.SilkS))
  (dimension 16 (width 0.3) (layer Dwgs.User)
    (gr_text "16.000 mm" (at 150 118.35) (layer Dwgs.User))
    (feature1 (pts (xy 158 115) (xy 158 119.7)))
    (feature2 (pts (xy 142 115) (xy 142 119.7)))
    (crossbar (pts (xy 142 117) (xy 158 117)))
    (arrow1a (pts (xy 158 117) (xy 156.873496 117.586421)))
    (arrow1b (pts (xy 158 117) (xy 156.873496 116.413579)))
    (arrow2a (pts (xy 142 117) (xy 143.126504 117.586421)))
    (arrow2b (pts (xy 142 117) (xy 143.126504 116.413579)))
  )
  (gr_text AXT624124 (at 150 100.5) (layer F.SilkS))
  (gr_text "23\n21\n19\n17\n15\n13\n11\n9\n7\n5\n3\n1" (at 150 96.75 90) (layer F.SilkS))
  (gr_text "24\n22\n20\n18\n16\n14\n12\n10\n8\n6\n4\n2" (at 150 112.5 90) (layer F.SilkS))
  (dimension 21 (width 0.3) (layer Dwgs.User)
    (gr_text "21.000 mm" (at 164.35 104.5 270) (layer Dwgs.User))
    (feature1 (pts (xy 158 115) (xy 165.7 115)))
    (feature2 (pts (xy 158 94) (xy 165.7 94)))
    (crossbar (pts (xy 163 94) (xy 163 115)))
    (arrow1a (pts (xy 163 115) (xy 162.413579 113.873496)))
    (arrow1b (pts (xy 163 115) (xy 163.586421 113.873496)))
    (arrow2a (pts (xy 163 94) (xy 162.413579 95.126504)))
    (arrow2b (pts (xy 163 94) (xy 163.586421 95.126504)))
  )
  (gr_text 2 (at 148 109) (layer F.SilkS))
  (gr_text 1 (at 152 109) (layer F.SilkS))
  (gr_line (start 142 95) (end 142 114) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 157 94) (end 143 94) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 158 114) (end 158 95) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 143 115) (end 157 115) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 143 114) (end 143 115) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 143 95) (end 142 95) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 157 95) (end 157 94) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 157 114) (end 158 114) (angle 90) (layer Edge.Cuts) (width 0.15))
)
