<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="55.55" y2="0" width="0" layer="20"/>
<wire x1="55.55" y1="0" x2="55.55" y2="50.79" width="0" layer="20"/>
<wire x1="55.55" y1="50.79" x2="0" y2="50.79" width="0" layer="20"/>
<wire x1="0" y1="50.79" x2="0" y2="0" width="0" layer="20"/>
<hole x="2.54" y="48.26" drill="3.2"/>
<hole x="53.34" y="48.26" drill="3.2"/>
<hole x="53.34" y="2.54" drill="3.2"/>
<hole x="2.54" y="2.54" drill="3.2"/>
<text>NO</text>
<text>COM</text>
<text>NC</text>
<text>Fubar.gr</text>
<text>Green Button to SET
Red Button to RESET</text>
<text>+12V</text>
<text>GND</text>
<text>Soft-Latching Relay</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="DO41-10">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 2.54 mm, horizontal, grid 10.16 mm</description>
</package>
<package name="0207/9">
</package>
</packages>
</library>
<library name="con-wago-500">
<description>&lt;b&gt;Wago Screw Clamps&lt;/b&gt;&lt;p&gt;
Grid 5.00 mm&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="W237-102">
<description>&lt;b&gt;WAGO SCREW CLAMP&lt;/b&gt;</description>
</package>
<package name="W237-103">
<description>&lt;b&gt;WAGO SCREW CLAMP&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TO-92">
<description>&lt;b&gt;TO 92&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="custom">
<packages>
<package name="TO-92">
<description>&lt;b&gt;TO 92&lt;/b&gt;</description>
</package>
<package name="FINDER_41.52">
<description>Finder 41.52 series PCB relay</description>
</package>
<package name="FUBAR_LOGO">
</package>
</packages>
</library>
<library name="SparkFun-LED_Tactile_Button">
<description>Device for SparkFun Electronics' LED Tactile Button.
COM-10439, COM-10440, COM-10441, COM-10442, COM-10443</description>
<packages>
<package name="LED_TACTILE_BUTTON_SFE">
<description>&lt;h1&gt;LED Tactile Button&lt;/h1&gt;
&lt;p&gt;
Package for SparkFun Electronics' LED Tactile Button.
&lt;/p&gt;
&lt;p&gt;
Derived from BOB-10467 - LED Tactile Button Breakout.&lt;br /&gt;
Released under the Creative Commons Attribution Share-Alike 3.0 License&lt;br /&gt;
http://creativecommons.org/licenses/by-sa/3.0
&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="D1" library="adafruit" package="DO41-10" value="1N4004">
<attribute name="NAME"/>
</element>
<element name="D2" library="adafruit" package="DO41-10" value="1N4004">
<attribute name="NAME"/>
</element>
<element name="POWER" library="con-wago-500" package="W237-102" value="">
<attribute name="MPN" value="237-102"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="70K9898"/>
</element>
<element name="Q1" library="SparkFun-DiscreteSemi" package="TO-92" value="MOSFET-NCHANNEL2N7000">
<attribute name="NAME"/>
</element>
<element name="Q2" library="custom" package="TO-92" value="VP2106">
<attribute name="NAME"/>
</element>
<element name="R1" library="adafruit" package="0207/9" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="adafruit" package="0207/9" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="adafruit" package="0207/9" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RLY_CONTACT" library="con-wago-500" package="W237-103" value="">
<attribute name="MPN" value="237-103"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="18M7116"/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="RESET" library="SparkFun-LED_Tactile_Button" package="LED_TACTILE_BUTTON_SFE" value="LED_TACTILE_BUTTONSFE"/>
<element name="SET" library="SparkFun-LED_Tactile_Button" package="LED_TACTILE_BUTTON_SFE" value="LED_TACTILE_BUTTONSFE"/>
<element name="RLY1" library="custom" package="FINDER_41.52" value="FINDER_41.52"/>
<element name="U$1" library="custom" package="FUBAR_LOGO" value=""/>
</elements>
<signals>
<signal name="N$1">
<contactref element="POWER" pad="1"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="GND">
<contactref element="POWER" pad="2"/>
<contactref element="R1" pad="1"/>
<contactref element="Q1" pad="1"/>
<contactref element="R3" pad="2"/>
<contactref element="RESET" pad="1"/>
</signal>
<signal name="+12V">
<contactref element="D1" pad="C"/>
<contactref element="SET" pad="4"/>
<contactref element="RLY1" pad="9"/>
<contactref element="R2" pad="2"/>
<contactref element="Q2" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="R1" pad="2"/>
<contactref element="SET" pad="C"/>
</signal>
<signal name="COM_NODE">
<contactref element="SET" pad="2"/>
<contactref element="D2" pad="C"/>
<contactref element="Q2" pad="2"/>
<contactref element="RLY1" pad="11"/>
<contactref element="RLY1" pad="1"/>
<contactref element="SET" pad="A"/>
</signal>
<signal name="NC">
<contactref element="RLY1" pad="4"/>
<contactref element="RLY_CONTACT" pad="1"/>
</signal>
<signal name="NO">
<contactref element="RLY1" pad="8"/>
<contactref element="RLY_CONTACT" pad="3"/>
</signal>
<signal name="N$4">
<contactref element="Q1" pad="3"/>
<contactref element="D2" pad="A"/>
<contactref element="RLY1" pad="16"/>
</signal>
<signal name="N$5">
<contactref element="Q1" pad="2"/>
<contactref element="R2" pad="1"/>
<contactref element="RESET" pad="3"/>
</signal>
<signal name="N$2">
<contactref element="RESET" pad="C"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="MOSFET_DRAIN">
<contactref element="Q2" pad="3"/>
<contactref element="RESET" pad="A"/>
</signal>
<signal name="COM">
<contactref element="RLY_CONTACT" pad="2"/>
<contactref element="RLY1" pad="6"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
