(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "GerberSeed_PCBway_Funbox_v3p2/")
    )
  )
  (net 0 "")
  (net 1 "unconnected-(A1-USB_ID-Pad1)")
  (net 2 "DIP1")
  (net 3 "SW3_LEFT")
  (net 4 "DIP2")
  (net 5 "FOOT_SWITCH_2")
  (net 6 "FOOT_SWITCH_1")
  (net 7 "SW3_RIGHT")
  (net 8 "DIP3")
  (net 9 "SW2_LEFT")
  (net 10 "unconnected-(A1-I2C1_SCL-Pad12)")
  (net 11 "unconnected-(A1-SPI1_SCK-Pad9)")
  (net 12 "unconnected-(A1-I2C1_SDA-Pad13)")
  (net 13 "unconnected-(A1-SPI1_POCI-Pad10)")
  (net 14 "AUDIO_IN_BUFFER_LEFT")
  (net 15 "AUDIO_OUT_BUFFER_LEFT")
  (net 16 "GND")
  (net 17 "POT_1")
  (net 18 "POT_2")
  (net 19 "POT_3")
  (net 20 "POT_4")
  (net 21 "AUDIO_IN_BUFFER_RIGHT")
  (net 22 "AUDIO_OUT_BUFFER_RIGHT")
  (net 23 "LED_1")
  (net 24 "LED_2")
  (net 25 "unconnected-(A1-SAI2_MCLK-Pad31)")
  (net 26 "POT_5")
  (net 27 "unconnected-(A1-SAI2_FS-Pad34)")
  (net 28 "unconnected-(A1-SAI2_SCK-Pad35)")
  (net 29 "POT_6")
  (net 30 "MIDI_IN")
  (net 31 "Net-(In1-Pin_1)")
  (net 32 "Net-(C1-Pad2)")
  (net 33 "Net-(U1A-+)")
  (net 34 "Net-(U1B-+)")
  (net 35 "Net-(Out1-Pin_1)")
  (net 36 "Net-(U1B--)")
  (net 37 "Net-(9v1-Pin_1)")
  (net 38 "Net-(LED1-A)")
  (net 39 "Net-(LED2-A)")
  (net 40 "Net-(C5-Pad2)")
  (net 41 "SW2_RIGHT")
  (net 42 "3V3_D")
  (net 43 "VCC")
  (net 44 "5V")
  (net 45 "3V3_A")
  (net 46 "SW1_RIGHT")
  (net 47 "Net-(C12-Pad1)")
  (net 48 "DIP4")
  (net 49 "SW1_LEFT")
  (net 50 "Net-(In2-Pin_1)")
  (net 51 "Net-(C13-Pad1)")
  (net 52 "Net-(C14-Pad2)")
  (net 53 "Net-(U1D-+)")
  (net 54 "Net-(U1C-+)")
  (net 55 "Net-(Out2-Pin_1)")
  (net 56 "Net-(C17-Pad2)")
  (net 57 "Net-(U1D--)")
  (net 58 "Net-(D2-K)")
  (net 59 "MIDI_IN_JACK_PIN5")
  (net 60 "MIDI_IN_JACK_PIN4")
  (net 61 "unconnected-(U5-Pad3)")
  (net 62 "unconnected-(J6-PadR2)")
  (net 63 "unconnected-(J7-PadR2)")
  (net 64 "EXPRESSION_IN")
  (net 65 "unconnected-(A1-USB_D_--Pad36)")
  (net 66 "EXPRESSION_REF")
  (net 67 "EXPRESSION_IN_JACK")
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 132.055 66.375)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "Midi.kicad_sch")
    (property "Sheetname" "Midi and Expression")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R30" (at 3.7846 0.0254) (layer "F.Fab"))
    (fp_text value "220R" (at 3.9878 0.127) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 60 "MIDI_IN_JACK_PIN4") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 58 "Net-(D2-K)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Potentiometer_THT:Pot_RightAngle_LongPin_16mm" (layer "F.Cu")
    (at 168.2788 101.57 180)
    (property "Sheetfile" "funbox_v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Potentiometer, US symbol")
    (property "ki_keywords" "resistor variable")
    (attr through_hole)
    (fp_text reference "POT4" (at 0 -5.8 180 unlocked) (layer "F.Fab") hide)
    (fp_text value "10K" (at -0.25 -4.25 unlocked) (layer "B.SilkS"))
    (pad "1" thru_hole rect (at -5 -1.3 180) (size 2.75 2.75) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 16 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 -1.3 180) (size 2.75 2.75) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 20 "POT_4") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at 5 -1.3 180) (size 2.75 2.75) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 45 "3V3_A") (pinfunction "3") (pintype "passive"))
  )
  (footprint "TestPoint:TestPoint_THTPad_D2.0mm_Drill1.0mm" (layer "F.Cu")
    (at 174.75 66.15)
    (descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
    (tags "test point THT pad")
    (property "Sheetfile" "funbox_v2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr exclude_from_pos_files)
    (fp_text reference "OutR" (at 2.05 0.3 90) (layer "F.SilkS"))
    (fp_text value "~" (at 0 2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.05 0.25 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 55 "Net-(Out2-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "Capacitor_THT:C_Rect_L7.0mm_W6.0mm_P5.00mm" (layer "F.Cu")
    (at 145.161 89.448 -90)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*6mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 6mm Capacitor")
    (property "Sheetfile" "funbox_v2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C15" (at 2.5 0 -270) (layer "F.Fab"))
    (fp_text value "1UF" (at 2.627 0 -270) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 2.5 0 -270) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 51 "Net-(C13-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 53 "Net-(U1D-+)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L7.0mm_W6.0mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Potentiometer_THT:Pot_RightAngle_LongPin_16mm" (layer "F.Cu")
    (at 148.035 101.57 180)
    (property "Sheetfile" "funbox_v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Potentiometer, US symbol")
    (property "ki_keywords" "resistor variable")
    (attr through_hole)
    (fp_text reference "POT5" (at -0.047 -3.84 180 unlocked) (layer "F.Fab"))
    (fp_text value "10K" (at -0.174 -3.84 unlocked) (layer "B.SilkS"))
    (pad "1" thru_hole rect (at -5 -1.3 180) (size 2.75 2.75) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 16 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 -1.3 180) (size 2.75 2.75) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 26 "POT_5") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at 5 -1.3 180) (size 2.75 2.75) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 45 "3V3_A") (pinfunction "3") (pintype "passive"))
  )
  (footprint "Capacitor_THT:C_Rect_L7.0mm_W6.0mm_P5.00mm" (layer "F.Cu")
    (at 151.511 89.448 -90)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*6mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 6mm Capacitor")
    (property "Sheetfile" "funbox_v2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C4" (at 2.5 0 -270) (layer "F.Fab"))
    (fp_text value "1UF" (at 2.5 0 -270) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 2.5 0 -270) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 47 "Net-(C12-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 34 "Net-(U1B-+)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L7.0mm_W6.0mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Rect_L7.0mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (at 140.462 89.448 -90)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 2.5mm Capacitor")
    (property "Sheetfile" "funbox_v2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C13" (at 2.5 0 -270) (layer "F.Fab"))
    (fp_text value "2.2nF" (at 2.5 0 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 2.5 0 -270) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 51 "Net-(C13-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 16 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L7.0mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Potentiometer_THT:Pot_RightAngle_LongPin_16mm" (layer "F.Cu")
    (at 147.955 76.2 180)
    (property "Sheetfile" "funbox_v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Potentiometer, US symbol")
    (property "ki_keywords" "resistor variable")
    (attr through_hole)
    (fp_text reference "POT2" (at 0 -5.8 180 unlocked) (layer "F.Fab"))
    (fp_text value "10K" (at -0.25 -4.064 unlocked) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0.1 -4.15 180 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole rect (at -5 -1.3 180) (size 2.75 2.75) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 16 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 -1.3 180) (size 2.75 2.75) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 18 "POT_2") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at 5 -1.3 180) (size 2.75 2.75) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 45 "3V3_A") (pinfunction "3") (pintype "passive"))
  )
  (footprint "Potentiometer_THT:Pot_RightAngle_LongPin_16mm" (layer "F.Cu")
    (at 168.2788 76.17 180)
    (property "Sheetfile" "funbox_v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Potentiometer, US symbol")
    (property "ki_keywords" "resistor variable")
    (attr through_hole)
    (fp_text reference "POT1" (at 0 -5.8 180 unlocked) (layer "F.Fab"))
    (fp_text value "10K" (at 0.0038 -3.84 unlocked) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0.1 -4.15 180 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole rect (at -5 -1.3 180) (size 2.75 2.75) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 16 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 -1.3 180) (size 2.75 2.75) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 17 "POT_1") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at 5 -1.3 180) (size 2.75 2.75) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 45 "3V3_A") (pinfunction "3") (pintype "passive"))
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 138.925 68.99 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "Midi.kicad_sch")
    (property "Sheetname" "Midi and Expression")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R31" (at 4.2926 -0.1016 90) (layer "F.Fab"))
    (fp_text value "470R" (at 3.937 0.1524 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 45 "3V3_A") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 30 "MIDI_IN") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal" (layer "F.Cu")
    (at 136.175 68.965 -90)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (property "Sheetfile" "Midi.kicad_sch")
    (property "Sheetname" "Midi and Expression")
    (property "ki_description" "100V 0.15A standard switching diode, DO-35")
    (property "ki_keywords" "diode")
    (attr through_hole)
    (fp_text reference "D2" (at 3.81 -2.12 90) (layer "F.Fab"))
    (fp_text value "1N4148" (at 3.937 0.127 90) (layer "F.SilkS"))
    (fp_text user "K" (at 0 -1.8 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 4.11 0 90) (layer "F.Fab"))
    (fp_text user "K" (at 0 -1.8 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 58 "Net-(D2-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 59 "MIDI_IN_JACK_PIN5") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Audio_Module:TRRS-PJ-320A" (layer "F.Cu")
    (at 176.35 71.2 -90)
    (property "Sheetfile" "funbox_v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Audio Jack, 4 Poles (TRRS)")
    (property "ki_keywords" "audio jack receptacle stereo headphones TRRS connector")
    (attr through_hole)
    (fp_text reference "J7" (at 0 14.2 90) (layer "Dwgs.User"))
    (fp_text value "EXPRESSION" (at -1.6 4.9378 180) (layer "F.SilkS"))
    (fp_text user "Ring1" (at 0 6.25 90) (layer "F.Fab"))
    (fp_text user "Ring2" (at 0 3.25 90) (layer "F.Fab"))
    (fp_text user "Tip" (at 0 10 90) (layer "F.Fab"))
    (fp_text user "Sleeve" (at 0.25 11.4 90) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 1.6 270) (size 0.8 0.8) (drill 0.8) (layers "*.Cu" "*.Mask"))
    (pad "" np_thru_hole circle (at 0 8.6 270) (size 0.8 0.8) (drill 0.8) (layers "*.Cu" "*.Mask"))
    (pad "R1" thru_hole oval (at 2.3 6.2 270) (size 1.6 2) (drill oval 0.9 1.3) (layers "*.Cu" "*.Mask")
      (net 66 "EXPRESSION_REF") (pintype "passive"))
    (pad "R2" thru_hole oval (at 2.3 3.2 270) (size 1.6 2) (drill oval 0.9 1.3) (layers "*.Cu" "*.Mask")
      (net 63 "unconnected-(J7-PadR2)") (pintype "passive+no_connect"))
    (pad "S" thru_hole oval (at -2.3 11.3 270) (size 1.6 2) (drill oval 0.9 1.3) (layers "*.Cu" "*.Mask")
      (net 16 "GND") (pintype "passive"))
    (pad "T" thru_hole oval (at 2.3 10.2 270) (size 1.6 2) (drill oval 0.9 1.3) (layers "*.Cu" "*.Mask")
      (net 67 "EXPRESSION_IN_JACK") (pintype "passive"))
    (model "/Users/danny/syncproj/kicad-libs/footprints/Keebio-Parts.pretty/3dmodels/PJ-320A.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 180))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 134.239 86.487)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "funbox_v2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R12" (at 4.064 -0.127) (layer "F.Fab"))
    (fp_text value "1K" (at 4.073 -0.127) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 4.073 -0.17) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 52 "Net-(C14-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 54 "Net-(U1C-+)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-220-3_Vertical" (layer "F.Cu")
    (at 137.922 111.252 90)
    (descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (property "Sheetfile" "funbox_v2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Positive 1.5A 35V Linear Regulator, Fixed Output 5V, TO-220/TO-263/TO-252")
    (property "ki_keywords" "Voltage Regulator 1.5A Positive")
    (attr through_hole)
    (fp_text reference "U2" (at 2.5146 -1.8034 90) (layer "F.Fab"))
    (fp_text value "L7805" (at 2.54 2.159 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 2.477 -1.922 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.905 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 43 "VCC") (pinfunction "IN") (pintype "power_in"))
    (pad "2" thru_hole oval (at 2.54 0 90) (size 1.905 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 16 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "3" thru_hole oval (at 5.08 0 90) (size 1.905 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 44 "5V") (pinfunction "OUT") (pintype "power_out"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_THT:SW_Toggle_SPDT_lugs" (layer "F.Cu")
    (at 168.275 108.712 180)
    (descr "SW Toggle")
    (tags "SW Toggle")
    (property "Sheetfile" "funbox_v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Switch, single pole double throw")
    (property "ki_keywords" "switch single-pole double-throw spdt ON-ON")
    (attr through_hole)
    (fp_text reference "SW1" (at 0.124031 -8.249895) (layer "F.SilkS") hide)
    (fp_text value "SW_SPDT" (at 0 -6.35) (layer "F.Fab") hide)
    (pad "1" thru_hole oval (at -4.6736 0 180) (size 2.1 3.5) (drill oval 1 2.3) (layers "*.Cu" "*.Mask")
      (net 46 "SW1_RIGHT") (pinfunction "A") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 0 180) (size 2.1 3.5) (drill oval 1 2.3) (layers "*.Cu" "*.Mask")
      (net 16 "GND") (pinfunction "B") (pintype "passive"))
    (pad "3" thru_hole oval (at 4.7244 0 180) (size 2.1 3.5) (drill oval 1 2.3) (layers "*.Cu" "*.Mask")
      (net 49 "SW1_LEFT") (pinfunction "C") (pintype "passive"))
    (model "${KICAD_USER_3DMOD}/Toggle_SW_Blue_R0.step"
      (offset (xyz -6.5 4 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (footprint "Capacitor_THT:C_Rect_L7.0mm_W6.0mm_P5.00mm" (layer "F.Cu")
    (at 173.8122 89.6766 -90)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*6mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 6mm Capacitor")
    (property "Sheetfile" "funbox_v2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C5" (at 2.5 0 90) (layer "F.Fab"))
    (fp_text value "1UF" (at 2.5 0 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 35 "Net-(Out1-Pin_1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 40 "Net-(C5-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L7.0mm_W6.0mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_THTPad_D2.0mm_Drill1.0mm" (layer "F.Cu")
    (at 128.725 66.1)
    (descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
    (tags "test point THT pad")
    (property "Sheetfile" "funbox_v2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr exclude_from_pos_files)
    (fp_text reference "InG" (at 2.075 -1.05) (layer "F.SilkS"))
    (fp_text value "~" (at 0 2.05) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 2.075 -1.075) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 16 "GND") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 163.449 124.079 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "funbox_v2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R6" (at 4.064 0.127 90) (layer "F.Fab"))
    (fp_text value "1M" (at 3.937 0.127 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 34 "Net-(U1B-+)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 16 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Rect_L7.0mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (at 121.96 113.411)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 2.5mm Capacitor")
    (property "Sheetfile" "funbox_v2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C8" (at 2.5 0) (layer "F.Fab"))
    (fp_text value "100NF" (at 2.5 0.127) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 16 "GND") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 43 "VCC") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L7.0mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Rect_L7.0mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (at 139.025 126.875 180)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 2.5mm Capacitor")
    (property "Sheetfile" "funbox_v2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C9" (at 2.627 0) (layer "F.Fab"))
    (fp_text value "100NF" (at 2.5 0.127) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 16 "GND") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 44 "5V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L7.0mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Rect_L7.0mm_W6.0mm_P5.00mm" (layer "F.Cu")
    (at 133.096 89.448 -90)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*6mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 6mm Capacitor")
    (property "Sheetfile" "funbox_v2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C14" (at 2.627 0 90) (layer "F.Fab"))
    (fp_text value "1UF" (at 2.627 -0.127 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 50 "Net-(In2-Pin_1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 52 "Net-(C14-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L7.0mm_W6.0mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D8.0mm_P3.50mm" (layer "F.Cu")
    (at 130.875 122 90)
    (descr "CP, Radial series, Radial, pin pitch=3.50mm, , diameter=8mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 3.50mm  diameter 8mm Electrolytic Capacitor")
    (property "Sheetfile" "funbox_v2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C6" (at 1.779651 -1.905 90) (layer "F.Fab"))
    (fp_text value "100UF" (at 1.906651 2.159 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 1.75 -1.905 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 16 "GND") (pintype "passive"))
    (pad "2" thru_hole circle (at 3.5 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 43 "VCC") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D8.0mm_P3.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_THTPad_D2.0mm_Drill1.0mm" (layer "F.Cu")
    (at 121.3 66.1)
    (descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
    (tags "test point THT pad")
    (property "Sheetfile" "funbox_v2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr exclude_from_pos_files)
    (fp_text reference "InL" (at -2.25 -0.15 90) (layer "F.SilkS"))
    (fp_text value "~" (at 0 2.05) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at -2.25 -0.15 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 31 "Net-(In1-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 154.015 129.9)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "funbox_v2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R5" (at 3.81 0) (layer "F.Fab"))
    (fp_text value "1M" (at 3.81 0) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 44 "5V") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 34 "Net-(U1B-+)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Rect_L7.0mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (at 137.414 89.448 -90)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 2.5mm Capacitor")
    (property "Sheetfile" "funbox_v2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C11" (at 2.373 0 90) (layer "F.Fab"))
    (fp_text value "100pF" (at 2.373 0.127 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 50 "Net-(In2-Pin_1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 16 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L7.0mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_THTPad_D2.0mm_Drill1.0mm" (layer "F.Cu")
    (at 125.05 66.1)
    (descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
    (tags "test point THT pad")
    (property "Sheetfile" "funbox_v2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr exclude_from_pos_files)
    (fp_text reference "InR" (at -1.95 -0.175 90) (layer "F.SilkS"))
    (fp_text value "~" (at -27.559 1.161) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at -1.925 -0.15 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 50 "Net-(In2-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 166.497 124.079 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "funbox_v2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R16" (at 4.073 -0.254 90) (layer "F.Fab"))
    (fp_text value "1M" (at 3.81 -0.127 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 4.073 -0.17 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 54 "Net-(U1C-+)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 16 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_THTPad_D2.0mm_Drill1.0mm" (layer "F.Cu")
    (at 166.9 66.1)
    (descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
    (tags "test point THT pad")
    (property "Sheetfile" "funbox_v2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr exclude_from_pos_files)
    (fp_text reference "OutG" (at -1.9 -0.5 90) (layer "F.SilkS"))
    (fp_text value "~" (at 0 2.05) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at -1.9 -0.475 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 16 "GND") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "Button_Switch_THT:SW_Toggle_SPDT_lugs" (layer "F.Cu")
    (at 148.082 108.839 180)
    (descr "SW Toggle")
    (tags "SW Toggle")
    (property "Sheetfile" "funbox_v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Switch, single pole double throw")
    (property "ki_keywords" "switch single-pole double-throw spdt ON-ON")
    (attr through_hole)
    (fp_text reference "SW2" (at 0.124031 -8.249895) (layer "F.SilkS") hide)
    (fp_text value "SW_SPDT" (at 0 -6.35) (layer "F.Fab") hide)
    (pad "1" thru_hole oval (at -4.6736 0 180) (size 2.1 3.5) (drill oval 1 2.3) (layers "*.Cu" "*.Mask")
      (net 41 "SW2_RIGHT") (pinfunction "A") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 0 180) (size 2.1 3.5) (drill oval 1 2.3) (layers "*.Cu" "*.Mask")
      (net 16 "GND") (pinfunction "B") (pintype "passive"))
    (pad "3" thru_hole oval (at 4.7244 0 180) (size 2.1 3.5) (drill oval 1 2.3) (layers "*.Cu" "*.Mask")
      (net 9 "SW2_LEFT") (pinfunction "C") (pintype "passive"))
    (model "${KICAD_USER_3DMOD}/Toggle_SW_Blue_R0.step"
      (offset (xyz -6.5 4 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (at 130.942 129.794 -90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "funbox_v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (attr through_hole)
    (fp_text reference "LED2" (at 0.106 4.392 -90) (layer "F.SilkS"))
    (fp_text value "LED_2" (at 1.27 -5.715 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0.106 4.342 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 16 "GND") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 39 "Net-(LED2-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 143.865 129.9)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "funbox_v2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R1" (at 3.683 0) (layer "F.Fab"))
    (fp_text value "1M" (at 3.81 0) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 33 "Net-(U1A-+)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 16 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D6.0mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (at 133.425 68.925 -90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=6*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 6mm width 2.5mm Capacitor")
    (property "Sheetfile" "Midi.kicad_sch")
    (property "Sheetname" "Midi and Expression")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C30" (at 2.5654 -0.0254 -270) (layer "F.Fab"))
    (fp_text value "100NF" (at 2.534 0.0508 -270) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 2.5 0 -270) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 45 "3V3_A") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 16 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D6.0mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 160.401 124.079 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "funbox_v2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R4" (at 3.683 0 90) (layer "F.Fab"))
    (fp_text value "100" (at 3.937 0 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 36 "Net-(U1B--)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 40 "Net-(C5-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (at 167.4926 129.794 -90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "funbox_v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (attr through_hole)
    (fp_text reference "LED1" (at -1.905 0.9956 -180) (layer "F.SilkS"))
    (fp_text value "LED_1" (at 0 4.87 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at -1.905 1.1226) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 16 "GND") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 38 "Net-(LED1-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Rect_L7.0mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (at 169.545 119.039 -90)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 2.5mm Capacitor")
    (property "Sheetfile" "funbox_v2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C16" (at 2.373 0 90) (layer "F.Fab"))
    (fp_text value "1NF" (at 2.246 0 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 16 "GND") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 54 "Net-(U1C-+)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L7.0mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 161.417 94.488)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "funbox_v2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R11" (at 3.937 -0.127) (layer "F.Fab"))
    (fp_text value "3K3" (at 3.937 0) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 15 "AUDIO_OUT_BUFFER_LEFT") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 47 "Net-(C12-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DIP:DIP-14_W7.62mm" (layer "F.Cu")
    (at 138.953 124.069 90)
    (descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (property "Sheetfile" "funbox_v2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Quad Low-Noise JFET-Input Operational Amplifiers, DIP-14/SOIC-14")
    (property "ki_keywords" "quad opamp")
    (attr through_hole)
    (fp_text reference "U1" (at 4.054 2.144 90) (layer "F.Fab"))
    (fp_text value "MCP6024" (at 3.546 7.986 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.81 7.62 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 14 "AUDIO_IN_BUFFER_LEFT") (pintype "output"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 14 "AUDIO_IN_BUFFER_LEFT") (pinfunction "-") (pintype "input"))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 33 "Net-(U1A-+)") (pinfunction "+") (pintype "input"))
    (pad "4" thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 44 "5V") (pinfunction "V+") (pintype "power_in"))
    (pad "5" thru_hole oval (at 0 10.16 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 34 "Net-(U1B-+)") (pinfunction "+") (pintype "input"))
    (pad "6" thru_hole oval (at 0 12.7 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 36 "Net-(U1B--)") (pinfunction "-") (pintype "input"))
    (pad "7" thru_hole oval (at 0 15.24 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 36 "Net-(U1B--)") (pintype "output"))
    (pad "8" thru_hole oval (at 7.62 15.24 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 21 "AUDIO_IN_BUFFER_RIGHT") (pintype "output"))
    (pad "9" thru_hole oval (at 7.62 12.7 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 21 "AUDIO_IN_BUFFER_RIGHT") (pinfunction "-") (pintype "input"))
    (pad "10" thru_hole oval (at 7.62 10.16 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 54 "Net-(U1C-+)") (pinfunction "+") (pintype "input"))
    (pad "11" thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 16 "GND") (pinfunction "V-") (pintype "power_in"))
    (pad "12" thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 53 "Net-(U1D-+)") (pinfunction "+") (pintype "input"))
    (pad "13" thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 57 "Net-(U1D--)") (pinfunction "-") (pintype "input"))
    (pad "14" thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 57 "Net-(U1D--)") (pintype "output"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-14_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_THTPad_D2.0mm_Drill1.0mm" (layer "F.Cu")
    (at 170.625 66.175)
    (descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
    (tags "test point THT pad")
    (property "Sheetfile" "funbox_v2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr exclude_from_pos_files)
    (fp_text reference "OutL" (at 2 0 90) (layer "F.SilkS"))
    (fp_text value "~" (at 0 2.05) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 2.05 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 35 "Net-(Out1-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "TestPoint:TestPoint_THTPad_D2.0mm_Drill1.0mm" (layer "F.Cu")
    (at 144.25 66)
    (descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
    (tags "test point THT pad")
    (property "Sheetfile" "funbox_v2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr exclude_from_pos_files)
    (fp_text reference "9v" (at -1.95 -0.825) (layer "F.SilkS"))
    (fp_text value "~" (at 0 2.05) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at -2 -0.85) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 37 "Net-(9v1-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "Module:Electrosmith_Daisy_Seed" (layer "F.Cu")
    (at 123.7996 97.79 90)
    (descr "Embedded platform for audio applications. 96kHz / 24-bit audio hardware. 64MB of SDRAM for up to 10 minute long audio. ARM Cortex-M7 MCU, running at 480MHz. 31 total GPIO pins with configurable functionality. 12-bit Digital to Analog Converters (x2). SD card interfaces. PWM outputs. Serial Protocols for connecting external sensors and devices (SPI, UART, I2S, I2C). Dedicated VIN pin for power. Micro USB port, and additional USB pins for full OTG-support as host and device. https://static1.squarespace.com/static/58d03fdc1b10e3bf442567b8/t/6227e6236f02fb68d1577146/1646781988478/Daisy_Seed_datasheet_v1.0.3.pdf")
    (tags "Electrosmith Daisy Seed Microcontroller Module ARM Cortex-M7 Audio Codec")
    (property "Sheetfile" "funbox_v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Daisy is an embedded platform for music.")
    (property "ki_keywords" "Electrosmith Daisy Seed Microcontroller Module ARM Cortex-M7")
    (attr through_hole)
    (fp_text reference "A1" (at 2.4892 -0.3302 90) (layer "F.SilkS"))
    (fp_text value "Electrosmith_Daisy_Seed_Rev7" (at 7.62 51 90) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 1 "unconnected-(A1-USB_ID-Pad1)") (pinfunction "USB_ID") (pintype "bidirectional+no_connect"))
    (pad "2" thru_hole circle (at 0 2.54 90) (size 1.7 1.7) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 2 "DIP1") (pinfunction "SD_DATA_3") (pintype "bidirectional"))
    (pad "3" thru_hole circle (at 0 5.08 90) (size 1.7 1.7) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 3 "SW3_LEFT") (pinfunction "SD_DATA_2") (pintype "bidirectional"))
    (pad "4" thru_hole circle (at 0 7.62 90) (size 1.7 1.7) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 4 "DIP2") (pinfunction "SD_DATA_1") (pintype "bidirectional"))
    (pad "5" thru_hole circle (at 0 10.16 90) (size 1.7 1.7) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 7 "SW3_RIGHT") (pinfunction "SD_DATA_0") (pintype "bidirectional"))
    (pad "6" thru_hole circle (at 0 12.7 90) (size 1.7 1.7) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 8 "DIP3") (pinfunction "SD_CMD") (pintype "bidirectional"))
    (pad "7" thru_hole circle (at 0 15.24 90) (size 1.7 1.7) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 48 "DIP4") (pinfunction "SD_CLK") (pintype "bidirectional"))
    (pad "8" thru_hole circle (at 0 17.78 90) (size 1.7 1.7) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 9 "SW2_LEFT") (pinfunction "SPI1_CS") (pintype "bidirectional"))
    (pad "9" thru_hole circle (at 0 20.32 90) (size 1.7 1.7) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 11 "unconnected-(A1-SPI1_SCK-Pad9)") (pinfunction "SPI1_SCK") (pintype "bidirectional+no_connect"))
    (pad "10" thru_hole circle (at 0 22.86 90) (size 1.7 1.7) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 13 "unconnected-(A1-SPI1_POCI-Pad10)") (pinfunction "SPI1_POCI") (pintype "bidirectional+no_connect"))
    (pad "11" thru_hole circle (at 0 25.4 90) (size 1.7 1.7) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 41 "SW2_RIGHT") (pinfunction "SPI1_PICO") (pintype "bidirectional"))
    (pad "12" thru_hole circle (at 0 27.94 90) (size 1.7 1.7) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 10 "unconnected-(A1-I2C1_SCL-Pad12)") (pinfunction "I2C1_SCL") (pintype "bidirectional+no_connect"))
    (pad "13" thru_hole circle (at 0 30.48 90) (size 1.7 1.7) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 12 "unconnected-(A1-I2C1_SDA-Pad13)") (pinfunction "I2C1_SDA") (pintype "bidirectional+no_connect"))
    (pad "14" thru_hole circle (at 0 33.02 90) (size 1.7 1.7) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 46 "SW1_RIGHT") (pinfunction "USART1_TX") (pintype "bidirectional"))
    (pad "15" thru_hole circle (at 0 35.56 90) (size 1.7 1.7) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 49 "SW1_LEFT") (pinfunction "USART1_RX") (pintype "bidirectional"))
    (pad "16" thru_hole circle (at 0 38.1 90) (size 1.7 1.7) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 14 "AUDIO_IN_BUFFER_LEFT") (pinfunction "AUDIO_IN_1") (pintype "input"))
    (pad "17" thru_hole circle (at 0 40.64 90) (size 1.7 1.7) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 21 "AUDIO_IN_BUFFER_RIGHT") (pinfunction "AUDIO_IN_2") (pintype "input"))
    (pad "18" thru_hole circle (at 0 43.18 90) (size 1.7 1.7) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 15 "AUDIO_OUT_BUFFER_LEFT") (pinfunction "AUDIO_OUT_1") (pintype "output"))
    (pad "19" thru_hole circle (at 0 45.72 90) (size 1.7 1.7) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 22 "AUDIO_OUT_BUFFER_RIGHT") (pinfunction "AUDIO_OUT_2") (pintype "output"))
    (pad "20" thru_hole circle (at 0 48.26 90) (size 1.7 1.7) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 16 "GND") (pinfunction "AGND") (pintype "power_in"))
    (pad "21" thru_hole circle (at 15.24 48.26 90) (size 1.7 1.7) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 45 "3V3_A") (pinfunction "3V3_A") (pintype "power_out"))
    (pad "22" thru_hole circle (at 15.24 45.72 90) (size 1.7 1.7) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 64 "EXPRESSION_IN") (pinfunction "ADC_0") (pintype "bidirectional"))
    (pad "23" thru_hole circle (at 15.24 43.18 90) (size 1.7 1.7) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 17 "POT_1") (pinfunction "ADC_1") (pintype "bidirectional"))
    (pad "24" thru_hole circle (at 15.24 40.64 90) (size 1.7 1.7) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 18 "POT_2") (pinfunction "ADC_2") (pintype "bidirectional"))
    (pad "25" thru_hole circle (at 15.24 38.1 90) (size 1.7 1.7) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 19 "POT_3") (pinfunction "ADC_3") (pintype "bidirectional"))
    (pad "26" thru_hole circle (at 15.24 35.56 90) (size 1.7 1.7) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 20 "POT_4") (pinfunction "ADC_4") (pintype "bidirectional"))
    (pad "27" thru_hole circle (at 15.24 33.02 90) (size 1.7 1.7) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 26 "POT_5") (pinfunction "ADC_5") (pintype "bidirectional"))
    (pad "28" thru_hole circle (at 15.24 30.48 90) (size 1.7 1.7) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 29 "POT_6") (pinfunction "ADC_6") (pintype "bidirectional"))
    (pad "29" thru_hole circle (at 15.24 27.94 90) (size 1.7 1.7) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 23 "LED_1") (pinfunction "DAC_OUT2") (pintype "bidirectional"))
    (pad "30" thru_hole circle (at 15.24 25.4 90) (size 1.7 1.7) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 24 "LED_2") (pinfunction "DAC_OUT1") (pintype "bidirectional"))
    (pad "31" thru_hole circle (at 15.24 22.86 90) (size 1.7 1.7) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 25 "unconnected-(A1-SAI2_MCLK-Pad31)") (pinfunction "SAI2_MCLK") (pintype "bidirectional+no_connect"))
    (pad "32" thru_hole circle (at 15.24 20.32 90) (size 1.7 1.7) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 6 "FOOT_SWITCH_1") (pinfunction "SAI2_SD_B") (pintype "bidirectional"))
    (pad "33" thru_hole circle (at 15.24 17.78 90) (size 1.7 1.7) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 5 "FOOT_SWITCH_2") (pinfunction "SAI2_SD_A") (pintype "bidirectional"))
    (pad "34" thru_hole circle (at 15.24 15.24 90) (size 1.7 1.7) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 27 "unconnected-(A1-SAI2_FS-Pad34)") (pinfunction "SAI2_FS") (pintype "bidirectional+no_connect"))
    (pad "35" thru_hole circle (at 15.24 12.7 90) (size 1.7 1.7) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 28 "unconnected-(A1-SAI2_SCK-Pad35)") (pinfunction "SAI2_SCK") (pintype "bidirectional+no_connect"))
    (pad "36" thru_hole circle (at 15.24 10.16 90) (size 1.7 1.7) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 65 "unconnected-(A1-USB_D_--Pad36)") (pinfunction "USB_D_-") (pintype "bidirectional+no_connect"))
    (pad "37" thru_hole circle (at 15.24 7.62 90) (size 1.7 1.7) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 30 "MIDI_IN") (pinfunction "USB_D_+") (pintype "bidirectional"))
    (pad "38" thru_hole circle (at 15.24 5.08 90) (size 1.7 1.7) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 42 "3V3_D") (pinfunction "3V3_D") (pintype "power_out"))
    (pad "39" thru_hole circle (at 15.24 2.54 90) (size 1.7 1.7) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 43 "VCC") (pinfunction "VIN") (pintype "power_in"))
    (pad "40" thru_hole circle (at 15.24 0 90) (size 1.7 1.7) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 16 "GND") (pinfunction "DGND") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Module.3dshapes/Electrosmith_Daisy_Seed.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 154.94 126.873)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "funbox_v2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R15" (at 4.064 -0.127) (layer "F.Fab"))
    (fp_text value "1M" (at 4.064 -0.127) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 4.073 -0.17) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 44 "5V") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 54 "Net-(U1C-+)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Rect_L7.0mm_W6.0mm_P5.00mm" (layer "F.Cu")
    (at 157.353 89.448 -90)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*6mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 6mm Capacitor")
    (property "Sheetfile" "funbox_v2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C17" (at 2.5 0 -270) (layer "F.Fab"))
    (fp_text value "1UF" (at 2.5 0 -270) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 2.5 0 -270) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 55 "Net-(Out2-Pin_1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 56 "Net-(C17-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L7.0mm_W6.0mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-41_SOD81_P7.62mm_Horizontal" (layer "F.Cu")
    (at 124.079 86.487)
    (descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 7.62mm  length 5.2mm diameter 2.7mm")
    (property "Sheetfile" "funbox_v2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "20V 1A Schottky Barrier Rectifier Diode, DO-41")
    (property "ki_keywords" "diode Schottky")
    (attr through_hole)
    (fp_text reference "D1" (at 4.191 0) (layer "F.Fab"))
    (fp_text value "1N5817" (at 3.81 0) (layer "F.SilkS"))
    (fp_text user "K" (at 0 -2.1) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 4.2 0) (layer "F.Fab"))
    (fp_text user "K" (at 0 -2.1) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 2.2 2.2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 43 "VCC") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 2.2 2.2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 37 "Net-(9v1-Pin_1)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-41_SOD81_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DIP:DIP-8_W7.62mm" (layer "F.Cu")
    (at 152.85 74 90)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (property "Sheetfile" "Midi.kicad_sch")
    (property "Sheetname" "Midi and Expression")
    (property "ki_description" "1MHz, Low-Power Op Amp, DIP-8")
    (property "ki_keywords" "dual opamp")
    (attr through_hole)
    (fp_text reference "U3" (at 3.725 3.8 90) (layer "F.Fab"))
    (fp_text value "MCP6002" (at 3.675 4.15 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.81 3.81 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 66 "EXPRESSION_REF") (pintype "output"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 66 "EXPRESSION_REF") (pinfunction "-") (pintype "input"))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 45 "3V3_A") (pinfunction "+") (pintype "input"))
    (pad "4" thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 16 "GND") (pinfunction "V-") (pintype "power_in"))
    (pad "5" thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 67 "EXPRESSION_IN_JACK") (pinfunction "+") (pintype "input"))
    (pad "6" thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 64 "EXPRESSION_IN") (pinfunction "-") (pintype "input"))
    (pad "7" thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 64 "EXPRESSION_IN") (pintype "output"))
    (pad "8" thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 44 "5V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-8_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Potentiometer_THT:Pot_RightAngle_LongPin_16mm" (layer "F.Cu")
    (at 127.588 76.17 180)
    (property "Sheetfile" "funbox_v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Potentiometer, US symbol")
    (property "ki_keywords" "resistor variable")
    (attr through_hole)
    (fp_text reference "POT3" (at 0 -5.8 180 unlocked) (layer "F.Fab"))
    (fp_text value "10K" (at -0.25 -4.094 unlocked) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0.1 -4.15 180 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole rect (at -5 -1.3 180) (size 2.75 2.75) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 16 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 -1.3 180) (size 2.75 2.75) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 19 "POT_3") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at 5 -1.3 180) (size 2.75 2.75) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 45 "3V3_A") (pinfunction "3") (pintype "passive"))
  )
  (footprint "Button_Switch_THT:DS03-254-04BE-dip4" (layer "F.Cu")
    (at 123.81 116.97)
    (descr "2x-dip-switch SPST CTS_Series194-2MSTN, Piano, row spacing 7.62 mm (300 mils), body size  (see https://www.ctscorp.com/wp-content/uploads/194-195.pdf)")
    (tags "DIP Switch SPST Piano 7.62mm 300mil")
    (property "MANUFACTURER" "CUI Inc.")
    (property "MAXIMUM_PACKAGE_HEIGHT" "9.93 mm")
    (property "PARTREV" "V1.0")
    (property "STANDARD" "Manufacturer Recommendations")
    (property "Sheetfile" "funbox_v3.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "S1" (at -1.701 4.383 90) (layer "F.SilkS"))
    (fp_text value "DS03-254-04BE" (at -3.051 4.033 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at -1.905 4.572 90) (layer "F.Fab"))
    (pad "1A" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "DIP1") (pintype "passive"))
    (pad "1B" thru_hole oval (at 2.54 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 16 "GND") (pintype "passive"))
    (pad "2A" thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 4 "DIP2") (pintype "passive"))
    (pad "2B" thru_hole oval (at 2.54 2.54) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 16 "GND") (pintype "passive"))
    (pad "3A" thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 8 "DIP3") (pintype "passive"))
    (pad "3B" thru_hole oval (at 2.54 5.08) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 16 "GND") (pintype "passive"))
    (pad "4A" thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 48 "DIP4") (pintype "passive"))
    (pad "4B" thru_hole oval (at 2.54 7.62) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 16 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_DIP_SPSTx02_Piano_CTS_Series194-2MSTN_W7.62mm_P2.54mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 175.641 124.206 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "funbox_v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R8" (at 3.81 0 90) (layer "F.Fab"))
    (fp_text value "1K" (at 3.81 0 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 38 "Net-(LED1-A)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 23 "LED_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Rect_L7.0mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (at 169.378 86.487 180)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 2.5mm Capacitor")
    (property "Sheetfile" "funbox_v2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C12" (at 2.5 0) (layer "F.Fab"))
    (fp_text value "2.2nF" (at 1.992 0.127) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 47 "Net-(C12-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 16 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L7.0mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Rect_L7.0mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (at 129.707 113.411)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 2.5mm Capacitor")
    (property "Sheetfile" "funbox_v2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C7" (at 2.5 0) (layer "F.Fab"))
    (fp_text value "100NF" (at 2.5 0.127) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 16 "GND") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 43 "VCC") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L7.0mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 148.16 113.85 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "funbox_v2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R13" (at 4.073 -0.127) (layer "F.Fab"))
    (fp_text value "1M" (at 3.937 0) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 4.073 -0.17) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 44 "5V") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 53 "Net-(U1D-+)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Potentiometer_THT:Pot_RightAngle_LongPin_16mm" (layer "F.Cu")
    (at 127.6604 101.57 180)
    (property "Sheetfile" "funbox_v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Potentiometer, US symbol")
    (property "ki_keywords" "resistor variable")
    (attr through_hole)
    (fp_text reference "POT6" (at -0.1016 -3.84 180 unlocked) (layer "F.Fab"))
    (fp_text value "10K" (at -0.1016 -3.84 unlocked) (layer "B.SilkS"))
    (pad "1" thru_hole rect (at -5 -1.3 180) (size 2.75 2.75) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 16 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 -1.3 180) (size 2.75 2.75) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 29 "POT_6") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at 5 -1.3 180) (size 2.75 2.75) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 45 "3V3_A") (pinfunction "3") (pintype "passive"))
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 161.417 89.535)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "funbox_v2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R18" (at 4.064 -0.127) (layer "F.Fab"))
    (fp_text value "100K" (at 3.81 -0.127) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 4.073 -0.17) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 16 "GND") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 55 "Net-(Out2-Pin_1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (at 171.525 129.8 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "funbox_v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Push button switch, generic, two pins")
    (property "ki_keywords" "switch normally-open pushbutton push-button")
    (attr through_hole)
    (fp_text reference "FS1" (at 2.032 1.402 180) (layer "F.SilkS"))
    (fp_text value "Foot_Switch_1" (at 0 4.87 180) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 2.032 1.402) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 16 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 6 "FOOT_SWITCH_1") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 151.765 86.487 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "funbox_v2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R14" (at 3.937 -0.127) (layer "F.Fab"))
    (fp_text value "1M" (at 4.073 -0.127) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 4.073 -0.17) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 53 "Net-(U1D-+)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 16 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Rect_L7.0mm_W6.0mm_P5.00mm" (layer "F.Cu")
    (at 127.254 94.448 90)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*6mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 6mm Capacitor")
    (property "Sheetfile" "funbox_v2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C1" (at 2.373 -0.127 90) (layer "F.Fab"))
    (fp_text value "1UF" (at 2.5 0 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 31 "Net-(In1-Pin_1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 32 "Net-(C1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L7.0mm_W6.0mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Rect_L7.0mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (at 146.699 126.85 180)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 2.5mm Capacitor")
    (property "Sheetfile" "funbox_v2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C3" (at 2.627 0.127) (layer "F.Fab"))
    (fp_text value "1NF" (at 2.5 0.127) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 2.627 0.127) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 16 "GND") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 33 "Net-(U1A-+)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L7.0mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 135.89 116.459 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "funbox_v2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R3" (at 3.81 -0.127 90) (layer "F.Fab"))
    (fp_text value "1K" (at 3.81 0 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 32 "Net-(C1-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 33 "Net-(U1A-+)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Audio_Module:TRRS-PJ-320A" (layer "F.Cu")
    (at 119.6 71.1708 90)
    (property "Sheetfile" "funbox_v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Audio Jack, 4 Poles (TRRS)")
    (property "ki_keywords" "audio jack receptacle stereo headphones TRRS connector")
    (attr through_hole)
    (fp_text reference "J6" (at 0 14.2 90) (layer "Dwgs.User"))
    (fp_text value "MIDI IN" (at -2.1292 5.6193 180) (layer "F.SilkS"))
    (fp_text user "Ring2" (at 0 3.25 90) (layer "F.Fab"))
    (fp_text user "Sleeve" (at 0.25 11.4 90) (layer "F.Fab"))
    (fp_text user "Tip" (at 0 10 90) (layer "F.Fab"))
    (fp_text user "Ring1" (at 0 6.25 90) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 1.6 90) (size 0.8 0.8) (drill 0.8) (layers "*.Cu" "*.Mask"))
    (pad "" np_thru_hole circle (at 0 8.6 90) (size 0.8 0.8) (drill 0.8) (layers "*.Cu" "*.Mask"))
    (pad "R1" thru_hole oval (at 2.3 6.2 90) (size 1.6 2) (drill oval 0.9 1.3) (layers "*.Cu" "*.Mask")
      (net 60 "MIDI_IN_JACK_PIN4") (pintype "passive"))
    (pad "R2" thru_hole oval (at 2.3 3.2 90) (size 1.6 2) (drill oval 0.9 1.3) (layers "*.Cu" "*.Mask")
      (net 62 "unconnected-(J6-PadR2)") (pintype "passive+no_connect"))
    (pad "S" thru_hole oval (at -2.3 11.3 90) (size 1.6 2) (drill oval 0.9 1.3) (layers "*.Cu" "*.Mask")
      (net 16 "GND") (pintype "passive"))
    (pad "T" thru_hole oval (at 2.3 10.2 90) (size 1.6 2) (drill oval 0.9 1.3) (layers "*.Cu" "*.Mask")
      (net 59 "MIDI_IN_JACK_PIN5") (pintype "passive"))
    (model "/Users/danny/syncproj/kicad-libs/footprints/Keebio-Parts.pretty/3dmodels/PJ-320A.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 180))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (at 123.698 130.048 -90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "funbox_v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Push button switch, generic, two pins")
    (property "ki_keywords" "switch normally-open pushbutton push-button")
    (attr through_hole)
    (fp_text reference "FS2" (at -0.448 4.498 90) (layer "F.SilkS"))
    (fp_text value "Foot_Switch_2" (at 0 4.87 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at -0.448 4.498 -90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 16 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 5 "FOOT_SWITCH_2") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DIP:DIP-6_W7.62mm" (layer "F.Cu")
    (at 141.95 69.125)
    (descr "6-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (property "Sheetfile" "Midi.kicad_sch")
    (property "Sheetname" "Midi and Expression")
    (property "ki_description" "Schmitt Trigger Output Optocoupler, High Speed, DIP-6, 1.6mA turn on threshold")
    (property "ki_keywords" "High Speed Schmitt Optocoupler")
    (attr through_hole)
    (fp_text reference "U5" (at 3.7 2.575) (layer "F.Fab"))
    (fp_text value "H11L1" (at 4 2.375) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.81 2.54) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 58 "Net-(D2-K)") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 59 "MIDI_IN_JACK_PIN5") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 61 "unconnected-(U5-Pad3)") (pintype "no_connect"))
    (pad "4" thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 30 "MIDI_IN") (pintype "output"))
    (pad "5" thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 16 "GND") (pintype "power_in"))
    (pad "6" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 45 "3V3_A") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-6_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 162.9 66.415 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "Midi.kicad_sch")
    (property "Sheetname" "Midi and Expression")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R19" (at 3.81 0.025 90) (layer "F.Fab"))
    (fp_text value "2M" (at 3.695 0.075 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 67 "EXPRESSION_IN_JACK") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 16 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_THT:SW_Toggle_SPDT_lugs" (layer "F.Cu")
    (at 127.762 108.712 180)
    (descr "SW Toggle")
    (tags "SW Toggle")
    (property "Sheetfile" "funbox_v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Switch, single pole double throw")
    (property "ki_keywords" "switch single-pole double-throw spdt ON-ON")
    (attr through_hole)
    (fp_text reference "SW3" (at 0.124031 -8.249895) (layer "F.SilkS") hide)
    (fp_text value "SW_SPDT" (at 0 -6.35) (layer "F.Fab") hide)
    (pad "1" thru_hole oval (at -4.6736 0 180) (size 2.1 3.5) (drill oval 1 2.3) (layers "*.Cu" "*.Mask")
      (net 7 "SW3_RIGHT") (pinfunction "A") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 0 180) (size 2.1 3.5) (drill oval 1 2.3) (layers "*.Cu" "*.Mask")
      (net 16 "GND") (pinfunction "B") (pintype "passive"))
    (pad "3" thru_hole oval (at 4.7244 0 180) (size 2.1 3.5) (drill oval 1 2.3) (layers "*.Cu" "*.Mask")
      (net 3 "SW3_LEFT") (pinfunction "C") (pintype "passive"))
    (model "${KICAD_USER_3DMOD}/Toggle_SW_Blue_R0.step"
      (offset (xyz -6.5 4 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 130.429 127.127 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "funbox_v3.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R9" (at 3.81 0.0254) (layer "F.Fab"))
    (fp_text value "1K" (at 3.81 0.127) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 39 "Net-(LED2-A)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 24 "LED_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 133.809 129.9)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "funbox_v2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R2" (at 3.556 0) (layer "F.Fab"))
    (fp_text value "1M" (at 3.683 -0.127) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 44 "5V") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 33 "Net-(U1A-+)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 161.417 91.948)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "funbox_v2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R7" (at 3.937 0.127) (layer "F.Fab"))
    (fp_text value "100K" (at 3.937 0.127) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 16 "GND") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 35 "Net-(Out1-Pin_1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Rect_L7.0mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (at 172.593 119.039 -90)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 2.5mm Capacitor")
    (property "Sheetfile" "funbox_v2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C10" (at 2.5 0 90) (layer "F.Fab"))
    (fp_text value "100NF" (at 2.5 0.127 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 16 "GND") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 44 "5V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L7.0mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 161.925 86.487 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "funbox_v2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R10" (at 3.937 -0.127) (layer "F.Fab"))
    (fp_text value "3K3" (at 3.937 -0.127) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 4.073 -0.17) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 22 "AUDIO_OUT_BUFFER_RIGHT") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 51 "Net-(C13-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 157.353 124.079 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "funbox_v2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R17" (at 4.191 -0.127 90) (layer "F.Fab"))
    (fp_text value "100" (at 4.064 0 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 4.073 -0.17 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 57 "Net-(U1D--)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 56 "Net-(C17-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_THTPad_D2.0mm_Drill1.0mm" (layer "F.Cu")
    (at 148.225 66)
    (descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
    (tags "test point THT pad")
    (property "Sheetfile" "funbox_v2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr exclude_from_pos_files)
    (fp_text reference "Gnd" (at 2.625 -0.725 180) (layer "F.SilkS"))
    (fp_text value "~" (at 0 2.05) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 2.625 -0.75 180) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 16 "GND") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "Capacitor_THT:C_Rect_L7.0mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (at 122.555 94.488 90)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 2.5mm Capacitor")
    (property "Sheetfile" "funbox_v2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C2" (at 2.5 0 90) (layer "F.Fab"))
    (fp_text value "100pF" (at 2.5 0.127 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 31 "Net-(In1-Pin_1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 16 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L7.0mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_arc (start 177.800031 130.546974) (mid 177.428589 131.448207) (end 176.53 131.825999)
    (layer "Edge.Cuts"))
  (gr_arc (start 176.53 64.2874) (mid 177.428026 64.659374) (end 177.8 65.5574)
    (layer "Edge.Cuts"))
  (gr_line (start 176.53 131.825999) (end 119.38 131.826)
    (layer "Edge.Cuts"))
  (gr_line (start 119.38 64.2874) (end 176.53 64.2874)
    (layer "Edge.Cuts"))
  (gr_line (start 177.8 65.5574) (end 177.790974 130.546974)
    (layer "Edge.Cuts"))
  (gr_arc (start 119.38 131.826) (mid 118.481974 131.454026) (end 118.11 130.556)
    (layer "Edge.Cuts"))
  (gr_arc (start 118.11 65.5574) (mid 118.481974 64.659374) (end 119.38 64.2874)
    (layer "Edge.Cuts"))
  (gr_line (start 118.11 130.556) (end 118.11 65.5574)
    (layer "Edge.Cuts"))
  (gr_text "FunBox v3.2\n    GuitarML" (at 159.512 113.665 90) (layer "F.SilkS"))
  (zone (net 16) (net_name "GND") (layer "F.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 119.5324 64.2874)
        (xy 176.3776 64.2874)
        (xy 177.275626 64.659374)
        (xy 177.7492 65.4812)
        (xy 177.8 130.175)
        (xy 177.428026 131.327026)
        (xy 176.53 131.699)
        (xy 119.38 131.699)
        (xy 118.481974 131.327026)
        (xy 118.11 130.175)
        (xy 118.237 65.3288)
        (xy 118.634374 64.659374)
      )
    )
  )
  (zone (net 16) (net_name "GND") (layer "B.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 119.4562 64.3382)
        (xy 176.4538 64.3382)
        (xy 177.292 64.6684)
        (xy 177.6984 65.3542)
        (xy 177.8 130.175)
        (xy 177.428026 131.327026)
        (xy 176.53 131.699)
        (xy 119.38 131.699)
        (xy 118.481974 131.327026)
        (xy 118.11 130.175)
        (xy 118.237 65.3288)
        (xy 118.634374 64.643)
      )
    )
  )
)
