(kicad_pcb (version 20171130) (host pcbnew 5.1.6-c6e7f7d~87~ubuntu16.04.1)
  (general
    (thickness 1.6)
    (drawings 24)
    (tracks 174)
    (zones 0)
    (modules 19)
    (nets 34)
  )
  (page USLetter)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 1)
    (user_trace_width 0.5)
    (user_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.1)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.7 1.7)
    (pad_drill 1)
    (pad_to_mask_clearance 0.05)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(U2-Pad3)")
  (net 3 /5v)
  (net 4 /3.3v)
  (net 5 /SS)
  (net 6 /MOSI)
  (net 7 /MISO)
  (net 8 /SCK)
  (net 9 "Net-(J2-Pad1)")
  (net 10 "Net-(J2-Pad2)")
  (net 11 "Net-(J3-Pad1)")
  (net 12 "Net-(J3-Pad2)")
  (net 13 "Net-(J3-Pad5)")
  (net 14 "Net-(J4-Pad1)")
  (net 15 "Net-(J4-Pad2)")
  (net 16 "Net-(J4-Pad3)")
  (net 17 "Net-(J4-Pad4)")
  (net 18 "Net-(J4-Pad5)")
  (net 19 "Net-(J4-Pad6)")
  (net 20 "Net-(R1-Pad1)")
  (net 21 "Net-(U1-Pad5)")
  (net 22 "Net-(U1-Pad22)")
  (net 23 "Net-(U1-Pad12)")
  (net 24 "Net-(U2-Pad8)")
  (net 25 "Net-(U2-Pad7)")
  (net 26 "Net-(U2-Pad6)")
  (net 27 "Net-(R3-Pad1)")
  (net 28 "Net-(SW1-Pad3)")
  (net 29 "Net-(D1-Pad1)")
  (net 30 "Net-(D1-Pad2)")
  (net 31 "Net-(JP1-Pad1)")
  (net 32 "Net-(J4-Pad7)")
  (net 33 "Net-(J4-Pad8)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net /3.3v)
    (add_net /5v)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /SCK)
    (add_net /SS)
    (add_net GND)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(J3-Pad5)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(J4-Pad2)")
    (add_net "Net-(J4-Pad3)")
    (add_net "Net-(J4-Pad4)")
    (add_net "Net-(J4-Pad5)")
    (add_net "Net-(J4-Pad6)")
    (add_net "Net-(J4-Pad7)")
    (add_net "Net-(J4-Pad8)")
    (add_net "Net-(JP1-Pad1)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(SW1-Pad3)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U1-Pad22)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U2-Pad3)")
    (add_net "Net-(U2-Pad6)")
    (add_net "Net-(U2-Pad7)")
    (add_net "Net-(U2-Pad8)")
  )
  (module TerminalBlock_Phoenix:TerminalBlock_Phoenix_MPT-0,5-2-2.54_1x02_P2.54mm_Horizontal (layer F.Cu) (tedit 5B294F98)
    (at 167.513 117.221 270)
    (descr "Terminal Block Phoenix MPT-0,5-2-2.54, 2 pins, pitch 2.54mm, size 5.54x6.2mm^2, drill diamater 1.1mm, pad diameter 2.2mm, see http://www.mouser.com/ds/2/324/ItemDetail_1725656-920552.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
    (tags "THT Terminal Block Phoenix MPT-0,5-2-2.54 pitch 2.54mm size 5.54x6.2mm^2 drill 1.1mm pad 2.2mm")
    (fp_text reference J1 (at 2.921 -2.032 90) (layer F.SilkS))
    (fp_text value Conn_01x02_Male (at 0 4.87 90) (layer F.Fab))
    (fp_text user %R (at 0 1.27) (layer F.Fab))
    (pad "" np_thru_hole circle (at 2.54 2.54 270) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad "" np_thru_hole circle (at 0 2.54 270) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 30 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MPT-0,5-2-2.54_1x02_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module InAir4:TP4056 (layer F.Cu) (tedit 60348761)
    (at 202 106.25 270)
    (fp_text reference U3 (at -0.0272 14.9798 90) (layer F.SilkS))
    (fp_text value TP4056 (at 0 -2.54 90) (layer F.Fab))
    (pad 6 thru_hole circle (at 7 25 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(JP1-Pad1)"))
    (pad 5 thru_hole circle (at 4 25 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J2-Pad1)"))
    (pad 4 thru_hole circle (at -4 25 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J2-Pad2)"))
    (pad 3 thru_hole circle (at -7 25 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 7 2 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(D1-Pad1)"))
    (pad 1 thru_hole circle (at -7 2 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module InAir4:InAir9B (layer F.Cu) (tedit 603484AA)
    (at 177.5 83.7 270)
    (fp_text reference U2 (at 0.0184 -9.1392 270) (layer F.SilkS))
    (fp_text value InAir4 (at 0.21 -7.21 270) (layer F.Fab))
    (pad 8 thru_hole circle (at 11.43 -1.52 270) (size 1.7 1.7) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(U2-Pad8)"))
    (pad 9 thru_hole circle (at 11.43 -4.06 270) (size 1.7 1.7) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 10 thru_hole circle (at 11.43 -6.6 270) (size 1.7 1.7) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 /MOSI))
    (pad 11 thru_hole circle (at 11.43 -9.14 270) (size 1.7 1.7) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 /MISO))
    (pad 12 thru_hole circle (at 11.43 -11.68 270) (size 1.7 1.7) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 /SCK))
    (pad 13 thru_hole circle (at 11.43 -14.22 270) (size 1.7 1.7) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 /3.3v))
    (pad 14 thru_hole circle (at 11.43 -16.76 270) (size 1.7 1.7) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 7 thru_hole circle (at -11.43 -1.52 270) (size 1.7 1.7) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(U2-Pad7)"))
    (pad 6 thru_hole circle (at -11.43 -4.06 270) (size 1.7 1.7) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(U2-Pad6)"))
    (pad 5 thru_hole circle (at -11.43 -6.6 270) (size 1.7 1.7) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(U1-Pad5)"))
    (pad 4 thru_hole circle (at -11.43 -9.14 270) (size 1.7 1.7) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(U1-Pad12)"))
    (pad 3 thru_hole circle (at -11.43 -11.68 270) (size 1.7 1.7) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(U2-Pad3)"))
    (pad 2 thru_hole circle (at -11.43 -14.22 270) (size 1.7 1.7) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 /SS))
    (pad 1 thru_hole circle (at -11.43 -16.76 270) (size 1.7 1.7) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (module MountingHole:MountingHole_2.5mm_Pad (layer F.Cu) (tedit 603358CB)
    (at 199 73)
    (descr "Mounting Hole 2.5mm")
    (tags "mounting hole 2.5mm")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.5mm_Pad (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 2.5) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module MountingHole:MountingHole_2.5mm_Pad (layer F.Cu) (tedit 603358D3)
    (at 199 119)
    (descr "Mounting Hole 2.5mm")
    (tags "mounting hole 2.5mm")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.5mm_Pad (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 2.5) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module MountingHole:MountingHole_2.5mm_Pad (layer F.Cu) (tedit 603358BD)
    (at 153 119)
    (descr "Mounting Hole 2.5mm")
    (tags "mounting hole 2.5mm")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.5mm_Pad (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 2.5) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module MountingHole:MountingHole_2.5mm_Pad (layer F.Cu) (tedit 603358C4)
    (at 153 73)
    (descr "Mounting Hole 2.5mm")
    (tags "mounting hole 2.5mm")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.5mm_Pad (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 2.5) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical (layer F.Cu) (tedit 603864BE)
    (at 160.274 72.136 90)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (fp_text reference J6 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value Conn_01x06_Male (at 0 15.03 90) (layer F.Fab))
    (fp_text user %R (at 0 6.35) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /3.3v))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 4 /3.3v))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.4 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.4 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /5v))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /5v))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-24_W15.24mm_Socket_LongPads (layer F.Cu) (tedit 5CB66F85)
    (at 157.734 78.0415)
    (descr "24-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils), Socket, LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 15.24mm 600mil Socket LongPads")
    (fp_text reference U1 (at 7.5946 0.5207) (layer F.SilkS))
    (fp_text value ProMini (at 7.62 30.27) (layer F.Fab))
    (fp_text user %R (at 7.62 13.97) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.4 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J3-Pad1)"))
    (pad 13 thru_hole oval (at 15.24 27.94) (size 2.4 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 5 /SS))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.4 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J3-Pad2)"))
    (pad 14 thru_hole oval (at 15.24 25.4) (size 2.4 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 6 /MOSI))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.4 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J3-Pad5)"))
    (pad 15 thru_hole oval (at 15.24 22.86) (size 2.4 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 7 /MISO))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.4 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 16 thru_hole oval (at 15.24 20.32) (size 2.4 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 8 /SCK))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.4 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(U1-Pad5)"))
    (pad 17 thru_hole oval (at 15.24 17.78) (size 2.4 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(R1-Pad1)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.4 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J4-Pad1)"))
    (pad 18 thru_hole oval (at 15.24 15.24) (size 2.4 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(R3-Pad1)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.4 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J4-Pad2)"))
    (pad 19 thru_hole oval (at 15.24 12.7) (size 2.4 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(J4-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 2.4 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J4-Pad3)"))
    (pad 20 thru_hole oval (at 15.24 10.16) (size 2.4 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(J4-Pad8)"))
    (pad 9 thru_hole oval (at 0 20.32) (size 2.4 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J4-Pad4)"))
    (pad 21 thru_hole oval (at 15.24 7.62) (size 2.4 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 4 /3.3v))
    (pad 10 thru_hole oval (at 0 22.86) (size 2.4 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J4-Pad5)"))
    (pad 22 thru_hole oval (at 15.24 5.08) (size 2.4 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(U1-Pad22)"))
    (pad 11 thru_hole oval (at 0 25.4) (size 2.4 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J4-Pad6)"))
    (pad 23 thru_hole oval (at 15.24 2.54) (size 2.4 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 12 thru_hole oval (at 0 27.94) (size 2.4 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(U1-Pad12)"))
    (pad 24 thru_hole oval (at 15.24 0) (size 2.4 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 3 /5v))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-24_W15.24mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_PH_B2B-PH-K_1x02_P2.00mm_Vertical (layer F.Cu) (tedit 5B7745C2)
    (at 177.8 117.602)
    (descr "JST PH series connector, B2B-PH-K (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST PH side entry")
    (fp_text reference J2 (at 1 -2.9) (layer F.SilkS))
    (fp_text value Conn_01x02_Male (at 1 4) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask) (roundrect_rratio 0.208333)
      (net 9 "Net-(J2-Pad1)"))
    (pad 2 thru_hole oval (at 2 0) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask)
      (net 10 "Net-(J2-Pad2)"))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_PH_B2B-PH-K_1x02_P2.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical (layer F.Cu) (tedit 60348323)
    (at 152.146 79.2099)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x05_Male (at 0 12.49) (layer F.Fab))
    (fp_text user %R (at 0 5.08 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.4 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J3-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.4 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J3-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.4 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /3.3v))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.4 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.4 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J3-Pad5)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 165.0365 112.268)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R3 (at 2.4892 1.9304) (layer F.SilkS))
    (fp_text value 1M (at 2.54 1.92) (layer F.Fab))
    (fp_text user %R (at 2.54 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 27 "Net-(R3-Pad1)"))
    (pad 2 thru_hole oval (at 5.08 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 29 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 157.226 112.268)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R4 (at 2.4892 1.8923) (layer F.SilkS))
    (fp_text value 100K (at 2.54 1.92) (layer F.Fab))
    (fp_text user %R (at 2.54 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 5.08 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 27 "Net-(R3-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_THT:SW_CuK_OS102011MA1QN1_SPDT_Angled (layer F.Cu) (tedit 60334EB1)
    (at 187.4901 119.253)
    (descr "CuK miniature slide switch, OS series, SPDT, right angle, http://www.ckswitches.com/media/1428/os.pdf")
    (tags "switch SPDT")
    (fp_text reference SW1 (at 1.9304 2.3114) (layer F.SilkS))
    (fp_text value SW_SPDT (at 1.7 7.7) (layer F.Fab))
    (fp_text user %R (at 2.3 1.7) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.5 2.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 31 "Net-(JP1-Pad1)"))
    (pad 2 thru_hole oval (at 2 0) (size 1.5 2.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 /5v))
    (pad 3 thru_hole oval (at 4 0) (size 1.5 2.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 28 "Net-(SW1-Pad3)"))
    (pad "" thru_hole oval (at -2.1 0) (size 2.2 3.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad "" thru_hole oval (at 6.1 0) (size 2.2 3.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_CuK_OS102011MA1QN1_SPDT_Angled.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-34_SOD68_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE50CD5)
    (at 172.6311 110.2741 270)
    (descr "Diode, DO-34_SOD68 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=3.04*1.6mm^2, , https://www.nxp.com/docs/en/data-sheet/KTY83_SER.pdf")
    (tags "Diode DO-34_SOD68 series Axial Horizontal pin pitch 7.62mm  length 3.04mm diameter 1.6mm")
    (fp_text reference D1 (at 3.8227 1.9177 90) (layer F.SilkS))
    (fp_text value D_Small (at 3.81 1.92 90) (layer F.Fab))
    (fp_text user %R (at 4.038 0 90) (layer F.Fab))
    (fp_text user K (at 0 -1.75 90) (layer F.Fab))
    (fp_text user K (at 0 -1.75 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.5 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 29 "Net-(D1-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.5 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 30 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-34_SOD68_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm (layer F.Cu) (tedit 5B391E66)
    (at 188.5569 115.951)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP1 (at -2.9464 0.1397) (layer F.SilkS))
    (fp_text value Jumper_2_Open (at 0 1.9) (layer F.Fab))
    (pad 1 smd custom (at -0.65 0) (size 1 0.5) (layers F.Cu F.Mask)
      (net 31 "Net-(JP1-Pad1)") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy 0.5 -0.75) (xy 0.5 0.75) (xy 0 0.75)) (width 0))
      ))
    (pad 2 smd custom (at 0.65 0) (size 1 0.5) (layers F.Cu F.Mask)
      (net 3 /5v) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy -0.5 -0.75) (xy -0.5 0.75) (xy 0 0.75)) (width 0))
      ))
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 165.1 109.474)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R1 (at 2.54 -1.92) (layer F.SilkS))
    (fp_text value 1M (at 2.54 1.92) (layer F.Fab))
    (fp_text user %R (at 2.54 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 20 "Net-(R1-Pad1)"))
    (pad 2 thru_hole oval (at 5.08 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 /5v))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 157.226 109.474)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R2 (at 2.54 -1.92) (layer F.SilkS))
    (fp_text value 100K (at 2.54 1.92) (layer F.Fab))
    (fp_text user %R (at 2.54 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 5.08 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 20 "Net-(R1-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x08_P2.54mm_Vertical (layer F.Cu) (tedit 603482B9)
    (at 152.146 94.8055)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference J4 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x06_Male (at 0 20.11) (layer F.Fab))
    (fp_text user %R (at 0 8.89 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J4-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.2 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J4-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.2 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J4-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.2 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J4-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.2 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J4-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.2 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J4-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.2 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(J4-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 2.2 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(J4-Pad8)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text - (at 162.814 119.888 90) (layer F.SilkS))
  (gr_text + (at 162.814 117.094) (layer F.SilkS))
  (gr_text 3V (at 154.5336 84.201 270) (layer F.SilkS))
  (gr_text N7MCC (at 187.96 80.899) (layer B.SilkS))
  (gr_text A3 (at 154.432 112.776 270) (layer F.SilkS))
  (gr_text A2 (at 154.432 109.982 270) (layer F.SilkS))
  (gr_text "TMRR XPDR\nV3.0 8-2020\n" (at 187.579 78.486) (layer B.SilkS))
  (gr_text "v3.0.1\n2021.2" (at 158.623 120.142) (layer F.SilkS))
  (gr_text GND (at 154.5844 86.995 270) (layer F.SilkS))
  (gr_text D6 (at 154.432 102.362 270) (layer F.SilkS))
  (gr_text D5 (at 154.432 99.822 270) (layer F.SilkS))
  (gr_text D4 (at 154.432 97.282 270) (layer F.SilkS))
  (gr_text D3 (at 154.432 94.742 270) (layer F.SilkS))
  (gr_text RX (at 154.559 81.788 270) (layer F.SilkS))
  (gr_text TX (at 154.5336 79.1845 270) (layer F.SilkS))
  (gr_text 3V (at 161.3662 74.4474 180) (layer F.SilkS))
  (gr_text GND (at 166.5478 74.5236 180) (layer F.SilkS))
  (gr_text 5V (at 171.7548 74.5236 180) (layer F.SilkS))
  (gr_text D7 (at 154.432 104.902 270) (layer F.SilkS))
  (gr_text D8 (at 154.432 107.442 270) (layer F.SilkS))
  (gr_line (start 150 70) (end 150 122) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 202 122) (end 150 122) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 202 70) (end 202 122) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 150 70) (end 202 70) (layer Edge.Cuts) (width 0.1))
  (zone (net 3) (net_name /5v) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 201.168 113.792) (xy 175.768 113.792) (xy 175.768 73.406) (xy 201.168 73.406)
      )
    )
  )
  (zone (net 4) (net_name /3.3v) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 172.974 107.442) (xy 157.734 107.442) (xy 157.988 73.914) (xy 173.736 73.914)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 150.622 70.612) (xy 150.622 121.412) (xy 171.45 121.412) (xy 201.3077 121.3231) (xy 201.3077 113.5253)
        (xy 201.3077 70.5993)
      )
    )
  )
)
