(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 72)
    (no_connects 0)
    (area 124.499181 109.707799 142.50082 119.644224)
    (thickness 1.6)
    (drawings 10)
    (tracks 125)
    (zones 0)
    (modules 23)
    (nets 15)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.2032)
    (user_trace_width 0.1524)
    (user_trace_width 0.2032)
    (user_trace_width 0.254)
    (trace_clearance 0.2032)
    (zone_clearance 0.1524)
    (zone_45_only yes)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.7112)
    (via_drill 0.3048)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.7112)
    (uvia_drill 0.3048)
    (uvias_allowed no)
    (uvia_min_size 0.7112)
    (uvia_min_drill 0.3048)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.25 0.75)
    (pad_drill 0)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 126 118)
    (grid_origin 126.762 114.2535)
    (visible_elements 7FFEFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +3V3)
  (net 2 GND)
  (net 3 +BATT)
  (net 4 "Net-(C2-Pad2)")
  (net 5 "Net-(C4-Pad1)")
  (net 6 "Net-(C5-Pad1)")
  (net 7 "Net-(C6-Pad1)")
  (net 8 "Net-(C7-Pad1)")
  (net 9 "Net-(C7-Pad2)")
  (net 10 "Net-(R1-Pad2)")
  (net 11 "Net-(R3-Pad1)")
  (net 12 /EN)
  (net 13 "Net-(U4-Pad2)")
  (net 14 "Net-(D1-PadA)")
  (net_class Default "This is the default net class."
    (clearance 0.2032)
    (trace_width 0.2032)
    (via_dia 0.7112)
    (via_drill 0.3048)
    (uvia_dia 0.7112)
    (uvia_drill 0.3048)
    (add_net +3V3)
    (add_net +BATT)
    (add_net /EN)
    (add_net GND)
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(C7-Pad2)")
    (add_net "Net-(D1-PadA)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(U4-Pad2)")
  )
  (module TI_footprints:DBZ (layer F.Cu) (tedit 5AB76900)
    (at 132.477 116.0315 90)
    (tags "DBZ0003A, SOT-23(3)")
    (attr smd)
    (fp_text reference U2 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value DRV5032ZE (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.05 -0.95 180) (size 0.6 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3) (solder_mask_margin 0.07))
    (pad 3 smd rect (at 1.05 0 180) (size 0.6 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.07))
    (pad 2 smd rect (at -1.05 0.95 180) (size 0.6 1.3) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(R1-Pad2)") (solder_mask_margin 0.07))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module passives:R0603R (layer F.Cu) (tedit 5AB7693B)
    (at 130.064 113.111)
    (fp_text reference R5 (at 0 0) (layer F.SilkS) hide)
    (fp_text value 500 (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.725 0) (size 0.95 0.95) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C7-Pad1)") (solder_mask_margin 0.1))
    (pad 2 smd rect (at 0.725 0) (size 0.95 0.95) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D1-PadA)") (solder_mask_margin 0.1))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module passives:R0603R (layer B.Cu) (tedit 5AB7691C)
    (at 137.049 114.2535 90)
    (fp_text reference R4 (at 0 0 90) (layer B.SilkS) hide)
    (fp_text value 47k (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -0.725 0 90) (size 0.95 0.95) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3) (solder_mask_margin 0.1))
    (pad 2 smd rect (at 0.725 0 90) (size 0.95 0.95) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(C6-Pad1)") (solder_mask_margin 0.1))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module passives:R0603R (layer F.Cu) (tedit 5AB768F1)
    (at 132.858 113.111)
    (fp_text reference R3 (at 0 0) (layer F.SilkS) hide)
    (fp_text value 487 (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.725 0) (size 0.95 0.95) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(R3-Pad1)") (solder_mask_margin 0.1))
    (pad 2 smd rect (at 0.725 0) (size 0.95 0.95) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.1))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module passives:R0603R (layer B.Cu) (tedit 5AB76920)
    (at 131.588 115.0155)
    (fp_text reference R2 (at 0 0) (layer B.SilkS) hide)
    (fp_text value 100k (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -0.725 0) (size 0.95 0.95) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(C5-Pad1)") (solder_mask_margin 0.1))
    (pad 2 smd rect (at 0.725 0) (size 0.95 0.95) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(R1-Pad2)") (solder_mask_margin 0.1))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module passives:R0603R (layer F.Cu) (tedit 5AB76904)
    (at 130.064 116.413 90)
    (fp_text reference R1 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value 10k (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.725 0 90) (size 0.95 0.95) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3) (solder_mask_margin 0.1))
    (pad 2 smd rect (at 0.725 0 90) (size 0.95 0.95) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(R1-Pad2)") (solder_mask_margin 0.1))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module passives:D0603R (layer F.Cu) (tedit 5AB76937)
    (at 130.064 114.381 180)
    (fp_text reference D1 (at 0 0 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 0 180) (layer F.Fab))
    (pad A smd rect (at -0.8 0 180) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D1-PadA)") (solder_mask_margin 0.1))
    (pad K smd rect (at 0.8 0 180) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.1))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module passives:C0603R (layer B.Cu) (tedit 5AB76915)
    (at 134.5725 115.7775 270)
    (fp_text reference C9 (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value 100n (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.725 0 270) (size 0.95 0.95) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3) (solder_mask_margin 0.1))
    (pad 2 smd rect (at 0.725 0 270) (size 0.95 0.95) (layers B.Cu B.Paste B.Mask)
      (net 2 GND) (solder_mask_margin 0.1))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module passives:C0603R (layer F.Cu) (tedit 5AB768FA)
    (at 126.762 114.2535 270)
    (fp_text reference C8 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 10u (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.725 0 270) (size 0.95 0.95) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C7-Pad2)") (solder_mask_margin 0.1))
    (pad 2 smd rect (at 0.725 0 270) (size 0.95 0.95) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.1))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module passives:C0603R (layer F.Cu) (tedit 5AB768F5)
    (at 128.032 113.8725 270)
    (fp_text reference C7 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 10u (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.725 0 270) (size 0.95 0.95) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C7-Pad1)") (solder_mask_margin 0.1))
    (pad 2 smd rect (at 0.725 0 270) (size 0.95 0.95) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C7-Pad2)") (solder_mask_margin 0.1))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module passives:C0603R (layer B.Cu) (tedit 5AB7692B)
    (at 138.319 114.2535 270)
    (fp_text reference C6 (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value 100n (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.725 0 270) (size 0.95 0.95) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(C6-Pad1)") (solder_mask_margin 0.1))
    (pad 2 smd rect (at 0.725 0 270) (size 0.95 0.95) (layers B.Cu B.Paste B.Mask)
      (net 2 GND) (solder_mask_margin 0.1))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module passives:C0603R (layer B.Cu) (tedit 5AB76934)
    (at 130.699 113.7455 180)
    (fp_text reference C5 (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value 100n (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -0.725 0 180) (size 0.95 0.95) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(C5-Pad1)") (solder_mask_margin 0.1))
    (pad 2 smd rect (at 0.725 0 180) (size 0.95 0.95) (layers B.Cu B.Paste B.Mask)
      (net 2 GND) (solder_mask_margin 0.1))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module passives:C0603R (layer F.Cu) (tedit 5AB76941)
    (at 136.16 111.968)
    (fp_text reference C4 (at 0 0) (layer F.SilkS) hide)
    (fp_text value 3.3n (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.725 0) (size 0.95 0.95) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C4-Pad1)") (solder_mask_margin 0.1))
    (pad 2 smd rect (at 0.725 0) (size 0.95 0.95) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.1))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module passives:C0603R (layer F.Cu) (tedit 5AB76953)
    (at 139.335 114.635 180)
    (fp_text reference C3 (at 0 0 180) (layer F.SilkS) hide)
    (fp_text value 10u (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.725 0 180) (size 0.95 0.95) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C2-Pad2)") (solder_mask_margin 0.1))
    (pad 2 smd rect (at 0.725 0 180) (size 0.95 0.95) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.1))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module passives:C0603R (layer F.Cu) (tedit 5AB7694F)
    (at 139.335 113.365)
    (fp_text reference C2 (at 0 0) (layer F.SilkS) hide)
    (fp_text value 10u (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.725 0) (size 0.95 0.95) (layers F.Cu F.Paste F.Mask)
      (net 3 +BATT) (solder_mask_margin 0.1))
    (pad 2 smd rect (at 0.725 0) (size 0.95 0.95) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C2-Pad2)") (solder_mask_margin 0.1))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module passives:C0603R (layer F.Cu) (tedit 5AB76910)
    (at 136.033 117.302)
    (fp_text reference C1 (at 0 0) (layer F.SilkS) hide)
    (fp_text value 4.7uF (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.725 0) (size 0.95 0.95) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3) (solder_mask_margin 0.1))
    (pad 2 smd rect (at 0.725 0) (size 0.95 0.95) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.1))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TI_footprints:DBV (layer F.Cu) (tedit 5AB76918)
    (at 136.033 114.635 270)
    (tags "DBV0005A, SOT-23(5)")
    (attr smd)
    (fp_text reference U1 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value TPS709xxDBV (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.3 -0.95) (size 0.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 3 +BATT) (solder_mask_margin 0.07))
    (pad 5 smd rect (at 1.3 -0.95) (size 0.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3) (solder_mask_margin 0.07))
    (pad 2 smd rect (at -1.3 0) (size 0.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.07))
    (pad 3 smd rect (at -1.3 0.95) (size 0.6 1.1) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.07))
    (pad 4 smd rect (at 1.3 0.95) (size 0.6 1.1) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.07))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TI_footprints:DSG (layer F.Cu) (tedit 5AB76946)
    (at 132.858 111.206 180)
    (tags "DSG0008A, WSON(8)")
    (fp_text reference U3 (at 0 0 180) (layer F.SilkS) hide)
    (fp_text value TPS259571DSG (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 -0.75 180) (size 0.5 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C4-Pad1)") (solder_mask_margin 0.07))
    (pad 2 smd rect (at -0.95 -0.25 180) (size 0.5 0.25) (layers F.Cu F.Paste F.Mask)
      (net 12 /EN) (solder_mask_margin 0.07))
    (pad 3 smd rect (at -0.95 0.25 180) (size 0.5 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +BATT) (solder_mask_margin 0.07))
    (pad 4 smd rect (at -0.95 0.75 180) (size 0.5 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +BATT) (solder_mask_margin 0.07))
    (pad 8 smd rect (at 0.95 -0.75 180) (size 0.5 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.07))
    (pad 7 smd rect (at 0.95 -0.25 180) (size 0.5 0.25) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(R3-Pad1)") (solder_mask_margin 0.07))
    (pad 6 smd rect (at 0.95 0.25 180) (size 0.5 0.25) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.07))
    (pad 5 smd rect (at 0.95 0.75 180) (size 0.5 0.25) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C7-Pad1)") (solder_mask_margin 0.07))
    (pad 9 smd rect (at 0 0 180) (size 0.9 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.07))
    (pad 9 thru_hole circle (at 0 -0.55 270) (size 0.3048 0.3048) (drill 0.3048) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 9 thru_hole circle (at 0 0.55 270) (size 0.3048 0.3048) (drill 0.3048) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Housings_SON.3dshapes/X2SON-8_1.4x1mm_Pitch0.35mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TI_footprints:DCU (layer B.Cu) (tedit 5AB8F8B8)
    (at 134.255 113.1105)
    (tags "S-PDSO-G8, VSSOP(8)")
    (fp_text reference U4 (at 0 0) (layer B.SilkS) hide)
    (fp_text value SN74AUP1G74DCUR (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.55 0.75 270) (size 0.25 0.75) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(C5-Pad1)") (solder_mask_margin 0.05))
    (pad 8 smd rect (at 1.55 0.75 270) (size 0.25 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3) (solder_mask_margin 0.05))
    (pad 2 smd rect (at -1.55 0.25 270) (size 0.25 0.75) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(U4-Pad2)") (solder_mask_margin 0.05))
    (pad 7 smd rect (at 1.55 0.25 270) (size 0.25 0.75) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(C6-Pad1)") (solder_mask_margin 0.05))
    (pad 3 smd rect (at -1.55 -0.25 270) (size 0.25 0.75) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(U4-Pad2)") (solder_mask_margin 0.05))
    (pad 6 smd rect (at 1.55 -0.25 270) (size 0.25 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3) (solder_mask_margin 0.05))
    (pad 4 smd rect (at -1.55 -0.75 270) (size 0.25 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND) (solder_mask_margin 0.05))
    (pad 5 smd rect (at 1.55 -0.75 270) (size 0.25 0.75) (layers B.Cu B.Paste B.Mask)
      (net 12 /EN) (solder_mask_margin 0.05))
    (model Housings_SSOP.3dshapes/VSSOP-8_2.3x2mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module misc:SMD_PAD_2x3mm_plated (layer F.Cu) (tedit 5AB7694B)
    (at 139.25 111.25)
    (fp_text reference J1 (at 0 0) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 3 2) (layers F.Cu F.Paste F.Mask)
      (net 3 +BATT))
    (pad 1 thru_hole circle (at -1.143 -0.635) (size 0.7112 0.7112) (drill 0.3048) (layers *.Cu *.Mask)
      (net 3 +BATT))
    (pad 1 thru_hole circle (at 0 -0.635) (size 0.7112 0.7112) (drill 0.3048) (layers *.Cu *.Mask)
      (net 3 +BATT))
    (pad 1 thru_hole circle (at 1.143 -0.635) (size 0.7112 0.7112) (drill 0.3048) (layers *.Cu *.Mask)
      (net 3 +BATT))
    (pad 1 thru_hole circle (at -1.143 0.635) (size 0.7112 0.7112) (drill 0.3048) (layers *.Cu *.Mask)
      (net 3 +BATT))
    (pad 1 thru_hole circle (at 0 0.635) (size 0.7112 0.7112) (drill 0.3048) (layers *.Cu *.Mask)
      (net 3 +BATT))
    (pad 1 thru_hole circle (at 1.143 0.635) (size 0.7112 0.7112) (drill 0.3048) (layers *.Cu *.Mask)
      (net 3 +BATT))
    (pad 1 smd rect (at 0 0) (size 3 2) (layers B.Cu B.Paste B.Mask)
      (net 3 +BATT))
  )
  (module misc:SMD_PAD_2x3mm_plated (layer F.Cu) (tedit 5AB76956)
    (at 139.25 116.75)
    (fp_text reference J2 (at 0 0) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 3 2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at -1.143 -0.635) (size 0.7112 0.7112) (drill 0.3048) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 -0.635) (size 0.7112 0.7112) (drill 0.3048) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 1.143 -0.635) (size 0.7112 0.7112) (drill 0.3048) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at -1.143 0.635) (size 0.7112 0.7112) (drill 0.3048) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 0.635) (size 0.7112 0.7112) (drill 0.3048) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 1.143 0.635) (size 0.7112 0.7112) (drill 0.3048) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 0) (size 3 2) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
  )
  (module misc:SMD_PAD_2x3mm_plated (layer F.Cu) (tedit 5AB768E5)
    (at 127.75 111.25)
    (fp_text reference J3 (at 0 0) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 3 2) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C7-Pad1)"))
    (pad 1 thru_hole circle (at -1.143 -0.635) (size 0.7112 0.7112) (drill 0.3048) (layers *.Cu *.Mask)
      (net 8 "Net-(C7-Pad1)"))
    (pad 1 thru_hole circle (at 0 -0.635) (size 0.7112 0.7112) (drill 0.3048) (layers *.Cu *.Mask)
      (net 8 "Net-(C7-Pad1)"))
    (pad 1 thru_hole circle (at 1.143 -0.635) (size 0.7112 0.7112) (drill 0.3048) (layers *.Cu *.Mask)
      (net 8 "Net-(C7-Pad1)"))
    (pad 1 thru_hole circle (at -1.143 0.635) (size 0.7112 0.7112) (drill 0.3048) (layers *.Cu *.Mask)
      (net 8 "Net-(C7-Pad1)"))
    (pad 1 thru_hole circle (at 0 0.635) (size 0.7112 0.7112) (drill 0.3048) (layers *.Cu *.Mask)
      (net 8 "Net-(C7-Pad1)"))
    (pad 1 thru_hole circle (at 1.143 0.635) (size 0.7112 0.7112) (drill 0.3048) (layers *.Cu *.Mask)
      (net 8 "Net-(C7-Pad1)"))
    (pad 1 smd rect (at 0 0) (size 3 2) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(C7-Pad1)"))
  )
  (module misc:SMD_PAD_2x3mm_plated (layer F.Cu) (tedit 5AB7690A)
    (at 127.75 116.75)
    (fp_text reference J4 (at 0 0) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 3 2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at -1.143 -0.635) (size 0.7112 0.7112) (drill 0.3048) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 -0.635) (size 0.7112 0.7112) (drill 0.3048) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 1.143 -0.635) (size 0.7112 0.7112) (drill 0.3048) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at -1.143 0.635) (size 0.7112 0.7112) (drill 0.3048) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 0.635) (size 0.7112 0.7112) (drill 0.3048) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 1.143 0.635) (size 0.7112 0.7112) (drill 0.3048) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 0) (size 3 2) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
  )
  (gr_text v1.0a (at 132.477 117.1745) (layer B.SilkS))
  (gr_text magSW (at 133.747 110.9515) (layer B.SilkS))
  (gr_text GND (at 126.365 115.189) (layer B.SilkS))
  (gr_text +RX (at 126.365 113.03) (layer B.SilkS))
  (gr_text GND (at 137.684 117.1745) (layer B.SilkS))
  (gr_text +BAT (at 137.557 110.9515) (layer B.SilkS))
  (gr_line (start 126 118) (end 126 110) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 141 118) (end 126 118) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 141 110) (end 141 118) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 126 110) (end 141 110) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 8) (net_name "Net-(C7-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer))
    (polygon
      (pts
        (xy 126 109.999) (xy 131.0165 109.999) (xy 131.334 110.3165) (xy 131.334 110.507) (xy 131.334 110.698)
        (xy 131.334 111.0785) (xy 129.8735 112.539) (xy 129.8735 113.6185) (xy 127.524 113.6185) (xy 127.524 112.476)
        (xy 126 112.4755)
      )
    )
  )
  (zone (net 3) (net_name +BATT) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer))
    (polygon
      (pts
        (xy 134.1915 111.0785) (xy 134.763 111.0785) (xy 134.9535 111.269) (xy 137.4935 111.269) (xy 137.6205 111.396)
        (xy 137.6205 112.539) (xy 137.4935 112.666) (xy 136.668 112.666) (xy 136.668 113.936) (xy 139.335 113.936)
        (xy 139.335 112.6025) (xy 140.986 112.6025) (xy 140.986 109.999) (xy 134.1915 109.999)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer))
    (polygon
      (pts
        (xy 126 117.9365) (xy 140.986 117.9365) (xy 140.986 110.1895) (xy 126.127 110.1895) (xy 126 110.1895)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer))
    (polygon
      (pts
        (xy 126 114.444) (xy 128.3495 114.444) (xy 128.8575 113.936) (xy 129.683 113.936) (xy 129.683 114.7615)
        (xy 129.302 115.1425) (xy 129.302 118) (xy 126 118)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer))
    (polygon
      (pts
        (xy 140.986 118) (xy 140.986 115.333) (xy 139.335 115.333) (xy 139.335 114.1265) (xy 137.684 114.1265)
        (xy 137.684 116.7935) (xy 136.287 116.7935) (xy 136.2235 116.7935) (xy 136.2235 118) (xy 140.859 118)
      )
    )
  )
)
