(kicad_pcb (version 20171130) (host pcbnew 5.0.2-bee76a0~70~ubuntu18.04.1)
  (general
    (thickness 1.6)
    (drawings 7)
    (tracks 121)
    (zones 0)
    (modules 10)
    (nets 11)
  )
  (page A4)
  (title_block
    (title "ALERT Scint module")
    (date 2018-12-12)
    (rev v0)
    (comment 4 "Author: Whitney Armstrong")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.15)
    (edge_width 0.0254)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /p5_P)
  (net 2 /p5_N)
  (net 3 /p1_N)
  (net 4 /p1_P)
  (net 5 /p2_P)
  (net 6 /p2_N)
  (net 7 /p3_N)
  (net 8 /p3_P)
  (net 9 /p4_P)
  (net 10 /p4_N)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /p1_N)
    (add_net /p1_P)
    (add_net /p2_N)
    (add_net /p2_P)
    (add_net /p3_N)
    (add_net /p3_P)
    (add_net /p4_N)
    (add_net /p4_P)
    (add_net /p5_N)
    (add_net /p5_P)
  )
  (module Pin_Headers:Pin_Header_Straight_2x01_Pitch2.54mm (layer F.Cu) (tedit 5C115BC7)
    (at 252.8 82.3)
    (descr "Through hole straight pin header, 2x01, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x01 2.54mm double row")
    (fp_text reference J5 (at -2.2 -1.2) (layer F.SilkS))
    (fp_text value sipm5 (at -0.3 2.1) (layer F.Fab))
    (fp_text user %R (at 1.27 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /p5_N))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /p5_P))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x01_Pitch2.54mm (layer F.Cu) (tedit 5C115BC2)
    (at 256.9 87.7)
    (descr "Through hole straight pin header, 2x01, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x01 2.54mm double row")
    (fp_text reference J4 (at -2.2 1.2) (layer F.SilkS))
    (fp_text value sipm4 (at 0.2 -2.2) (layer F.Fab))
    (fp_text user %R (at 1.27 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /p4_P))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /p4_N))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x01_Pitch2.54mm (layer F.Cu) (tedit 5C115BCD)
    (at 261.4 82.3)
    (descr "Through hole straight pin header, 2x01, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x01 2.54mm double row")
    (fp_text reference J3 (at -2.2 -1.2) (layer F.SilkS))
    (fp_text value sipm3 (at 1.2 2.1) (layer F.Fab))
    (fp_text user %R (at 1.27 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /p3_N))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /p3_P))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x01_Pitch2.54mm (layer F.Cu) (tedit 5C115BBC)
    (at 265.6 87.6)
    (descr "Through hole straight pin header, 2x01, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x01 2.54mm double row")
    (fp_text reference J2 (at -2.26 1.2) (layer F.SilkS))
    (fp_text value sipm2 (at 1.3 -2.1) (layer F.Fab))
    (fp_text user %R (at 1.27 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /p2_P))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /p2_N))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x01_Pitch2.54mm (layer F.Cu) (tedit 5C115BD1)
    (at 270 82.3)
    (descr "Through hole straight pin header, 2x01, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x01 2.54mm double row")
    (fp_text reference J1 (at -2.2 -1.2) (layer F.SilkS))
    (fp_text value sipm1 (at 1.9 2) (layer F.Fab))
    (fp_text user %R (at 1.27 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /p1_N))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /p1_P))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module photo_detectors:SiPM_6050VE (layer B.Cu) (tedit 5AB085F7)
    (at 235 85)
    (fp_text reference D1 (at 0 -4) (layer B.SilkS))
    (fp_text value D_SiPM (at 0.25 4.5) (layer B.Fab))
    (fp_text user cathode (at 2.8194 0.0254 90) (layer B.SilkS))
    (fp_text user anode (at 0.5588 -0.0254 90) (layer B.SilkS))
    (pad 2 smd circle (at 1.25 1.25) (size 0.7 0.7) (layers B.Cu B.Paste B.Mask)
      (net 3 /p1_N))
    (pad 2 smd circle (at 1.25 -1.25) (size 0.7 0.7) (layers B.Cu B.Paste B.Mask)
      (net 3 /p1_N))
    (pad 2 smd circle (at -1.25 -1.25) (size 0.7 0.7) (layers B.Cu B.Paste B.Mask)
      (net 3 /p1_N))
    (pad 2 smd circle (at -1.25 1.25) (size 0.7 0.7) (layers B.Cu B.Paste B.Mask)
      (net 3 /p1_N))
    (pad 1 smd circle (at 2.5 2.5) (size 0.7 0.7) (layers B.Cu B.Paste B.Mask)
      (net 4 /p1_P))
    (pad 1 smd circle (at 2.5 -2.5) (size 0.7 0.7) (layers B.Cu B.Paste B.Mask)
      (net 4 /p1_P))
    (pad 1 smd circle (at -2.5 2.5) (size 0.7 0.7) (layers B.Cu B.Paste B.Mask)
      (net 4 /p1_P))
    (pad 1 smd circle (at -2.5 -2.5) (size 0.7 0.7) (layers B.Cu B.Paste B.Mask)
      (net 4 /p1_P))
  )
  (module photo_detectors:SiPM_6050VE (layer B.Cu) (tedit 5AB085F7)
    (at 205 85)
    (fp_text reference D2 (at 0 -4) (layer B.SilkS))
    (fp_text value D_SiPM (at 0.25 4.5) (layer B.Fab))
    (fp_text user anode (at 0.5588 -0.0254 90) (layer B.SilkS))
    (fp_text user cathode (at 2.8194 0.0254 90) (layer B.SilkS))
    (pad 1 smd circle (at -2.5 -2.5) (size 0.7 0.7) (layers B.Cu B.Paste B.Mask)
      (net 5 /p2_P))
    (pad 1 smd circle (at -2.5 2.5) (size 0.7 0.7) (layers B.Cu B.Paste B.Mask)
      (net 5 /p2_P))
    (pad 1 smd circle (at 2.5 -2.5) (size 0.7 0.7) (layers B.Cu B.Paste B.Mask)
      (net 5 /p2_P))
    (pad 1 smd circle (at 2.5 2.5) (size 0.7 0.7) (layers B.Cu B.Paste B.Mask)
      (net 5 /p2_P))
    (pad 2 smd circle (at -1.25 1.25) (size 0.7 0.7) (layers B.Cu B.Paste B.Mask)
      (net 6 /p2_N))
    (pad 2 smd circle (at -1.25 -1.25) (size 0.7 0.7) (layers B.Cu B.Paste B.Mask)
      (net 6 /p2_N))
    (pad 2 smd circle (at 1.25 -1.25) (size 0.7 0.7) (layers B.Cu B.Paste B.Mask)
      (net 6 /p2_N))
    (pad 2 smd circle (at 1.25 1.25) (size 0.7 0.7) (layers B.Cu B.Paste B.Mask)
      (net 6 /p2_N))
  )
  (module photo_detectors:SiPM_6050VE (layer B.Cu) (tedit 5AB085F7)
    (at 175 85)
    (fp_text reference D3 (at 0 -4) (layer B.SilkS))
    (fp_text value D_SiPM (at 0.25 4.5) (layer B.Fab))
    (fp_text user cathode (at 2.8194 0.0254 90) (layer B.SilkS))
    (fp_text user anode (at 0.5588 -0.0254 90) (layer B.SilkS))
    (pad 2 smd circle (at 1.25 1.25) (size 0.7 0.7) (layers B.Cu B.Paste B.Mask)
      (net 7 /p3_N))
    (pad 2 smd circle (at 1.25 -1.25) (size 0.7 0.7) (layers B.Cu B.Paste B.Mask)
      (net 7 /p3_N))
    (pad 2 smd circle (at -1.25 -1.25) (size 0.7 0.7) (layers B.Cu B.Paste B.Mask)
      (net 7 /p3_N))
    (pad 2 smd circle (at -1.25 1.25) (size 0.7 0.7) (layers B.Cu B.Paste B.Mask)
      (net 7 /p3_N))
    (pad 1 smd circle (at 2.5 2.5) (size 0.7 0.7) (layers B.Cu B.Paste B.Mask)
      (net 8 /p3_P))
    (pad 1 smd circle (at 2.5 -2.5) (size 0.7 0.7) (layers B.Cu B.Paste B.Mask)
      (net 8 /p3_P))
    (pad 1 smd circle (at -2.5 2.5) (size 0.7 0.7) (layers B.Cu B.Paste B.Mask)
      (net 8 /p3_P))
    (pad 1 smd circle (at -2.5 -2.5) (size 0.7 0.7) (layers B.Cu B.Paste B.Mask)
      (net 8 /p3_P))
  )
  (module photo_detectors:SiPM_6050VE (layer B.Cu) (tedit 5AB085F7)
    (at 145 85)
    (fp_text reference D4 (at 0 -4) (layer B.SilkS))
    (fp_text value D_SiPM (at 0.25 4.5) (layer B.Fab))
    (fp_text user anode (at 0.5588 -0.0254 90) (layer B.SilkS))
    (fp_text user cathode (at 2.8194 0.0254 90) (layer B.SilkS))
    (pad 1 smd circle (at -2.5 -2.5) (size 0.7 0.7) (layers B.Cu B.Paste B.Mask)
      (net 9 /p4_P))
    (pad 1 smd circle (at -2.5 2.5) (size 0.7 0.7) (layers B.Cu B.Paste B.Mask)
      (net 9 /p4_P))
    (pad 1 smd circle (at 2.5 -2.5) (size 0.7 0.7) (layers B.Cu B.Paste B.Mask)
      (net 9 /p4_P))
    (pad 1 smd circle (at 2.5 2.5) (size 0.7 0.7) (layers B.Cu B.Paste B.Mask)
      (net 9 /p4_P))
    (pad 2 smd circle (at -1.25 1.25) (size 0.7 0.7) (layers B.Cu B.Paste B.Mask)
      (net 10 /p4_N))
    (pad 2 smd circle (at -1.25 -1.25) (size 0.7 0.7) (layers B.Cu B.Paste B.Mask)
      (net 10 /p4_N))
    (pad 2 smd circle (at 1.25 -1.25) (size 0.7 0.7) (layers B.Cu B.Paste B.Mask)
      (net 10 /p4_N))
    (pad 2 smd circle (at 1.25 1.25) (size 0.7 0.7) (layers B.Cu B.Paste B.Mask)
      (net 10 /p4_N))
  )
  (module photo_detectors:SiPM_6050VE (layer B.Cu) (tedit 5AB085F7)
    (at 115 85)
    (fp_text reference D5 (at 0 -4) (layer B.SilkS))
    (fp_text value D_SiPM (at 0.25 4.5) (layer B.Fab))
    (fp_text user cathode (at 2.8194 0.0254 90) (layer B.SilkS))
    (fp_text user anode (at 0.5588 -0.0254 90) (layer B.SilkS))
    (pad 2 smd circle (at 1.25 1.25) (size 0.7 0.7) (layers B.Cu B.Paste B.Mask)
      (net 2 /p5_N))
    (pad 2 smd circle (at 1.25 -1.25) (size 0.7 0.7) (layers B.Cu B.Paste B.Mask)
      (net 2 /p5_N))
    (pad 2 smd circle (at -1.25 -1.25) (size 0.7 0.7) (layers B.Cu B.Paste B.Mask)
      (net 2 /p5_N))
    (pad 2 smd circle (at -1.25 1.25) (size 0.7 0.7) (layers B.Cu B.Paste B.Mask)
      (net 2 /p5_N))
    (pad 1 smd circle (at 2.5 2.5) (size 0.7 0.7) (layers B.Cu B.Paste B.Mask)
      (net 1 /p5_P))
    (pad 1 smd circle (at 2.5 -2.5) (size 0.7 0.7) (layers B.Cu B.Paste B.Mask)
      (net 1 /p5_P))
    (pad 1 smd circle (at -2.5 2.5) (size 0.7 0.7) (layers B.Cu B.Paste B.Mask)
      (net 1 /p5_P))
    (pad 1 smd circle (at -2.5 -2.5) (size 0.7 0.7) (layers B.Cu B.Paste B.Mask)
      (net 1 /p5_P))
  )
  (gr_line (start 250 90) (end 275 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 250 80) (end 275 80) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 100 80) (end 100 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 275 80) (end 275 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 250 90) (end 100 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 250 80) (end 100 80) (layer Edge.Cuts) (width 0.0254))
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 100 80) (xy 100 90) (xy 275 90) (xy 275 80)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 100 80) (xy 100 90) (xy 275 90) (xy 275 80)
      )
    )
  )
)
