(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 158)
    (no_connects 0)
    (area 76.589999 77.809999 141.690001 107.920001)
    (thickness 1.6)
    (drawings 14)
    (tracks 662)
    (zones 0)
    (modules 51)
    (nets 27)
  )
  (page A4)
  (title_block
    (title OA_IMU)
    (date 2018-03-10)
    (rev 0)
    (company OpenAvionics)
  )
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (44 Edge.Cuts user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 1)
    (user_trace_width 0.01)
    (user_trace_width 0.02)
    (user_trace_width 0.05)
    (user_trace_width 0.1)
    (user_trace_width 0.2)
    (user_trace_width 1)
    (trace_clearance 0.1)
    (zone_clearance 0.25)
    (zone_45_only no)
    (trace_min 0.01)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 0.5 0.5)
    (mod_text_width 0.15)
    (pad_size 2.75 2.75)
    (pad_drill 2.75)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x01330_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 4)
      (mirror false)
      (drillshape 2)
      (scaleselection 1)
      (outputdirectory meta/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(C1-Pad1)")
  (net 3 "Net-(C2-Pad1)")
  (net 4 SCL1)
  (net 5 SDA1)
  (net 6 TX)
  (net 7 RX)
  (net 8 ID_SD)
  (net 9 ID_SC)
  (net 10 +5V)
  (net 11 +3V3)
  (net 12 "Net-(C13-Pad1)")
  (net 13 "Net-(C14-Pad1)")
  (net 14 "Net-(D2-Pad2)")
  (net 15 "Net-(J3-Pad2)")
  (net 16 "Net-(L1-Pad2)")
  (net 17 "Net-(R7-Pad1)")
  (net 18 "Net-(F1-Pad1)")
  (net 19 "Net-(F2-Pad1)")
  (net 20 "Net-(R1-Pad2)")
  (net 21 "Net-(C15-Pad1)")
  (net 22 "Net-(J4-Pad1)")
  (net 23 "Net-(R10-Pad2)")
  (net 24 "Net-(R8-Pad1)")
  (net 25 "Net-(BT1-Pad1)")
  (net 26 "Net-(D1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.1)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net GND)
    (add_net ID_SC)
    (add_net ID_SD)
    (add_net "Net-(BT1-Pad1)")
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C13-Pad1)")
    (add_net "Net-(C14-Pad1)")
    (add_net "Net-(C15-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(F1-Pad1)")
    (add_net "Net-(F2-Pad1)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(L1-Pad2)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R10-Pad2)")
    (add_net "Net-(R7-Pad1)")
    (add_net "Net-(R8-Pad1)")
    (add_net RX)
    (add_net SCL1)
    (add_net SDA1)
    (add_net TX)
  )
  (module Diodes_SMD:D_SMB (layer F.Cu) (tedit 5AB4E2BA)
    (at 78.85 96.6 270)
    (descr "Diode SMB (DO-214AA)")
    (tags "Diode SMB (DO-214AA)")
    (attr smd)
    (fp_text reference D2 (at 1.7188 1.6322 270) (layer F.SilkS))
    (fp_text value RS2A+ (at -0.9482 1.6322 270) (layer F.Fab))
    (pad 1 smd rect (at -2.15 0 270) (size 2.5 2.3) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C13-Pad1)"))
    (pad 2 smd rect (at 2.15 0 270) (size 2.5 2.3) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SMB.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5AE765B5)
    (at 94.7 92.55 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at -0.15 -0.15 270) (layer F.SilkS))
    (fp_text value 4.7k (at -1.9 -0.15 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 +3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 SCL1))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module OA_pretty:SMA-CONN (layer F.Cu) (tedit 5AEF1021)
    (at 128.9 104.05 180)
    (tags "SMA Connector")
    (fp_text reference J4 (at -5.25 -8.2 180) (layer F.SilkS))
    (fp_text value Conn_SMA (at -8.95 -5.35 180) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 180) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(J4-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 -2.54 180) (size 2.6 2.6) (drill 1.6) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole circle (at -2.54 -2.54 180) (size 2.6 2.6) (drill 1.6) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole circle (at -2.54 2.54 180) (size 2.6 2.6) (drill 1.6) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.54 2.54 180) (size 2.6 2.6) (drill 1.6) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model connectors/sma.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz -90 0 -90))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5AE76563)
    (at 122.35 100.8 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C6 (at 0.1002 -0.058 90) (layer F.SilkS))
    (fp_text value 100n (at -1.1498 -0.058 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 11 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5AECB023)
    (at 113.75 87.1)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at -1.4 -0.8) (layer F.SilkS))
    (fp_text value 4.7k (at 0 0.05) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 ID_SC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RPi_Hat:RPi_Hat_Mounting_Hole locked (layer F.Cu) (tedit 5ABBBD7C)
    (at 80.14 81.383)
    (descr "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -4.0005) (layer F.SilkS) hide)
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 -0.013) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask)
      (solder_mask_margin 1.725) (clearance 1.725))
  )
  (module RPi_Hat:RPi_Hat_Mounting_Hole locked (layer F.Cu) (tedit 55217C7B)
    (at 138.14 81.37)
    (descr "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -4.0005) (layer F.SilkS) hide)
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask)
      (solder_mask_margin 1.725) (clearance 1.725))
  )
  (module RPi_Hat:RPi_Hat_Mounting_Hole locked (layer F.Cu) (tedit 55217CCB)
    (at 138.14 104.37)
    (descr "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -4.0005) (layer F.SilkS) hide)
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask)
      (solder_mask_margin 1.725) (clearance 1.725))
  )
  (module Pin_Headers:Pin_Header_Straight_2x20_Pitch2.54mm locked (layer F.Cu) (tedit 5ABB9681)
    (at 84.92 82.645 90)
    (descr "Through hole straight pin header, 2x20, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x20 2.54mm double row")
    (fp_text reference J1 (at 5.81 -1.481 180) (layer F.SilkS))
    (fp_text value "RPi Zero Headers 02x20" (at 5.75 9.47 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 +5V))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 SDA1))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 +5V))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 SCL1))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 TX))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 RX))
    (pad 11 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 12 thru_hole oval (at 2.54 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 13 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 14 thru_hole oval (at 2.54 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 15 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 16 thru_hole oval (at 2.54 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 17 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 18 thru_hole oval (at 2.54 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 19 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 20 thru_hole oval (at 2.54 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 21 thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 22 thru_hole oval (at 2.54 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 23 thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 24 thru_hole oval (at 2.54 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 25 thru_hole oval (at 0 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 26 thru_hole oval (at 2.54 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 27 thru_hole oval (at 0 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 ID_SD))
    (pad 28 thru_hole oval (at 2.54 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 ID_SC))
    (pad 29 thru_hole oval (at 0 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 30 thru_hole oval (at 2.54 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 31 thru_hole oval (at 0 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 32 thru_hole oval (at 2.54 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 33 thru_hole oval (at 0 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 34 thru_hole oval (at 2.54 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 35 thru_hole oval (at 0 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 36 thru_hole oval (at 2.54 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 37 thru_hole oval (at 0 45.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 38 thru_hole oval (at 2.54 45.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 39 thru_hole oval (at 0 48.26 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 40 thru_hole oval (at 2.54 48.26 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x20_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module OA_pretty:LGA-24L_3x3.5mm_Pitch0.43mm (layer F.Cu) (tedit 5AECAC90)
    (at 122.2 105)
    (descr "LGA 24L 3x3.5mm Pitch 0.43mm")
    (tags "LGA 24L 3x3.5mm Pitch 0.43mm")
    (attr smd)
    (fp_text reference U1 (at -0.55 -0.55 180) (layer F.SilkS))
    (fp_text value LSM9DS1 (at 1.25 2.2 180) (layer F.Fab))
    (pad 1 smd rect (at -1.505 -1.225) (size 0.23 0.35) (layers F.Cu F.Paste F.Mask)
      (net 11 +3V3))
    (pad 2 smd rect (at -1.475 -0.645) (size 0.35 0.23) (layers F.Cu F.Paste F.Mask)
      (net 4 SCL1))
    (pad 17 smd rect (at 1.475 -0.645) (size 0.35 0.23) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.475 -0.215) (size 0.35 0.23) (layers F.Cu F.Paste F.Mask)
      (net 11 +3V3))
    (pad 16 smd rect (at 1.475 -0.215) (size 0.35 0.23) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -1.475 0.215) (size 0.35 0.23) (layers F.Cu F.Paste F.Mask)
      (net 5 SDA1))
    (pad 15 smd rect (at 1.475 0.215) (size 0.35 0.23) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at -1.475 0.645) (size 0.35 0.23) (layers F.Cu F.Paste F.Mask)
      (net 11 +3V3))
    (pad 14 smd rect (at 1.475 0.645) (size 0.35 0.23) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 24 smd rect (at -1.075 -1.225) (size 0.23 0.35) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 23 smd rect (at -0.645 -1.225) (size 0.23 0.35) (layers F.Cu F.Paste F.Mask)
      (net 11 +3V3))
    (pad 22 smd rect (at -0.215 -1.225) (size 0.23 0.35) (layers F.Cu F.Paste F.Mask)
      (net 11 +3V3))
    (pad 21 smd rect (at 0.215 -1.225) (size 0.23 0.35) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 20 smd rect (at 0.645 -1.225) (size 0.23 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 19 smd rect (at 1.075 -1.225) (size 0.23 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 18 smd rect (at 1.505 -1.225) (size 0.23 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -1.505 1.225) (size 0.23 0.35) (layers F.Cu F.Paste F.Mask)
      (net 11 +3V3))
    (pad 7 smd rect (at -1.075 1.225) (size 0.23 0.35) (layers F.Cu F.Paste F.Mask)
      (net 11 +3V3))
    (pad 8 smd rect (at -0.645 1.225) (size 0.23 0.35) (layers F.Cu F.Paste F.Mask)
      (net 11 +3V3))
    (pad 9 smd rect (at -0.215 1.225) (size 0.23 0.35) (layers F.Cu F.Paste F.Mask))
    (pad 10 smd rect (at 0.215 1.225) (size 0.23 0.35) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd rect (at 0.645 1.225) (size 0.23 0.35) (layers F.Cu F.Paste F.Mask))
    (pad 12 smd rect (at 1.075 1.225) (size 0.23 0.35) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at 1.505 1.225) (size 0.23 0.35) (layers F.Cu F.Paste F.Mask))
  )
  (module OA_pretty:HLGA-10L (layer F.Cu) (tedit 5AF18B0D)
    (at 110.25 102.05 270)
    (descr "HLGA Package; 10-Lead Plastic (2mm x 2mm) (see ST TN1198.pdf)")
    (tags HLGA-10L)
    (attr smd)
    (fp_text reference U2 (at -1.45 1.65 360) (layer F.SilkS))
    (fp_text value LPS22HB (at -1.5 -0.7 360) (layer F.Fab))
    (pad 7 smd rect (at 0.75 -0.25 270) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 0.75 0.25 270) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 11 +3V3))
    (pad 5 smd rect (at 0.5 0.75 270) (size 0.35 0.375) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0 0.75 270) (size 0.35 0.375) (layers F.Cu F.Paste F.Mask)
      (net 4 SCL1))
    (pad 3 smd rect (at -0.5 0.75 270) (size 0.35 0.375) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -0.75 0.25 270) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 5 SDA1))
    (pad 1 smd rect (at -0.75 -0.25 270) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 11 +3V3))
    (pad 10 smd rect (at -0.5 -0.75 270) (size 0.35 0.375) (layers F.Cu F.Paste F.Mask)
      (net 11 +3V3))
    (pad 9 smd rect (at 0 -0.75 270) (size 0.35 0.375) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 8 smd rect (at 0.5 -0.75 270) (size 0.35 0.375) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Housings_DFN_QFN.3dshapes/DFN-12-1EP_4x4mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module OA_pretty:HLGA-10L (layer F.Cu) (tedit 5AF46389)
    (at 99.9 101.95 270)
    (descr "HLGA Package; 10-Lead Plastic (2mm x 2mm) (see ST TN1198.pdf)")
    (tags HLGA-10L)
    (attr smd)
    (fp_text reference U3 (at -1.55 1.5 360) (layer F.SilkS))
    (fp_text value LPS22HB (at 1.35 0.4 360) (layer F.Fab))
    (pad 7 smd rect (at 0.75 -0.25 270) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 0.75 0.25 270) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 11 +3V3))
    (pad 5 smd rect (at 0.5 0.75 270) (size 0.35 0.375) (layers F.Cu F.Paste F.Mask)
      (net 11 +3V3))
    (pad 4 smd rect (at 0 0.75 270) (size 0.35 0.375) (layers F.Cu F.Paste F.Mask)
      (net 4 SCL1))
    (pad 3 smd rect (at -0.5 0.75 270) (size 0.35 0.375) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -0.75 0.25 270) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 5 SDA1))
    (pad 1 smd rect (at -0.75 -0.25 270) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 11 +3V3))
    (pad 10 smd rect (at -0.5 -0.75 270) (size 0.35 0.375) (layers F.Cu F.Paste F.Mask)
      (net 11 +3V3))
    (pad 9 smd rect (at 0 -0.75 270) (size 0.35 0.375) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 8 smd rect (at 0.5 -0.75 270) (size 0.35 0.375) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Housings_DFN_QFN.3dshapes/DFN-12-1EP_4x4mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5ABA67D1)
    (at 82.296 85.979 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C12 (at -0.9398 1.3462 180) (layer F.SilkS))
    (fp_text value 10u (at 1.016 1.3462 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 10 +5V))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module OA_pretty:UTDFN-6 (layer F.Cu) (tedit 5AECAC4C)
    (at 94.5 87.35 90)
    (fp_text reference U6 (at 1.3462 -0.3302 180) (layer F.SilkS))
    (fp_text value ISL9021A (at 2.6 -1.2 180) (layer F.Fab))
    (pad 1 smd rect (at 0.5 -0.6 90) (size 0.25 0.7) (layers F.Cu F.Paste F.Mask)
      (net 10 +5V))
    (pad 2 smd rect (at 0 -0.7 90) (size 0.25 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at -0.5 -0.7 90) (size 0.25 0.5) (layers F.Cu F.Paste F.Mask)
      (net 10 +5V))
    (pad 4 smd rect (at -0.5 0.7 90) (size 0.25 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 0 0.7 90) (size 0.25 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 0.5 0.7 90) (size 0.25 0.5) (layers F.Cu F.Paste F.Mask)
      (net 11 +3V3))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5ABA6796)
    (at 77.85 88.15 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C14 (at 1.3462 -1.016 90) (layer F.SilkS))
    (fp_text value 3.3nF (at -0.5842 -1.1176 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C14-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5ABA6806)
    (at 83.5 87.5 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at -0.8636 -1.2192 90) (layer F.SilkS))
    (fp_text value 100k (at 0.9144 -1.2446 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(R7-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 +5V))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DFN_QFN:QFN-16-1EP_3x3mm_Pitch0.5mm_ThermalVias (layer F.Cu) (tedit 5ABBB109)
    (at 80.7 89.1 180)
    (descr "16-Lead Plastic Quad Flat, No Lead Package (NG) - 3x3x0.9 mm Body [QFN]; (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFN 0.5")
    (attr smd)
    (fp_text reference U7 (at 1.4732 2.3114 180) (layer F.SilkS))
    (fp_text value TPS62143 (at -0.9652 2.3114 180) (layer F.Fab))
    (pad 1 smd oval (at -1.475 -0.75 180) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(L1-Pad2)"))
    (pad 2 smd oval (at -1.475 -0.25 180) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(L1-Pad2)"))
    (pad 3 smd oval (at -1.475 0.25 180) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(L1-Pad2)"))
    (pad 4 smd oval (at -1.475 0.75 180) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(R7-Pad1)"))
    (pad 5 smd oval (at -0.75 1.475 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd oval (at -0.25 1.475 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 7 smd oval (at 0.25 1.475 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 8 smd oval (at 0.75 1.475 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd oval (at 1.475 0.75 180) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C14-Pad1)"))
    (pad 10 smd oval (at 1.475 0.25 180) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C13-Pad1)"))
    (pad 11 smd oval (at 1.475 -0.25 180) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C13-Pad1)"))
    (pad 12 smd oval (at 1.475 -0.75 180) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C13-Pad1)"))
    (pad 13 smd oval (at 0.75 -1.475 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C13-Pad1)"))
    (pad 14 smd oval (at 0.25 -1.475 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 10 +5V))
    (pad 15 smd oval (at -0.25 -1.475 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 16 smd oval (at -0.75 -1.475 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 17 smd rect (at 0.45 0.45 180) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 17 smd rect (at 0.45 -0.45 180) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 17 smd rect (at -0.45 0.45 180) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 17 smd rect (at -0.45 -0.45 180) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 17 thru_hole circle (at 0 0 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND))
    (pad 17 thru_hole circle (at -0.5 -0.5 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND))
    (pad 17 thru_hole circle (at 0.5 -0.5 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND))
    (pad 17 thru_hole circle (at 0.5 0.5 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND))
    (pad 17 thru_hole circle (at -0.5 0.5 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND))
    (model Housings_DFN_QFN.3dshapes/QFN-16-1EP_3x3mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module OA_pretty:L_Coilcraft_4mmx4mm (layer F.Cu) (tedit 5ABA7CCD)
    (at 86.487 87.503 270)
    (fp_text reference L1 (at -0.2032 1.2954 360) (layer F.SilkS))
    (fp_text value 2.2uH (at 0.2286 -0.762 360) (layer F.Fab))
    (pad 1 smd rect (at -1.2 0 270) (size 1 3.4) (layers F.Cu F.Paste F.Mask)
      (net 10 +5V))
    (pad 2 smd rect (at 1.2 0 270) (size 1 3.4) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(L1-Pad2)"))
  )
  (module OA_pretty:Molex_2p (layer F.Cu) (tedit 5ABA6C98)
    (at 86.25 101.7)
    (descr "Bornier d'alimentation 2 pins")
    (tags DEV)
    (fp_text reference J2 (at -1.4986 8.1534) (layer F.SilkS))
    (fp_text value "12V in" (at -0.127 9.7028) (layer F.Fab))
    (pad 1 thru_hole rect (at -1.27 0) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 18 "Net-(F1-Pad1)"))
    (pad 2 thru_hole circle (at 1.27 0) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 19 "Net-(F2-Pad1)"))
    (model Connect.3dshapes/bornier2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 5ABBAE7B)
    (at 80.95 93)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C13 (at 0.254 0.381) (layer F.SilkS))
    (fp_text value 47uF (at 0 -0.381) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C13-Pad1)"))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SMB (layer F.Cu) (tedit 5ABB9833)
    (at 88.9 96.5 90)
    (descr "Diode SMB (DO-214AA)")
    (tags "Diode SMB (DO-214AA)")
    (attr smd)
    (fp_text reference D3 (at -1.651 -1.5748 90) (layer F.SilkS))
    (fp_text value SMBJ5.0A (at 0.0762 1.5494 90) (layer F.Fab))
    (pad 1 smd rect (at -2.15 0 90) (size 2.5 2.3) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D2-Pad2)"))
    (pad 2 smd rect (at 2.15 0 90) (size 2.5 2.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SMB.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:GS2 (layer F.Cu) (tedit 5AECB002)
    (at 110.1 86.6 90)
    (descr "2-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J3 (at 1.65 -0.7 180) (layer F.SilkS))
    (fp_text value GS2 (at 1.65 0.55 180) (layer F.Fab))
    (pad 1 smd rect (at 0 -0.64 90) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 11 +3V3))
    (pad 2 smd rect (at 0 0.64 90) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(J3-Pad2)"))
  )
  (module Housings_DFN_QFN:DFN-8-1EP_2x3mm_Pitch0.5mm (layer F.Cu) (tedit 5AFACC84)
    (at 116.9 86.35 180)
    (descr "DDB Package; 8-Lead Plastic DFN (3mm x 2mm) (see Linear Technology DFN_8_05-08-1702.pdf)")
    (tags "DFN 0.5")
    (attr smd)
    (fp_text reference U5 (at -1.2 2.1 270) (layer F.SilkS))
    (fp_text value M24C16 (at 0.1 -0.05 270) (layer F.Fab))
    (pad 1 smd rect (at -0.925 -0.75 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -0.925 -0.25 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -0.925 0.25 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -0.925 0.75 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 0.925 0.75 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 8 ID_SD))
    (pad 6 smd rect (at 0.925 0.25 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 9 ID_SC))
    (pad 7 smd rect (at 0.925 -0.25 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(J3-Pad2)"))
    (pad 8 smd rect (at 0.925 -0.75 180) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 11 +3V3))
    (pad 9 smd rect (at 0 0.55 180) (size 0.61 1.1) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 9 smd rect (at 0 -0.55 180) (size 0.61 1.1) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin_ratio -0.2))
    (model ${KISYS3DMOD}/Housings_DFN_QFN.3dshapes/DFN-8-1EP_2x3mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5AF189B8)
    (at 99.95 104.2)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at -1.85 0.1 180) (layer F.SilkS))
    (fp_text value 100n (at -0.1 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 11 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5AECB073)
    (at 116.75 88.8)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C8 (at 0.65 0.85) (layer F.SilkS))
    (fp_text value 100n (at 0 0.05) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 11 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5ABE6AD0)
    (at 96.65 87.35 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C10 (at -1.1656 1.1892 270) (layer F.SilkS))
    (fp_text value 4.7uF (at 0.0344 -0.3608 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 11 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fuse_Holders_and_Fuses:Fuse_SMD1206_Reflow (layer F.Cu) (tedit 5AF2E8BA)
    (at 83.65 98.9 180)
    (descr "Fuse, Sicherung, SMD1206, Littlefuse-Wickmann, Reflow,")
    (tags "Fuse Sicherung SMD1206 Littlefuse-Wickmann Reflow ")
    (attr smd)
    (fp_text reference F1 (at 1.75 1.4 180) (layer F.SilkS))
    (fp_text value 1206L150TH (at -0.2 0.15 180) (layer F.Fab))
    (pad 1 smd rect (at -1.305 0 270) (size 2.03 1.14) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(F1-Pad1)"))
    (pad 2 smd rect (at 1.295 0 270) (size 2.03 1.14) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D2-Pad2)"))
  )
  (module Fuse_Holders_and_Fuses:Fuse_SMD1206_Reflow (layer F.Cu) (tedit 5ABE67E5)
    (at 83.6 96.5 180)
    (descr "Fuse, Sicherung, SMD1206, Littlefuse-Wickmann, Reflow,")
    (tags "Fuse Sicherung SMD1206 Littlefuse-Wickmann Reflow ")
    (attr smd)
    (fp_text reference F2 (at -0.1 -2.75 180) (layer F.SilkS))
    (fp_text value 1206L150TH (at -0.381 1.524 180) (layer F.Fab))
    (pad 1 smd rect (at -1.305 0 270) (size 2.03 1.14) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(F2-Pad1)"))
    (pad 2 smd rect (at 1.295 0 270) (size 2.03 1.14) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5ABE6A93)
    (at 92.583 87.249 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C11 (at 0.101 0.933 270) (layer F.SilkS))
    (fp_text value 100n (at -0.099 0.033 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 10 +5V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5AF18B3A)
    (at 110.35 104.35)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at -1.75 -0.75 180) (layer F.SilkS))
    (fp_text value 100n (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 11 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5AE7649D)
    (at 123.55 101.8 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 0.1 0.1 90) (layer F.SilkS))
    (fp_text value 100n (at -0.15 0.85 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5AE765D6)
    (at 121.15 101.9 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at -0.1 -0.05 90) (layer F.SilkS))
    (fp_text value 10n (at 1.4 -0.05 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5AF460C9)
    (at 119.95 101.9 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at 1.95 0 90) (layer F.SilkS))
    (fp_text value 100n (at 0.1 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 11 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5AFAD277)
    (at 119.6 87.55 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at -1.55 0.6 270) (layer F.SilkS))
    (fp_text value 470R (at -0.05 0.05 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 RX))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(R1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5AECB05D)
    (at 113.75 85.45)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 1.1 0.95) (layer F.SilkS))
    (fp_text value 4.7k (at -0.05 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 ID_SD))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5AE765C8)
    (at 96.3 92.55 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at 0.1 -0.15 270) (layer F.SilkS))
    (fp_text value 4.7k (at -1.9 0.1 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 +3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 SDA1))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module OA_pretty:XA1100 (layer F.Cu) (tedit 5AECB08E)
    (at 130.7 91.95 90)
    (fp_text reference U4 (at 3.2316 3.437 90) (layer F.SilkS))
    (fp_text value XA1100 (at -0.25 1 90) (layer F.Fab))
    (pad 19 smd rect (at 3.6 -6.25 90) (size 0.6 2) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(R1-Pad2)"))
    (pad 20 smd rect (at 2.4 -6.25 90) (size 0.6 2) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(R10-Pad2)"))
    (pad 21 smd rect (at 1.2 -6.25 90) (size 0.6 2) (layers F.Cu F.Paste F.Mask))
    (pad 22 smd rect (at -1.2 -6.25 90) (size 0.6 2) (layers F.Cu F.Paste F.Mask))
    (pad 23 smd rect (at -2.4 -6.25 90) (size 0.6 2) (layers F.Cu F.Paste F.Mask))
    (pad 24 smd rect (at -3.6 -6.25 90) (size 0.6 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 18 smd rect (at 6.25 -3 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 17 smd rect (at 6.25 -1.8 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 16 smd rect (at 6.25 -0.6 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(R8-Pad1)"))
    (pad 15 smd rect (at 6.25 0.6 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at 6.25 1.8 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -6.25 -3 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -6.25 -1.8 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(J4-Pad1)"))
    (pad 3 smd rect (at -6.25 -0.6 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -6.25 0.6 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at -6.25 1.8 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -6.25 3 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 8 smd rect (at -2.4 6.25 90) (size 0.6 2) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(BT1-Pad1)"))
    (pad 7 smd rect (at -3.6 6.25 90) (size 0.6 2) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(C15-Pad1)"))
    (pad 9 smd rect (at -1.2 6.25 90) (size 0.6 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 10 smd rect (at 1.2 6.25 90) (size 0.6 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 11 smd rect (at 2.4 6.25 90) (size 0.6 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 12 smd rect (at 3.6 6.25 90) (size 0.6 2) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at 6.25 3 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5AEF47C4)
    (at 140.05 98.65)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C15 (at 2.4 0.15) (layer F.SilkS))
    (fp_text value 100n (at -0.05 0) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(C15-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_0603 (layer F.Cu) (tedit 5AEF2E49)
    (at 121.9 97.1)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L2 (at -1.05 -0.9) (layer F.SilkS))
    (fp_text value 33nF (at 0.05 0.05) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(J4-Pad1)"))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5AEF46DB)
    (at 123 85.1 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at 1.7 0.25 180) (layer F.SilkS))
    (fp_text value 10k (at -0.05 0.05 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(R8-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5AFAD04A)
    (at 140 94.5)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R9 (at -0.55 -0.95) (layer F.SilkS))
    (fp_text value 1k (at -0.1 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(BT1-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5AFAD28C)
    (at 121.2 89.95 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R10 (at -0.6 1.1 90) (layer F.SilkS))
    (fp_text value 10k (at -0.05 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(R10-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5AFAD283)
    (at 119.6 89.95 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R11 (at 1.15 -1 90) (layer F.SilkS))
    (fp_text value 10k (at 0 0.05 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(R1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5AEF2E78)
    (at 122.15 94.9 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C7 (at -0.7 -0.85 90) (layer F.SilkS))
    (fp_text value 4.7u (at 0.05 0.05 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 11 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5AEF47C8)
    (at 140.05 100)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C9 (at 2.2 0.1) (layer F.SilkS))
    (fp_text value 4.7u (at 0 0.05) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(C15-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5AFACCAD)
    (at 121.2 87.55 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at -0.8 -0.9 270) (layer F.SilkS))
    (fp_text value 470R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 TX))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(R10-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_0603 (layer F.Cu) (tedit 5AEF477C)
    (at 137.9 99.05 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L3 (at 0 -1.9 90) (layer F.SilkS))
    (fp_text value Bead (at 0 -0.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(C15-Pad1)"))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-523 (layer F.Cu) (tedit 5AFAD056)
    (at 140 95.95 180)
    (descr "http://www.diodes.com/datasheets/ap02001.pdf p.144")
    (tags "Diode SOD523")
    (attr smd)
    (fp_text reference D1 (at 0.75 -0.95 180) (layer F.SilkS))
    (fp_text value CDBU70 (at -3.25 -0.15 180) (layer F.Fab))
    (pad 2 smd rect (at 0.7 0) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(C15-Pad1)"))
    (pad 1 smd rect (at -0.7 0) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-523.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module OA_pretty:P2Case (layer F.Cu) (tedit 5AF30BEF)
    (at 105.15 107.9)
    (fp_text reference REF** (at 0.2 3.9) (layer F.SilkS))
    (fp_text value P2Case (at 0.25 2) (layer F.Fab))
    (pad "" thru_hole circle (at 0 -8) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 0 -2.5) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 10.5 -8) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 10.5 -2.5) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -10.5 -2.5) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -10.5 -8) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask))
  )
  (module OA_pretty:RPi_pHat_Mounting_Hole locked (layer F.Cu) (tedit 5AF3147C)
    (at 80.15 104.35)
    (descr "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -4.0005) (layer F.SilkS) hide)
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask))
  )
  (module OA_pretty:BatCellLi3V (layer F.Cu) (tedit 5AFAC975)
    (at 141 88.05 180)
    (fp_text reference BT1 (at 3.05 4.7 180) (layer F.SilkS))
    (fp_text value Li3V (at -2.15 -0.55 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 -0.75 180) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 25 "Net-(BT1-Pad1)"))
    (pad 2 thru_hole circle (at 0 0.75 180) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (gr_arc (start 79.64 104.87) (end 79.64 107.87) (angle 90) (layer Edge.Cuts) (width 0.1))
  (dimension 3.5 (width 0.3) (layer Dwgs.User)
    (gr_text "3,5 mm" (at 150 105 90) (layer Dwgs.User))
    (feature1 (pts (xy 144 104.5) (xy 148.2 104.5)))
    (feature2 (pts (xy 144 108) (xy 148.2 108)))
    (crossbar (pts (xy 145.5 108) (xy 145.5 104.5)))
    (arrow1a (pts (xy 145.5 104.5) (xy 146.086421 105.626504)))
    (arrow1b (pts (xy 145.5 104.5) (xy 144.913579 105.626504)))
    (arrow2a (pts (xy 145.5 108) (xy 146.086421 106.873496)))
    (arrow2b (pts (xy 145.5 108) (xy 144.913579 106.873496)))
  )
  (dimension 3.5 (width 0.3) (layer Dwgs.User)
    (gr_text "3,5 mm" (at 141 115.5) (layer Dwgs.User))
    (feature1 (pts (xy 141.5 109.5) (xy 141.5 113.7)))
    (feature2 (pts (xy 138 109.5) (xy 138 113.7)))
    (crossbar (pts (xy 138 111) (xy 141.5 111)))
    (arrow1a (pts (xy 141.5 111) (xy 140.373496 111.586421)))
    (arrow1b (pts (xy 141.5 111) (xy 140.373496 110.413579)))
    (arrow2a (pts (xy 138 111) (xy 139.126504 111.586421)))
    (arrow2b (pts (xy 138 111) (xy 139.126504 110.413579)))
  )
  (dimension 30 (width 0.3) (layer Dwgs.User)
    (gr_text "30 mm" (at 65.65 93 90) (layer Dwgs.User))
    (feature1 (pts (xy 76 78) (xy 64.3 78)))
    (feature2 (pts (xy 76 108) (xy 64.3 108)))
    (crossbar (pts (xy 67 108) (xy 67 78)))
    (arrow1a (pts (xy 67 78) (xy 67.586421 79.126504)))
    (arrow1b (pts (xy 67 78) (xy 66.413579 79.126504)))
    (arrow2a (pts (xy 67 108) (xy 67.586421 106.873496)))
    (arrow2b (pts (xy 67 108) (xy 66.413579 106.873496)))
  )
  (dimension 23 (width 0.3) (layer Dwgs.User)
    (gr_text "23 mm" (at 71.85 92.87 90) (layer Dwgs.User))
    (feature1 (pts (xy 75.64 81.37) (xy 71.04 81.37)))
    (feature2 (pts (xy 75.64 104.37) (xy 71.04 104.37)))
    (crossbar (pts (xy 73.14 104.37) (xy 73.14 81.37)))
    (arrow1a (pts (xy 73.14 81.37) (xy 73.726421 82.496504)))
    (arrow1b (pts (xy 73.14 81.37) (xy 72.553579 82.496504)))
    (arrow2a (pts (xy 73.14 104.37) (xy 73.726421 103.243496)))
    (arrow2b (pts (xy 73.14 104.37) (xy 72.553579 103.243496)))
  )
  (gr_arc (start 138.64 80.87) (end 138.64 77.87) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 79.64 77.87) (end 138.64 77.87) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 79.64 80.86) (end 76.64 80.86) (angle 90) (layer Edge.Cuts) (width 0.1))
  (dimension 58 (width 0.3) (layer Dwgs.User)
    (gr_text "58 mm" (at 109.14 72.52) (layer Dwgs.User))
    (feature1 (pts (xy 138.14 76.37) (xy 138.14 71.17)))
    (feature2 (pts (xy 80.14 76.37) (xy 80.14 71.17)))
    (crossbar (pts (xy 80.14 73.87) (xy 138.14 73.87)))
    (arrow1a (pts (xy 138.14 73.87) (xy 137.013496 74.456421)))
    (arrow1b (pts (xy 138.14 73.87) (xy 137.013496 73.283579)))
    (arrow2a (pts (xy 80.14 73.87) (xy 81.266504 74.456421)))
    (arrow2b (pts (xy 80.14 73.87) (xy 81.266504 73.283579)))
  )
  (dimension 65 (width 0.3) (layer Dwgs.User)
    (gr_text "65 mm" (at 109.14 68) (layer Dwgs.User))
    (feature1 (pts (xy 141.64 76.37) (xy 141.64 66.67)))
    (feature2 (pts (xy 76.64 76.37) (xy 76.64 66.67)))
    (crossbar (pts (xy 76.64 69.37) (xy 141.64 69.37)))
    (arrow1a (pts (xy 141.64 69.37) (xy 140.513496 69.956421)))
    (arrow1b (pts (xy 141.64 69.37) (xy 140.513496 68.783579)))
    (arrow2a (pts (xy 76.64 69.37) (xy 77.766504 69.956421)))
    (arrow2b (pts (xy 76.64 69.37) (xy 77.766504 68.783579)))
  )
  (gr_arc (start 138.64 104.87) (end 141.64 104.87) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 76.64 80.37) (end 76.64 104.87) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 79.64 107.87) (end 138.64 107.87) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 141.64 80.37) (end 141.64 104.87) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.25))
    (min_thickness 0.1)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 96.47 84.328) (xy 86.250259 84.328) (xy 86.3 95.1) (xy 77.2 95.1) (xy 77.2 85.15)
        (xy 83.3 85.15) (xy 83.3 84.3) (xy 83.312 84.3) (xy 83.312 78.74) (xy 96.47 78.74)
      )
    )
  )
  (zone (net 10) (net_name +5V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.25))
    (min_thickness 0.1)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 88.646 84.455) (xy 88.646 86.741) (xy 83.312 86.741) (xy 83.312 84.328) (xy 83.312 78.74)
        (xy 88.646 78.74)
      )
    )
  )
  (zone (net 16) (net_name "Net-(L1-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.099))
    (min_thickness 0.1)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 82.2 88.85) (xy 88.65 88.85) (xy 88.65 89.65) (xy 82.85 89.65) (xy 82.2 89.85)
        (xy 82.2 89.4)
      )
    )
  )
  (zone (net 12) (net_name "Net-(C13-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.099))
    (min_thickness 0.1)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 78.5 88.8) (xy 79.2 88.8) (xy 79.2 90.55) (xy 80.1 90.6) (xy 80.1 91.2)
        (xy 78.7 92.2) (xy 77.45 92.2) (xy 77.45 89.95) (xy 78.5 89.45) (xy 78.5 89.4)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.099))
    (min_thickness 0.1)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 79.8 88.3) (xy 79.8 87.8) (xy 77.2 87.75) (xy 77.2 85.15) (xy 82 85.15)
        (xy 82.05 87.65) (xy 81.6 88.2)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.099))
    (min_thickness 0.1)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 80.85 89.95) (xy 80.85 95.1) (xy 86.2 95.1) (xy 86.3 95.1) (xy 86.3 90.4)
        (xy 81.6 90.4) (xy 81.6 89.95)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.25))
    (min_thickness 0.1)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 141.65 100.4) (xy 118.95 100.4) (xy 118.9 89.25) (xy 118.9 84.55) (xy 141.65 84.55)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.25))
    (min_thickness 0.1)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 125.65 107.35) (xy 125.65 98.95) (xy 132.45 98.95) (xy 132.45 107.35)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.1)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 106.65 98.4) (xy 114.15 98.4) (xy 114.15 106.9) (xy 106.65 106.9)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.25))
    (min_thickness 0.1)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 103.65 98.4) (xy 103.65 106.9) (xy 96.15 106.9) (xy 96.15 98.4)
      )
    )
  )
)
