(kicad_pcb (version 20171130) (host pcbnew "(5.1.5-0-10_14)")
  (general
    (thickness 1.6)
    (drawings 26)
    (tracks 374)
    (zones 0)
    (modules 25)
    (nets 52)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.1)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(C1-Pad1)")
  (net 3 VCC)
  (net 4 "Net-(D1-Pad1)")
  (net 5 "Net-(D1-Pad2)")
  (net 6 "Net-(J1-Pad1)")
  (net 7 "Net-(J1-Pad2)")
  (net 8 "Net-(J1-Pad3)")
  (net 9 "Net-(J1-Pad4)")
  (net 10 "Net-(J1-Pad5)")
  (net 11 "Net-(J1-Pad6)")
  (net 12 "Net-(J1-Pad7)")
  (net 13 "Net-(J1-Pad8)")
  (net 14 "Net-(J1-Pad10)")
  (net 15 "Net-(J1-Pad11)")
  (net 16 "Net-(J1-Pad12)")
  (net 17 "Net-(J1-Pad13)")
  (net 18 "Net-(J1-Pad14)")
  (net 19 "Net-(J2-Pad1)")
  (net 20 "Net-(J3-Pad1)")
  (net 21 "Net-(J3-Pad2)")
  (net 22 "Net-(J3-Pad3)")
  (net 23 "Net-(J3-Pad4)")
  (net 24 "Net-(J3-Pad5)")
  (net 25 "Net-(J4-Pad5)")
  (net 26 "Net-(J5-Pad2)")
  (net 27 "Net-(J5-Pad3)")
  (net 28 "Net-(J6-Pad4)")
  (net 29 "Net-(J6-Pad3)")
  (net 30 "Net-(J6-Pad2)")
  (net 31 "Net-(J6-Pad1)")
  (net 32 "Net-(J6-Pad7)")
  (net 33 "Net-(J6-Pad8)")
  (net 34 "Net-(J6-Pad9)")
  (net 35 "Net-(J7-Pad4)")
  (net 36 "Net-(J7-Pad3)")
  (net 37 "Net-(J7-Pad2)")
  (net 38 "Net-(J7-Pad1)")
  (net 39 "Net-(J8-Pad1)")
  (net 40 "Net-(J8-Pad2)")
  (net 41 "Net-(J8-Pad3)")
  (net 42 "Net-(JP2-Pad2)")
  (net 43 "Net-(S1-Pad1)")
  (net 44 "Net-(U1-Pad4)")
  (net 45 "Net-(U2-Pad20)")
  (net 46 "Net-(U2-Pad27)")
  (net 47 "Net-(U2-Pad28)")
  (net 48 "Net-(U3-Pad11)")
  (net 49 "Net-(J5-Pad4)")
  (net 50 "Net-(J5-Pad5)")
  (net 51 "Net-(J7-Pad10)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad11)")
    (add_net "Net-(J1-Pad12)")
    (add_net "Net-(J1-Pad13)")
    (add_net "Net-(J1-Pad14)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J3-Pad4)")
    (add_net "Net-(J3-Pad5)")
    (add_net "Net-(J4-Pad5)")
    (add_net "Net-(J5-Pad2)")
    (add_net "Net-(J5-Pad3)")
    (add_net "Net-(J5-Pad4)")
    (add_net "Net-(J5-Pad5)")
    (add_net "Net-(J6-Pad1)")
    (add_net "Net-(J6-Pad2)")
    (add_net "Net-(J6-Pad3)")
    (add_net "Net-(J6-Pad4)")
    (add_net "Net-(J6-Pad7)")
    (add_net "Net-(J6-Pad8)")
    (add_net "Net-(J6-Pad9)")
    (add_net "Net-(J7-Pad1)")
    (add_net "Net-(J7-Pad10)")
    (add_net "Net-(J7-Pad2)")
    (add_net "Net-(J7-Pad3)")
    (add_net "Net-(J7-Pad4)")
    (add_net "Net-(J8-Pad1)")
    (add_net "Net-(J8-Pad2)")
    (add_net "Net-(J8-Pad3)")
    (add_net "Net-(JP2-Pad2)")
    (add_net "Net-(S1-Pad1)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U2-Pad20)")
    (add_net "Net-(U2-Pad27)")
    (add_net "Net-(U2-Pad28)")
    (add_net "Net-(U3-Pad11)")
    (add_net VCC)
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Horizontal (layer F.Cu) (tedit 5EB352E2)
    (at 203 79 90)
    (descr "Through hole angled pin header, 1x02, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x02 2.54mm single row")
    (fp_text reference J9 (at 4.385 -2.27 90) (layer F.SilkS) hide)
    (fp_text value "Power OUT (to PSP)" (at 4.385 4.81 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 5EB0B66B)
    (at 203 75.9 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value "Power IN" (at 0 4.87 90) (layer F.Fab))
    (fp_text user %R (at 0 1.27 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J2-Pad1)"))
  )
  (module L102011ML04Q (layer F.Cu) (tedit 5EB0B646)
    (at 193 107.5 270)
    (descr "L102 (ML)")
    (tags Switch)
    (fp_text reference S1 (at -1.245 0 90) (layer F.SilkS) hide)
    (fp_text value L102021ML04Q (at -1.245 0 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -7.62 4.75) (size 2.775 2.775) (drill 1.85) (layers *.Cu *.Mask F.SilkS)
      (net 43 "Net-(S1-Pad1)"))
    (pad 2 thru_hole circle (at -7.62 -4.75) (size 2.775 2.775) (drill 1.85) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(J2-Pad1)"))
    (pad 3 thru_hole circle (at -7.62 0) (size 2.775 2.775) (drill 1.85) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(C1-Pad1)"))
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 196.5 94.275 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C1 (at 0 -1.43 -90) (layer F.SilkS) hide)
    (fp_text value "1 uF" (at 0 1.43 -90) (layer F.Fab))
    (fp_text user %R (at 0 0 -90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 188.6 94.3 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C2 (at 0 -1.43 270) (layer F.SilkS) hide)
    (fp_text value "1 uF" (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VCC))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 167.7 92.025 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C3 (at 0 -1.43 90) (layer F.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VCC))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBE)
    (at 198.1 83.775 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C4 (at 0 1.43 90) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.43 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 182 92.025 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C5 (at 0 -1.43 90) (layer F.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VCC))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B4B45C9)
    (at 190.7 104.2 90)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (attr smd)
    (fp_text reference D1 (at 0 -1.43 90) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(D1-Pad1)"))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 56D1B4CB)
    (at 163.3 72.8)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference H1 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 56D1B4CB)
    (at 206.1 72.7)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference H2 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 56D1B4CB)
    (at 163.4 104.7)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference H3 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 56D1B4CB)
    (at 206 104.7)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference H4 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module 1-1734592-4:TE_1-1734592-4 (layer F.Cu) (tedit 5E169627)
    (at 192.9 88.7 180)
    (fp_text reference J1 (at -4.04944 -1.70629) (layer F.SilkS) hide)
    (fp_text value "right ribbon" (at 0.28252 5.1008) (layer F.Fab))
    (pad 1 smd rect (at -3.25 0 180) (size 0.3 1.1) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J1-Pad1)"))
    (pad 2 smd rect (at -2.75 0 180) (size 0.3 1.1) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J1-Pad2)"))
    (pad 3 smd rect (at -2.25 0 180) (size 0.3 1.1) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J1-Pad3)"))
    (pad 4 smd rect (at -1.75 0 180) (size 0.3 1.1) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J1-Pad4)"))
    (pad 5 smd rect (at -1.25 0 180) (size 0.3 1.1) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J1-Pad5)"))
    (pad 6 smd rect (at -0.75 0 180) (size 0.3 1.1) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J1-Pad6)"))
    (pad 7 smd rect (at -0.25 0 180) (size 0.3 1.1) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(J1-Pad7)"))
    (pad 8 smd rect (at 0.25 0 180) (size 0.3 1.1) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(J1-Pad8)"))
    (pad 9 smd rect (at 0.75 0 180) (size 0.3 1.1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 10 smd rect (at 1.25 0 180) (size 0.3 1.1) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(J1-Pad10)"))
    (pad 11 smd rect (at 1.75 0 180) (size 0.3 1.1) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(J1-Pad11)"))
    (pad 12 smd rect (at 2.25 0 180) (size 0.3 1.1) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(J1-Pad12)"))
    (pad 13 smd rect (at 2.75 0 180) (size 0.3 1.1) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(J1-Pad13)"))
    (pad 14 smd rect (at 3.25 0 180) (size 0.3 1.1) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(J1-Pad14)"))
    (pad S1 smd rect (at -4.92 1.7 180) (size 2.3 3.1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad S2 smd rect (at 4.92 1.7 180) (size 2.3 3.1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module 1-1734592-0:TE_1-1734592-0 (layer B.Cu) (tedit 5E1685EA)
    (at 165.7 85.92 90)
    (fp_text reference J3 (at -2.329175 1.888395 90) (layer B.SilkS) hide)
    (fp_text value "left ribbon" (at 3.39419 -6.003415 90) (layer B.Fab))
    (pad 1 smd rect (at -2.25 0 90) (size 0.3 1.1) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(J3-Pad1)"))
    (pad 2 smd rect (at -1.75 0 90) (size 0.3 1.1) (layers B.Cu B.Paste B.Mask)
      (net 21 "Net-(J3-Pad2)"))
    (pad 3 smd rect (at -1.25 0 90) (size 0.3 1.1) (layers B.Cu B.Paste B.Mask)
      (net 22 "Net-(J3-Pad3)"))
    (pad 4 smd rect (at -0.75 0 90) (size 0.3 1.1) (layers B.Cu B.Paste B.Mask)
      (net 23 "Net-(J3-Pad4)"))
    (pad 5 smd rect (at -0.25 0 90) (size 0.3 1.1) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(J3-Pad5)"))
    (pad 6 smd rect (at 0.25 0 90) (size 0.3 1.1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 7 smd rect (at 0.75 0 90) (size 0.3 1.1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 8 smd rect (at 1.25 0 90) (size 0.3 1.1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 9 smd rect (at 1.75 0 90) (size 0.3 1.1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 10 smd rect (at 2.25 0 90) (size 0.3 1.1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad S1 smd rect (at -3.92 -1.7 90) (size 2.3 3.1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad S2 smd rect (at 3.92 -1.7 90) (size 2.3 3.1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 172.2 78.6 90)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference J4 (at 1.27 -2.33 90) (layer F.SilkS) hide)
    (fp_text value AVR-ISP-6 (at 1.27 7.41 90) (layer F.Fab))
    (fp_text user %R (at 1.27 2.54 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(J3-Pad2)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(J3-Pad1)"))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(J3-Pad3)"))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(J4-Pad5)"))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Horizontal (layer F.Cu) (tedit 59FED5CB)
    (at 180.5 103.3 270)
    (descr "Through hole angled pin header, 1x06, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x06 2.54mm single row")
    (fp_text reference J5 (at 4.385 -2.27 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x06 (at 4.385 14.97 90) (layer F.Fab))
    (fp_text user %R (at 2.77 6.35) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(J5-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(J5-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 "Net-(J5-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 "Net-(J5-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(J4-Pad5)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector:ps2_connector (layer F.Cu) (tedit 5EAF6840)
    (at 213.5 88.8 270)
    (fp_text reference J6 (at 0 0.5 90) (layer F.SilkS) hide)
    (fp_text value "PS2 Controller" (at 0 -0.5 90) (layer F.Fab))
    (pad 5 connect rect (at 0 3 270) (size 2 4) (layers F.Cu F.Mask)
      (net 3 VCC))
    (pad 4 connect rect (at -4 3 270) (size 2 4) (layers F.Cu F.Mask)
      (net 28 "Net-(J6-Pad4)"))
    (pad 3 connect rect (at -8 3 270) (size 2 4) (layers F.Cu F.Mask)
      (net 29 "Net-(J6-Pad3)"))
    (pad 2 connect rect (at -12 3 270) (size 2 4) (layers F.Cu F.Mask)
      (net 30 "Net-(J6-Pad2)"))
    (pad 1 connect rect (at -16 3 270) (size 2 4) (layers F.Cu F.Mask)
      (net 31 "Net-(J6-Pad1)"))
    (pad 6 connect rect (at 4 3 270) (size 2 4) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 7 connect rect (at 8 3 270) (size 2 4) (layers F.Cu F.Mask)
      (net 32 "Net-(J6-Pad7)"))
    (pad 8 connect rect (at 12 3 270) (size 2 4) (layers F.Cu F.Mask)
      (net 33 "Net-(J6-Pad8)"))
    (pad 9 connect rect (at 16 3 270) (size 2 4) (layers F.Cu F.Mask)
      (net 34 "Net-(J6-Pad9)"))
    (pad 10 connect rect (at 0 3 270) (size 4 4) (layers B.Cu B.Mask)
      (net 1 GND))
  )
  (module 1-1734592-0:TE_1-1734592-0 (layer B.Cu) (tedit 5E1685EA)
    (at 165.7 96.98 90)
    (fp_text reference J7 (at -2.329175 1.888395 -90) (layer B.SilkS) hide)
    (fp_text value "center ribbon" (at 3.39419 -6.003415 -90) (layer B.Fab))
    (pad S2 smd rect (at 3.92 -1.7 90) (size 2.3 3.1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad S1 smd rect (at -3.92 -1.7 90) (size 2.3 3.1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 10 smd rect (at 2.25 0 90) (size 0.3 1.1) (layers B.Cu B.Paste B.Mask)
      (net 51 "Net-(J7-Pad10)"))
    (pad 9 smd rect (at 1.75 0 90) (size 0.3 1.1) (layers B.Cu B.Paste B.Mask)
      (net 50 "Net-(J5-Pad5)"))
    (pad 8 smd rect (at 1.25 0 90) (size 0.3 1.1) (layers B.Cu B.Paste B.Mask)
      (net 49 "Net-(J5-Pad4)"))
    (pad 7 smd rect (at 0.75 0 90) (size 0.3 1.1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 0.25 0 90) (size 0.3 1.1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 5 smd rect (at -0.25 0 90) (size 0.3 1.1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -0.75 0 90) (size 0.3 1.1) (layers B.Cu B.Paste B.Mask)
      (net 35 "Net-(J7-Pad4)"))
    (pad 3 smd rect (at -1.25 0 90) (size 0.3 1.1) (layers B.Cu B.Paste B.Mask)
      (net 36 "Net-(J7-Pad3)"))
    (pad 2 smd rect (at -1.75 0 90) (size 0.3 1.1) (layers B.Cu B.Paste B.Mask)
      (net 37 "Net-(J7-Pad2)"))
    (pad 1 smd rect (at -2.25 0 90) (size 0.3 1.1) (layers B.Cu B.Paste B.Mask)
      (net 38 "Net-(J7-Pad1)"))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 190.5 77.9 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J8 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value Analog (at 0 7.41 90) (layer F.Fab))
    (fp_text user %R (at 0 2.3 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 "Net-(J8-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 "Net-(J8-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 "Net-(J8-Pad3)"))
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm (layer F.Cu) (tedit 5B391E66)
    (at 174.8 83.5)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP2 (at 0 -1.8) (layer F.SilkS) hide)
    (fp_text value SolderJumper_2_Open (at 0 1.9) (layer F.Fab))
    (pad 1 smd custom (at -0.65 0) (size 1 0.5) (layers F.Cu F.Mask)
      (net 1 GND) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy 0.5 -0.75) (xy 0.5 0.75) (xy 0 0.75)) (width 0))
      ))
    (pad 2 smd custom (at 0.65 0) (size 1 0.5) (layers F.Cu F.Mask)
      (net 42 "Net-(JP2-Pad2)") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy -0.5 -0.75) (xy -0.5 0.75) (xy 0 0.75)) (width 0))
      ))
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 195.5 104.275 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 68 (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-5 (layer F.Cu) (tedit 5A02FF57)
    (at 192.9 94.25 180)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U1 (at 0 -2.9 180) (layer F.SilkS) hide)
    (fp_text value MIC5504-3.3YM5 (at 0 2.9 180) (layer F.Fab))
    (fp_text user %R (at 0 0 -90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at -1.1 0 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.1 0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 4 smd rect (at 1.1 0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(U1-Pad4)"))
    (pad 5 smd rect (at 1.1 -0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_QFP:TQFP-32_7x7mm_P0.8mm (layer F.Cu) (tedit 5A02F146)
    (at 174.8 92 180)
    (descr "32-Lead Plastic Thin Quad Flatpack (PT) - 7x7x1.0 mm Body, 2.00 mm [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (attr smd)
    (fp_text reference U2 (at 0 -6.05) (layer F.SilkS) hide)
    (fp_text value ATmega328PB-AU (at 0 6.05) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -4.25 -2.8 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(J6-Pad4)"))
    (pad 2 smd rect (at -4.25 -2 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(J6-Pad8)"))
    (pad 3 smd rect (at -4.25 -1.2 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(J6-Pad9)"))
    (pad 4 smd rect (at -4.25 -0.4 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 5 smd rect (at -4.25 0.4 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -4.25 1.2 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D1-Pad2)"))
    (pad 7 smd rect (at -4.25 2 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J1-Pad5)"))
    (pad 8 smd rect (at -4.25 2.8 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(J1-Pad10)"))
    (pad 9 smd rect (at -2.8 4.25 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(J1-Pad11)"))
    (pad 10 smd rect (at -2 4.25 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(J1-Pad12)"))
    (pad 11 smd rect (at -1.2 4.25 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(J1-Pad13)"))
    (pad 12 smd rect (at -0.4 4.25 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(J1-Pad14)"))
    (pad 13 smd rect (at 0.4 4.25 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(J3-Pad5)"))
    (pad 14 smd rect (at 1.2 4.25 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(J3-Pad4)"))
    (pad 15 smd rect (at 2 4.25 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(J3-Pad3)"))
    (pad 16 smd rect (at 2.8 4.25 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(J3-Pad2)"))
    (pad 17 smd rect (at 4.25 2.8 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(J3-Pad1)"))
    (pad 18 smd rect (at 4.25 2 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 19 smd rect (at 4.25 1.2 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(JP2-Pad2)"))
    (pad 20 smd rect (at 4.25 0.4 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(U2-Pad20)"))
    (pad 21 smd rect (at 4.25 -0.4 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 22 smd rect (at 4.25 -1.2 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(J7-Pad10)"))
    (pad 23 smd rect (at 4.25 -2 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(J7-Pad4)"))
    (pad 24 smd rect (at 4.25 -2.8 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(J7-Pad3)"))
    (pad 25 smd rect (at 2.8 -4.25 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(J7-Pad2)"))
    (pad 26 smd rect (at 2 -4.25 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(J7-Pad1)"))
    (pad 27 smd rect (at 1.2 -4.25 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(U2-Pad27)"))
    (pad 28 smd rect (at 0.4 -4.25 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(U2-Pad28)"))
    (pad 29 smd rect (at -0.4 -4.25 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(J4-Pad5)"))
    (pad 30 smd rect (at -1.2 -4.25 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(J5-Pad5)"))
    (pad 31 smd rect (at -2 -4.25 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(J5-Pad4)"))
    (pad 32 smd rect (at -2.8 -4.25 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(J6-Pad3)"))
    (model ${KISYS3DMOD}/Package_QFP.3dshapes/TQFP-32_7x7mm_P0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MCP4651-103E_ST:SOP65P640X120-14N (layer B.Cu) (tedit 5E13DE35)
    (at 193.2 83.9)
    (fp_text reference U3 (at 0.63588 4.09506 180) (layer B.SilkS) hide)
    (fp_text value MCP4651-103E_ST (at 12.13581 -3.99439 180) (layer B.Fab))
    (fp_text user * (at -3.66254 2.18735 180) (layer B.Fab))
    (pad 1 smd rect (at -2.8194 1.9558) (size 1.4732 0.3556) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -2.8194 1.2954) (size 1.4732 0.3556) (layers B.Cu B.Paste B.Mask)
      (net 47 "Net-(U2-Pad28)"))
    (pad 3 smd rect (at -2.8194 0.6604) (size 1.4732 0.3556) (layers B.Cu B.Paste B.Mask)
      (net 46 "Net-(U2-Pad27)"))
    (pad 4 smd rect (at -2.8194 0) (size 1.4732 0.3556) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 5 smd rect (at -2.8194 -0.6604) (size 1.4732 0.3556) (layers B.Cu B.Paste B.Mask)
      (net 40 "Net-(J8-Pad2)"))
    (pad 6 smd rect (at -2.8194 -1.2954) (size 1.4732 0.3556) (layers B.Cu B.Paste B.Mask)
      (net 39 "Net-(J8-Pad1)"))
    (pad 7 smd rect (at -2.8194 -1.9558) (size 1.4732 0.3556) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 8 smd rect (at 2.8194 -1.9558) (size 1.4732 0.3556) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 9 smd rect (at 2.8194 -1.2954) (size 1.4732 0.3556) (layers B.Cu B.Paste B.Mask)
      (net 41 "Net-(J8-Pad3)"))
    (pad 10 smd rect (at 2.8194 -0.6604) (size 1.4732 0.3556) (layers B.Cu B.Paste B.Mask)
      (net 40 "Net-(J8-Pad2)"))
    (pad 11 smd rect (at 2.8194 0) (size 1.4732 0.3556) (layers B.Cu B.Paste B.Mask)
      (net 48 "Net-(U3-Pad11)"))
    (pad 12 smd rect (at 2.8194 0.6604) (size 1.4732 0.3556) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 13 smd rect (at 2.8194 1.2954) (size 1.4732 0.3556) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 14 smd rect (at 2.8194 1.9558) (size 1.4732 0.3556) (layers B.Cu B.Paste B.Mask)
      (net 3 VCC))
  )
  (gr_text 0.1uF (at 199.5 83.8 270) (layer B.SilkS))
  (gr_text ??? (at 172.6 83.5 90) (layer F.SilkS))
  (gr_text Y (at 195.6 75.7) (layer B.SilkS))
  (gr_text H (at 193 75.7) (layer B.SilkS))
  (gr_text X (at 190.5 75.7) (layer B.SilkS))
  (gr_text 5v (at 204.4 73.8) (layer F.SilkS))
  (gr_text GND (at 179.6 76.1) (layer F.SilkS))
  (gr_text ISP (at 174.8 80.9) (layer F.SilkS))
  (gr_text CENTER (at 167.5 97 270) (layer B.SilkS))
  (gr_text LEFT (at 167.5 85.9 270) (layer B.SilkS))
  (gr_text SERIAL (at 174.2 101.2) (layer F.SilkS))
  (gr_text RIGHT (at 192.9 90.3) (layer F.SilkS))
  (gr_text 1uF (at 197.8 94.3 90) (layer F.SilkS))
  (gr_text 1uF (at 187.4 94.3 90) (layer F.SilkS))
  (gr_text 0.1uF (at 166.4 92 90) (layer F.SilkS))
  (gr_text 0.1uF (at 183.3 92 90) (layer F.SilkS))
  (gr_text 68Ω (at 196.8 104.2 90) (layer F.SilkS))
  (gr_text LED (at 189.2 104.3 90) (layer F.SilkS))
  (gr_text - (at 205.6 80.8) (layer F.SilkS))
  (gr_text + (at 203 80.8) (layer F.SilkS))
  (gr_text OUT (at 200 79.1) (layer F.SilkS))
  (gr_text IN (at 200.8 76) (layer F.SilkS))
  (gr_line (start 160.6 70.2) (end 212.7 70) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 160.6 107.4) (end 160.6 70.2) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 212.6 107.3) (end 160.6 107.4) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 212.7 70) (end 212.6 107.3) (layer Edge.Cuts) (width 0.1))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 209.8 102.8) (xy 180.2 101.4) (xy 179.8 80.6) (xy 179.8 80.5) (xy 210 77.8)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 212.6 107.3) (xy 160.6 107.3) (xy 160.7 70.3) (xy 212.6 70)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 212.5 107.3) (xy 160.6 107.3) (xy 160.7 70.2) (xy 212.7 69.9)
      )
    )
  )
)
