(kicad_pcb (version 20171130) (host pcbnew 5.0.0+dfsg1-2)
  (general
    (thickness 1.6)
    (drawings 46)
    (tracks 93)
    (zones 0)
    (modules 20)
    (nets 1)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.6)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.6)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module WaterSensorProngs (layer B.Cu) (tedit 5BB992DA)
    (at 139.7 135.255)
    (fp_text reference REF** (at 0 -30.48) (layer B.SilkS) hide)
    (fp_text value WaterSensorProngs (at 0 20.32) (layer B.Fab))
    (pad 2 smd trapezoid (at 0 0 180) (size 7 50.8) (rect_delta 14 0 ) (drill (offset 3.5 0)) (layers B.Cu B.Paste B.Mask))
    (pad 1 smd trapezoid (at -25.4 0) (size 7 50.8) (rect_delta 14 0 ) (drill (offset 3.5 0)) (layers B.Cu B.Paste B.Mask))
  )
  (module WaterSensorProngs (layer F.Cu) (tedit 5BB992DA)
    (at 139.7 135.255)
    (fp_text reference REF** (at 0 30.48) (layer F.SilkS) hide)
    (fp_text value WaterSensorProngs (at 0 -20.32) (layer F.Fab))
    (pad 1 smd trapezoid (at -25.4 0) (size 7 50.8) (rect_delta 14 0 ) (drill (offset 3.5 0)) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd trapezoid (at 0 0 180) (size 7 50.8) (rect_delta 14 0 ) (drill (offset 3.5 0)) (layers F.Cu F.Paste F.Mask))
  )
  (module LOGO (layer F.Cu) (tedit 0)
    (at 127 93.345)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module LOGO (layer F.Cu) (tedit 0)
    (at 127 93.345)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module cr2032 (layer B.Cu) (tedit 5BB93E97)
    (at 127 97.155 90)
    (fp_text reference BAT1 (at 0 10.16 90) (layer B.SilkS))
    (fp_text value cr2032 (at 0 17.78 90) (layer B.Fab))
    (pad 1 smd rect (at 12.7 0 90) (size 2.54 5.08) (drill (offset -1.27 0)) (layers B.Cu B.Paste B.Mask))
    (pad 1 smd rect (at -12.7 0 90) (size 2.54 5.08) (drill (offset 1.27 0)) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd circle (at 0 0 90) (size 17.78 17.78) (layers B.Cu B.Paste B.Mask))
  )
  (module LED_THT:LED_Rectangular_W5.0mm_H2.0mm (layer F.Cu) (tedit 5BB93A71)
    (at 125.73 33.02)
    (descr "LED_Rectangular, Rectangular,  Rectangular size 5.0x2.0mm^2, 2 pins, http://www.kingbright.com/attachments/file/psearch/000/00/00/L-169XCGDK(Ver.9B).pdf")
    (tags "LED_Rectangular Rectangular  Rectangular size 5.0x2.0mm^2 2 pins")
    (fp_text reference LED1 (at 1.27 -2.06) (layer F.SilkS))
    (fp_text value LED_Rectangular_W5.0mm_H2.0mm (at 1.27 2.06) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_Rectangular_W5.0mm_H2.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Vertical (layer F.Cu) (tedit 5BB94511)
    (at 129.54 37.465)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R10 (at 7.62 0) (layer F.SilkS))
    (fp_text value R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Vertical (at 2.54 1.92) (layer F.Fab))
    (fp_text user %R (at 2.54 -1.92) (layer F.Fab))
    (pad 2 thru_hole oval (at 5.08 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_A-405_P5.08mm_Vertical_KathodeUp (layer F.Cu) (tedit 5BBA708D)
    (at 126.365 46.355 90)
    (descr "Diode, A-405 series, Axial, Vertical, pin pitch=5.08mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/A-405.pdf")
    (tags "Diode A-405 series Axial Vertical pin pitch 5.08mm  length 5.2mm diameter 2.7mm")
    (fp_text reference D1 (at 8.255 0 90) (layer F.SilkS))
    (fp_text value D_A-405_P5.08mm_Vertical_KathodeUp (at 2.54 2.47 90) (layer F.Fab))
    (fp_text user K (at 6.985 1.905 270) (layer F.SilkS) hide)
    (fp_text user K (at 1.6 0.9 90) (layer F.Fab))
    (fp_text user %R (at 2.54 -2.47 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_A-405_P5.08mm_Vertical_KathodeUp.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Vertical (layer F.Cu) (tedit 5BB94509)
    (at 129.54 45.085)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R8 (at 7.62 0) (layer F.SilkS))
    (fp_text value R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Vertical (at 2.54 1.92) (layer F.Fab))
    (fp_text user %R (at 2.54 -1.92) (layer F.Fab))
    (pad 2 thru_hole oval (at 5.08 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Vertical (layer F.Cu) (tedit 5BB9450D)
    (at 129.54 41.275)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R9 (at 7.62 0) (layer F.SilkS))
    (fp_text value R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Vertical (at 2.54 1.92) (layer F.Fab))
    (fp_text user %R (at 2.54 -1.92) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 5.08 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Vertical (layer F.Cu) (tedit 5BB94506)
    (at 129.54 48.895)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R7 (at 7.62 0) (layer F.SilkS))
    (fp_text value R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Vertical (at 2.54 1.92) (layer F.Fab))
    (fp_text user %R (at 2.54 -1.92) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 5.08 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Vertical (layer F.Cu) (tedit 5BB91C63)
    (at 119.38 75.565 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R1 (at -2.54 0 180) (layer F.SilkS))
    (fp_text value R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Vertical (at 2.54 1.92 90) (layer F.Fab))
    (fp_text user %R (at 2.54 -1.92 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Vertical (layer F.Cu) (tedit 5BB94500)
    (at 123.19 55.245 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R6 (at 7.62 0 90) (layer F.SilkS))
    (fp_text value R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Vertical (at 2.54 1.92 90) (layer F.Fab))
    (fp_text user %R (at 2.54 -1.92 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Vertical (layer F.Cu) (tedit 5BB944F8)
    (at 123.19 62.865 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R5 (at 2.54 1.905 90) (layer F.SilkS))
    (fp_text value R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Vertical (at 2.54 1.92 90) (layer F.Fab))
    (fp_text user %R (at 2.54 -1.92 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-8_W7.62mm (layer F.Cu) (tedit 5BB944ED)
    (at 127 52.705)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U2 (at 10.16 0) (layer F.SilkS))
    (fp_text value DIP-8_W7.62mm (at 3.81 9.95) (layer F.Fab))
    (fp_text user %R (at 3.81 3.81) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-8_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Vertical (layer F.Cu) (tedit 5BB944E4)
    (at 123.19 70.485 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R3 (at 2.54 -1.905 90) (layer F.SilkS))
    (fp_text value R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Vertical (at 2.54 1.92 90) (layer F.Fab))
    (fp_text user %R (at 2.54 -1.92 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Vertical (layer F.Cu) (tedit 5BB944E0)
    (at 123.19 78.105 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R2 (at -2.54 0 180) (layer F.SilkS))
    (fp_text value R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Vertical (at 2.54 1.92 90) (layer F.Fab))
    (fp_text user %R (at 2.54 -1.92 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-8_W7.62mm (layer F.Cu) (tedit 5BB91C75)
    (at 127 67.945)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U1 (at 10.16 0) (layer F.SilkS))
    (fp_text value DIP-8_W7.62mm (at 3.81 9.95) (layer F.Fab))
    (fp_text user %R (at 3.81 3.81) (layer F.Fab))
    (pad 8 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-8_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Vertical (layer F.Cu) (tedit 5BB944E9)
    (at 129.54 79.375)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R4 (at 2.54 2.54) (layer F.SilkS))
    (fp_text value R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Vertical (at 2.54 1.92) (layer F.Fab))
    (fp_text user %R (at 2.54 -1.92) (layer F.Fab))
    (pad 2 thru_hole oval (at 5.08 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5BB944D4)
    (at 119.38 60.325 90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C1 (at 2.5 -2.5 90) (layer F.SilkS))
    (fp_text value C_Disc_D5.0mm_W2.5mm_P5.00mm (at 2.5 2.5 90) (layer F.Fab))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 121.92 121.285) (end 121.92 130.175) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 123.19 131.445) (end 121.92 130.175) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 121.92 133.985) (end 123.19 131.445) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 123.19 135.255) (end 121.92 133.985) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 121.92 137.795) (end 123.19 135.255) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 123.19 139.065) (end 121.92 137.795) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 121.92 141.605) (end 123.19 139.065) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 123.19 142.875) (end 121.92 141.605) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 121.92 145.415) (end 123.19 142.875) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 123.19 146.685) (end 121.92 145.415) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 121.92 149.225) (end 123.19 146.685) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 123.19 150.495) (end 121.92 149.225) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 121.92 153.035) (end 123.19 150.495) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 132.08 121.285) (end 132.08 130.175) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 130.81 131.445) (end 132.08 130.175) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 132.08 133.985) (end 130.81 131.445) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 130.81 135.255) (end 132.08 133.985) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 132.08 137.795) (end 130.81 135.255) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 130.81 139.065) (end 132.08 137.795) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 132.08 141.605) (end 130.81 139.065) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 130.81 142.875) (end 132.08 141.605) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 132.08 145.415) (end 130.81 142.875) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 130.81 146.685) (end 132.08 145.415) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 132.08 149.225) (end 130.81 146.685) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 130.81 150.495) (end 132.08 149.225) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 132.08 153.035) (end 130.81 150.495) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 114.3 168.275) (end 121.92 153.035) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 114.3 161.925) (end 114.3 168.275) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 139.7 168.275) (end 139.7 161.925) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 132.08 153.035) (end 139.7 168.275) (layer Edge.Cuts) (width 0.15))
  (gr_text "Water plant\nwhen \nflashing" (at 134.62 33.02) (layer B.SilkS))
  (gr_text "Water plant\nwhen \nflashing" (at 134.62 33.02) (layer F.SilkS))
  (gr_text "Ellie D. Martin-Eberhardt\ngithub.com/diodelass/florablinker" (at 120.015 40.005 90) (layer B.SilkS))
  (gr_text "FloraBlinker v0.5" (at 117.475 40.005 90) (layer B.SilkS))
  (gr_text "FloraBlinker v0.5" (at 117.475 40.005 90) (layer F.SilkS))
  (gr_text "Ellie D. Martin-Eberhardt\ngithub.com/diodelass/florablinker" (at 120.015 40.005 90) (layer F.SilkS))
  (gr_line (start 121.92 112.395) (end 121.92 121.285) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 132.08 121.285) (end 132.08 112.395) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 127 117.475) (end 132.08 112.395) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 121.92 112.395) (end 127 117.475) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 114.3 161.925) (end 114.3 97.155) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 139.7 160.655) (end 139.7 161.925) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 139.7 97.155) (end 139.7 160.655) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 114.3 28.575) (end 114.3 97.155) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 139.7 28.575) (end 114.3 28.575) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 139.7 97.155) (end 139.7 28.575) (layer Edge.Cuts) (width 0.2))
)
