(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (title_block
    (title "Eurorack State-Variable Filter")
    (date "2022-11-23")
    (rev "1.2")
    (company "Len Popp")
    (comment 1 "Copyright © 2022 Len Popp CC BY")
    (comment 2 "Board settings comply with requirements of OSH Park https://oshpark.com/")
    (comment 3 "CEM3320 state-variable VCF module - Eurorack 10HP")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0.0508)
    (pcbplotparams
      (layerselection 0x00010f0_ffffffff)
      (disableapertmacros false)
      (usegerberextensions true)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile false)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers/controls/")
    )
  )
  (net 0 "")
  (net 1 "+12V")
  (net 2 "GND")
  (net 3 "OUT-HP")
  (net 4 "Net-(J4-PadT)")
  (net 5 "OUT-LP")
  (net 6 "IN-AUDIO")
  (net 7 "CV-FREQ-1VOCT")
  (net 8 "IN-CV-BUS")
  (net 9 "Net-(J3-PadT)")
  (net 10 "CV-RES-MOD-N")
  (net 11 "unconnected-(J6-PadTN)")
  (net 12 "OUT-AUDIO-LP-HP")
  (net 13 "unconnected-(J5-PadTN)")
  (net 14 "OUT-AUDIO-BP")
  (net 15 "CV-FREQ-POT")
  (net 16 "CV-FREQ-MOD")
  (net 17 "CV-RES-POT")
  (net 18 "OUT-LP-HP")
  (net 19 "CV-RES-MOD-P")
  (net 20 "Net-(J5-PadT)")
  (net 21 "Net-(J6-PadT)")
  (footprint "-lmp-synth:Jack_3.5mm_QingPu_WQP-PJ398SM_Vertical" (layer "F.Cu")
    (tedit 622780AA)
    (at 106.58 118.2878)
    (descr "TS mono 3.5mm, vertical, Thonkiconn, PCB mount, (http://www.qingpu-electronics.com/en/products/WQP-PJ398SM-362.html)")
    (tags "WQP-PJ398SM WQP-PJ301M-12 TS 3.5mm mono vertical jack thonkiconn qingpu")
    (property "Distributor" "Thonk")
    (property "Distributor2" "SynthCube")
    (property "Distributor3" "Adafruit")
    (property "DistributorPartLink" "https://www.thonk.co.uk/shop/thonkiconn/")
    (property "DistributorPartLink2" "https://synthcube.com/cart/3-5mm-euro-jacks")
    (property "DistributorPartLink3" "https://www.adafruit.com/product/4031")
    (property "DistributorPartNum" "PJ398SM")
    (property "DistributorPartNum2" "WQP518MA")
    (property "DistributorPartNum3" "4031")
    (property "Label" "IN-AUDIO")
    (property "Manufacturer" "QingPu / Thonk")
    (property "ManufacturerPartNum" "PJ398SM / WQP518MA")
    (property "Sheetfile" "PanelPower.kicad_sch")
    (property "Sheetname" "PanelPower")
    (attr through_hole)
    (fp_text reference "J1" (at -4.03 1.08) (layer "F.SilkS"))
    (fp_text value "WQP-PJ398" (at 0 5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 8) (layer "F.Fab"))
    (pad "S" thru_hole oval (at 0 0 180) (size 2.75 1.75) (drill oval 1.65 0.65) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (pad "T" thru_hole oval (at 0 11.4 180) (size 2.75 1.75) (drill oval 1.65 0.65) (layers *.Cu *.Mask)
      (net 6 "IN-AUDIO") (pintype "passive"))
    (pad "TN" thru_hole oval (at 0 3.1 180) (size 2.75 1.75) (drill oval 1.65 0.65) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD_USER_3DMODEL_DIR}/AudioJacks.3dshapes/PJ398SM.step"
      (offset (xyz 0 -6.45 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (footprint "-lmp-synth:Potentiometer_Alpha_RD901F-40-00D_Single_Vertical" (layer "F.Cu")
    (tedit 62126752)
    (at 122.936 55.144 90)
    (descr "Potentiometer, Alpha, RD901F, vertical, 9mm, single, http://www.taiwanalpha.com.tw/downloads?target=products&id=113")
    (tags "potentiometer vertical 9mm single")
    (property "Distributor" "Thonk")
    (property "Distributor2" "Mouser")
    (property "Distributor3" "SynthCube")
    (property "DistributorPartLink" "https://www.thonk.co.uk/shop/alpha-9mm-pots/")
    (property "DistributorPartLink2" "https://www.mouser.ca/c/passive-components/potentiometers-trimmers-rheostats/potentiometers/?q=RD901F&orientation=Vertical")
    (property "DistributorPartLink3" "https://synthcube.com/cart/alpha-9mm-potentiometer-right-angle-pcb-mount-6-35mm-round-shaft")
    (property "DistributorPartNum" "Group_Pot_Alpha_6.35mm")
    (property "DistributorPartNum2" "311-1940F-*")
    (property "DistributorPartNum3" "9MMALPHAPOTMSTR")
    (property "Label" "CUTOFF")
    (property "Manufacturer" "Alpha")
    (property "ManufacturerPartNum" "RD901F-*")
    (property "Sheetfile" "PanelPower.kicad_sch")
    (property "Sheetname" "PanelPower")
    (property "Value2" "LIN")
    (attr through_hole)
    (fp_text reference "RV1" (at -2.286 2.4892) (layer "F.SilkS"))
    (fp_text value "100K" (at 0 9.86 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 7.62 2.54 90) (layer "F.Fab"))
    (pad "" thru_hole oval (at 7.5 7.3 180) (size 2.72 3.24) (drill oval 1.1 1.8) (layers *.Cu *.Mask))
    (pad "" thru_hole oval (at 7.5 -2.3 180) (size 2.72 3.24) (drill oval 1.1 1.8) (layers *.Cu *.Mask))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 2.5 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 15 "CV-FREQ-POT") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at 0 5 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 "+12V") (pinfunction "3") (pintype "passive"))
    (model "${KICAD_USER_3DMODEL_DIR}/RD901F-40-15R1-B100K-00DL1.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (footprint "-lmp-synth:Potentiometer_Alpha_RD901F-40-00D_Single_Vertical" (layer "F.Cu")
    (tedit 62126752)
    (at 134.29 86.497 90)
    (descr "Potentiometer, Alpha, RD901F, vertical, 9mm, single, http://www.taiwanalpha.com.tw/downloads?target=products&id=113")
    (tags "potentiometer vertical 9mm single")
    (property "Distributor" "Thonk")
    (property "Distributor2" "Mouser")
    (property "Distributor3" "SynthCube")
    (property "DistributorPartLink" "https://www.thonk.co.uk/shop/alpha-9mm-pots/")
    (property "DistributorPartLink2" "https://www.mouser.ca/c/passive-components/potentiometers-trimmers-rheostats/potentiometers/?q=RD901F&orientation=Vertical")
    (property "DistributorPartLink3" "https://synthcube.com/cart/alpha-9mm-potentiometer-right-angle-pcb-mount-6-35mm-round-shaft")
    (property "DistributorPartNum" "Group_Pot_Alpha_6.35mm")
    (property "DistributorPartNum2" "311-1940F-*")
    (property "DistributorPartNum3" "9MMALPHAPOTMSTR")
    (property "Label" "RESONANCE")
    (property "Manufacturer" "Alpha")
    (property "ManufacturerPartNum" "RD901F-*")
    (property "Sheetfile" "PanelPower.kicad_sch")
    (property "Sheetname" "PanelPower")
    (property "Value2" "LIN")
    (attr through_hole)
    (fp_text reference "RV3" (at -2.413 2.4892) (layer "F.SilkS"))
    (fp_text value "100K" (at 0 9.86 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 7.62 2.54 90) (layer "F.Fab"))
    (pad "" thru_hole oval (at 7.5 -2.3 180) (size 2.72 3.24) (drill oval 1.1 1.8) (layers *.Cu *.Mask))
    (pad "" thru_hole oval (at 7.5 7.3 180) (size 2.72 3.24) (drill oval 1.1 1.8) (layers *.Cu *.Mask))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 "+12V") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 2.5 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 17 "CV-RES-POT") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at 0 5 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "3") (pintype "passive"))
    (model "${KICAD_USER_3DMODEL_DIR}/RD901F-40-15R1-B100K-00DL1.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (footprint "-lmp-synth:Potentiometer_SongHuei_Single_Vertical" (layer "F.Cu")
    (tedit 62126785)
    (at 111.53225 75.497 90)
    (descr "Potentiometer, Song Huei, R0904N, vertical, 9mm, single, ")
    (tags "potentiometer vertical 9mm single")
    (property "Distributor" "SynthCube")
    (property "Distributor2" "Thonk")
    (property "Distributor3" "SynthCube")
    (property "DistributorPartLink" "https://synthcube.com/cart/9mm-trimmer-pots")
    (property "DistributorPartLink2" "https://www.thonk.co.uk/shop/ttpots/")
    (property "DistributorPartLink3" "https://synthcube.com/cart/alpha-9mm-potentiometer-right-angle-pcb-mount-6-35mm-round-shaft")
    (property "DistributorPartNum" "SH9MMTPOTMSTR")
    (property "DistributorPartNum2" "Group_SongHuei_TTP")
    (property "DistributorPartNum3" "9MMALPHAPOTMSTR")
    (property "Label" "CV-FREQ-AMT")
    (property "Manufacturer" "Song Huei")
    (property "ManufacturerPartNum" "R0904N*")
    (property "Sheetfile" "PanelPower.kicad_sch")
    (property "Sheetname" "PanelPower")
    (property "Value2" "LIN")
    (attr through_hole)
    (fp_text reference "RV2" (at -2.276 2.51375 180) (layer "F.SilkS"))
    (fp_text value "100K" (at 0 9.86 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 7.62 2.54 90) (layer "F.Fab"))
    (pad "" thru_hole oval (at 7.5 -2.3 180) (size 2.72 3.24) (drill oval 1.5 2) (layers *.Cu *.Mask))
    (pad "" thru_hole oval (at 7.5 7.3 180) (size 2.72 3.24) (drill oval 1.5 2) (layers *.Cu *.Mask))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 2.5 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 16 "CV-FREQ-MOD") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at 0 5 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J3-PadT)") (pinfunction "3") (pintype "passive"))
    (model "${KICAD_USER_3DMODEL_DIR}/RD901F-40-15R1-B100K-00DL1.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (footprint "-lmp-synth:Potentiometer_SongHuei_Single_Vertical" (layer "F.Cu")
    (tedit 62126785)
    (at 134.29 106.68 90)
    (descr "Potentiometer, Song Huei, R0904N, vertical, 9mm, single, ")
    (tags "potentiometer vertical 9mm single")
    (property "Distributor" "SynthCube")
    (property "Distributor2" "Thonk")
    (property "Distributor3" "SynthCube")
    (property "DistributorPartLink" "https://synthcube.com/cart/9mm-trimmer-pots")
    (property "DistributorPartLink2" "https://www.thonk.co.uk/shop/ttpots/")
    (property "DistributorPartLink3" "https://synthcube.com/cart/alpha-9mm-potentiometer-right-angle-pcb-mount-6-35mm-round-shaft")
    (property "DistributorPartNum" "SH9MMTPOTMSTR")
    (property "DistributorPartNum2" "Group_SongHuei_TTP")
    (property "DistributorPartNum3" "9MMALPHAPOTMSTR")
    (property "Label" "CV-RES-AMT")
    (property "Manufacturer" "Song Huei")
    (property "ManufacturerPartNum" "R0904N*")
    (property "Sheetfile" "PanelPower.kicad_sch")
    (property "Sheetname" "PanelPower")
    (property "Value2" "LIN")
    (attr through_hole)
    (fp_text reference "RV4" (at -2.286 2.489 180) (layer "F.SilkS"))
    (fp_text value "100K" (at 0 9.86 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 7.62 2.54 90) (layer "F.Fab"))
    (pad "" thru_hole oval (at 7.5 -2.3 180) (size 2.72 3.24) (drill oval 1.5 2) (layers *.Cu *.Mask))
    (pad "" thru_hole oval (at 7.5 7.3 180) (size 2.72 3.24) (drill oval 1.5 2) (layers *.Cu *.Mask))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 19 "CV-RES-MOD-P") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 2.5 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J4-PadT)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at 0 5 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 10 "CV-RES-MOD-N") (pinfunction "3") (pintype "passive"))
    (model "${KICAD_USER_3DMODEL_DIR}/RD901F-40-15R1-B100K-00DL1.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (footprint "-lmp-synth:Jack_3.5mm_QingPu_WQP-PJ398SM_Vertical" (layer "F.Cu")
    (tedit 622780AA)
    (at 119.13 118.2878)
    (descr "TS mono 3.5mm, vertical, Thonkiconn, PCB mount, (http://www.qingpu-electronics.com/en/products/WQP-PJ398SM-362.html)")
    (tags "WQP-PJ398SM WQP-PJ301M-12 TS 3.5mm mono vertical jack thonkiconn qingpu")
    (property "Distributor" "Thonk")
    (property "Distributor2" "SynthCube")
    (property "Distributor3" "Adafruit")
    (property "DistributorPartLink" "https://www.thonk.co.uk/shop/thonkiconn/")
    (property "DistributorPartLink2" "https://synthcube.com/cart/3-5mm-euro-jacks")
    (property "DistributorPartLink3" "https://www.adafruit.com/product/4031")
    (property "DistributorPartNum" "PJ398SM")
    (property "DistributorPartNum2" "WQP518MA")
    (property "DistributorPartNum3" "4031")
    (property "Label" "IN-CV-FREQ-1VOCT")
    (property "Manufacturer" "QingPu / Thonk")
    (property "ManufacturerPartNum" "PJ398SM / WQP518MA")
    (property "Sheetfile" "PanelPower.kicad_sch")
    (property "Sheetname" "PanelPower")
    (attr through_hole)
    (fp_text reference "J2" (at -4.03 1.08) (layer "F.SilkS"))
    (fp_text value "WQP-PJ398" (at 0 5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 8) (layer "F.Fab"))
    (pad "S" thru_hole oval (at 0 0 180) (size 2.75 1.75) (drill oval 1.65 0.65) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (pad "T" thru_hole oval (at 0 11.4 180) (size 2.75 1.75) (drill oval 1.65 0.65) (layers *.Cu *.Mask)
      (net 7 "CV-FREQ-1VOCT") (pintype "passive"))
    (pad "TN" thru_hole oval (at 0 3.1 180) (size 2.75 1.75) (drill oval 1.65 0.65) (layers *.Cu *.Mask)
      (net 8 "IN-CV-BUS") (pintype "passive"))
    (model "${KICAD_USER_3DMODEL_DIR}/AudioJacks.3dshapes/PJ398SM.step"
      (offset (xyz 0 -6.45 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (footprint "-lmp-synth:Jack_3.5mm_QingPu_WQP-PJ398SM_Vertical" (layer "F.Cu")
    (tedit 622780AA)
    (at 131.63 118.2878)
    (descr "TS mono 3.5mm, vertical, Thonkiconn, PCB mount, (http://www.qingpu-electronics.com/en/products/WQP-PJ398SM-362.html)")
    (tags "WQP-PJ398SM WQP-PJ301M-12 TS 3.5mm mono vertical jack thonkiconn qingpu")
    (property "Distributor" "Thonk")
    (property "Distributor2" "SynthCube")
    (property "Distributor3" "Adafruit")
    (property "DistributorPartLink" "https://www.thonk.co.uk/shop/thonkiconn/")
    (property "DistributorPartLink2" "https://synthcube.com/cart/3-5mm-euro-jacks")
    (property "DistributorPartLink3" "https://www.adafruit.com/product/4031")
    (property "DistributorPartNum" "PJ398SM")
    (property "DistributorPartNum2" "WQP518MA")
    (property "DistributorPartNum3" "4031")
    (property "Label" "IN-CV-FREQ-MOD")
    (property "Manufacturer" "QingPu / Thonk")
    (property "ManufacturerPartNum" "PJ398SM / WQP518MA")
    (property "Sheetfile" "PanelPower.kicad_sch")
    (property "Sheetname" "PanelPower")
    (attr through_hole)
    (fp_text reference "J3" (at -4.03 1.08) (layer "F.SilkS"))
    (fp_text value "WQP-PJ398" (at 0 5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 8) (layer "F.Fab"))
    (pad "S" thru_hole oval (at 0 0 180) (size 2.75 1.75) (drill oval 1.65 0.65) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (pad "T" thru_hole oval (at 0 11.4 180) (size 2.75 1.75) (drill oval 1.65 0.65) (layers *.Cu *.Mask)
      (net 9 "Net-(J3-PadT)") (pintype "passive"))
    (pad "TN" thru_hole oval (at 0 3.1 180) (size 2.75 1.75) (drill oval 1.65 0.65) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD_USER_3DMODEL_DIR}/AudioJacks.3dshapes/PJ398SM.step"
      (offset (xyz 0 -6.45 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (footprint "-lmp-synth:Jack_3.5mm_QingPu_WQP-PJ398SM_Vertical" (layer "F.Cu")
    (tedit 622780AA)
    (at 144.33 118.2878)
    (descr "TS mono 3.5mm, vertical, Thonkiconn, PCB mount, (http://www.qingpu-electronics.com/en/products/WQP-PJ398SM-362.html)")
    (tags "WQP-PJ398SM WQP-PJ301M-12 TS 3.5mm mono vertical jack thonkiconn qingpu")
    (property "Distributor" "Thonk")
    (property "Distributor2" "SynthCube")
    (property "Distributor3" "Adafruit")
    (property "DistributorPartLink" "https://www.thonk.co.uk/shop/thonkiconn/")
    (property "DistributorPartLink2" "https://synthcube.com/cart/3-5mm-euro-jacks")
    (property "DistributorPartLink3" "https://www.adafruit.com/product/4031")
    (property "DistributorPartNum" "PJ398SM")
    (property "DistributorPartNum2" "WQP518MA")
    (property "DistributorPartNum3" "4031")
    (property "Label" "IN-CV-RES")
    (property "Manufacturer" "QingPu / Thonk")
    (property "ManufacturerPartNum" "PJ398SM / WQP518MA")
    (property "Sheetfile" "PanelPower.kicad_sch")
    (property "Sheetname" "PanelPower")
    (attr through_hole)
    (fp_text reference "J4" (at -4.03 1.08) (layer "F.SilkS"))
    (fp_text value "WQP-PJ398" (at 0 5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 8) (layer "F.Fab"))
    (pad "S" thru_hole oval (at 0 0 180) (size 2.75 1.75) (drill oval 1.65 0.65) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (pad "T" thru_hole oval (at 0 11.4 180) (size 2.75 1.75) (drill oval 1.65 0.65) (layers *.Cu *.Mask)
      (net 4 "Net-(J4-PadT)") (pintype "passive"))
    (pad "TN" thru_hole oval (at 0 3.1 180) (size 2.75 1.75) (drill oval 1.65 0.65) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD_USER_3DMODEL_DIR}/AudioJacks.3dshapes/PJ398SM.step"
      (offset (xyz 0 -6.45 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (footprint "-lmp-synth:Jack_3.5mm_QingPu_WQP-PJ398SM_Vertical" (layer "F.Cu")
    (tedit 622780AA)
    (at 112.855 132.334)
    (descr "TS mono 3.5mm, vertical, Thonkiconn, PCB mount, (http://www.qingpu-electronics.com/en/products/WQP-PJ398SM-362.html)")
    (tags "WQP-PJ398SM WQP-PJ301M-12 TS 3.5mm mono vertical jack thonkiconn qingpu")
    (property "Distributor" "Thonk")
    (property "Distributor2" "SynthCube")
    (property "Distributor3" "Adafruit")
    (property "DistributorPartLink" "https://www.thonk.co.uk/shop/thonkiconn/")
    (property "DistributorPartLink2" "https://synthcube.com/cart/3-5mm-euro-jacks")
    (property "DistributorPartLink3" "https://www.adafruit.com/product/4031")
    (property "DistributorPartNum" "PJ398SM")
    (property "DistributorPartNum2" "WQP518MA")
    (property "DistributorPartNum3" "4031")
    (property "Label" "OUT-AUDIO-LP-HP")
    (property "Manufacturer" "QingPu / Thonk")
    (property "ManufacturerPartNum" "PJ398SM / WQP518MA")
    (property "Sheetfile" "PanelPower.kicad_sch")
    (property "Sheetname" "PanelPower")
    (attr through_hole)
    (fp_text reference "J5" (at -4.03 1.08) (layer "F.SilkS"))
    (fp_text value "WQP-PJ398" (at 0 5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 8) (layer "F.Fab"))
    (pad "S" thru_hole oval (at 0 0 180) (size 2.75 1.75) (drill oval 1.65 0.65) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (pad "T" thru_hole oval (at 0 11.4 180) (size 2.75 1.75) (drill oval 1.65 0.65) (layers *.Cu *.Mask)
      (net 20 "Net-(J5-PadT)") (pintype "passive"))
    (pad "TN" thru_hole oval (at 0 3.1 180) (size 2.75 1.75) (drill oval 1.65 0.65) (layers *.Cu *.Mask)
      (net 13 "unconnected-(J5-PadTN)") (pintype "passive+no_connect"))
    (model "${KICAD_USER_3DMODEL_DIR}/AudioJacks.3dshapes/PJ398SM.step"
      (offset (xyz 0 -6.45 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (footprint "-lmp-misc:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 102.235 143.256 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Distributor" "Mouser")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/Vishay-Dale/CCF071K00JKE36?qs=sGAEpiMZZMsPqMdJzcrNwqw41JD0NFylHV1MADcQnpo%3D")
    (property "DistributorPartNum" "71-CCF071K00JKE36")
    (property "Manufacturer" "Vishay / Dale")
    (property "ManufacturerPartNum" "CCF071K00JKE36")
    (property "Note" "Output limiting")
    (property "Sheetfile" "PanelPower.kicad_sch")
    (property "Sheetname" "PanelPower")
    (property "Value2" "5%, 1/4 W")
    (attr through_hole)
    (fp_text reference "R31" (at 5.08 3.175) (layer "F.SilkS"))
    (fp_text value "1K" (at 5.08 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(J5-PadT)") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "OUT-AUDIO-LP-HP") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "-lmp-misc:Logo_OSHW" locked (layer "F.Cu")
    (tedit 60F495A1)
    (at 135.763 65.151)
    (descr "Open Source Hardware logo")
    (tags "Open Source Hardware logo")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "G3" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "Logo_OSHW" (at 0.75 0) (layer "F.SilkS") hide)
  )
  (footprint "-lmp-misc:Logo_CC_BY" locked (layer "F.Cu")
    (tedit 0)
    (at 144.907 65.278)
    (attr through_hole)
    (fp_text reference "G1" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "Logo_CC_BY" (at 0.75 0) (layer "F.SilkS") hide)
  )
  (footprint "-lmp-misc:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 123.19 143.256 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Distributor" "Mouser")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/Vishay-Dale/CCF071K00JKE36?qs=sGAEpiMZZMsPqMdJzcrNwqw41JD0NFylHV1MADcQnpo%3D")
    (property "DistributorPartNum" "71-CCF071K00JKE36")
    (property "Manufacturer" "Vishay / Dale")
    (property "ManufacturerPartNum" "CCF071K00JKE36")
    (property "Note" "Output limiting")
    (property "Sheetfile" "PanelPower.kicad_sch")
    (property "Sheetname" "PanelPower")
    (property "Value2" "5%, 1/4 W")
    (attr through_hole)
    (fp_text reference "R32" (at 5.08 3.175) (layer "F.SilkS"))
    (fp_text value "1K" (at 5.08 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(J6-PadT)") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "OUT-AUDIO-BP") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "-lmp-synth:Potentiometer_Alpha_RD901F-40-00D_Single_Vertical" (layer "F.Cu")
    (tedit 62126752)
    (at 111.53225 106.68 90)
    (descr "Potentiometer, Alpha, RD901F, vertical, 9mm, single, http://www.taiwanalpha.com.tw/downloads?target=products&id=113")
    (tags "potentiometer vertical 9mm single")
    (property "Distributor" "Thonk")
    (property "Distributor2" "Mouser")
    (property "Distributor3" "SynthCube")
    (property "DistributorPartLink" "https://www.thonk.co.uk/shop/alpha-9mm-pots/")
    (property "DistributorPartLink2" "https://www.mouser.ca/c/passive-components/potentiometers-trimmers-rheostats/potentiometers/?q=RD901F&orientation=Vertical")
    (property "DistributorPartLink3" "https://synthcube.com/cart/alpha-9mm-potentiometer-right-angle-pcb-mount-6-35mm-round-shaft")
    (property "DistributorPartNum" "Group_Pot_Alpha_6.35mm")
    (property "DistributorPartNum2" "311-1940F-*")
    (property "DistributorPartNum3" "9MMALPHAPOTMSTR")
    (property "Label" "LP-HP-SHAPE")
    (property "Manufacturer" "Alpha")
    (property "ManufacturerPartNum" "RD901F-*")
    (property "Sheetfile" "PanelPower.kicad_sch")
    (property "Sheetname" "PanelPower")
    (property "Value2" "LIN")
    (attr through_hole)
    (fp_text reference "RV5" (at -2.286 2.51375 180) (layer "F.SilkS"))
    (fp_text value "100K" (at 0 9.86 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 7.62 2.54 90) (layer "F.Fab"))
    (pad "" thru_hole oval (at 7.5 7.3 180) (size 2.72 3.24) (drill oval 1.1 1.8) (layers *.Cu *.Mask))
    (pad "" thru_hole oval (at 7.5 -2.3 180) (size 2.72 3.24) (drill oval 1.1 1.8) (layers *.Cu *.Mask))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 5 "OUT-LP") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 2.5 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 18 "OUT-LP-HP") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at 0 5 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 3 "OUT-HP") (pinfunction "3") (pintype "passive"))
    (model "${KICAD_USER_3DMODEL_DIR}/RD901F-40-15R1-B100K-00DL1.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (footprint "-lmp-synth:Jack_3.5mm_QingPu_WQP-PJ398SM_Vertical" (layer "F.Cu")
    (tedit 622780AA)
    (at 137.98 132.334)
    (descr "TS mono 3.5mm, vertical, Thonkiconn, PCB mount, (http://www.qingpu-electronics.com/en/products/WQP-PJ398SM-362.html)")
    (tags "WQP-PJ398SM WQP-PJ301M-12 TS 3.5mm mono vertical jack thonkiconn qingpu")
    (property "Distributor" "Thonk")
    (property "Distributor2" "SynthCube")
    (property "Distributor3" "Adafruit")
    (property "DistributorPartLink" "https://www.thonk.co.uk/shop/thonkiconn/")
    (property "DistributorPartLink2" "https://synthcube.com/cart/3-5mm-euro-jacks")
    (property "DistributorPartLink3" "https://www.adafruit.com/product/4031")
    (property "DistributorPartNum" "PJ398SM")
    (property "DistributorPartNum2" "WQP518MA")
    (property "DistributorPartNum3" "4031")
    (property "Label" "OUT-AUDIO-BP")
    (property "Manufacturer" "QingPu / Thonk")
    (property "ManufacturerPartNum" "PJ398SM / WQP518MA")
    (property "Sheetfile" "PanelPower.kicad_sch")
    (property "Sheetname" "PanelPower")
    (attr through_hole)
    (fp_text reference "J6" (at -4.03 1.08) (layer "F.SilkS"))
    (fp_text value "WQP-PJ398" (at 0 5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 8) (layer "F.Fab"))
    (pad "S" thru_hole oval (at 0 0 180) (size 2.75 1.75) (drill oval 1.65 0.65) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (pad "T" thru_hole oval (at 0 11.4 180) (size 2.75 1.75) (drill oval 1.65 0.65) (layers *.Cu *.Mask)
      (net 21 "Net-(J6-PadT)") (pintype "passive"))
    (pad "TN" thru_hole oval (at 0 3.1 180) (size 2.75 1.75) (drill oval 1.65 0.65) (layers *.Cu *.Mask)
      (net 11 "unconnected-(J6-PadTN)") (pintype "passive+no_connect"))
    (model "${KICAD_USER_3DMODEL_DIR}/AudioJacks.3dshapes/PJ398SM.step"
      (offset (xyz 0 -6.45 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (footprint "-lmp-holes:MountingHole_PCB_3.2mm_M3" locked (layer "F.Cu")
    (tedit 622675F6)
    (at 129.5702 134.112)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm m3")
    (property "Sheetfile" "PanelPower.kicad_sch")
    (property "Sheetname" "PanelPower")
    (property "exclude_from_bom" "")
    (clearance 1.15)
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "H2" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_M3" (at 0 0.009) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "-lmp-holes:MountingHole_PCB_3.2mm_M3" locked (layer "F.Cu")
    (tedit 622675F6)
    (at 103.632 54.61)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm m3")
    (property "Sheetfile" "PanelPower.kicad_sch")
    (property "Sheetname" "PanelPower")
    (property "exclude_from_bom" "")
    (clearance 1.15)
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "H1" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_M3" (at 0 0.009) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x15_P2.54mm_Vertical" (layer "B.Cu")
    (tedit 5A19A41D)
    (at 101.6 59.69 180)
    (descr "Through hole straight socket strip, 1x15, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x15 2.54mm single row")
    (property "Distributor" "Adafruit")
    (property "Distributor2" "Mouser")
    (property "DistributorPartLink" "https://www.adafruit.com/product/598")
    (property "DistributorPartLink2" "https://www.mouser.ca/ProductDetail/Wurth-Elektronik/61303211821?qs=ZtY9WdtwX55M%2FH%2FSrHZ9xA%3D%3D")
    (property "DistributorPartNum" "598")
    (property "DistributorPartNum2" "710-61303211821")
    (property "Sheetfile" "PanelPower.kicad_sch")
    (property "Sheetname" "PanelPower")
    (attr through_hole)
    (fp_text reference "J10" (at -0.508 -37.973) (layer "B.SilkS"))
    (fp_text value "Conn_Front_Left_Top" (at 0 -38.33) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -17.78 90) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "+12V") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "CV-FREQ-POT") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "CV-RES-POT") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "CV-RES-MOD-N") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "CV-RES-MOD-P") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "CV-FREQ-MOD") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "CV-FREQ-1VOCT") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 0 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "OUT-HP") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval (at 0 -20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "OUT-LP-HP") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval (at 0 -22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "OUT-LP") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole oval (at 0 -25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "IN-CV-BUS") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole oval (at 0 -27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "IN-AUDIO") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole oval (at 0 -30.48 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "OUT-AUDIO-BP") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole oval (at 0 -33.02 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "OUT-AUDIO-LP-HP") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" thru_hole oval (at 0 -35.56 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_15") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x15_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 150.83 42.164) (end 150.83 145.034) (layer "Edge.Cuts") (width 0.1524))
  (gr_line (start 150.83 145.034) (end 100.33 145.034) (layer "Edge.Cuts") (width 0.1524))
  (gr_line (start 100.33 42.164) (end 150.83 42.164) (layer "Edge.Cuts") (width 0.1524))
  (gr_line (start 100.33 145.034) (end 100.33 42.164) (layer "Edge.Cuts") (width 0.1524))
  (gr_text "https://len42.github.io/Synth/" (at 149.225 61.341) (layer "F.SilkS"))
  (gr_text "rev ${REVISION}" (at 149.225 57.277) (layer "F.SilkS"))
  (gr_text "© 2022 Len Popp" (at 149.225 59.309) (layer "F.SilkS"))
  (gr_text "SV-VCF" (at 149.225 52.705) (layer "F.SilkS"))
  (gr_text "Controls" (at 149.225 55.245) (layer "F.SilkS"))
  (zone (net 2) (net_name "GND") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2032))
    (min_thickness 0.2032) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.381) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 151.765 145.415)
        (xy 99.695 145.415)
        (xy 99.695 41.021)
        (xy 151.765 41.021)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 137.9516 140.3555)
        (xy 138.4151 140.2821)
        (xy 138.8333 140.069)
        (xy 139.1651 139.7372)
        (xy 139.3782 139.319)
        (xy 139.4516 138.8555)
        (xy 139.3782 138.392)
        (xy 139.1651 137.9738)
        (xy 138.8333 137.642)
        (xy 138.4151 137.4289)
        (xy 137.9516 137.3555)
        (xy 137.4881 137.4289)
        (xy 137.0699 137.642)
        (xy 136.7381 137.9738)
        (xy 136.525 138.392)
        (xy 136.4516 138.8555)
        (xy 136.525 139.319)
        (xy 136.7381 139.7372)
        (xy 137.0699 140.069)
        (xy 137.4881 140.2821)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 106.640839 126.269529)
        (xy 107.104339 126.196129)
        (xy 107.522539 125.983029)
        (xy 107.854339 125.651229)
        (xy 108.067439 125.233029)
        (xy 108.140839 124.769529)
        (xy 108.067439 124.306029)
        (xy 107.854339 123.887829)
        (xy 107.522539 123.556029)
        (xy 107.104339 123.342929)
        (xy 106.640839 123.269529)
        (xy 106.177339 123.342929)
        (xy 105.759139 123.556029)
        (xy 105.427339 123.887829)
        (xy 105.214239 124.306029)
        (xy 105.140839 124.769529)
        (xy 105.214239 125.233029)
        (xy 105.427339 125.651229)
        (xy 105.759139 125.983029)
        (xy 106.177339 126.196129)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 144.296 126.214)
        (xy 144.7595 126.1406)
        (xy 145.1777 125.9275)
        (xy 145.5095 125.5957)
        (xy 145.7226 125.1775)
        (xy 145.796 124.714)
        (xy 145.7226 124.2505)
        (xy 145.5095 123.8323)
        (xy 145.1777 123.5005)
        (xy 144.7595 123.2874)
        (xy 144.296 123.214)
        (xy 143.8325 123.2874)
        (xy 143.4143 123.5005)
        (xy 143.0825 123.8323)
        (xy 142.8694 124.2505)
        (xy 142.796 124.714)
        (xy 142.8694 125.1775)
        (xy 143.0825 125.5957)
        (xy 143.4143 125.9275)
        (xy 143.8325 126.1406)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 119.1556 126.269529)
        (xy 119.6191 126.196129)
        (xy 120.0373 125.983029)
        (xy 120.3691 125.651229)
        (xy 120.5822 125.233029)
        (xy 120.6556 124.769529)
        (xy 120.5822 124.306029)
        (xy 120.3691 123.887829)
        (xy 120.0373 123.556029)
        (xy 119.6191 123.342929)
        (xy 119.1556 123.269529)
        (xy 118.6921 123.342929)
        (xy 118.2739 123.556029)
        (xy 117.9421 123.887829)
        (xy 117.729 124.306029)
        (xy 117.6556 124.769529)
        (xy 117.729 125.233029)
        (xy 117.9421 125.651229)
        (xy 118.2739 125.983029)
        (xy 118.6921 126.196129)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 112.8957 140.315729)
        (xy 113.3592 140.242329)
        (xy 113.7774 140.029229)
        (xy 114.1092 139.697429)
        (xy 114.3223 139.279229)
        (xy 114.3957 138.815729)
        (xy 114.3223 138.352229)
        (xy 114.1092 137.934029)
        (xy 113.7774 137.602229)
        (xy 113.3592 137.389129)
        (xy 112.8957 137.315729)
        (xy 112.4322 137.389129)
        (xy 112.014 137.602229)
        (xy 111.6822 137.934029)
        (xy 111.4691 138.352229)
        (xy 111.3957 138.815729)
        (xy 111.4691 139.279229)
        (xy 111.6822 139.697429)
        (xy 112.014 140.029229)
        (xy 112.4322 140.242329)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 131.6165 126.294929)
        (xy 132.08 126.221529)
        (xy 132.4982 126.008429)
        (xy 132.83 125.676629)
        (xy 133.0431 125.258429)
        (xy 133.1165 124.794929)
        (xy 133.0431 124.331429)
        (xy 132.83 123.913229)
        (xy 132.4982 123.581429)
        (xy 132.08 123.368329)
        (xy 131.6165 123.294929)
        (xy 131.153 123.368329)
        (xy 130.7348 123.581429)
        (xy 130.403 123.913229)
        (xy 130.1899 124.331429)
        (xy 130.1165 124.794929)
        (xy 130.1899 125.258429)
        (xy 130.403 125.676629)
        (xy 130.7348 126.008429)
        (xy 131.153 126.221529)
      )
    )
  )
)
