(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 16)
    (no_connects 0)
    (area 111.049999 95.809999 127.075001 110.565001)
    (thickness 1.6)
    (drawings 18)
    (tracks 46)
    (zones 0)
    (modules 4)
    (nets 9)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.3048)
    (user_trace_width 0.4064)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad2)")
  (net 2 "Net-(J1-Pad4)")
  (net 3 "Net-(J1-Pad1)")
  (net 4 "Net-(J1-Pad3)")
  (net 5 "Net-(J2-Pad1)")
  (net 6 "Net-(J2-Pad2)")
  (net 7 "Net-(J2-Pad3)")
  (net 8 "Net-(J2-Pad4)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad4)")
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 5D82A55C)
    (at 114.3 99.06)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value CONN_01X04 (at 0 9.95) (layer F.Fab))
    (fp_text user %R (at 0 3.81 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad4)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 5D82A54D)
    (at 116.84 100.33)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value CONN_01X04 (at 0 9.95) (layer F.Fab))
    (fp_text user %R (at 0 3.81 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J2-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J2-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J2-Pad4)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_SH_SM08B-SRSS-TB_08x1.00mm_Angled (layer B.Cu) (tedit 5D82A4B4)
    (at 123.19 102.87 270)
    (descr http://www.jst-mfg.com/product/pdf/eng/eSH.pdf)
    (tags "connector jst sh")
    (attr smd)
    (fp_text reference J3 (at -3.5 4 270) (layer B.SilkS) hide)
    (fp_text value CONN_01X08 (at 0 -4.5 270) (layer B.Fab))
    (pad 1 smd rect (at -3.5 1.9375 270) (size 0.6 1.55) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(J1-Pad1)"))
    (pad 2 smd rect (at -2.5 1.9375 270) (size 0.6 1.55) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(J2-Pad1)"))
    (pad 3 smd rect (at -1.5 1.9375 270) (size 0.6 1.55) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(J1-Pad2)"))
    (pad 4 smd rect (at -0.5 1.9375 270) (size 0.6 1.55) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(J2-Pad2)"))
    (pad 5 smd rect (at 0.5 1.9375 270) (size 0.6 1.55) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(J1-Pad3)"))
    (pad 6 smd rect (at 1.5 1.9375 270) (size 0.6 1.55) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(J2-Pad3)"))
    (pad 7 smd rect (at 2.5 1.9375 270) (size 0.6 1.55) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(J1-Pad4)"))
    (pad 8 smd rect (at 3.5 1.9375 270) (size 0.6 1.55) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(J2-Pad4)"))
    (pad "" smd rect (at -4.8 -1.9375 270) (size 1.2 1.8) (layers B.Cu B.Paste B.Mask))
    (pad "" smd rect (at 4.8 -1.9375 270) (size 1.2 1.8) (layers B.Cu B.Paste B.Mask))
  )
  (module Connectors_JST:JST_SH_BM08B-SRSS-TB_08x1.00mm_Straight (layer F.Cu) (tedit 5D82A4AE)
    (at 123.19 102.87 270)
    (descr http://www.jst-mfg.com/product/pdf/eng/eSH.pdf)
    (tags "connector jst sh")
    (attr smd)
    (fp_text reference J4 (at -3.5 -3.5 270) (layer F.SilkS) hide)
    (fp_text value CONN_01X08 (at 0 3.5 270) (layer F.Fab))
    (pad 1 smd rect (at -3.5 1.2625 270) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad1)"))
    (pad 2 smd rect (at -2.5 1.2625 270) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J2-Pad1)"))
    (pad 3 smd rect (at -1.5 1.2625 270) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J1-Pad2)"))
    (pad 4 smd rect (at -0.5 1.2625 270) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J2-Pad2)"))
    (pad 5 smd rect (at 0.5 1.2625 270) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-Pad3)"))
    (pad 6 smd rect (at 1.5 1.2625 270) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J2-Pad3)"))
    (pad 7 smd rect (at 2.5 1.2625 270) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad4)"))
    (pad 8 smd rect (at 3.5 1.2625 270) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J2-Pad4)"))
    (pad "" smd rect (at -4.8 -1.2625 270) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask))
    (pad "" smd rect (at 4.8 -1.2625 270) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask))
  )
  (gr_line (start 124.46 110.49) (end 113.665 110.49) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 113.665 95.885) (end 124.46 95.885) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "JST SH 8POS" (at 118.745 109.855) (layer F.SilkS))
  (gr_text "JST SH 8POS" (at 118.745 109.855) (layer B.SilkS))
  (gr_text BM08B-SRSS (at 118.11 97.155) (layer B.SilkS))
  (gr_text SM08B-SRSS (at 118.11 97.155) (layer F.SilkS))
  (gr_text "2\n4\n6\n8" (at 118.745 104.14) (layer B.SilkS))
  (gr_text "1\n3\n5\n7" (at 112.395 102.87) (layer B.SilkS))
  (gr_text "2\n4\n6\n8" (at 118.745 104.14) (layer F.SilkS))
  (gr_text "1\n3\n5\n7" (at 112.395 102.87) (layer F.SilkS))
  (gr_line (start 111.125 99.06) (end 111.125 98.425) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 127 99.06) (end 127 98.425) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 127 107.95) (end 127 99.06) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 111.125 99.06) (end 111.125 107.95) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 113.665 107.95) (end 113.665 110.49) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 124.46 107.95) (end 127 107.95) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 124.46 98.425) (end 124.46 95.885) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 113.665 98.425) (end 111.125 98.425) (angle 90) (layer Edge.Cuts) (width 0.15))
)
