<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="12.68" y2="0" width="0" layer="20"/>
<wire x1="12.68" y1="0" x2="12.68" y2="12.37" width="0" layer="20"/>
<wire x1="12.68" y1="12.37" x2="0" y2="12.37" width="0" layer="20"/>
<wire x1="0" y1="12.37" x2="0" y2="0" width="0" layer="20"/>
<text>MAX17050
Fuel Gauge</text>
<text>rev1.3</text>
<text>OSH</text>
<text>Designed in 
Thailand
By TinLethax</text>
<text>+</text>
<text>-</text>
<text>1.V_I2C
2.SCL
3.SDA
4.GND</text>
<text>1</text>
<text>4</text>
<text>MAX17050 MOD</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X04">
<description>&lt;h3&gt;Plated Through Hole - 4 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="C1206">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="R2512">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="max17050">
<description>MAX17050</description>
<packages>
<package name="BGA9C40P3X3_145X147X69N">
<description>9-BGA, collapsing, 0.40 mm pitch, 1.46 X 1.47 X 0.69 mm body
&lt;p&gt;9-pin collapsing BGA package with 0.40 mm col pitch and 0.40 mm row pitch with body size 1.46 X 1.47 X 0.69 mm&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="testpad">
<description>&lt;b&gt;Test Pins/Pads&lt;/b&gt;&lt;p&gt;
Cream on SMD OFF.&lt;br&gt;
new: Attribute TP_SIGNAL_NAME&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TP10R">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="BAT" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-09696"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="adafruit" package="C1206" value="0.1uf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="adafruit" package="C1206" value="0.1uf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="I2C" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-09696"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="adafruit" package="R2512" value="10m">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="adafruit" package="R0603" value="4.7k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="adafruit" package="R0603" value="4.7k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="max17050" package="BGA9C40P3X3_145X147X69N" value="MAX17050">
<attribute name="NAME"/>
<attribute name="PART_NO" value="MAX17050"/>
<attribute name="VALUE"/>
</element>
<element name="ALRT" library="testpad" package="TP10R" value="TPSQTP10R">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="I2C_SCL">
<contactref element="U1" pad="A2"/>
<contactref element="R2" pad="1"/>
<contactref element="I2C" pad="2"/>
</signal>
<signal name="I2C_SDA">
<contactref element="U1" pad="C1"/>
<contactref element="R3" pad="1"/>
<contactref element="I2C" pad="3"/>
</signal>
<signal name="V_I2C">
<contactref element="R2" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="I2C" pad="1"/>
</signal>
<signal name="V-">
<contactref element="U1" pad="C3"/>
<contactref element="R1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="BAT" pad="2"/>
<contactref element="BAT" pad="1"/>
</signal>
<signal name="REG">
<contactref element="U1" pad="B3"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="VBATT">
<contactref element="C1" pad="1"/>
<contactref element="U1" pad="B1"/>
<contactref element="BAT" pad="3"/>
<contactref element="BAT" pad="4"/>
<contactref element="U1" pad="A1"/>
</signal>
<signal name="GND">
<contactref element="I2C" pad="4"/>
<contactref element="R1" pad="2"/>
<contactref element="U1" pad="A3"/>
</signal>
<signal name="ALERT">
<contactref element="U1" pad="B2"/>
<contactref element="ALRT" pad="TP"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
