(kicad_pcb (version 4) (host pcbnew "(2016-05-05 BZR 6775)-product")
  (general
    (links 133)
    (no_connects 0)
    (area 54.724999 40.224999 99.775001 85.275001)
    (thickness 1.6)
    (drawings 121)
    (tracks 668)
    (zones 0)
    (modules 59)
    (nets 36)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (1 In1.Cu signal hide)
    (2 In2.Cu signal hide)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.15)
    (user_trace_width 0.15)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.8)
    (user_trace_width 1.5)
    (trace_clearance 0.149)
    (zone_clearance 0.2)
    (zone_45_only no)
    (trace_min 0.15)
    (segment_width 0.05)
    (edge_width 0.05)
    (via_size 0.6)
    (via_drill 0.3)
    (via_min_size 0.6)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0.1)
    (pad_to_paste_clearance -0.01)
    (aux_axis_origin 54.75 40.25)
    (grid_origin 54.75 40.25)
    (visible_elements FFFEFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.020000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (psnegative false)
      (psa4output false)
      (plotreference false)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory export/ruuvitag_revb3_gerbers/))
  )
  (net 0 "")
  (net 1 VDD)
  (net 2 GND)
  (net 3 "Net-(C3-Pad1)")
  (net 4 "Net-(C4-Pad2)")
  (net 5 "Net-(C5-Pad2)")
  (net 6 "Net-(C6-Pad2)")
  (net 7 "Net-(C7-Pad1)")
  (net 8 "Net-(C11-Pad2)")
  (net 9 "Net-(C12-Pad2)")
  (net 10 "Net-(C13-Pad2)")
  (net 11 /XC1)
  (net 12 /ANTENNA)
  (net 13 /XC2)
  (net 14 /LED1)
  (net 15 "Net-(D1-Pad2)")
  (net 16 "Net-(D2-Pad2)")
  (net 17 "Net-(L1-Pad1)")
  (net 18 "Net-(L2-Pad1)")
  (net 19 /SWDIO)
  (net 20 /SWDCLK)
  (net 21 /SWO)
  (net 22 /RESET)
  (net 23 /BUTTON1)
  (net 24 /SPI_ACC_CS)
  (net 25 /SPI_HUMI_CS)
  (net 26 /ACC_INT1)
  (net 27 /SPI_MOSI)
  (net 28 /SPI_MISO)
  (net 29 /SPI_SCK)
  (net 30 "Net-(P18-Pad1)")
  (net 31 /LED2)
  (net 32 "Net-(C1-Pad1)")
  (net 33 "Net-(P10-Pad1)")
  (net 34 "Net-(P11-Pad1)")
  (net 35 /ACC_INT2)
  (net_class Default "This is the default net class."
    (clearance 0.149)
    (trace_width 0.15)
    (via_dia 0.6)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /ACC_INT1)
    (add_net /ACC_INT2)
    (add_net /ANTENNA)
    (add_net /BUTTON1)
    (add_net /LED1)
    (add_net /LED2)
    (add_net /RESET)
    (add_net /SPI_ACC_CS)
    (add_net /SPI_HUMI_CS)
    (add_net /SPI_MISO)
    (add_net /SPI_MOSI)
    (add_net /SPI_SCK)
    (add_net /SWDCLK)
    (add_net /SWDIO)
    (add_net /SWO)
    (add_net /XC1)
    (add_net /XC2)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C11-Pad2)")
    (add_net "Net-(C12-Pad2)")
    (add_net "Net-(C13-Pad2)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C4-Pad2)")
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(C6-Pad2)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(L1-Pad1)")
    (add_net "Net-(L2-Pad1)")
    (add_net "Net-(P10-Pad1)")
    (add_net "Net-(P11-Pad1)")
    (add_net "Net-(P18-Pad1)")
    (add_net VDD)
  )
  (module RuuviTag:ABG-96_POS_BATT_CONTACT (layer F.Cu) (tedit 5695E335)
    (at 66.75 52.25 135)
    (fp_text reference P5 (at 0 0 135) (layer F.SilkS))
    (fp_text value GND (at -9 0 135) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 135) (size 3 3) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KIPRJMOD}/../kicad_lib/3d/ABG96-POS.wrl
      (at (xyz -0.23 0 -0.135))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Ruuvi:RUUVI_LOGO_BENDED_RUUVITAG_REVB2 (layer F.Cu) (tedit 56934F1B)
    (at 77.22 78.59)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value RUUVI_LOGO_BENDED_RUUVITAG_REVB2 (at 0.75 0) (layer F.SilkS) hide)
  )
  (module RuuviTag:NFC_RUUVITAG_REVB2 (layer F.Cu) (tedit 5693421E)
    (at 72.42 75.96 340)
    (fp_text reference P4 (at 0 0 340) (layer F.SilkS) hide)
    (fp_text value NFC (at 0.75 0 340) (layer F.SilkS) hide)
    (pad 1 smd rect (at -12.93 -3.76 20) (size 0.18 0.18) (layers F.Cu)
      (net 6 "Net-(C6-Pad2)"))
    (pad 2 smd rect (at -11.76 -7.65 13) (size 0.2 0.2) (layers F.Cu)
      (net 7 "Net-(C7-Pad1)"))
  )
  (module RuuviTag:0402_RES (layer F.Cu) (tedit 5695EDCA)
    (at 84.5 51.5 327)
    (tags 0402)
    (attr smd)
    (fp_text reference R2 (at 0 0 327) (layer F.SilkS))
    (fp_text value 470 (at 0 0 327) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 327) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(D2-Pad2)"))
    (pad 2 smd rect (at 0.55 0 327) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RuuviTag:0402_RES (layer F.Cu) (tedit 5695EDCA)
    (at 70 51.5 212)
    (tags 0402)
    (attr smd)
    (fp_text reference R1 (at 0 0 212) (layer F.SilkS))
    (fp_text value 470 (at 0 0 212) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 212) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(D1-Pad2)"))
    (pad 2 smd rect (at 0.55 0 212) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RuuviTag:0402_IND (layer F.Cu) (tedit 5695EDCA)
    (at 83.23 46.31 340)
    (tags 0402)
    (attr smd)
    (fp_text reference L3 (at 0 0 340) (layer F.SilkS))
    (fp_text value 3n9 (at 0 0 340) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 340) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0.55 0 340) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 12 /ANTENNA))
    (model Diodes_SMD.3dshapes/SMA_Standard.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module RuuviTag:0603_IND (layer F.Cu) (tedit 5691107A)
    (at 73.24 41.57 11)
    (tags 0603)
    (attr smd)
    (fp_text reference L2 (at 0 0 11) (layer F.SilkS))
    (fp_text value 10u (at 0 0 11) (layer F.Fab))
    (pad 1 smd rect (at -0.7 0 11) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(L2-Pad1)"))
    (pad 2 smd rect (at 0.7 0 11) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(L1-Pad1)"))
    (model Diodes_SMD.3dshapes/SMA_Standard.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.12 0.12 0.12))
      (rotate (xyz 0 0 0))
    )
  )
  (module RuuviTag:0402_IND (layer F.Cu) (tedit 5695EDCA)
    (at 75.24 41.13 5)
    (tags 0402)
    (attr smd)
    (fp_text reference L1 (at 0 0 5) (layer F.SilkS))
    (fp_text value 15n (at 0 0 5) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 5) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(L1-Pad1)"))
    (pad 2 smd rect (at 0.55 0 5) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (model Diodes_SMD.3dshapes/SMA_Standard.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.08 0.08 0.08))
      (rotate (xyz 0 0 0))
    )
  )
  (module RuuviTag:0402_CAP (layer F.Cu) (tedit 5695EDCA)
    (at 83.27 47.75 249)
    (tags 0402)
    (attr smd)
    (fp_text reference C19 (at 0 0 249) (layer F.SilkS))
    (fp_text value NA (at 0 0 249) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 249) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 12 /ANTENNA))
    (pad 2 smd rect (at 0.55 0 249) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RuuviTag:0603_CAP (layer F.Cu) (tedit 5691107A)
    (at 61.22 49.2 140)
    (tags 0603)
    (attr smd)
    (fp_text reference C18 (at 0 0 140) (layer F.SilkS))
    (fp_text value 4u7 (at 0 0 140) (layer F.Fab))
    (pad 1 smd rect (at -0.7 0 140) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 0.7 0 140) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RuuviTag:0402_CAP (layer F.Cu) (tedit 5695EDCA)
    (at 81.04 41.88 259.5)
    (tags 0402)
    (attr smd)
    (fp_text reference C16 (at 0 0 259.5) (layer F.SilkS))
    (fp_text value 12p (at 0 0 259.5) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 259.5) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.55 0 259.5) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 13 /XC2))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RuuviTag:0402_CAP (layer F.Cu) (tedit 5695EDCA)
    (at 85.09 43.06 248.5)
    (tags 0402)
    (attr smd)
    (fp_text reference C14 (at 0 0 248.5) (layer F.SilkS))
    (fp_text value 12p (at 0 0 248.5) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 248.5) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.55 0 248.5) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 11 /XC1))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RuuviTag:0402_CAP (layer F.Cu) (tedit 5695EDCA)
    (at 82.23 44.6 165)
    (tags 0402)
    (attr smd)
    (fp_text reference C13 (at 0 0 165) (layer F.SilkS))
    (fp_text value 100p (at 0 0 165) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 165) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.55 0 165) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C13-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RuuviTag:0402_CAP (layer F.Cu) (tedit 5695EDCA)
    (at 84.31 45.08 248.5)
    (tags 0402)
    (attr smd)
    (fp_text reference C12 (at 0 0 248.5) (layer F.SilkS))
    (fp_text value NA (at 0 0 248.5) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 248.5) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.55 0 248.5) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C12-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RuuviTag:0402_CAP (layer F.Cu) (tedit 5695EDCA)
    (at 71.2 43.37 17)
    (tags 0402)
    (attr smd)
    (fp_text reference C11 (at 0 0 17) (layer F.SilkS))
    (fp_text value 100n (at 0 0 17) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 17) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.55 0 17) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C11-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RuuviTag:0603_CAP (layer F.Cu) (tedit 5691107A)
    (at 70.84 42.19 17)
    (tags 0603)
    (attr smd)
    (fp_text reference C10 (at 0 0 17) (layer F.SilkS))
    (fp_text value 4u7 (at 0 0 17) (layer F.Fab))
    (pad 1 smd rect (at -0.7 0 17) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.7 0 17) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RuuviTag:0402_CAP (layer F.Cu) (tedit 5695EDCA)
    (at 79.64 41.13 354)
    (tags 0402)
    (attr smd)
    (fp_text reference C9 (at 0 0 354) (layer F.SilkS))
    (fp_text value 100n (at 0 0 354) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 354) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.55 0 354) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RuuviTag:0402_CAP (layer F.Cu) (tedit 5695EDCA)
    (at 74.73 49.71 12)
    (tags 0402)
    (attr smd)
    (fp_text reference C8 (at 0 0 12) (layer F.SilkS))
    (fp_text value 100n (at 0 0 12) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 12) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.55 0 12) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RuuviTag:0402_CAP (layer F.Cu) (tedit 5695EDCA)
    (at 63.75 62.75 90)
    (tags 0402)
    (attr smd)
    (fp_text reference C7 (at 0 0 90) (layer F.SilkS))
    (fp_text value NFCTUN2 (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at 0.55 0 90) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RuuviTag:0402_CAP (layer F.Cu) (tedit 5695EDCA)
    (at 62.5 62.75 270)
    (tags 0402)
    (attr smd)
    (fp_text reference C6 (at 0 0 270) (layer F.SilkS))
    (fp_text value NFCTUN1 (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.55 0 270) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C6-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RuuviTag:0402_CAP (layer F.Cu) (tedit 5695EDCA)
    (at 67.45 45.55 30)
    (tags 0402)
    (attr smd)
    (fp_text reference C5 (at 0 0 30) (layer F.SilkS))
    (fp_text value 12p (at 0 0 30) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 30) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.55 0 30) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C5-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RuuviTag:0402_CAP (layer F.Cu) (tedit 5695EDCA)
    (at 68.94 43.26 293)
    (tags 0402)
    (attr smd)
    (fp_text reference C4 (at 0 0 293) (layer F.SilkS))
    (fp_text value 12p (at 0 0 293) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 293) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.55 0 293) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C4-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RuuviTag:0402_CAP (layer F.Cu) (tedit 5695EDCA)
    (at 77.1 41.02 1)
    (tags 0402)
    (attr smd)
    (fp_text reference C3 (at 0 0 1) (layer F.SilkS))
    (fp_text value 1u (at 0 0 1) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 1) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 0.55 0 1) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RuuviTag:0402_CAP (layer F.Cu) (tedit 5695EDCA)
    (at 69.75 50 30)
    (tags 0402)
    (attr smd)
    (fp_text reference C2 (at 0 0 30) (layer F.SilkS))
    (fp_text value 100n (at 0 0 30) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 30) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 0.55 0 30) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RuuviTag:0402_CAP (layer F.Cu) (tedit 5695EDCA)
    (at 81.65 46.04 75)
    (tags 0402)
    (attr smd)
    (fp_text reference C1 (at 0 0 75) (layer F.SilkS))
    (fp_text value 0p8 (at 0 0 75) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 75) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0.55 0 75) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RuuviTag:BME280 (layer F.Cu) (tedit 569478D5)
    (at 68.75 48.25 120)
    (solder_mask_margin 0.07)
    (attr smd)
    (fp_text reference U2 (at 0 0 120) (layer F.SilkS))
    (fp_text value BME280 (at 0 0 120) (layer F.Fab))
    (pad 1 smd rect (at 1.025 -0.975 120) (size 0.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.025 -0.325 120) (size 0.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 25 /SPI_HUMI_CS))
    (pad 3 smd rect (at 1.025 0.325 120) (size 0.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 27 /SPI_MOSI))
    (pad 4 smd rect (at 1.025 0.975 120) (size 0.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 29 /SPI_SCK))
    (pad 5 smd rect (at -1.025 0.975 120) (size 0.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 28 /SPI_MISO))
    (pad 6 smd rect (at -1.025 0.325 120) (size 0.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 7 smd rect (at -1.025 -0.325 120) (size 0.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 8 smd rect (at -1.025 -0.975 120) (size 0.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (model Housings_DFN_QFN.3dshapes/DFN-8-1EP_2x2mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1.2 1.2 1.2))
      (rotate (xyz 0 0 0))
    )
  )
  (module RuuviTag:TEST_POINT_SMD_1MM (layer B.Cu) (tedit 569630FE)
    (at 69.75 49.75)
    (fp_text reference P11 (at 0 0) (layer B.SilkS))
    (fp_text value TP (at 0 0) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers B.Cu B.Mask)
      (net 34 "Net-(P11-Pad1)"))
  )
  (module RuuviTag:TEST_POINT_SMD_1MM (layer B.Cu) (tedit 569630FE)
    (at 72.5 45.5)
    (fp_text reference P10 (at 0 0) (layer B.SilkS))
    (fp_text value TP (at 0 0) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers B.Cu B.Mask)
      (net 33 "Net-(P10-Pad1)"))
  )
  (module RuuviTag:SOT-23 (layer F.Cu) (tedit 56939B92)
    (at 64.09 56.91 246)
    (descr SOT-23)
    (tags "SOT-23 SOT23")
    (attr smd)
    (fp_text reference Q1 (at 0 0 246) (layer F.SilkS))
    (fp_text value Q_PMOS_GSD (at 0 0 246) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.00076 246) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.95 1.00076 246) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 3 smd rect (at 0 -0.99822 246) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(P18-Pad1)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RuuviTag:ARM_DEBUG_CONNECTOR_10PIN (layer F.Cu) (tedit 56910E97)
    (at 58.25 62.75 90)
    (fp_text reference P1 (at 0 0 90) (layer F.SilkS))
    (fp_text value ARM_DEBUG (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -0.635 -2.54 315) (size 0.9 0.9) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 VDD))
    (pad 2 thru_hole rect (at 0.635 -2.54 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 19 /SWDIO))
    (pad 3 thru_hole rect (at -0.635 -1.27 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole rect (at 0.635 -1.27 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 20 /SWDCLK))
    (pad 5 thru_hole rect (at -0.635 0 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole rect (at 0.635 0 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 21 /SWO))
    (pad 7 thru_hole rect (at -0.635 1.27 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad 8 thru_hole rect (at 0.635 1.27 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad 9 thru_hole rect (at -0.635 2.54 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 10 thru_hole rect (at 0.635 2.54 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 22 /RESET))
  )
  (module RuuviTag:FIDUCIAL_1MM (layer F.Cu) (tedit 569630B7)
    (at 58.25 54.25)
    (fp_text reference P6 (at 0 0) (layer F.SilkS))
    (fp_text value FIDUCIAL (at 0 0) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.4) (clearance 0.5))
  )
  (module RuuviTag:FIDUCIAL_1MM (layer F.Cu) (tedit 569630B7)
    (at 86.5 44)
    (fp_text reference P7 (at 0 0) (layer F.SilkS))
    (fp_text value FIDUCIAL (at 0 0) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.4) (clearance 0.5))
  )
  (module RuuviTag:32X15MM_2PIN_CRYSTAL (layer F.Cu) (tedit 56933C54)
    (at 66.7 44.32 210)
    (fp_text reference Y1 (at 0 0 210) (layer F.SilkS))
    (fp_text value 32K (at 0 0 210) (layer F.Fab))
    (pad 1 smd rect (at -1.2 0 210) (size 0.8 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C4-Pad2)"))
    (pad 2 smd rect (at 1.2 0 210) (size 0.8 1.5) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C5-Pad2)"))
    (model Oscillators.3dshapes/KXO-200.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.15 0.1 0.15))
      (rotate (xyz 0 0 0))
    )
  )
  (module Ruuvi:OSHWMASK5MM (layer B.Cu) (tedit 0)
    (at 77.25 79.37 180)
    (solder_mask_margin 0.001)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value OSHWMASK5MM (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module RuuviTag:TEST_POINT_SMD_1MM (layer B.Cu) (tedit 569630FE)
    (at 63.25 46.5)
    (fp_text reference P2 (at 0 0) (layer B.SilkS))
    (fp_text value TP (at 0 0) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers B.Cu B.Mask)
      (net 29 /SPI_SCK))
  )
  (module RuuviTag:TEST_POINT_SMD_1MM (layer B.Cu) (tedit 569630FE)
    (at 68.5 43.5)
    (fp_text reference P3 (at 0 0) (layer B.SilkS))
    (fp_text value TP (at 0 0) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers B.Cu B.Mask)
      (net 28 /SPI_MISO))
  )
  (module RuuviTag:TEST_POINT_SMD_1MM (layer B.Cu) (tedit 569630FE)
    (at 66.25 46.75)
    (fp_text reference P12 (at 0 0) (layer B.SilkS))
    (fp_text value TP (at 0 0) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers B.Cu B.Mask)
      (net 27 /SPI_MOSI))
  )
  (module RuuviTag:TEST_POINT_SMD_1MM (layer B.Cu) (tedit 569630FE)
    (at 81.5 49.75)
    (fp_text reference P13 (at 0 0) (layer B.SilkS))
    (fp_text value TP (at 0 0) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers B.Cu B.Mask)
      (net 31 /LED2))
  )
  (module RuuviTag:TEST_POINT_SMD_1MM (layer B.Cu) (tedit 569630FE)
    (at 72.5 49.25)
    (fp_text reference P14 (at 0 0) (layer B.SilkS))
    (fp_text value TP (at 0 0) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers B.Cu B.Mask)
      (net 14 /LED1))
  )
  (module RuuviTag:TEST_POINT_SMD_1MM (layer B.Cu) (tedit 569630FE)
    (at 64.25 53.75)
    (fp_text reference P15 (at 0 0) (layer B.SilkS))
    (fp_text value TP (at 0 0) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers B.Cu B.Mask)
      (net 23 /BUTTON1))
  )
  (module RuuviTag:TEST_POINT_SMD_1MM (layer B.Cu) (tedit 569630FE)
    (at 58.25 52.75)
    (fp_text reference P16 (at 0 0) (layer B.SilkS))
    (fp_text value TP (at 0 0) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers B.Cu B.Mask)
      (net 2 GND))
  )
  (module RuuviTag:TEST_POINT_SMD_1MM (layer B.Cu) (tedit 569630FE)
    (at 58.75 56.25)
    (fp_text reference P17 (at 0 0) (layer B.SilkS))
    (fp_text value TP (at 0 0) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers B.Cu B.Mask)
      (net 1 VDD))
  )
  (module RuuviTag:TEST_POINT_SMD_1MM (layer B.Cu) (tedit 569630FE)
    (at 62.5 57.25)
    (fp_text reference P18 (at 0 0) (layer B.SilkS))
    (fp_text value TP (at 0 0) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers B.Cu B.Mask)
      (net 30 "Net-(P18-Pad1)"))
  )
  (module RuuviTag:QFN-48_6X6MM_BOTPAD locked (layer F.Cu) (tedit 56986E9A)
    (at 77.25 45.75)
    (solder_mask_margin 0.08)
    (solder_paste_margin -0.01)
    (attr smd)
    (fp_text reference U1 (at 0 0) (layer F.SilkS))
    (fp_text value nRF52832 (at 0 0) (layer F.Fab))
    (pad 49 smd rect (at 0 1.52) (size 1.52 1.52) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin -0.25) (zone_connect 0))
    (pad 49 smd rect (at 1.52 0) (size 1.52 1.52) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin -0.25) (zone_connect 0))
    (pad 49 smd rect (at -1.52 0) (size 1.52 1.52) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin -0.25) (zone_connect 0))
    (pad 49 smd rect (at 0 0) (size 1.52 1.52) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin -0.25))
    (pad 49 smd rect (at 0 -1.52) (size 1.52 1.52) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin -0.25) (zone_connect 0))
    (pad 1 smd rect (at -2.86 -2.2 90) (size 0.25 0.68) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C11-Pad2)"))
    (pad 2 smd rect (at -2.86 -1.8 90) (size 0.25 0.68) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C4-Pad2)"))
    (pad 3 smd rect (at -2.86 -1.4 90) (size 0.25 0.68) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C5-Pad2)"))
    (pad 4 smd rect (at -2.86 -1 90) (size 0.25 0.68) (layers F.Cu F.Paste F.Mask)
      (net 26 /ACC_INT1))
    (pad 5 smd rect (at -2.86 -0.6 90) (size 0.25 0.68) (layers F.Cu F.Paste F.Mask)
      (net 25 /SPI_HUMI_CS))
    (pad 6 smd rect (at -2.86 -0.2 90) (size 0.25 0.68) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(P10-Pad1)"))
    (pad 7 smd rect (at -2.86 0.2 90) (size 0.25 0.68) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(P11-Pad1)"))
    (pad 8 smd rect (at -2.86 0.6 90) (size 0.25 0.68) (layers F.Cu F.Paste F.Mask)
      (net 35 /ACC_INT2))
    (pad 9 smd rect (at -2.86 1 90) (size 0.25 0.68) (layers F.Cu F.Paste F.Mask))
    (pad 10 smd rect (at -2.86 1.4 90) (size 0.25 0.68) (layers F.Cu F.Paste F.Mask)
      (net 24 /SPI_ACC_CS))
    (pad 11 smd rect (at -2.86 1.8 90) (size 0.25 0.68) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C6-Pad2)"))
    (pad 12 smd rect (at -2.86 2.2 90) (size 0.25 0.68) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C7-Pad1)"))
    (pad 13 smd rect (at -2.2 2.86) (size 0.25 0.68) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 14 smd rect (at -1.8 2.86) (size 0.25 0.68) (layers F.Cu F.Paste F.Mask))
    (pad 15 smd rect (at -1.4 2.86) (size 0.25 0.68) (layers F.Cu F.Paste F.Mask))
    (pad 16 smd rect (at -1 2.86) (size 0.25 0.68) (layers F.Cu F.Paste F.Mask)
      (net 23 /BUTTON1))
    (pad 17 smd rect (at -0.6 2.86) (size 0.25 0.68) (layers F.Cu F.Paste F.Mask))
    (pad 18 smd rect (at -0.2 2.86) (size 0.25 0.68) (layers F.Cu F.Paste F.Mask))
    (pad 19 smd rect (at 0.2 2.86) (size 0.25 0.68) (layers F.Cu F.Paste F.Mask))
    (pad 20 smd rect (at 0.6 2.86) (size 0.25 0.68) (layers F.Cu F.Paste F.Mask)
      (net 14 /LED1))
    (pad 21 smd rect (at 1 2.86) (size 0.25 0.68) (layers F.Cu F.Paste F.Mask)
      (net 21 /SWO))
    (pad 22 smd rect (at 1.4 2.86) (size 0.25 0.68) (layers F.Cu F.Paste F.Mask)
      (net 31 /LED2))
    (pad 23 smd rect (at 1.8 2.86) (size 0.25 0.68) (layers F.Cu F.Paste F.Mask))
    (pad 24 smd rect (at 2.2 2.86) (size 0.25 0.68) (layers F.Cu F.Paste F.Mask)
      (net 22 /RESET))
    (pad 25 smd rect (at 2.86 2.2 90) (size 0.25 0.68) (layers F.Cu F.Paste F.Mask)
      (net 20 /SWDCLK))
    (pad 26 smd rect (at 2.86 1.8 90) (size 0.25 0.68) (layers F.Cu F.Paste F.Mask)
      (net 19 /SWDIO))
    (pad 27 smd rect (at 2.86 1.4 90) (size 0.25 0.68) (layers F.Cu F.Paste F.Mask))
    (pad 28 smd rect (at 2.86 1 90) (size 0.25 0.68) (layers F.Cu F.Paste F.Mask))
    (pad 29 smd rect (at 2.86 0.6 90) (size 0.25 0.68) (layers F.Cu F.Paste F.Mask))
    (pad 30 smd rect (at 2.86 0.2 90) (size 0.25 0.68) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(C1-Pad1)"))
    (pad 31 smd rect (at 2.86 -0.2 90) (size 0.25 0.68) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 32 smd rect (at 2.86 -0.6 90) (size 0.25 0.68) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C12-Pad2)"))
    (pad 33 smd rect (at 2.86 -1 90) (size 0.25 0.68) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C13-Pad2)"))
    (pad 34 smd rect (at 2.86 -1.4 90) (size 0.25 0.68) (layers F.Cu F.Paste F.Mask)
      (net 11 /XC1))
    (pad 35 smd rect (at 2.86 -1.8 90) (size 0.25 0.68) (layers F.Cu F.Paste F.Mask)
      (net 13 /XC2))
    (pad 36 smd rect (at 2.86 -2.2 90) (size 0.25 0.68) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 37 smd rect (at 2.2 -2.86) (size 0.25 0.68) (layers F.Cu F.Paste F.Mask)
      (net 27 /SPI_MOSI))
    (pad 38 smd rect (at 1.8 -2.86) (size 0.25 0.68) (layers F.Cu F.Paste F.Mask))
    (pad 39 smd rect (at 1.4 -2.86) (size 0.25 0.68) (layers F.Cu F.Paste F.Mask))
    (pad 40 smd rect (at 1 -2.86) (size 0.25 0.68) (layers F.Cu F.Paste F.Mask)
      (net 28 /SPI_MISO))
    (pad 41 smd rect (at 0.6 -2.86) (size 0.25 0.68) (layers F.Cu F.Paste F.Mask)
      (net 29 /SPI_SCK))
    (pad 42 smd rect (at 0.2 -2.86) (size 0.25 0.68) (layers F.Cu F.Paste F.Mask))
    (pad 43 smd rect (at -0.2 -2.86) (size 0.25 0.68) (layers F.Cu F.Paste F.Mask))
    (pad 44 smd rect (at -0.6 -2.86) (size 0.25 0.68) (layers F.Cu F.Paste F.Mask))
    (pad 45 smd rect (at -1 -2.86) (size 0.25 0.68) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 46 smd rect (at -1.4 -2.86) (size 0.25 0.68) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (pad 47 smd rect (at -1.8 -2.86) (size 0.25 0.68) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(L2-Pad1)"))
    (pad 48 smd rect (at -2.2 -2.86) (size 0.25 0.68) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 49 smd rect (at -1.52 -1.52) (size 1.52 1.52) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin -0.25) (zone_connect 0))
    (pad 49 smd rect (at 1.52 -1.52) (size 1.52 1.52) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin -0.25) (zone_connect 0))
    (pad 49 smd rect (at 1.52 1.52) (size 1.52 1.52) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin -0.25) (zone_connect 0))
    (pad 49 smd rect (at -1.52 1.52) (size 1.52 1.52) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin -0.25) (zone_connect 0))
    (pad 49 thru_hole circle (at -1.5 -1.5) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND))
    (pad 49 thru_hole circle (at -0.5 -1.5) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND))
    (pad 49 thru_hole circle (at 0.5 -1.5) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND))
    (pad 49 thru_hole circle (at 1.5 -1.5) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND))
    (pad 49 thru_hole circle (at -1.5 -0.5) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND))
    (pad 49 thru_hole circle (at -0.5 -0.5) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND))
    (pad 49 thru_hole circle (at 0.5 -0.5) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND))
    (pad 49 thru_hole circle (at 1.5 -0.5) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND))
    (pad 49 thru_hole circle (at -1.5 0.5) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND))
    (pad 49 thru_hole circle (at -0.5 0.5) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND))
    (pad 49 thru_hole circle (at 0.5 0.5) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND))
    (pad 49 thru_hole circle (at 1.5 0.5) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND))
    (pad 49 thru_hole circle (at -1.5 1.5) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND))
    (pad 49 thru_hole circle (at -0.5 1.5) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND))
    (pad 49 thru_hole circle (at 0.5 1.5) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND))
    (pad 49 thru_hole circle (at 1.5 1.5) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND))
    (model Housings_DFN_QFN.3dshapes/UQFN-48-1EP_6x6mm_Pitch0.4mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RuuviTag:TEST_POINT_SMD_1MM (layer B.Cu) (tedit 569630FE)
    (at 56.25 58.25)
    (fp_text reference P19 (at 0 0) (layer B.SilkS))
    (fp_text value TP (at 0 0) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers B.Cu B.Mask)
      (net 19 /SWDIO))
  )
  (module RuuviTag:TEST_POINT_SMD_1MM (layer B.Cu) (tedit 569630FE)
    (at 62.75 61.25)
    (fp_text reference P20 (at 0 0) (layer B.SilkS))
    (fp_text value TP (at 0 0) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers B.Cu B.Mask)
      (net 20 /SWDCLK))
  )
  (module RuuviTag:TEST_POINT_SMD_1MM (layer B.Cu) (tedit 569630FE)
    (at 58.75 59.75)
    (fp_text reference P21 (at 0 0) (layer B.SilkS))
    (fp_text value TP (at 0 0) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers B.Cu B.Mask)
      (net 21 /SWO))
  )
  (module RuuviTag:TEST_POINT_SMD_1MM (layer B.Cu) (tedit 569630FE)
    (at 61.25 53.75)
    (fp_text reference P22 (at 0 0) (layer B.SilkS))
    (fp_text value TP (at 0 0) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers B.Cu B.Mask)
      (net 22 /RESET))
  )
  (module RuuviTag:TEST_POINT_SMD_1MM (layer B.Cu) (tedit 569630FE)
    (at 61.5 49.25)
    (fp_text reference P23 (at 0 0) (layer B.SilkS))
    (fp_text value TP (at 0 0) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers B.Cu B.Mask)
      (net 2 GND))
  )
  (module RuuviTag:0603_LED (layer F.Cu) (tedit 56933288)
    (at 72.25 50.25 202)
    (tags "0603 LED")
    (attr smd)
    (fp_text reference D1 (at 0 0 202) (layer F.SilkS))
    (fp_text value LED1 (at 0 0 202) (layer F.Fab))
    (pad 1 smd rect (at -0.725 0 202) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 14 /LED1))
    (pad 2 smd rect (at 0.725 0 202) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(D1-Pad2)"))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RuuviTag:0603_LED (layer F.Cu) (tedit 56933288)
    (at 82.25 50.25 335)
    (tags "0603 LED")
    (attr smd)
    (fp_text reference D2 (at 0 0 335) (layer F.SilkS))
    (fp_text value LED2 (at 0 0 335) (layer F.Fab))
    (pad 1 smd rect (at -0.725 0 335) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 31 /LED2))
    (pad 2 smd rect (at 0.725 0 335) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(D2-Pad2)"))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RuuviTag:CR2450-BATTERY-3D (layer F.Cu) (tedit 56B46875)
    (at 77.25 62.75)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value CR2450-BATTERY-3D (at 0 0) (layer F.Fab) hide)
    (model ${KIPRJMOD}/../kicad_lib/3d/CR2450.wrl
      (at (xyz 0 0 0.07000000000000001))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 180 0 180))
    )
  )
  (module RuuviTag:SKRKAEE010_BUTTON (layer F.Cu) (tedit 5752FB21)
    (at 60.75 52.5 327)
    (solder_mask_margin 0.1)
    (fp_text reference SW1 (at 0 0 327) (layer F.SilkS))
    (fp_text value SW_PUSH (at 0 0 327) (layer F.Fab))
    (pad 1 smd rect (at -2.1 0 327) (size 0.8 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 2.1 0 327) (size 0.8 1.6) (layers F.Cu F.Paste F.Mask)
      (net 23 /BUTTON1))
  )
  (module RuuviTag:SKRKAEE010_BUTTON (layer F.Cu) (tedit 5752FB21)
    (at 58.5 57.25 343.5)
    (solder_mask_margin 0.1)
    (fp_text reference SW2 (at 0 0 343.5) (layer F.SilkS))
    (fp_text value SW_PUSH (at 0 0 343.5) (layer F.Fab))
    (pad 1 smd rect (at -2.1 0 343.5) (size 0.8 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 2.1 0 343.5) (size 0.8 1.6) (layers F.Cu F.Paste F.Mask)
      (net 22 /RESET))
  )
  (module RuuviTag:LGA12_2X2MM (layer F.Cu) (tedit 5752E357)
    (at 63.15 47.85 223)
    (solder_mask_margin 0.0825)
    (attr smd)
    (fp_text reference U4 (at 0 0 223) (layer F.SilkS))
    (fp_text value LIS2DH12 (at 0 0 223) (layer F.Fab))
    (pad 1 smd rect (at -0.775 -0.75 223) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 29 /SPI_SCK))
    (pad 2 smd rect (at -0.775 -0.25 223) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 24 /SPI_ACC_CS))
    (pad 3 smd rect (at -0.775 0.25 223) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 28 /SPI_MISO))
    (pad 4 smd rect (at -0.775 0.75 223) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 27 /SPI_MOSI))
    (pad 5 smd rect (at -0.25 0.75 313) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at 0.25 0.75 313) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at 0.775 0.75 223) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 8 smd rect (at 0.775 0.25 223) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 9 smd rect (at 0.775 -0.25 223) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 10 smd rect (at 0.775 -0.75 223) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 11 smd rect (at 0.25 -0.75 313) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 35 /ACC_INT2))
    (pad 12 smd rect (at -0.25 -0.75 313) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 26 /ACC_INT1))
    (model Housings_DFN_QFN.3dshapes/DFN-8-1EP_2x2mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RuuviTag:WIDE_PLATED_HOLE locked (layer F.Cu) (tedit 57540909)
    (at 69.075 54.575 225)
    (fp_text reference P8 (at 0 0 225) (layer F.SilkS))
    (fp_text value +BATT (at 0 0 225) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 225) (size 7.4 1.6) (drill oval 7 1.2) (layers *.Cu *.Mask)
      (net 30 "Net-(P18-Pad1)"))
  )
  (module RuuviTag:WIDE_PLATED_HOLE locked (layer F.Cu) (tedit 57540909)
    (at 69.075 70.925 315)
    (fp_text reference P9 (at 0 0 315) (layer F.SilkS))
    (fp_text value +BATT (at 0 0 315) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 315) (size 7.4 1.6) (drill oval 7 1.2) (layers *.Cu *.Mask)
      (net 30 "Net-(P18-Pad1)"))
  )
  (module Ruuvi:G_LOGO (layer B.Cu) (tedit 57547E72)
    (at 86.54 48.72 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value G_LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module RuuviTag:20X16MM_4PIN_CRYSTAL (layer F.Cu) (tedit 5695EE52)
    (at 83.01 42.79 74)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference Y2 (at 0 0 74) (layer F.SilkS))
    (fp_text value 32M (at 0 0 74) (layer F.Fab))
    (pad 4 smd rect (at -0.725 -0.575 74) (size 0.95 0.85) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.725 0.575 74) (size 0.95 0.85) (layers F.Cu F.Paste F.Mask)
      (net 11 /XC1))
    (pad 2 smd rect (at 0.725 0.575 74) (size 0.95 0.85) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 0.725 -0.575 74) (size 0.95 0.85) (layers F.Cu F.Paste F.Mask)
      (net 13 /XC2))
    (model Oscillators.3dshapes/KXO-200.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 85.85 71.85) (end 85.4 72.25) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 86.45 71.25) (end 85.85 71.85) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 86.6 71.1) (end 86.45 71.25) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 88.6 71.65) (end 88.6 72.65) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 87.4 71.65) (end 87.4 72.65) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 87.4 52.85) (end 87.4 53.85) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 88.6 52.85) (end 88.6 53.85) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 69.35 70.65) (end 70.7 73.4) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 66.6 69.3) (end 69.35 70.65) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 69.35 54.85) (end 70.7 52.1) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 66.6 56.2) (end 69.35 54.85) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 88.6 59.05) (end 88.6 58.75) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 88.775 59.675) (end 88.6 59.05) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 88.95 60.425) (end 88.775 59.675) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 89.075 61.175) (end 88.95 60.425) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 89.15 61.975) (end 89.075 61.175) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 89.175 62.75) (end 89.15 61.975) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 89.15 63.65) (end 89.175 62.75) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 89.05 64.5) (end 89.15 63.65) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 88.95 65.1) (end 89.05 64.5) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 88.8 65.75) (end 88.95 65.1) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 88.6 66.45) (end 88.8 65.75) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 88.6 66.75) (end 88.6 66.45) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_circle (center 88.75 45.75) (end 88.25 45.75) (layer Edge.Cuts) (width 0.05))
  (gr_circle (center 91.75 76.25) (end 91.75 76.75) (layer Edge.Cuts) (width 0.05))
  (gr_circle (center 61.75 70.75) (end 61.75 71.25) (layer Edge.Cuts) (width 0.05))
  (gr_text B3 (at 73.86 44) (layer B.Mask))
  (gr_line (start 91 68.35) (end 91 73.65) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 89.8 73.65) (end 89.8 67.75) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 91 57.15) (end 91 51.85) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 89.8 51.85) (end 89.8 57.75) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 85.9 53.7) (end 85.4 53.25) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 86.45 54.3) (end 85.9 53.7) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 86.6 54.4) (end 86.45 54.3) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 86.75 54.45) (end 86.6 54.4) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 86.8 54.45) (end 86.75 54.45) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 86.75 71.05) (end 86.6 71.1) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 86.8 71.05) (end 86.75 71.05) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 86.8 71.65) (end 86.8 71.05) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 88 72.65) (end 88 73.25) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 86.8 53.85) (end 87.4 53.85) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 88 52.85) (end 87.4 52.85) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 85.25 72.35) (end 85.4 72.25) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 88.6 66.75) (end 88.6 71.65) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 88.6 53.85) (end 88.6 58.75) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 88 52.85) (end 88 52.25) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 88 72.65) (end 88.6 72.65) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 91.75 63.85) (end 91.75 65.55) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 92.75 65.75) (end 92.75 63.85) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 92.75 59.75) (end 92.75 61.65) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 91.75 61.65) (end 91.75 59.95) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 92.25 63.85) (end 92.25 63.35) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 92.25 63.85) (end 91.75 63.85) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 92.25 61.65) (end 92.75 61.65) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 92.25 61.65) (end 92.25 62.15) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 90.55 59.95) (end 90.55 65.55) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 91 68.35) (end 91.35 68.35) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 90.4 67.15) (end 91.35 67.15) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 90.4 58.35) (end 91.35 58.35) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 91 57.15) (end 91.35 57.15) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 93.95 59.75) (end 93.95 65.75) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 91.35 59.75) (end 91.35 57.15) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 91.35 65.75) (end 93.95 65.75) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 91.35 65.75) (end 92.75 65.75) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 91.35 59.75) (end 91.35 58.35) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 90.4 73.65) (end 91 73.65) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 90.4 73.65) (end 90.4 74.25) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 90.4 67.75) (end 89.8 67.75) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 90.4 51.85) (end 90.4 51.25) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 90.4 51.85) (end 89.8 51.85) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 90.4 57.75) (end 90.4 58.35) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 91.15 65.55) (end 91.75 65.55) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 91.15 65.55) (end 91.15 66.15) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 91.15 59.95) (end 91.15 59.35) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 91.15 59.95) (end 90.55 59.95) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 64.775 61.95) (end 64.75 62.75) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 64.825 61.375) (end 64.775 61.95) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 64.975 60.375) (end 64.825 61.375) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 65.25 59.25) (end 64.975 60.375) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 65.5 58.475) (end 65.25 59.25) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 65.85 57.6) (end 65.5 58.475) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 66.225 56.85) (end 65.85 57.6) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 66.6 56.2) (end 66.225 56.85) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 71.4 51.7) (end 70.7 52.1) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 72.275 51.275) (end 71.4 51.7) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 73.325 50.875) (end 72.275 51.275) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 74.4 50.575) (end 73.325 50.875) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 75.475 50.375) (end 74.4 50.575) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 76.475 50.275) (end 75.475 50.375) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 77.25 50.25) (end 76.475 50.275) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 64.775 63.575) (end 64.75 62.75) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 64.875 64.525) (end 64.775 63.575) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 65.05 65.475) (end 64.875 64.525) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 65.3 66.425) (end 65.05 65.475) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 65.65 67.425) (end 65.3 66.425) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 66.125 68.45) (end 65.65 67.425) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 66.6 69.3) (end 66.125 68.45) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 71.475 73.85) (end 70.7 73.4) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 72.475 74.3) (end 71.475 73.85) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 73.475 74.675) (end 72.475 74.3) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 74.525 74.95) (end 73.475 74.675) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 75.475 75.125) (end 74.525 74.95) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 76.4 75.225) (end 75.475 75.125) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 77.25 75.25) (end 76.4 75.225) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 84.4 73) (end 85.25 72.35) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 83.3 73.7) (end 84.4 73) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 82.05 74.3) (end 83.3 73.7) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 80.95 74.7) (end 82.05 74.3) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 79.75 75) (end 80.95 74.7) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 78.45 75.2) (end 79.75 75) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 77.25 75.25) (end 78.45 75.2) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 84.25 52.4) (end 85.4 53.25) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 82.9 51.6) (end 84.25 52.4) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 81.4 50.95) (end 82.9 51.6) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 80 50.55) (end 81.4 50.95) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 78.45 50.3) (end 80 50.55) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 77.25 50.25) (end 78.45 50.3) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_circle (center 77.25 62.75) (end 54.75 62.75) (layer Edge.Cuts) (width 0.05))
  (gr_text ruuvi.com (at 77.13 83.02) (layer B.Mask))
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.2) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 74.75 43.25) (xy 79.75 43.25) (xy 79.75 48.25) (xy 74.75 48.25)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.2) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 78.75 40.8) (xy 79.95 40.9) (xy 81.15 41.1) (xy 82.5 41.35) (xy 84.45 41.95)
        (xy 85.05 42.15) (xy 83.901424 45.183418) (xy 83.47 45.02) (xy 82.66 44.74) (xy 81.88 44.53)
        (xy 81.15 44.37) (xy 80.49 44.26) (xy 79.55 44.11) (xy 79.55 46.65) (xy 80.27 46.76)
        (xy 81 46.93) (xy 81.71 47.11) (xy 82.58 47.37) (xy 83.012136 47.532051) (xy 81.840339 50.626798)
        (xy 81 50.3) (xy 80 50.05) (xy 79.2 49.9) (xy 78.3 49.8) (xy 77.25 49.75)
        (xy 76.15 49.8) (xy 74.7 50) (xy 73.7 50.25) (xy 72.5 50.65) (xy 71.1 51.3)
        (xy 70.1 51.9) (xy 69.2 52.55) (xy 68.45 53.2) (xy 68.05 53.55) (xy 67.3 54.4)
        (xy 66.6 55.3) (xy 66.05 56.15) (xy 65.55 57.1) (xy 65.1 58.15) (xy 64.75 59.15)
        (xy 64.45 60.5) (xy 64.3 61.6) (xy 64.25 62.75) (xy 55.25 62.75) (xy 55.35 60.5)
        (xy 55.6 58.65) (xy 55.9 57.35) (xy 56.35 55.75) (xy 56.8 54.55) (xy 57.4 53.2)
        (xy 58.15 51.8) (xy 59.15 50.2) (xy 60.1 48.95) (xy 60.852603 48.0859) (xy 62.9 49.8)
        (xy 65 47.75) (xy 63.238961 45.768831) (xy 63.95 45.2) (xy 65.75 43.95) (xy 67.4 43.05)
        (xy 69.05 42.3) (xy 70.85 41.65) (xy 72.15 41.3) (xy 73.65 41) (xy 75.2 40.8)
        (xy 76.45 40.75) (xy 77.25 40.75) (xy 78.75 40.8)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.2) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 78.75 40.8) (xy 79.95 40.9) (xy 81.15 41.1) (xy 82.5 41.35) (xy 84.45 41.95)
        (xy 85.05 42.15) (xy 83.901424 45.183418) (xy 83.47 45.02) (xy 82.66 44.74) (xy 81.88 44.53)
        (xy 81.15 44.37) (xy 80.49 44.26) (xy 79.55 44.11) (xy 79.55 46.65) (xy 80.27 46.76)
        (xy 81 46.93) (xy 81.71 47.11) (xy 82.58 47.37) (xy 83.012136 47.532051) (xy 81.840339 50.626798)
        (xy 81 50.3) (xy 80 50.05) (xy 79.2 49.9) (xy 78.3 49.8) (xy 77.25 49.75)
        (xy 76.15 49.8) (xy 74.7 50) (xy 73.7 50.25) (xy 72.5 50.65) (xy 71.1 51.3)
        (xy 70.1 51.9) (xy 69.2 52.55) (xy 68.45 53.2) (xy 68.05 53.55) (xy 67.3 54.4)
        (xy 66.6 55.3) (xy 66.05 56.15) (xy 65.55 57.1) (xy 65.1 58.15) (xy 64.75 59.15)
        (xy 64.45 60.5) (xy 64.3 61.6) (xy 64.25 62.75) (xy 55.25 62.75) (xy 55.35 60.5)
        (xy 55.6 58.65) (xy 55.9 57.35) (xy 56.35 55.75) (xy 56.8 54.55) (xy 57.4 53.2)
        (xy 58.15 51.8) (xy 59.15 50.2) (xy 60.1 48.95) (xy 61.45 47.4) (xy 62.7 46.2)
        (xy 63.95 45.2) (xy 65.75 43.95) (xy 67.4 43.05) (xy 69.05 42.3) (xy 70.85 41.65)
        (xy 72.15 41.3) (xy 73.65 41) (xy 75.2 40.8) (xy 76.45 40.75) (xy 77.25 40.75)
        (xy 78.75 40.8)
      )
    )
  )
  (zone (net 1) (net_name VDD) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.2) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 78.75 40.8) (xy 79.95 40.9) (xy 81.15 41.1) (xy 82.5 41.35) (xy 84.45 41.95)
        (xy 85.05 42.15) (xy 83.901424 45.183418) (xy 83.47 45.02) (xy 82.66 44.74) (xy 81.88 44.53)
        (xy 81.15 44.37) (xy 80.49 44.26) (xy 79.55 44.11) (xy 79.55 46.65) (xy 80.27 46.76)
        (xy 81 46.93) (xy 81.71 47.11) (xy 82.58 47.37) (xy 83.012136 47.532051) (xy 81.840339 50.626798)
        (xy 81 50.3) (xy 80 50.05) (xy 79.2 49.9) (xy 78.3 49.8) (xy 77.25 49.75)
        (xy 76.15 49.8) (xy 74.7 50) (xy 73.7 50.25) (xy 72.5 50.65) (xy 71.1 51.3)
        (xy 70.1 51.9) (xy 69.2 52.55) (xy 68.45 53.2) (xy 68.05 53.55) (xy 67.3 54.4)
        (xy 66.6 55.3) (xy 66.05 56.15) (xy 65.55 57.1) (xy 65.1 58.15) (xy 64.75 59.15)
        (xy 64.45 60.5) (xy 64.3 61.6) (xy 64.25 62.75) (xy 55.25 62.75) (xy 55.35 60.5)
        (xy 55.6 58.65) (xy 55.9 57.35) (xy 56.35 55.75) (xy 56.8 54.55) (xy 57.4 53.2)
        (xy 58.15 51.8) (xy 59.15 50.2) (xy 60.1 48.95) (xy 61.45 47.4) (xy 62.7 46.2)
        (xy 63.95 45.2) (xy 65.75 43.95) (xy 67.4 43.05) (xy 69.05 42.3) (xy 70.85 41.65)
        (xy 72.15 41.3) (xy 73.65 41) (xy 75.2 40.8) (xy 76.45 40.75) (xy 77.25 40.75)
        (xy 78.75 40.8)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.2) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 78.75 40.8) (xy 79.95 40.9) (xy 81.15 41.1) (xy 82.5 41.35) (xy 84.45 41.95)
        (xy 85.05 42.15) (xy 85.63 42.4) (xy 82.34 50.82) (xy 81.839537 50.628914) (xy 81.839241 50.629697)
        (xy 81.54 50.51) (xy 81 50.3) (xy 80 50.05) (xy 79.2 49.9) (xy 78.924316 49.869368)
        (xy 78.3 49.8) (xy 77.25 49.75) (xy 76.15 49.8) (xy 74.7 50) (xy 73.7 50.25)
        (xy 72.5 50.65) (xy 71.1 51.3) (xy 70.1 51.9) (xy 69.2 52.55) (xy 68.45 53.2)
        (xy 68.05 53.55) (xy 67.3 54.4) (xy 66.6 55.3) (xy 66.05 56.15) (xy 65.55 57.1)
        (xy 65.1 58.15) (xy 64.75 59.15) (xy 64.45 60.5) (xy 64.3 61.6) (xy 64.25 62.75)
        (xy 55.25 62.75) (xy 55.35 60.5) (xy 55.6 58.65) (xy 55.9 57.35) (xy 56.35 55.75)
        (xy 56.8 54.55) (xy 57.4 53.2) (xy 58.15 51.8) (xy 59.15 50.2) (xy 60.1 48.95)
        (xy 61.45 47.4) (xy 62.7 46.2) (xy 63.95 45.2) (xy 65.75 43.95) (xy 67.4 43.05)
        (xy 69.05 42.3) (xy 70.85 41.65) (xy 72.15 41.3) (xy 73.65 41) (xy 75.2 40.8)
        (xy 76.45 40.75) (xy 77.25 40.75) (xy 78.75 40.8)
      )
    )
  )
)
