(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 24)
    (no_connects 0)
    (area 154.864999 63.995 201.662 93.83319)
    (thickness 1.6)
    (drawings 20)
    (tracks 77)
    (zones 0)
    (modules 9)
    (nets 15)
  )
  (page A4)
  (title_block
    (title "GMC/Opel Setter")
    (date 2017-03-08)
    (rev 0.3)
    (company "Andreas Könecke")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.2032)
    (trace_clearance 0.2032)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.762)
    (via_drill 0.3556)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VCC)
  (net 2 Earth)
  (net 3 VIO)
  (net 4 "Net-(D1-Pad2)")
  (net 5 /CANH)
  (net 6 /CANL)
  (net 7 LED)
  (net 8 UP)
  (net 9 CENTER)
  (net 10 DOWN)
  (net 11 LEFT)
  (net 12 RIGHT)
  (net 13 TXD)
  (net 14 RXD)
  (net_class Default "Dies ist die voreingestellte Netzklasse."
    (clearance 0.2032)
    (trace_width 0.2032)
    (via_dia 0.762)
    (via_drill 0.3556)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net CENTER)
    (add_net DOWN)
    (add_net LEFT)
    (add_net RIGHT)
    (add_net RXD)
    (add_net TXD)
    (add_net UP)
    (add_net VIO)
  )
  (net_class CAN ""
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.762)
    (via_drill 0.3556)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /CANH)
    (add_net /CANL)
    (add_net LED)
    (add_net "Net-(D1-Pad2)")
  )
  (net_class Power ""
    (clearance 0.381)
    (trace_width 0.381)
    (via_dia 0.762)
    (via_drill 0.3556)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net Earth)
    (add_net VCC)
  )
  (module Teensy:Teensy30_31_32_LC_OPads (layer F.Cu) (tedit 58BD9A4C)
    (at 172.831 76.286)
    (fp_text reference U2 (at 0 -10.16) (layer F.Fab))
    (fp_text value Teensy_3.1_3.2 (at 0 10.16) (layer F.Fab))
    (pad 19 thru_hole circle (at 1.27 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 10 DOWN))
    (pad 13 thru_hole circle (at 16.51 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 12 thru_hole circle (at 16.51 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 14 thru_hole circle (at 13.97 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 15 thru_hole circle (at 11.43 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 16 thru_hole circle (at 8.89 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 8 UP))
    (pad 17 thru_hole circle (at 6.35 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 18 thru_hole circle (at 3.81 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 11 LEFT))
    (pad 20 thru_hole circle (at -1.27 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 21 thru_hole circle (at -3.81 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 7 LED))
    (pad 22 thru_hole circle (at -6.35 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 23 thru_hole circle (at -8.89 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 35 thru_hole circle (at -11.43 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 3 VIO))
    (pad 36 thru_hole circle (at -13.97 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 37 thru_hole circle (at -16.51 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 11 thru_hole circle (at 13.97 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 10 thru_hole circle (at 11.43 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 9 thru_hole circle (at 8.89 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 9 CENTER))
    (pad 8 thru_hole circle (at 6.35 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 7 thru_hole circle (at 3.81 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 12 RIGHT))
    (pad 6 thru_hole circle (at 1.27 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 5 thru_hole circle (at -1.27 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 4 thru_hole circle (at -3.81 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 14 RXD))
    (pad 3 thru_hole circle (at -6.35 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 13 TXD))
    (pad 2 thru_hole circle (at -8.89 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole circle (at -11.43 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 0 thru_hole circle (at -13.97 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 34 thru_hole rect (at -16.51 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 2 Earth))
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58BDA449)
    (at 162.052 77.363 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 15.113 -4.953 270) (layer F.Fab))
    (fp_text value 100n (at 0 1.397 270) (layer F.SilkS))
    (fp_text user %R (at 14.732 -1.905 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 Earth))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58BDA41B)
    (at 167.152 71.755)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 0.127 -6.604) (layer F.Fab))
    (fp_text value 100n (at 0 1.397) (layer F.SilkS))
    (fp_text user %R (at -2.667 -6.858) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 VIO))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x02_Pitch2.54mm (layer F.Cu) (tedit 58BDA0E4)
    (at 187.706 77.851 90)
    (descr "Through hole straight pin header, 2x02, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x02 2.54mm double row")
    (fp_text reference J1 (at 0.508 7.493 90) (layer F.Fab))
    (fp_text value CONN_02X02 (at 1.143 10.033 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /CANH))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /CANL))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 Earth))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x02_Pitch2.54mm.wrl
      (at (xyz 0.05 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58BDA3F4)
    (at 182.626 77.851 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at -8.763 12.446 90) (layer F.Fab))
    (fp_text value 120R (at -2.159 1.524 270) (layer F.SilkS))
    (fp_text user %R (at -5.08 12.827 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 /CANH))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 /CANL))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58BDA3E4)
    (at 182.626 72.771 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 4.572 14.605 90) (layer F.Fab))
    (fp_text value 20R (at -0.127 1.524 90) (layer F.SilkS))
    (fp_text user %R (at 0.889 12.7 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 LED))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_footprints:SKQU_5-way-switch (layer F.Cu) (tedit 58BDA106)
    (at 175.895 76.2 270)
    (fp_text reference S1 (at 14.224 -7.493 270) (layer F.Fab))
    (fp_text value SKQU_5-Way-Switch (at 0.635 -24.511 270) (layer F.Fab))
    (pad 1 thru_hole circle (at -5.15 -3.25 270) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 8 UP))
    (pad 6 thru_hole circle (at 5.15 -3.25 270) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 9 CENTER))
    (pad 3 thru_hole circle (at -5.15 3.25 270) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 10 DOWN))
    (pad 4 thru_hole circle (at 5.15 3.25 270) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 Earth))
    (pad 2 thru_hole circle (at -5.15 0.45 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 11 LEFT))
    (pad 5 thru_hole circle (at 5.15 0.45 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 12 RIGHT))
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 58BDA439)
    (at 166.37 77.47 90)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1 (at 0.127 3.429 90) (layer F.SilkS))
    (fp_text value TJA1051/3 (at -3.429 26.924 90) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 TXD))
    (pad 2 smd rect (at -2.7 -0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 Earth))
    (pad 3 smd rect (at -2.7 0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 4 smd rect (at -2.7 1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 RXD))
    (pad 5 smd rect (at 2.7 1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 VIO))
    (pad 6 smd rect (at 2.7 0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 /CANL))
    (pad 7 smd rect (at 2.7 -0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 /CANH))
    (pad 8 smd rect (at 2.7 -1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 Earth))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_1206_Symb_Silk (layer F.Cu) (tedit 58BDA3D3)
    (at 187.198 71.501 180)
    (descr "LED 1206 smd package")
    (tags "LED led 1206 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D1 (at -10.16 -15.494 180) (layer F.Fab))
    (fp_text value LED (at 0 -1.651 180) (layer F.SilkS))
    (pad 2 smd rect (at 1.65 0) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -1.65 0) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 Earth))
    (model LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (gr_text 1 (at 164.465 78.74 90) (layer F.SilkS))
  (gr_text "A. Könecke\n2017" (at 159.385 81.28) (layer F.SilkS))
  (gr_text "GMC/Opel\nCAN Setter" (at 159.766 71.755) (layer F.SilkS))
  (gr_text "VCC 5V" (at 156.337 69.977 180) (layer F.SilkS))
  (gr_text "VIO 3.3V" (at 161.417 69.977 180) (layer F.SilkS))
  (gr_text GND (at 156.337 82.55) (layer F.SilkS))
  (gr_text TXD (at 166.497 82.55) (layer F.SilkS))
  (gr_text RXD (at 169.037 82.55) (layer F.SilkS))
  (gr_line (start 154.94 67.31) (end 154.94 85.217) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 191.77 67.31) (end 191.77 85.217) (layer Edge.Cuts) (width 0.15))
  (gr_text LED (at 169.037 69.977 180) (layer F.SilkS))
  (gr_text Down (at 174.117 69.977 180) (layer F.SilkS))
  (gr_text Left (at 176.657 69.977 180) (layer F.SilkS))
  (gr_text Up (at 181.737 69.977 180) (layer F.SilkS))
  (gr_text Right (at 176.657 82.55) (layer F.SilkS))
  (gr_text Center (at 181.737 82.55) (layer F.SilkS))
  (gr_text CANH (at 185.039 77.851) (layer F.SilkS))
  (gr_text CANL (at 184.912 75.311) (layer F.SilkS))
  (gr_line (start 154.94 85.217) (end 191.77 85.217) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 154.94 67.31) (end 191.77 67.31) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name Earth) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 155.067 67.437) (xy 191.643 67.437) (xy 191.643 84.963) (xy 155.067 84.963)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 172.847 81.534) (xy 175.514 81.534) (xy 176.657 83.947) (xy 174.117 83.947) (xy 171.704 83.947)
        (xy 172.974 81.534)
      )
    )
  )
)
