(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (grid_origin 148.59 104.521)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "/V_TARG")
  (net 2 "/TMS")
  (net 3 "GND")
  (net 4 "/TCK")
  (net 5 "/TDO")
  (net 6 "/TDI")
  (net 7 "/RST")
  (net 8 "unconnected-(J2-Pad7)")
  (net 9 "unconnected-(J2-Pad8)")
  (footprint "t_headers:CONN_20021521-00010T1LF_AMP" (layer "F.Cu")
    (tedit 0)
    (at 153.7462 96.901 -90)
    (tags "20021521-00010T1LF ")
    (property "Sheetfile" "PSOC_Adapter.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "J1" (at -6.477 4.1402 unlocked) (layer "F.SilkS"))
    (fp_text value "0.05 Pins SMT" (at 0 0 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -2.54 1.950001 270) (size 0.762 2.3876) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/V_TARG") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd rect (at -2.54 -1.950001 270) (size 0.762 2.3876) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/TMS") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" smd rect (at -1.27 1.950001 270) (size 0.762 2.3876) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "GND") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" smd rect (at -1.27 -1.950001 270) (size 0.762 2.3876) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/TCK") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" smd rect (at 0 1.950001 270) (size 0.762 2.3876) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "GND") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" smd rect (at 0 -1.950001 270) (size 0.762 2.3876) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "/TDO") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" smd rect (at 1.27 1.950001 270) (size 0.762 2.3876) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "GND") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" smd rect (at 1.27 -1.950001 270) (size 0.762 2.3876) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "/TDI") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" smd rect (at 2.54 1.950001 270) (size 0.762 2.3876) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "GND") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" smd rect (at 2.54 -1.950001 270) (size 0.762 2.3876) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "/RST") (pinfunction "Pin_10") (pintype "passive"))
    (model "${T_LIBS}/3d/t_header/1.27mm/20021521-00010T1LF.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_2x05_P2.54mm_Vertical_SMD" (layer "B.Cu")
    (tedit 5A19A425)
    (at 153.6954 96.9264 180)
    (descr "surface-mounted straight socket strip, 2x05, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated")
    (tags "Surface mounted socket strip SMD 2x05 2.54mm double row")
    (property "Sheetfile" "PSOC_Adapter.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "J2" (at 4.0894 6.6294) (layer "B.SilkS"))
    (fp_text value "0.100 Socket SMT" (at 0 -7.85) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd rect (at 2.52 5.08 180) (size 3 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "/TCK") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd rect (at -2.52 5.08 180) (size 3 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 3 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" smd rect (at 2.52 2.54 180) (size 3 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 5 "/TDO") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" smd rect (at -2.52 2.54 180) (size 3 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "/V_TARG") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" smd rect (at 2.52 0 180) (size 3 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "/TMS") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" smd rect (at -2.52 0 180) (size 3 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "/RST") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" smd rect (at 2.52 -2.54 180) (size 3 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 8 "unconnected-(J2-Pad7)") (pinfunction "Pin_7") (pintype "passive+no_connect"))
    (pad "8" smd rect (at -2.52 -2.54 180) (size 3 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "unconnected-(J2-Pad8)") (pinfunction "Pin_8") (pintype "passive+no_connect"))
    (pad "9" smd rect (at 2.52 -5.08 180) (size 3 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 6 "/TDI") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" smd rect (at -2.52 -5.08 180) (size 3 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 3 "GND") (pinfunction "Pin_10") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x05_P2.54mm_Vertical_SMD.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_rect (start 148.59 89.281) (end 158.75 104.521) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_text "PSOC Prog Adapter" (at 157.861 96.901 90) (layer "F.SilkS"))
)
