(kicad_pcb (version 20171130) (host pcbnew "(5.0.1)-4")
  (general
    (thickness 1.6)
    (drawings 17)
    (tracks 87)
    (zones 0)
    (modules 15)
    (nets 11)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.762)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 1.016)
    (via_drill 0.508)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 -15V)
  (net 2 GND)
  (net 3 +15V)
  (net 4 "Net-(C3-Pad2)")
  (net 5 "Net-(C5-Pad1)")
  (net 6 "Net-(D1-Pad2)")
  (net 7 "Net-(J1-Pad1)")
  (net 8 "Net-(J3-Pad1)")
  (net 9 "Net-(R1-Pad1)")
  (net 10 "Net-(J2-Pad4)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.762)
    (via_dia 1.016)
    (via_drill 0.508)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +15V)
    (add_net -15V)
    (add_net GND)
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(R1-Pad1)")
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5C9A56CB)
    (at 157.1952 49.403)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at -0.1216 -2.8194) (layer F.SilkS))
    (fp_text value .1uf (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 -15V))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5C9A572A)
    (at 140.4166 51.943)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at -0.3102 -2.5146) (layer F.SilkS))
    (fp_text value .1uf (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +15V))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5C9A5742)
    (at 142.0314 76.2762)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at -0.0454 -2.3622) (layer F.SilkS))
    (fp_text value 1pf (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5C9A5764)
    (at 142.0568 83.7946 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at -0.0816 -2.4384 180) (layer F.SilkS))
    (fp_text value 1pf (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_Tantal_D4.5mm_P5.00mm (layer B.Cu) (tedit 597C781B)
    (at 92.456 90.678)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=4.5mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 4.5mm Tantal Electrolytic Capacitor")
    (fp_text reference C5 (at 8.8646 3.4544) (layer B.SilkS))
    (fp_text value 6.8uf (at 9.0678 -3.1242) (layer B.Fab))
    (fp_text user %R (at 8.763 -0.0254) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C5-Pad1)"))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_Tantal_D4.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_Tantal_D4.5mm_P5.00mm (layer B.Cu) (tedit 597C781B)
    (at 92.456 79.270144)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=4.5mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 4.5mm Tantal Electrolytic Capacitor")
    (fp_text reference C6 (at 9.1186 2.848056) (layer B.SilkS))
    (fp_text value 6.8uf (at 8.9154 -2.587544) (layer B.Fab))
    (fp_text user %R (at 8.9408 0.003256) (layer B.Fab))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C5-Pad1)"))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_Tantal_D4.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VEMD2000:vemd2000 (layer F.Cu) (tedit 5C9A578D)
    (at 152.654 80.01)
    (tags "photo diode")
    (attr smd)
    (fp_text reference D1 (at 0.2286 3.0734) (layer F.SilkS))
    (fp_text value D_Photo_DUT (at -0.3556 -4.0386) (layer F.SilkS))
    (pad 2 smd rect (at 2.95 0) (size 1.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -2.95 0) (size 1.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad2)"))
  )
  (module Connectors:SMA_THT_Jack_Straight (layer F.Cu) (tedit 5C9A58B7)
    (at 263.8298 99.3648 90)
    (descr "SMA pcb through hole jack")
    (tags "SMA THT Jack Straight")
    (fp_text reference J1 (at -0.0762 5.0292 90) (layer F.SilkS))
    (fp_text value VDC_In (at 0 5 90) (layer F.Fab))
    (fp_text user %R (at 0 -5 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 1.5) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 2.54 90) (size 2.2 2.2) (drill 1.7) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 2.54 -2.54 90) (size 2.2 2.2) (drill 1.7) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -2.54 -2.54 90) (size 2.2 2.2) (drill 1.7) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -2.54 2.54 90) (size 2.2 2.2) (drill 1.7) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Connectors_Phoenix:PhoenixContact_MCV-G_06x3.50mm_Vertical (layer F.Cu) (tedit 5C9A58A5)
    (at 259.3594 71.4756 270)
    (descr "Generic Phoenix Contact connector footprint for series: MCV-G; number of pins: 06; pin pitch: 3.50mm; Vertical || order number: 1843648 8A 160V")
    (tags "phoenix_contact connector MCV_01x06_G_3.5mm")
    (fp_text reference J2 (at 5.7912 -9.3218 270) (layer F.SilkS))
    (fp_text value "6   5   4   3   2   1" (at 8.763 -4.3688 270) (layer F.Fab))
    (fp_text user %R (at 4.9784 -6.6294 270) (layer F.Fab))
    (pad 6 thru_hole oval (at 17.5 0 270) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 6 "Net-(D1-Pad2)"))
    (pad 5 thru_hole oval (at 14 0 270) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad2)"))
    (pad 4 thru_hole oval (at 10.5 0 270) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 10 "Net-(J2-Pad4)"))
    (pad 3 thru_hole oval (at 7 0 270) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad1)"))
    (pad 2 thru_hole oval (at 3.5 0 270) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 5 "Net-(C5-Pad1)"))
    (model ${KISYS3DMOD}/Connectors_Phoenix.3dshapes/PhoenixContact_MCV-G_06x3.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:SMA_THT_Jack_Straight (layer F.Cu) (tedit 5C9A5892)
    (at 263.6012 60.4266 90)
    (descr "SMA pcb through hole jack")
    (tags "SMA THT Jack Straight")
    (fp_text reference J3 (at -0.127 5.2578 90) (layer F.SilkS))
    (fp_text value Monitor_Out (at 0 5 90) (layer F.Fab))
    (fp_text user %R (at 0 -5 90) (layer F.Fab))
    (pad 2 thru_hole circle (at -2.54 2.54 90) (size 2.2 2.2) (drill 1.7) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -2.54 -2.54 90) (size 2.2 2.2) (drill 1.7) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 2.54 -2.54 90) (size 2.2 2.2) (drill 1.7) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 2.54 2.54 90) (size 2.2 2.2) (drill 1.7) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 1.5) (layers *.Cu *.Mask)
      (net 8 "Net-(J3-Pad1)"))
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5C9A56F5)
    (at 156.337 58.1114 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at -0.2756 -3.0226) (layer F.SilkS))
    (fp_text value 50 (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J3-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5C9A5752)
    (at 142.0152 79.9084)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at -3.509 -1.6256) (layer F.SilkS))
    (fp_text value 1k (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad2)"))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J2-Pad4)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometers:Potentiometer_Trimmer_Bourns_3296Y (layer F.Cu) (tedit 5C9A585D)
    (at 247.523 77.089)
    (descr "Spindle Trimmer Potentiometer, Bourns 3296Y, https://www.bourns.com/pdfs/3296.pdf")
    (tags "Spindle Trimmer Potentiometer   Bourns 3296Y")
    (fp_text reference "DUT Response Adj." (at -2.2352 -3.1496 180) (layer F.SilkS))
    (fp_text value Response_Adj (at -2.54 4.94) (layer F.Fab))
    (pad 3 thru_hole circle (at -5.08 0) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -2.54 2.54) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(D1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(D1-Pad2)"))
    (model Potentiometers.3dshapes/Potentiometer_Trimmer_Bourns_3296Y.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module SMD_Packages:SOIC-8-N (layer F.Cu) (tedit 5C9A5712)
    (at 148.844 51.308 90)
    (descr "Module Narrow CMS SOJ 8 pins large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference U1 (at -4.7244 -0.1016 180) (layer F.SilkS))
    (fp_text value LM7171 (at 0 1.27 90) (layer F.Fab))
    (pad 1 smd rect (at -1.905 3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -0.635 3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(R1-Pad1)"))
    (pad 3 smd rect (at 0.635 3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D1-Pad2)"))
    (pad 4 smd rect (at 1.905 3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 1 -15V))
    (pad 5 smd rect (at 1.905 -3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 0.635 -3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(R1-Pad1)"))
    (pad 7 smd rect (at -0.635 -3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 3 +15V))
    (pad 8 smd rect (at -1.905 -3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (model SMD_Packages.3dshapes/SOIC-8-N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.38 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module Photo_Diode:PDQ15D (layer B.Cu) (tedit 5BFC1687)
    (at 104.648 67.840144)
    (fp_text reference U2 (at 7.5184 -10.817144) (layer B.SilkS))
    (fp_text value "+/-15V DC-DC" (at 11.811 -7.616744) (layer B.Fab))
    (pad 3 thru_hole circle (at -20.4 -20.3) (size 2.032 2.032) (drill 1.0668) (layers *.Cu *.Mask)
      (net 3 +15V))
    (pad 4 thru_hole circle (at -10.2 -20.3) (size 2.032 2.032) (drill 1.0668) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 5 thru_hole circle (at 0 -20.3) (size 2.032 2.032) (drill 1.0668) (layers *.Cu *.Mask)
      (net 1 -15V))
    (pad 1 thru_hole circle (at -12.7 0) (size 2.032 2.032) (drill 1.0668) (layers *.Cu *.Mask)
      (net 5 "Net-(C5-Pad1)"))
    (pad 2 thru_hole circle (at -7.6 0) (size 2.032 2.032) (drill 1.0668) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.0668) (layers *.Cu *.Mask))
  )
  (gr_text Monitor_Out (at 252.2982 62.865 90) (layer F.SilkS))
  (gr_text DUT_Vdc_In (at 252.2982 97.79 90) (layer F.SilkS))
  (gr_text 1 (at 264.8458 71.3232 90) (layer F.SilkS))
  (gr_text Photo_Diode_DUT_RevA/BN (at 209.042 122.7836) (layer F.SilkS))
  (gr_line (start 232.5878 105.4608) (end 270.4592 105.4608) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 232.5624 130.1242) (end 232.5624 105.4608) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 232.6132 54.737) (end 270.4338 54.737) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 232.5878 30.0228) (end 232.5878 54.737) (layer Edge.Cuts) (width 0.15))
  (dimension 159.918418 (width 0.3) (layer Dwgs.User)
    (gr_text "6.2960 in" (at 152.611765 11.655194 359.972699) (layer Dwgs.User))
    (feature1 (pts (xy 232.5624 29.6672) (xy 232.570243 13.206873)))
    (feature2 (pts (xy 72.644 29.591) (xy 72.651843 13.130673)))
    (crossbar (pts (xy 72.651564 13.717094) (xy 232.569964 13.793294)))
    (arrow1a (pts (xy 232.569964 13.793294) (xy 231.443181 14.379178)))
    (arrow1b (pts (xy 232.569964 13.793294) (xy 231.44374 13.206337)))
    (arrow2a (pts (xy 72.651564 13.717094) (xy 73.777788 14.304051)))
    (arrow2b (pts (xy 72.651564 13.717094) (xy 73.778347 13.13121)))
  )
  (dimension 159.867602 (width 0.3) (layer Dwgs.User)
    (gr_text "6.2940 in" (at 152.580721 148.594128 0.00910323785) (layer Dwgs.User))
    (feature1 (pts (xy 232.5116 130.2004) (xy 232.51428 147.067849)))
    (feature2 (pts (xy 72.644 130.2258) (xy 72.64668 147.093249)))
    (crossbar (pts (xy 72.646587 146.506828) (xy 232.514187 146.481428)))
    (arrow1a (pts (xy 232.514187 146.481428) (xy 231.387776 147.068028)))
    (arrow1b (pts (xy 232.514187 146.481428) (xy 231.38759 145.895186)))
    (arrow2a (pts (xy 72.646587 146.506828) (xy 73.773184 147.09307)))
    (arrow2b (pts (xy 72.646587 146.506828) (xy 73.772998 145.920228)))
  )
  (dimension 25.4 (width 0.3) (layer Dwgs.User)
    (gr_text "1.0000 in" (at 284.796622 92.8116 270) (layer Dwgs.User))
    (feature1 (pts (xy 270.834822 105.5116) (xy 283.283043 105.5116)))
    (feature2 (pts (xy 270.834822 80.1116) (xy 283.283043 80.1116)))
    (crossbar (pts (xy 282.696622 80.1116) (xy 282.696622 105.5116)))
    (arrow1a (pts (xy 282.696622 105.5116) (xy 282.110201 104.385096)))
    (arrow1b (pts (xy 282.696622 105.5116) (xy 283.283043 104.385096)))
    (arrow2a (pts (xy 282.696622 80.1116) (xy 282.110201 81.238104)))
    (arrow2b (pts (xy 282.696622 80.1116) (xy 283.283043 81.238104)))
  )
  (dimension 25.4 (width 0.3) (layer Dwgs.User)
    (gr_text "1.0000 in" (at 284.695022 67.322875 90) (layer Dwgs.User))
    (feature1 (pts (xy 270.911022 54.622875) (xy 283.181443 54.622875)))
    (feature2 (pts (xy 270.911022 80.022875) (xy 283.181443 80.022875)))
    (crossbar (pts (xy 282.595022 80.022875) (xy 282.595022 54.622875)))
    (arrow1a (pts (xy 282.595022 54.622875) (xy 283.181443 55.749379)))
    (arrow1b (pts (xy 282.595022 54.622875) (xy 282.008601 55.749379)))
    (arrow2a (pts (xy 282.595022 80.022875) (xy 283.181443 78.896371)))
    (arrow2b (pts (xy 282.595022 80.022875) (xy 282.008601 78.896371)))
  )
  (dimension 50.012658 (width 0.3) (layer Dwgs.User)
    (gr_text "1.9690 in" (at 290.248942 54.974767 270.0872967) (layer Dwgs.User))
    (feature1 (pts (xy 271.2974 80.01) (xy 288.773464 79.983373)))
    (feature2 (pts (xy 271.2212 29.9974) (xy 288.697264 29.970773)))
    (crossbar (pts (xy 288.110844 29.971667) (xy 288.187044 79.984267)))
    (arrow1a (pts (xy 288.187044 79.984267) (xy 287.598908 78.858658)))
    (arrow1b (pts (xy 288.187044 79.984267) (xy 288.771748 78.856871)))
    (arrow2a (pts (xy 288.110844 29.971667) (xy 287.52614 31.099063)))
    (arrow2b (pts (xy 288.110844 29.971667) (xy 288.69898 31.097276)))
  )
  (gr_line (start 72.644 130.048) (end 72.644 29.972) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 232.5624 130.1242) (end 72.644 130.048) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 270.4338 54.737) (end 270.4592 105.4608) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 72.644 29.972) (end 232.5878 30.0228) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 71.8566 29.083) (xy 272.034 29.083) (xy 272.2372 131.1402) (xy 71.5772 131.2672)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 72.1868 29.1338) (xy 271.907 29.337) (xy 271.5006 131.064) (xy 71.9074 131.2672)
      )
    )
  )
)
