<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="24.765" y1="10.16" x2="1.905" y2="10.16" width="0" layer="20"/>
<wire x1="0.635" y1="8.89" x2="1.905" y2="1.905" width="0" layer="20"/>
<wire x1="4.445" y1="0" x2="22.225" y2="0" width="0" layer="20"/>
<wire x1="0.635" y1="8.89" x2="1.905" y2="10.16" width="0" layer="20" curve="-90"/>
<wire x1="24.765" y1="10.16" x2="26.035" y2="8.255" width="0" layer="20" curve="-90"/>
<wire x1="4.445" y1="0" x2="1.905" y2="1.905" width="0" layer="20" curve="-90"/>
<wire x1="24.765" y1="1.905" x2="22.225" y2="0" width="0" layer="20" curve="-90"/>
<wire x1="24.765" y1="1.905" x2="26.035" y2="8.255" width="0" layer="20"/>
<text>Implant 4.7</text>
<text>POS</text>
<text>NEG</text>
<text>FB</text>
<text>NEG</text>
<text>POS</text>
<text>FB1</text>
<text>FB2</text>
</plain>
<libraries>
<library name="Andy-library">
<packages>
<package name="0805">
</package>
<package name="LED10MM">
</package>
<package name="USB_VERT_MICRO_SMD">
</package>
<package name="LASERDIODE_5.6">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R2" library="Andy-library" package="0805" value="20k">
<attribute name="VALUE"/>
</element>
<element name="ALT_PWR" library="Andy-library" package="LED10MM" value=""/>
<element name="U$2" library="Andy-library" package="USB_VERT_MICRO_SMD" value="USB_MICRO_SOCKET_VERT"/>
<element name="U$1" library="Andy-library" package="LASERDIODE_5.6" value="LASERDIODE5.6MM"/>
<element name="U$3" library="Andy-library" package="LASERDIODE_5.6" value="LASERDIODE5.6MM"/>
<element name="R1" library="Andy-library" package="0805" value="20k">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="LD+">
<contactref element="U$2" pad="P5"/>
<contactref element="U$1" pad="2"/>
<contactref element="U$3" pad="2"/>
<contactref element="ALT_PWR" pad="A"/>
</signal>
<signal name="LD-">
<contactref element="U$1" pad="1"/>
<contactref element="U$3" pad="1"/>
<contactref element="U$2" pad="P1"/>
<contactref element="ALT_PWR" pad="C"/>
</signal>
<signal name="FDBK">
<contactref element="U$2" pad="P3"/>
<contactref element="U$1" pad="3"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="GND">
<contactref element="U$2" pad="P$1"/>
<contactref element="U$2" pad="P$2"/>
<contactref element="U$2" pad="P$3"/>
<contactref element="R1" pad="1"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="U$3" pad="3"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$2">
</signal>
<signal name="N$3">
</signal>
</signals>
</board>
</drawing>
</eagle>
