(kicad_pcb (version 20171130) (host pcbnew "(5.1.12)-1")
  (general
    (thickness 1.6)
    (drawings 12)
    (tracks 295)
    (zones 0)
    (modules 12)
    (nets 29)
  )
  (page A)
  (title_block
    (title "Beetje 32U4 Blok")
    (date 2018-08-10)
    (rev 0.0)
    (company www.MakersBox.us)
    (comment 1 648.ken@gmail.com)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.3048)
    (user_trace_width 0.3556)
    (user_trace_width 0.4064)
    (user_trace_width 0.6096)
    (trace_clearance 0.2)
    (zone_clearance 0.35)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.15)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.5 3.500001)
    (pad_drill 0)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions true)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers/"))
  )
  (net 0 "")
  (net 1 /10)
  (net 2 /01)
  (net 3 /02)
  (net 4 /04)
  (net 5 /05)
  (net 6 /06)
  (net 7 /07)
  (net 8 /08)
  (net 9 /09)
  (net 10 /11)
  (net 11 /12)
  (net 12 /13)
  (net 13 /14)
  (net 14 /15)
  (net 15 /16)
  (net 16 /17)
  (net 17 /18)
  (net 18 /19)
  (net 19 /20)
  (net 20 /03)
  (net 21 /D2_SDA)
  (net 22 GND)
  (net 23 /D3_SCL)
  (net 24 +5V)
  (net 25 /RESET)
  (net 26 /A)
  (net 27 "Net-(R1-Pad1)")
  (net 28 "Net-(U1-Pad7)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.254)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net /01)
    (add_net /02)
    (add_net /03)
    (add_net /04)
    (add_net /05)
    (add_net /06)
    (add_net /07)
    (add_net /08)
    (add_net /09)
    (add_net /10)
    (add_net /11)
    (add_net /12)
    (add_net /13)
    (add_net /14)
    (add_net /15)
    (add_net /16)
    (add_net /17)
    (add_net /18)
    (add_net /19)
    (add_net /20)
    (add_net /A)
    (add_net /D2_SDA)
    (add_net /D3_SCL)
    (add_net /RESET)
    (add_net GND)
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(U1-Pad7)")
  )
  (module footprints:MEC8-113-CARD_2 locked (layer F.Cu) (tedit 637EA67F)
    (at 0 -0.1 90)
    (fp_text reference X0 (at 4.375 -1.25 90) (layer F.Fab))
    (fp_text value "Card Edge" (at 10.9 -1 90) (layer F.Fab))
    (fp_line (start 21 50.5) (end 21 47.5) (layer Edge.Cuts) (width 0.12))
    (fp_line (start 19 51.5) (end 20 51.5) (layer Edge.Cuts) (width 0.12))
    (fp_line (start 0 51.5) (end 1 51.5) (layer Edge.Cuts) (width 0.12))
    (fp_line (start -1 50.5) (end -1 47.5) (layer Edge.Cuts) (width 0.12))
    (fp_line (start 19 6.5) (end 20 6.5) (layer Edge.Cuts) (width 0.12))
    (fp_line (start 0 6.5) (end 1 6.5) (layer Edge.Cuts) (width 0.12))
    (fp_line (start 17 0) (end 11.3 0) (layer Edge.Cuts) (width 0.12))
    (fp_line (start 3 0) (end 7.9 0) (layer Edge.Cuts) (width 0.12))
    (fp_line (start 9.4 6.5) (end 9.8 6.5) (layer Edge.Cuts) (width 0.12))
    (fp_line (start 10.8 5.5) (end 10.8 0.5) (layer Edge.Cuts) (width 0.12))
    (fp_line (start 8.4 0.5) (end 8.4 5.5) (layer Edge.Cuts) (width 0.12))
    (fp_line (start 2.5 0.5) (end 2.5 5.5) (layer Edge.Cuts) (width 0.12))
    (fp_line (start 17.5 0.5) (end 17.5 5.5) (layer Edge.Cuts) (width 0.12))
    (fp_line (start 18.5 6.5) (end 19 6.5) (layer Edge.Cuts) (width 0.12))
    (fp_line (start 1 6.5) (end 1.5 6.5) (layer Edge.Cuts) (width 0.12))
    (fp_line (start 8.5 51.5) (end 1 51.5) (layer Edge.Cuts) (width 0.12))
    (fp_line (start 11.5 51.5) (end 19 51.5) (layer Edge.Cuts) (width 0.12))
    (fp_line (start 21 7.5) (end 21 47.5) (layer Edge.Cuts) (width 0.12))
    (fp_line (start -1 47.5) (end -1 7.5) (layer Edge.Cuts) (width 0.12))
    (fp_arc (start 10 51.5) (end 11.5 51.5) (angle -180) (layer Edge.Cuts) (width 0.12))
    (fp_arc (start 20 50.5) (end 20 51.5) (angle -90) (layer Edge.Cuts) (width 0.12))
    (fp_arc (start 0 50.5) (end -1 50.5) (angle -90) (layer Edge.Cuts) (width 0.12))
    (fp_arc (start 0 7.5) (end 0 6.5) (angle -90) (layer Edge.Cuts) (width 0.12))
    (fp_arc (start 20 7.5) (end 21 7.5) (angle -90) (layer Edge.Cuts) (width 0.12))
    (fp_arc (start 18.5 5.5) (end 17.5 5.5) (angle -90) (layer Edge.Cuts) (width 0.12))
    (fp_arc (start 1.5 5.5) (end 1.5 6.5) (angle -90) (layer Edge.Cuts) (width 0.12))
    (fp_arc (start 9.4 5.5) (end 8.4 5.5) (angle -90) (layer Edge.Cuts) (width 0.12))
    (fp_arc (start 9.8 5.5) (end 9.8 6.5) (angle -90) (layer Edge.Cuts) (width 0.12))
    (fp_arc (start 7.9 0.5) (end 8.4 0.5) (angle -90) (layer Edge.Cuts) (width 0.12))
    (fp_arc (start 11.3 0.5) (end 11.3 0) (angle -90) (layer Edge.Cuts) (width 0.12))
    (fp_arc (start 17 0.5) (end 17.5 0.5) (angle -90) (layer Edge.Cuts) (width 0.12))
    (fp_arc (start 3 0.5) (end 3 0) (angle -90) (layer Edge.Cuts) (width 0.12))
    (pad 14 smd rect (at 3.6 2.25 90) (size 0.5 3.5) (layers F.Cu F.Paste F.Mask)
      (net 10 /11))
    (pad 1 smd rect (at 3.6 2.25 90) (size 0.5 3.5) (layers B.Cu B.Paste B.Mask)
      (net 2 /01))
    (pad 15 smd rect (at 4.4 2.25 90) (size 0.5 3.5) (layers F.Cu F.Paste F.Mask)
      (net 11 /12))
    (pad 2 smd rect (at 4.4 2.25 90) (size 0.5 3.5) (layers B.Cu B.Paste B.Mask)
      (net 3 /02))
    (pad 16 smd rect (at 5.2 2.25 90) (size 0.5 3.5) (layers F.Cu F.Paste F.Mask)
      (net 12 /13))
    (pad 3 smd rect (at 5.2 2.25 90) (size 0.5 3.5) (layers B.Cu B.Paste B.Mask)
      (net 20 /03))
    (pad 17 smd rect (at 6 2.25 90) (size 0.5 3.5) (layers F.Cu F.Paste F.Mask)
      (net 13 /14))
    (pad 4 smd rect (at 6 2.25 90) (size 0.5 3.5) (layers B.Cu B.Paste B.Mask)
      (net 4 /04))
    (pad 18 smd rect (at 6.8 2.25 90) (size 0.5 3.5) (layers F.Cu F.Paste F.Mask)
      (net 14 /15))
    (pad 5 smd rect (at 6.8 2.25 90) (size 0.5 3.5) (layers B.Cu B.Paste B.Mask)
      (net 5 /05))
    (pad 19 smd rect (at 7.6 2.25 90) (size 0.5 3.5) (layers F.Cu F.Paste F.Mask)
      (net 15 /16))
    (pad 6 smd rect (at 7.6 2.25 90) (size 0.5 3.5) (layers B.Cu B.Paste B.Mask)
      (net 6 /06))
    (pad 20 smd rect (at 11.6 2.25 90) (size 0.5 3.5) (layers F.Cu F.Paste F.Mask)
      (net 16 /17))
    (pad 7 smd rect (at 11.6 2.25 90) (size 0.5 3.5) (layers B.Cu B.Paste B.Mask)
      (net 7 /07))
    (pad 21 smd rect (at 12.4 2.25 90) (size 0.5 3.5) (layers F.Cu F.Paste F.Mask)
      (net 17 /18))
    (pad 8 smd rect (at 12.4 2.25 90) (size 0.5 3.5) (layers B.Cu B.Paste B.Mask)
      (net 8 /08))
    (pad 22 smd rect (at 13.2 2.25 90) (size 0.5 3.5) (layers F.Cu F.Paste F.Mask)
      (net 18 /19))
    (pad 9 smd rect (at 13.2 2.25 90) (size 0.5 3.5) (layers B.Cu B.Paste B.Mask)
      (net 9 /09))
    (pad 23 smd rect (at 14 2.25 90) (size 0.5 3.5) (layers F.Cu F.Paste F.Mask)
      (net 19 /20))
    (pad 10 smd rect (at 14 2.25 90) (size 0.5 3.5) (layers B.Cu B.Paste B.Mask)
      (net 1 /10))
    (pad 24 smd rect (at 14.8 2.25 90) (size 0.5 3.5) (layers F.Cu F.Paste F.Mask)
      (net 23 /D3_SCL))
    (pad 11 smd rect (at 14.8 2.25 90) (size 0.5 3.5) (layers B.Cu B.Paste B.Mask)
      (net 25 /RESET))
    (pad 25 smd rect (at 15.6 2.25 90) (size 0.5 3.5) (layers F.Cu F.Paste F.Mask)
      (net 21 /D2_SDA))
    (pad 12 smd rect (at 15.6 2.25 90) (size 0.5 3.5) (layers B.Cu B.Paste B.Mask)
      (net 26 /A))
    (pad 26 smd rect (at 16.4 2.25 90) (size 0.5 3.5) (layers F.Cu F.Paste F.Mask)
      (net 22 GND))
    (pad 13 smd rect (at 16.4 2.25 90) (size 0.5 3.5) (layers B.Cu B.Paste B.Mask)
      (net 24 +5V))
  )
  (module footprints:G125-MS10605L0P (layer F.Cu) (tedit 0)
    (at 35.875 -10.25)
    (descr G125-MS10605L0P)
    (tags Connector)
    (attr smd)
    (fp_text reference J11 (at 0 0) (layer F.SilkS) hide)
    (fp_text value "Gecko 12p" (at 0 0) (layer F.SilkS) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -3.125 1.85) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 /01))
    (pad 2 smd rect (at -1.875 1.85) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 3 /02))
    (pad 3 smd rect (at -0.625 1.85) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 20 /03))
    (pad 4 smd rect (at 0.625 1.85) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 4 /04))
    (pad 5 smd rect (at 1.875 1.85) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 5 /05))
    (pad 6 smd rect (at 3.125 1.85) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 6 /06))
    (pad 7 smd rect (at -3.125 -1.85) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 7 /07))
    (pad 8 smd rect (at -1.875 -1.85) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 8 /08))
    (pad 9 smd rect (at -0.625 -1.85) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 9 /09))
    (pad 10 smd rect (at 0.625 -1.85) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 1 /10))
    (pad 11 smd rect (at 1.875 -1.85) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 10 /11))
    (pad 12 smd rect (at 3.125 -1.85) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 11 /12))
    (model G125-MS11205L0P.stp
      (offset (xyz 0 0 1.999999969963015))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module footprints:test_pads_125mm_x06 (layer F.Cu) (tedit 63842995)
    (at 32.75 -13.5)
    (descr "Harwin Gecko Connector, 6 pins, dual row female, vertical entry, PN:G125-FVX0605L0X")
    (tags "connector harwin gecko")
    (fp_text reference J3 (at 1 1.5) (layer F.SilkS) hide)
    (fp_text value "test points" (at 4 -1.5) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 3 thru_hole circle (at 2.5 0) (size 0.95 0.95) (drill 0.3) (layers *.Cu *.Mask)
      (net 9 /09))
    (pad 2 thru_hole circle (at 1.25 0) (size 0.95 0.95) (drill 0.3) (layers *.Cu *.Mask)
      (net 8 /08))
    (pad 1 thru_hole circle (at 0 0) (size 0.95 0.95) (drill 0.3) (layers *.Cu *.Mask)
      (net 7 /07))
    (pad 4 thru_hole circle (at 3.75 0) (size 0.95 0.95) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 /10))
    (pad 5 thru_hole circle (at 5 0) (size 0.95 0.95) (drill 0.3) (layers *.Cu *.Mask)
      (net 10 /11))
    (pad 6 thru_hole circle (at 6.25 0) (size 0.95 0.95) (drill 0.3) (layers *.Cu *.Mask)
      (net 11 /12))
    (model ${KISYS3DMOD}/Connector_Harwin.3dshapes/Harwin_Gecko-G125-FVX0605L0X_2x03_P1.25mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:Harwin_Gecko-G125-MVX1205L0X_2x06_P1.25mm_Vertical (layer F.Cu) (tedit 63711ABB)
    (at 32.75 -9.5)
    (descr "Harwin Gecko Connector, 12 pins, dual row male, vertical entry, no latches, PN:G125-MVX1205L0X")
    (tags "connector harwin gecko")
    (fp_text reference J2 (at 3 -4.5) (layer F.SilkS) hide)
    (fp_text value "Gecko 12p" (at 3.5 8.25) (layer F.SilkS))
    (fp_text user %R (at 3.125 0) (layer F.Fab))
    (fp_text user G125-MV11605L0P (at 3 1.5) (layer B.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 2 /01))
    (pad 2 thru_hole circle (at 1.25 0) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 3 /02))
    (pad 3 thru_hole circle (at 2.5 0) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 20 /03))
    (pad 4 thru_hole circle (at 3.75 0) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 4 /04))
    (pad 5 thru_hole circle (at 5 0) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 5 /05))
    (pad 6 thru_hole circle (at 6.25 0) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 6 /06))
    (pad 7 thru_hole circle (at 0 -1.25) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 7 /07))
    (pad 8 thru_hole circle (at 1.25 -1.25) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 8 /08))
    (pad 9 thru_hole circle (at 2.5 -1.25) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 9 /09))
    (pad 10 thru_hole circle (at 3.75 -1.25) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 1 /10))
    (pad 11 thru_hole circle (at 5 -1.25) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 10 /11))
    (pad 12 thru_hole circle (at 6.25 -1.25) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 11 /12))
    (model ${KIPRJMOD}/3D/G125-MV11205L0P.stp
      (offset (xyz 3 0.5 1.5))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module footprints:test_pads_125mm_x06 (layer F.Cu) (tedit 63842995)
    (at 32.75 -7)
    (descr "Harwin Gecko Connector, 6 pins, dual row female, vertical entry, PN:G125-FVX0605L0X")
    (tags "connector harwin gecko")
    (fp_text reference J6 (at 1 1.5) (layer F.SilkS) hide)
    (fp_text value "test points" (at 4 -1.5) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 6 thru_hole circle (at 6.25 0) (size 0.95 0.95) (drill 0.3) (layers *.Cu *.Mask)
      (net 6 /06))
    (pad 5 thru_hole circle (at 5 0) (size 0.95 0.95) (drill 0.3) (layers *.Cu *.Mask)
      (net 5 /05))
    (pad 4 thru_hole circle (at 3.75 0) (size 0.95 0.95) (drill 0.3) (layers *.Cu *.Mask)
      (net 4 /04))
    (pad 1 thru_hole circle (at 0 0) (size 0.95 0.95) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 /01))
    (pad 2 thru_hole circle (at 1.25 0) (size 0.95 0.95) (drill 0.3) (layers *.Cu *.Mask)
      (net 3 /02))
    (pad 3 thru_hole circle (at 2.5 0) (size 0.95 0.95) (drill 0.3) (layers *.Cu *.Mask)
      (net 20 /03))
    (model ${KISYS3DMOD}/Connector_Harwin.3dshapes/Harwin_Gecko-G125-FVX0605L0X_2x03_P1.25mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0603 (layer F.Cu) (tedit 636E7A48)
    (at 47.25 -18 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 1.905 0 270) (layer Dwgs.User))
    (fp_text value 10K (at 2 0) (layer F.SilkS))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 26 /A))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:AR_logo_18mm (layer F.Cu) (tedit 63780F59)
    (at 46.7 -3.2)
    (fp_text reference G1 (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer Dwgs.User))
  )
  (module footprints:Harwin_Gecko-G125-MVX2005L0X_2x10_P1.25mm_Vertical (layer F.Cu) (tedit 63726BC9)
    (at 11.25 -9.5)
    (descr "Harwin Gecko Connector, 20 pins, dual row male, vertical entry, no latches, PN:G125-MVX2005L0X")
    (tags "connector harwin gecko")
    (fp_text reference J1 (at 5 -5) (layer F.SilkS) hide)
    (fp_text value "Gecko 20P" (at 5.26 8.23) (layer F.SilkS))
    (fp_text user %R (at 5.625 0) (layer F.Fab))
    (fp_text user G125-MV12005L0P (at 5.83 1.5) (layer B.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 2 /01))
    (pad 2 thru_hole circle (at 1.25 0) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 3 /02))
    (pad 3 thru_hole circle (at 2.5 0) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 20 /03))
    (pad 4 thru_hole circle (at 3.75 0) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 4 /04))
    (pad 5 thru_hole circle (at 5 0) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 5 /05))
    (pad 6 thru_hole circle (at 6.25 0) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 6 /06))
    (pad 7 thru_hole circle (at 7.5 0) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 7 /07))
    (pad 8 thru_hole circle (at 8.75 0) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 8 /08))
    (pad 9 thru_hole circle (at 10 0) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 9 /09))
    (pad 10 thru_hole circle (at 11.25 0) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 1 /10))
    (pad 11 thru_hole circle (at 0 -1.25) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 10 /11))
    (pad 12 thru_hole circle (at 1.25 -1.25) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 11 /12))
    (pad 13 thru_hole circle (at 2.5 -1.25) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 12 /13))
    (pad 14 thru_hole circle (at 3.75 -1.25) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 13 /14))
    (pad 15 thru_hole circle (at 5 -1.25) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 14 /15))
    (pad 16 thru_hole circle (at 6.25 -1.25) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 15 /16))
    (pad 17 thru_hole circle (at 7.5 -1.25) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 16 /17))
    (pad 18 thru_hole circle (at 8.75 -1.25) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 17 /18))
    (pad 19 thru_hole circle (at 10 -1.25) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 18 /19))
    (pad 20 thru_hole circle (at 11.25 -1.25) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 19 /20))
    (model ${KIPRJMOD}/3D/G125-MV12005L0P.stp
      (offset (xyz 5.5 0.5 1.5))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module footprints:test_pads_125mm_x10 (layer F.Cu) (tedit 6384296E)
    (at 11.25 -6.985)
    (descr "Harwin Gecko Connector, 6 pins, dual row female, vertical entry, PN:G125-FVX0605L0X")
    (tags "connector harwin gecko")
    (fp_text reference J4 (at 1 1.5) (layer F.SilkS) hide)
    (fp_text value "test points" (at 5.5 -1.5) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 10 thru_hole circle (at 11.25 0) (size 0.95 0.95) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 /10))
    (pad 9 thru_hole circle (at 10 0) (size 0.95 0.95) (drill 0.3) (layers *.Cu *.Mask)
      (net 9 /09))
    (pad 8 thru_hole circle (at 8.75 0) (size 0.95 0.95) (drill 0.3) (layers *.Cu *.Mask)
      (net 8 /08))
    (pad 7 thru_hole circle (at 7.5 0) (size 0.95 0.95) (drill 0.3) (layers *.Cu *.Mask)
      (net 7 /07))
    (pad 6 thru_hole circle (at 6.25 0) (size 0.95 0.95) (drill 0.3) (layers *.Cu *.Mask)
      (net 6 /06))
    (pad 5 thru_hole circle (at 5 0) (size 0.95 0.95) (drill 0.3) (layers *.Cu *.Mask)
      (net 5 /05))
    (pad 4 thru_hole circle (at 3.75 0) (size 0.95 0.95) (drill 0.3) (layers *.Cu *.Mask)
      (net 4 /04))
    (pad 1 thru_hole circle (at 0 0) (size 0.95 0.95) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 /01))
    (pad 2 thru_hole circle (at 1.25 0) (size 0.95 0.95) (drill 0.3) (layers *.Cu *.Mask)
      (net 3 /02))
    (pad 3 thru_hole circle (at 2.5 0) (size 0.95 0.95) (drill 0.3) (layers *.Cu *.Mask)
      (net 20 /03))
    (model ${KISYS3DMOD}/Connector_Harwin.3dshapes/Harwin_Gecko-G125-FVX0605L0X_2x03_P1.25mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:test_pads_125mm_x10 (layer F.Cu) (tedit 6384296E)
    (at 11.25 -13.5)
    (descr "Harwin Gecko Connector, 6 pins, dual row female, vertical entry, PN:G125-FVX0605L0X")
    (tags "connector harwin gecko")
    (fp_text reference J5 (at 1 1.5) (layer F.SilkS) hide)
    (fp_text value "test points" (at 5.5 -1.5) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 3 thru_hole circle (at 2.5 0) (size 0.95 0.95) (drill 0.3) (layers *.Cu *.Mask)
      (net 12 /13))
    (pad 2 thru_hole circle (at 1.25 0) (size 0.95 0.95) (drill 0.3) (layers *.Cu *.Mask)
      (net 11 /12))
    (pad 1 thru_hole circle (at 0 0) (size 0.95 0.95) (drill 0.3) (layers *.Cu *.Mask)
      (net 10 /11))
    (pad 4 thru_hole circle (at 3.75 0) (size 0.95 0.95) (drill 0.3) (layers *.Cu *.Mask)
      (net 13 /14))
    (pad 5 thru_hole circle (at 5 0) (size 0.95 0.95) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /15))
    (pad 6 thru_hole circle (at 6.25 0) (size 0.95 0.95) (drill 0.3) (layers *.Cu *.Mask)
      (net 15 /16))
    (pad 7 thru_hole circle (at 7.5 0) (size 0.95 0.95) (drill 0.3) (layers *.Cu *.Mask)
      (net 16 /17))
    (pad 8 thru_hole circle (at 8.75 0) (size 0.95 0.95) (drill 0.3) (layers *.Cu *.Mask)
      (net 17 /18))
    (pad 9 thru_hole circle (at 10 0) (size 0.95 0.95) (drill 0.3) (layers *.Cu *.Mask)
      (net 18 /19))
    (pad 10 thru_hole circle (at 11.25 0) (size 0.95 0.95) (drill 0.3) (layers *.Cu *.Mask)
      (net 19 /20))
    (model ${KISYS3DMOD}/Connector_Harwin.3dshapes/Harwin_Gecko-G125-FVX0605L0X_2x03_P1.25mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:DFN-8-1EP_3x2mm (layer F.Cu) (tedit 638826C0)
    (at 44.25 -18 180)
    (descr "8-Lead Plastic Dual Flat, No Lead Package (8MA2) - 2x3x0.6 mm Body [UDFN] (see Atmel-8815-SEEPROM-AT24CS01-02-Datasheet.pdf)")
    (tags "DFN 0.5")
    (attr smd)
    (fp_text reference U1 (at 0 -2.55 180) (layer F.SilkS) hide)
    (fp_text value 24LC32 (at 0 2 180) (layer F.SilkS))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad "" smd rect (at 0.325 0.375 180) (size 0.5 0.6) (layers F.Paste))
    (pad "" smd rect (at 0.325 -0.375 180) (size 0.5 0.6) (layers F.Paste))
    (pad "" smd rect (at -0.325 0.375 180) (size 0.5 0.6) (layers F.Paste))
    (pad "" smd rect (at -0.325 -0.375 180) (size 0.5 0.6) (layers F.Paste))
    (pad 9 smd rect (at 0 0 180) (size 1.3 1.5) (layers F.Cu F.Mask))
    (pad 8 smd rect (at 1.45 -0.75 180) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 24 +5V))
    (pad 7 smd rect (at 1.45 -0.25 180) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(U1-Pad7)"))
    (pad 6 smd rect (at 1.45 0.25 180) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 23 /D3_SCL))
    (pad 5 smd rect (at 1.45 0.75 180) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 21 /D2_SDA))
    (pad 4 smd rect (at -1.45 0.75 180) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 22 GND))
    (pad 3 smd rect (at -1.45 0.25 180) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 22 GND))
    (pad 2 smd rect (at -1.45 -0.25 180) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 22 GND))
    (pad 1 smd rect (at -1.45 -0.75 180) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(R1-Pad1)"))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/DFN-8-1EP_3x2mm_P0.5mm_EP1.3x1.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:G125-MS11005L0P (layer F.Cu) (tedit 0)
    (at 16.9 -10.2)
    (descr G125-MS11005L0P)
    (tags Connector)
    (attr smd)
    (fp_text reference J10 (at 0 0) (layer F.SilkS) hide)
    (fp_text value "Gecko 20P" (at 0 0) (layer F.SilkS) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -5.625 1.85) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 /01))
    (pad 2 smd rect (at -4.375 1.85) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 3 /02))
    (pad 3 smd rect (at -3.125 1.85) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 20 /03))
    (pad 4 smd rect (at -1.875 1.85) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 4 /04))
    (pad 5 smd rect (at -0.625 1.85) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 5 /05))
    (pad 6 smd rect (at 0.625 1.85) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 6 /06))
    (pad 7 smd rect (at 1.875 1.85) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 7 /07))
    (pad 8 smd rect (at 3.125 1.85) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 8 /08))
    (pad 9 smd rect (at 4.375 1.85) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 9 /09))
    (pad 10 smd rect (at 5.625 1.85) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 1 /10))
    (pad 11 smd rect (at -5.625 -1.85) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 10 /11))
    (pad 12 smd rect (at -4.375 -1.85) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 11 /12))
    (pad 13 smd rect (at -3.125 -1.85) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 12 /13))
    (pad 14 smd rect (at -1.875 -1.85) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 13 /14))
    (pad 15 smd rect (at -0.625 -1.85) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 14 /15))
    (pad 16 smd rect (at 0.625 -1.85) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 15 /16))
    (pad 17 smd rect (at 1.875 -1.85) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 16 /17))
    (pad 18 smd rect (at 3.125 -1.85) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 17 /18))
    (pad 19 smd rect (at 4.375 -1.85) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 18 /19))
    (pad 20 smd rect (at 5.625 -1.85) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 19 /20))
    (model G125-MS12005L0P.stp
      (offset (xyz 0 0 1.999999969963015))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (gr_text "7\n8\n9\n10\n11\n12" (at 35.75 -14 90) (layer F.SilkS))
  (gr_text "11\n12\n13\n14\n15\n16\n17\n18\n19\n20" (at 16.75 -14 90) (layer F.SilkS))
  (gr_text "1\n2\n3\n4\n5\n6" (at 36 -6.35 90) (layer F.SilkS))
  (gr_text "1\n2\n3\n4\n5\n6\n7\n8\n9\n10" (at 17 -6.35 90) (layer F.SilkS))
  (gr_text "Harwin Gecko G125" (at 27.3 -18) (layer F.SilkS))
  (gr_text "Rev 0.0\nMar 2023" (at 49.53 -1.27) (layer B.SilkS))
  (gr_text github.com/aspro648/RPB (at 27 -1.5) (layer B.SilkS))
  (gr_text Template (at 27.5 -2) (layer Dwgs.User))
  (gr_text "Rapid Prototyping Card" (at 27 -3) (layer B.SilkS))
)
