(kicad_pcb (version 20171130) (host pcbnew 5.1.12-84ad8e8a86~92~ubuntu21.04.1)
  (general
    (thickness 1.6)
    (drawings 31)
    (tracks 247)
    (zones 0)
    (modules 42)
    (nets 47)
  )
  (page USLetter)
  (title_block
    (title "DE0-NANO RGB2VGA")
    (date 2021-11-15)
    (rev 003)
    (company "Brian K. White - b.kenyon.w@gmail.com")
    (comment 1 "Original Design: Luis Antoniosi")
  )
  (layers
    (0 Top signal)
    (31 Bottom signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.2)
    (user_trace_width 0.3048)
    (user_trace_width 0.4)
    (trace_clearance 0.2)
    (zone_clearance 0.2)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.6)
    (via_drill 0.3)
    (via_min_size 0.5)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 4 4)
    (pad_drill 3.200001)
    (pad_to_mask_clearance 0)
    (solder_mask_min_width 0.22)
    (aux_axis_origin 139.7 100.965)
    (grid_origin 139.7 100.965)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "GERBER_rgb2vga_v003.8"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 /CSYNC)
  (net 3 /RSET)
  (net 4 /DIFFG)
  (net 5 /HSYNC)
  (net 6 /VSYNC)
  (net 7 /DIFFB)
  (net 8 /DIFFR)
  (net 9 /DIFF_N)
  (net 10 +5V)
  (net 11 /_BRIGHT)
  (net 12 /D0)
  (net 13 /D1)
  (net 14 /_VSYNC)
  (net 15 /D2)
  (net 16 /_HSYNC)
  (net 17 /R2)
  (net 18 /R1)
  (net 19 /R0)
  (net 20 /G2)
  (net 21 /G1)
  (net 22 /G0)
  (net 23 /B1)
  (net 24 /B2)
  (net 25 /B0)
  (net 26 /HS)
  (net 27 /VS)
  (net 28 "Net-(JP2-Pad1)")
  (net 29 "Net-(JP3-Pad1)")
  (net 30 /RED)
  (net 31 /GREEN)
  (net 32 /BLUE)
  (net 33 "Net-(R12-Pad2)")
  (net 34 "Net-(R14-Pad2)")
  (net 35 /BRIGHT)
  (net 36 "Net-(J1-Pad27)")
  (net 37 "Net-(J1-Pad25)")
  (net 38 "Net-(J1-Pad23)")
  (net 39 "Net-(J1-Pad21)")
  (net 40 "Net-(J1-Pad19)")
  (net 41 "Net-(J1-Pad17)")
  (net 42 "Net-(J1-Pad15)")
  (net 43 "Net-(J1-Pad13)")
  (net 44 "Net-(J6-Pad14)")
  (net 45 "Net-(J6-Pad13)")
  (net 46 "Net-(C1-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.6)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net /B0)
    (add_net /B1)
    (add_net /B2)
    (add_net /BLUE)
    (add_net /BRIGHT)
    (add_net /CSYNC)
    (add_net /D0)
    (add_net /D1)
    (add_net /D2)
    (add_net /DIFFB)
    (add_net /DIFFG)
    (add_net /DIFFR)
    (add_net /DIFF_N)
    (add_net /G0)
    (add_net /G1)
    (add_net /G2)
    (add_net /GREEN)
    (add_net /HS)
    (add_net /HSYNC)
    (add_net /R0)
    (add_net /R1)
    (add_net /R2)
    (add_net /RED)
    (add_net /RSET)
    (add_net /VS)
    (add_net /VSYNC)
    (add_net /_BRIGHT)
    (add_net /_HSYNC)
    (add_net /_VSYNC)
    (add_net GND)
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(J1-Pad13)")
    (add_net "Net-(J1-Pad15)")
    (add_net "Net-(J1-Pad17)")
    (add_net "Net-(J1-Pad19)")
    (add_net "Net-(J1-Pad21)")
    (add_net "Net-(J1-Pad23)")
    (add_net "Net-(J1-Pad25)")
    (add_net "Net-(J1-Pad27)")
    (add_net "Net-(J6-Pad13)")
    (add_net "Net-(J6-Pad14)")
    (add_net "Net-(JP2-Pad1)")
    (add_net "Net-(JP3-Pad1)")
    (add_net "Net-(R12-Pad2)")
    (add_net "Net-(R14-Pad2)")
  )
  (module 000_LOCAL:DE0-Nano (layer Top) (tedit 619543BB)
    (at 143.7 103.765 270)
    (attr virtual)
    (fp_text reference REF** (at 0 2 90) (layer F.SilkS) hide)
    (fp_text value DE0-Nano (at 0 -2 90) (layer F.Fab))
    (model ${KIPRJMOD}/000_LOCAL.pretty/3dshapes/DE0-Nano.step
      (offset (xyz 0 0 -14.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000_LOCAL:C025-025X050 (layer Top) (tedit 6192B1FC)
    (at 151.765 104.14)
    (descr "<b>CAPACITOR</b><p>\ngrid 2.5 mm, outline 2.5 x 5 mm")
    (fp_text reference C1 (at -1.8415 -1.397 unlocked) (layer F.SilkS))
    (fp_text value 0.1u (at 1.2065 -1.397 unlocked) (layer F.SilkS))
    (pad 2 thru_hole circle (at 1.27 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 46 "Net-(C1-Pad2)") (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at -1.27 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 2 /CSYNC) (solder_mask_margin 0.1016))
    (model ${KIPRJMOD}/000_LOCAL.pretty/3dshapes/C_Disc_D3.8mm_W2.6mm_P2.50mm.step
      (offset (xyz -1.27 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000_LOCAL:C025-025X050 (layer Top) (tedit 6192B1FC)
    (at 151.765 107.95)
    (descr "<b>CAPACITOR</b><p>\ngrid 2.5 mm, outline 2.5 x 5 mm")
    (fp_text reference C2 (at -1.8415 -1.397 unlocked) (layer F.SilkS))
    (fp_text value 0.1u (at 1.2065 -1.397 unlocked) (layer F.SilkS))
    (pad 2 thru_hole circle (at 1.27 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 3 /RSET) (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at -1.27 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (model ${KIPRJMOD}/000_LOCAL.pretty/3dshapes/C_Disc_D3.8mm_W2.6mm_P2.50mm.step
      (offset (xyz -1.27 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000_LOCAL:0207_10 (layer Top) (tedit 618DF372)
    (at 154.94 111.125)
    (descr "<b>RESISTOR</b><p>\ntype 0207, grid 10 mm")
    (fp_text reference R13 (at -5.08 -0.762 unlocked) (layer F.SilkS))
    (fp_text value 680K (at 0 0.5 unlocked) (layer F.SilkS))
    (fp_text user %R (at 0 0.1) (layer F.Fab))
    (pad 2 thru_hole circle (at 5.08 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at -5.08 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 3 /RSET) (solder_mask_margin 0.1016))
    (model ${KIPRJMOD}/000_LOCAL.pretty/3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.step
      (offset (xyz -5.08 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000_LOCAL:0207_10 (layer Top) (tedit 618DF372)
    (at 154.94 126.365)
    (descr "<b>RESISTOR</b><p>\ntype 0207, grid 10 mm")
    (fp_text reference R11 (at -5.08 -0.762 unlocked) (layer F.SilkS))
    (fp_text value 2K (at 0 0.5 unlocked) (layer F.SilkS))
    (fp_text user %R (at 0 0.1) (layer F.Fab))
    (pad 2 thru_hole circle (at 5.08 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 9 /DIFF_N) (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at -5.08 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 15 /D2) (solder_mask_margin 0.1016))
    (model ${KIPRJMOD}/000_LOCAL.pretty/3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.step
      (offset (xyz -5.08 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000_LOCAL:0207_10 (layer Top) (tedit 618DF372)
    (at 154.94 123.825)
    (descr "<b>RESISTOR</b><p>\ntype 0207, grid 10 mm")
    (fp_text reference R16 (at -5.08 -0.762 unlocked) (layer F.SilkS))
    (fp_text value 1K (at 0 0.5 unlocked) (layer F.SilkS))
    (fp_text user %R (at 0 0.1) (layer F.Fab))
    (pad 2 thru_hole circle (at 5.08 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 33 "Net-(R12-Pad2)") (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at -5.08 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 9 /DIFF_N) (solder_mask_margin 0.1016))
    (model ${KIPRJMOD}/000_LOCAL.pretty/3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.step
      (offset (xyz -5.08 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000_LOCAL:0207_10 (layer Top) (tedit 618DF372)
    (at 154.94 121.285)
    (descr "<b>RESISTOR</b><p>\ntype 0207, grid 10 mm")
    (fp_text reference R12 (at -5.08 -0.762 unlocked) (layer F.SilkS))
    (fp_text value 2K (at 0 0.5 unlocked) (layer F.SilkS))
    (fp_text user %R (at 0 0.1) (layer F.Fab))
    (pad 2 thru_hole circle (at 5.08 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 33 "Net-(R12-Pad2)") (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at -5.08 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 13 /D1) (solder_mask_margin 0.1016))
    (model ${KIPRJMOD}/000_LOCAL.pretty/3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.step
      (offset (xyz -5.08 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000_LOCAL:0207_10 (layer Top) (tedit 618DF372)
    (at 154.94 118.745)
    (descr "<b>RESISTOR</b><p>\ntype 0207, grid 10 mm")
    (fp_text reference R15 (at -5.08 -0.762 unlocked) (layer F.SilkS))
    (fp_text value 1K (at 0 0.5 unlocked) (layer F.SilkS))
    (fp_text user %R (at 0 0.1) (layer F.Fab))
    (pad 2 thru_hole circle (at 5.08 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 34 "Net-(R14-Pad2)") (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at -5.08 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 33 "Net-(R12-Pad2)") (solder_mask_margin 0.1016))
    (model ${KIPRJMOD}/000_LOCAL.pretty/3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.step
      (offset (xyz -5.08 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000_LOCAL:0207_10 (layer Top) (tedit 618DF372)
    (at 154.94 116.205)
    (descr "<b>RESISTOR</b><p>\ntype 0207, grid 10 mm")
    (fp_text reference R14 (at -5.08 -0.762 unlocked) (layer F.SilkS))
    (fp_text value 2K (at 0 0.5 unlocked) (layer F.SilkS))
    (fp_text user %R (at 0 0.1) (layer F.Fab))
    (pad 2 thru_hole circle (at 5.08 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 34 "Net-(R14-Pad2)") (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at -5.08 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 12 /D0) (solder_mask_margin 0.1016))
    (model ${KIPRJMOD}/000_LOCAL.pretty/3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.step
      (offset (xyz -5.08 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000_LOCAL:0207_10 (layer Top) (tedit 618DF372)
    (at 154.94 113.665)
    (descr "<b>RESISTOR</b><p>\ntype 0207, grid 10 mm")
    (fp_text reference R17 (at -5.08 -0.762 unlocked) (layer F.SilkS))
    (fp_text value 2K (at 0 0.5 unlocked) (layer F.SilkS))
    (fp_text user %R (at 0 0.1) (layer F.Fab))
    (pad 2 thru_hole circle (at 5.08 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 34 "Net-(R14-Pad2)") (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at -5.08 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (model ${KIPRJMOD}/000_LOCAL.pretty/3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.step
      (offset (xyz -5.08 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000_LOCAL:0207_10 (layer Top) (tedit 618DF372)
    (at 154.94 100.965)
    (descr "<b>RESISTOR</b><p>\ntype 0207, grid 10 mm")
    (fp_text reference R1 (at -5.08 -0.762 unlocked) (layer F.SilkS))
    (fp_text value 390 (at 0 0.5 unlocked) (layer F.SilkS))
    (fp_text user %R (at 0 0.1) (layer F.Fab))
    (pad 2 thru_hole circle (at 5.08 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 30 /RED) (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at -5.08 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 17 /R2) (solder_mask_margin 0.1016))
    (model ${KIPRJMOD}/000_LOCAL.pretty/3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.step
      (offset (xyz -5.08 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000_LOCAL:0207_10 (layer Top) (tedit 618DF372)
    (at 154.94 98.425)
    (descr "<b>RESISTOR</b><p>\ntype 0207, grid 10 mm")
    (fp_text reference R2 (at -5.08 -0.762 unlocked) (layer F.SilkS))
    (fp_text value 820 (at 0 0.5 unlocked) (layer F.SilkS))
    (fp_text user %R (at 0 0.1) (layer F.Fab))
    (pad 2 thru_hole circle (at 5.08 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 30 /RED) (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at -5.08 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 18 /R1) (solder_mask_margin 0.1016))
    (model ${KIPRJMOD}/000_LOCAL.pretty/3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.step
      (offset (xyz -5.08 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000_LOCAL:0207_10 (layer Top) (tedit 618DF372)
    (at 154.94 95.885)
    (descr "<b>RESISTOR</b><p>\ntype 0207, grid 10 mm")
    (fp_text reference R3 (at -5.08 -0.762 unlocked) (layer F.SilkS))
    (fp_text value 1.8K (at 0 0.5 unlocked) (layer F.SilkS))
    (fp_text user %R (at 0 0.1) (layer F.Fab))
    (pad 2 thru_hole circle (at 5.08 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 30 /RED) (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at -5.08 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 19 /R0) (solder_mask_margin 0.1016))
    (model ${KIPRJMOD}/000_LOCAL.pretty/3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.step
      (offset (xyz -5.08 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000_LOCAL:0207_10 (layer Top) (tedit 618DF372)
    (at 154.94 93.345)
    (descr "<b>RESISTOR</b><p>\ntype 0207, grid 10 mm")
    (fp_text reference R4 (at -5.08 -0.762 unlocked) (layer F.SilkS))
    (fp_text value 390 (at 0 0.5 unlocked) (layer F.SilkS))
    (fp_text user %R (at 0 0.1) (layer F.Fab))
    (pad 2 thru_hole circle (at 5.08 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 31 /GREEN) (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at -5.08 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 20 /G2) (solder_mask_margin 0.1016))
    (model ${KIPRJMOD}/000_LOCAL.pretty/3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.step
      (offset (xyz -5.08 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000_LOCAL:0207_10 (layer Top) (tedit 618DF372)
    (at 154.94 90.805)
    (descr "<b>RESISTOR</b><p>\ntype 0207, grid 10 mm")
    (fp_text reference R5 (at -5.08 -0.762 unlocked) (layer F.SilkS))
    (fp_text value 820 (at 0 0.5 unlocked) (layer F.SilkS))
    (fp_text user %R (at 0 0.1) (layer F.Fab))
    (pad 2 thru_hole circle (at 5.08 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 31 /GREEN) (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at -5.08 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 21 /G1) (solder_mask_margin 0.1016))
    (model ${KIPRJMOD}/000_LOCAL.pretty/3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.step
      (offset (xyz -5.08 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000_LOCAL:0207_10 (layer Top) (tedit 618DF372)
    (at 154.94 88.265)
    (descr "<b>RESISTOR</b><p>\ntype 0207, grid 10 mm")
    (fp_text reference R6 (at -5.08 -0.762 unlocked) (layer F.SilkS))
    (fp_text value 1.8K (at 0 0.5 unlocked) (layer F.SilkS))
    (fp_text user %R (at 0 0.1) (layer F.Fab))
    (pad 2 thru_hole circle (at 5.08 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 31 /GREEN) (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at -5.08 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 22 /G0) (solder_mask_margin 0.1016))
    (model ${KIPRJMOD}/000_LOCAL.pretty/3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.step
      (offset (xyz -5.08 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000_LOCAL:0207_10 (layer Top) (tedit 618DF372)
    (at 154.94 85.725)
    (descr "<b>RESISTOR</b><p>\ntype 0207, grid 10 mm")
    (fp_text reference R7 (at -5.08 -0.762 unlocked) (layer F.SilkS))
    (fp_text value 390 (at 0 0.5 unlocked) (layer F.SilkS))
    (fp_text user %R (at 0 0.1) (layer F.Fab))
    (pad 2 thru_hole circle (at 5.08 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 32 /BLUE) (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at -5.08 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 24 /B2) (solder_mask_margin 0.1016))
    (model ${KIPRJMOD}/000_LOCAL.pretty/3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.step
      (offset (xyz -5.08 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000_LOCAL:0207_10 (layer Top) (tedit 618DF372)
    (at 154.94 83.185)
    (descr "<b>RESISTOR</b><p>\ntype 0207, grid 10 mm")
    (fp_text reference R8 (at -5.08 -0.762 unlocked) (layer F.SilkS))
    (fp_text value 820 (at 0 0.5 unlocked) (layer F.SilkS))
    (fp_text user %R (at 0 0.1) (layer F.Fab))
    (pad 2 thru_hole circle (at 5.08 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 32 /BLUE) (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at -5.08 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 23 /B1) (solder_mask_margin 0.1016))
    (model ${KIPRJMOD}/000_LOCAL.pretty/3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.step
      (offset (xyz -5.08 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000_LOCAL:0207_10 (layer Top) (tedit 618DF372)
    (at 154.94 80.645)
    (descr "<b>RESISTOR</b><p>\ntype 0207, grid 10 mm")
    (fp_text reference R26 (at -5.08 -0.762 unlocked) (layer F.SilkS))
    (fp_text value 1.8K (at 0 0.5 unlocked) (layer F.SilkS))
    (fp_text user %R (at 0 0.1) (layer F.Fab))
    (pad 2 thru_hole circle (at 5.08 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 32 /BLUE) (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at -5.08 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 25 /B0) (solder_mask_margin 0.1016))
    (model ${KIPRJMOD}/000_LOCAL.pretty/3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.step
      (offset (xyz -5.08 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000_LOCAL:0207_10 (layer Top) (tedit 618DF372)
    (at 154.94 78.105)
    (descr "<b>RESISTOR</b><p>\ntype 0207, grid 10 mm")
    (fp_text reference R10 (at -5.08 -0.762 unlocked) (layer F.SilkS))
    (fp_text value 47 (at 0 0.5 unlocked) (layer F.SilkS))
    (fp_text user %R (at 0 0.1) (layer F.Fab))
    (pad 2 thru_hole circle (at 5.08 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 45 "Net-(J6-Pad13)") (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at -5.08 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 26 /HS) (solder_mask_margin 0.1016))
    (model ${KIPRJMOD}/000_LOCAL.pretty/3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.step
      (offset (xyz -5.08 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000_LOCAL:0207_10 (layer Top) (tedit 618DF372)
    (at 154.94 75.565)
    (descr "<b>RESISTOR</b><p>\ntype 0207, grid 10 mm")
    (fp_text reference R9 (at -5.08 -0.762 unlocked) (layer F.SilkS))
    (fp_text value 47 (at 0 0.5 unlocked) (layer F.SilkS))
    (fp_text user %R (at 0 0.1) (layer F.Fab))
    (pad 2 thru_hole circle (at 5.08 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 44 "Net-(J6-Pad14)") (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at -5.08 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 27 /VS) (solder_mask_margin 0.1016))
    (model ${KIPRJMOD}/000_LOCAL.pretty/3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.step
      (offset (xyz -5.08 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000_LOCAL:0207_10 (layer Top) (tedit 618DF372)
    (at 130.81 81.915)
    (descr "<b>RESISTOR</b><p>\ntype 0207, grid 10 mm")
    (fp_text reference R23 (at -5.08 -0.762 unlocked) (layer F.SilkS))
    (fp_text value 82 (at 0 0.5 unlocked) (layer F.SilkS))
    (fp_text user %R (at 0 0.1) (layer F.Fab))
    (pad 2 thru_hole circle (at 5.08 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at -5.08 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 8 /DIFFR) (solder_mask_margin 0.1016))
    (model ${KIPRJMOD}/000_LOCAL.pretty/3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.step
      (offset (xyz -5.08 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000_LOCAL:0207_10 (layer Top) (tedit 618DF372)
    (at 130.81 79.375)
    (descr "<b>RESISTOR</b><p>\ntype 0207, grid 10 mm")
    (fp_text reference R22 (at -5.08 -0.762 unlocked) (layer F.SilkS))
    (fp_text value 82 (at 0 0.5 unlocked) (layer F.SilkS))
    (fp_text user %R (at 0 0.1) (layer F.Fab))
    (pad 2 thru_hole circle (at 5.08 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at -5.08 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 7 /DIFFB) (solder_mask_margin 0.1016))
    (model ${KIPRJMOD}/000_LOCAL.pretty/3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.step
      (offset (xyz -5.08 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000_LOCAL:0207_10 (layer Top) (tedit 618DF372)
    (at 130.81 76.835)
    (descr "<b>RESISTOR</b><p>\ntype 0207, grid 10 mm")
    (fp_text reference R25 (at -5.08 -0.762 unlocked) (layer F.SilkS))
    (fp_text value 82 (at 0 0.5 unlocked) (layer F.SilkS))
    (fp_text user %R (at 0 0.1) (layer F.Fab))
    (pad 2 thru_hole circle (at 5.08 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at -5.08 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 4 /DIFFG) (solder_mask_margin 0.1016))
    (model ${KIPRJMOD}/000_LOCAL.pretty/3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.step
      (offset (xyz -5.08 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000_LOCAL:0207_10 (layer Top) (tedit 618DF372)
    (at 130.81 125.095)
    (descr "<b>RESISTOR</b><p>\ntype 0207, grid 10 mm")
    (fp_text reference R20 (at -5.08 -0.762 unlocked) (layer F.SilkS))
    (fp_text value 1.2K (at 0 0.5 unlocked) (layer F.SilkS))
    (fp_text user %R (at 0 0.1) (layer F.Fab))
    (pad 2 thru_hole circle (at 5.08 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 16 /_HSYNC) (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at -5.08 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 5 /HSYNC) (solder_mask_margin 0.1016))
    (model ${KIPRJMOD}/000_LOCAL.pretty/3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.step
      (offset (xyz -5.08 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000_LOCAL:0207_10 (layer Top) (tedit 618DF372)
    (at 130.81 122.555)
    (descr "<b>RESISTOR</b><p>\ntype 0207, grid 10 mm")
    (fp_text reference R21 (at -5.08 -0.762 unlocked) (layer F.SilkS))
    (fp_text value 6.8K (at 0 0.5 unlocked) (layer F.SilkS))
    (fp_text user %R (at 0 0.1) (layer F.Fab))
    (pad 2 thru_hole circle (at 5.08 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 16 /_HSYNC) (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at -5.08 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (model ${KIPRJMOD}/000_LOCAL.pretty/3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.step
      (offset (xyz -5.08 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000_LOCAL:0207_10 (layer Top) (tedit 618DF372)
    (at 130.81 120.015)
    (descr "<b>RESISTOR</b><p>\ntype 0207, grid 10 mm")
    (fp_text reference R19 (at -5.08 -0.762 unlocked) (layer F.SilkS))
    (fp_text value 1.2K (at 0 0.5 unlocked) (layer F.SilkS))
    (fp_text user %R (at 0 0.1) (layer F.Fab))
    (pad 2 thru_hole circle (at 5.08 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 14 /_VSYNC) (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at -5.08 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 6 /VSYNC) (solder_mask_margin 0.1016))
    (model ${KIPRJMOD}/000_LOCAL.pretty/3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.step
      (offset (xyz -5.08 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000_LOCAL:0207_10 (layer Top) (tedit 618DF372)
    (at 130.81 117.475)
    (descr "<b>RESISTOR</b><p>\ntype 0207, grid 10 mm")
    (fp_text reference R18 (at -5.08 -0.762 unlocked) (layer F.SilkS))
    (fp_text value 6.8K (at 0 0.5 unlocked) (layer F.SilkS))
    (fp_text user %R (at 0 0.1) (layer F.Fab))
    (pad 2 thru_hole circle (at 5.08 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 14 /_VSYNC) (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at -5.08 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (model ${KIPRJMOD}/000_LOCAL.pretty/3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.step
      (offset (xyz -5.08 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000_LOCAL:0207_10 (layer Top) (tedit 618DF372)
    (at 117.729 111.125 90)
    (descr "<b>RESISTOR</b><p>\ntype 0207, grid 10 mm")
    (fp_text reference R28 (at -5.08 -0.762 90 unlocked) (layer F.SilkS))
    (fp_text value 1K (at 0 0.5 90 unlocked) (layer F.SilkS))
    (fp_text user %R (at 0 0.1 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5.08 0 90) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 11 /_BRIGHT) (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at -5.08 0 90) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (model ${KIPRJMOD}/000_LOCAL.pretty/3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.step
      (offset (xyz -5.08 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000_LOCAL:0207_10 (layer Top) (tedit 618DF2D3)
    (at 117.729 99.06 90)
    (descr "<b>RESISTOR</b><p>\ntype 0207, grid 10 mm")
    (fp_text reference R27 (at -5.08 -0.889 90 unlocked) (layer F.SilkS))
    (fp_text value 1K (at 0 0.5 90 unlocked) (layer F.SilkS))
    (fp_text user %R (at 0 0.1 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5.08 0 90) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 35 /BRIGHT) (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at -5.08 0 90) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 11 /_BRIGHT) (solder_mask_margin 0.1016))
    (model ${KIPRJMOD}/000_LOCAL.pretty/3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.step
      (offset (xyz -5.08 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000_LOCAL:HD15-SN-25 (layer Top) (tedit 6187BD36)
    (at 172.085 100.965 90)
    (descr "15-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.29x1.98mm, pin-PCB-offset 3.0300000000000002mm, distance of mounting holes 25mm, distance of mounting holes to PCB edge 4.9399999999999995mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
    (tags "15-pin D-Sub connector horizontal angled 90deg THT female pitch 2.29x1.98mm pin-PCB-offset 3.0300000000000002mm mounting-holes-distance 25mm mounting-hole-offset 25mm")
    (fp_text reference J6 (at 6.604 -1.905) (layer F.SilkS))
    (fp_text value VGA_OUT (at -16.637 0) (layer F.SilkS))
    (fp_text user %R (at 0 8.34 90) (layer F.Fab))
    (pad 0 thru_hole circle (at 12.5 0 90) (size 4.064 4.064) (drill 3.2004) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 0 thru_hole circle (at -12.5 0 90) (size 4.064 4.064) (drill 3.2004) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 15 thru_hole circle (at -4.834 1.98 90) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask))
    (pad 14 thru_hole circle (at -2.544 1.98 90) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 44 "Net-(J6-Pad14)"))
    (pad 13 thru_hole circle (at -0.254 1.98 90) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 45 "Net-(J6-Pad13)"))
    (pad 12 thru_hole circle (at 2.036 1.98 90) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask))
    (pad 11 thru_hole circle (at 4.326 1.98 90) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask))
    (pad 10 thru_hole circle (at -3.689 0 90) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 9 thru_hole circle (at -1.399 0 90) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 8 thru_hole circle (at 0.891 0 90) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole circle (at 3.181 0 90) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole circle (at 5.471 0 90) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole circle (at -4.834 -1.98 90) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole circle (at -2.544 -1.98 90) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at -0.254 -1.98 90) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 32 /BLUE))
    (pad 2 thru_hole circle (at 2.036 -1.98 90) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 31 /GREEN))
    (pad 1 thru_hole roundrect (at 4.326 -1.98 90) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 30 /RED))
    (model ${KIPRJMOD}/000_LOCAL.pretty/3dshapes/HD15-SN-25.step
      (offset (xyz -6.858 5.4991 -5.715))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 90 -180))
    )
  )
  (module 000_LOCAL:HD15-SN-25 (layer Top) (tedit 6187BD36)
    (at 107.315 100.965 270)
    (descr "15-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.29x1.98mm, pin-PCB-offset 3.0300000000000002mm, distance of mounting holes 25mm, distance of mounting holes to PCB edge 4.9399999999999995mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
    (tags "15-pin D-Sub connector horizontal angled 90deg THT female pitch 2.29x1.98mm pin-PCB-offset 3.0300000000000002mm mounting-holes-distance 25mm mounting-hole-offset 25mm")
    (fp_text reference J2 (at 6.858 -2.032) (layer F.SilkS))
    (fp_text value RGB_IN (at 0 -5.08 90) (layer F.SilkS))
    (fp_text user %R (at 0 8.34 90) (layer F.Fab))
    (pad 0 thru_hole circle (at 12.5 0 270) (size 4.064 4.064) (drill 3.2004) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 0 thru_hole circle (at -12.5 0 270) (size 4.064 4.064) (drill 3.2004) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 15 thru_hole circle (at -4.834 1.98 270) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask))
    (pad 14 thru_hole circle (at -2.544 1.98 270) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask))
    (pad 13 thru_hole circle (at -0.254 1.98 270) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 2 /CSYNC))
    (pad 12 thru_hole circle (at 2.036 1.98 270) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask))
    (pad 11 thru_hole circle (at 4.326 1.98 270) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask))
    (pad 10 thru_hole circle (at -3.689 0 270) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 9 thru_hole circle (at -1.399 0 270) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 8 thru_hole circle (at 0.891 0 270) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole circle (at 3.181 0 270) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole circle (at 5.471 0 270) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole circle (at -4.834 -1.98 270) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole circle (at -2.544 -1.98 270) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 35 /BRIGHT))
    (pad 3 thru_hole circle (at -0.254 -1.98 270) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 7 /DIFFB))
    (pad 2 thru_hole circle (at 2.036 -1.98 270) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 4 /DIFFG))
    (pad 1 thru_hole roundrect (at 4.326 -1.98 270) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 8 /DIFFR))
    (model ${KIPRJMOD}/000_LOCAL.pretty/3dshapes/HD15-SN-25.step
      (offset (xyz -6.858 5.4991 -5.715))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 90 -180))
    )
  )
  (module 000_LOCAL:IDC-Header_2x05_P2.54mm_Horizontal (layer Top) (tedit 61879164)
    (at 107.569 79.375 90)
    (descr "Through hole IDC box header, 2x05, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0")
    (tags "Through hole horizontal IDC box header THT 2x05 2.54mm double row")
    (fp_text reference J3 (at 5.1435 5.08) (layer F.SilkS))
    (fp_text value COCO3_RGB_IN (at -3.429 5.08 180) (layer F.SilkS))
    (fp_text user %R (at 8.83 5.08) (layer F.Fab))
    (pad 10 thru_hole circle (at 2.54 10.16 90) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at 2.54 7.62 90) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask)
      (net 5 /HSYNC))
    (pad 6 thru_hole circle (at 2.54 5.08 90) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at 2.54 2.54 90) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask)
      (net 4 /DIFFG))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 9 thru_hole circle (at 0 10.16 90) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask)
      (net 6 /VSYNC))
    (pad 7 thru_hole circle (at 0 7.62 90) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at 0 5.08 90) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask)
      (net 7 /DIFFB))
    (pad 3 thru_hole circle (at 0 2.54 90) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask)
      (net 8 /DIFFR))
    (pad 1 thru_hole roundrect (at 0 0 90) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask) (roundrect_rratio 0.147)
      (net 1 GND))
    (model ${KIPRJMOD}/000_LOCAL.pretty/3dshapes/IDC-Header_2x05_P2.54mm_Horizontal.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000_LOCAL:PinSocket_2x20_P2.54mm_Vertical (layer Bottom) (tedit 61876BA9)
    (at 164.0586 76.835 180)
    (descr "Through hole straight socket strip, 2x20, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 2x20 2.54mm double row")
    (fp_text reference J5 (at 0 1.905 270 unlocked) (layer B.SilkS))
    (fp_text value GPIO_1 (at -5.715 -1.27 270 unlocked) (layer B.SilkS))
    (fp_text user %R (at 2.54 -3.048 90) (layer B.Fab))
    (pad 40 thru_hole circle (at -2.54 -48.26 180) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask))
    (pad 39 thru_hole circle (at 0 -48.26 180) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask))
    (pad 38 thru_hole circle (at -2.54 -45.72 180) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask))
    (pad 37 thru_hole circle (at 0 -45.72 180) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask))
    (pad 36 thru_hole circle (at -2.54 -43.18 180) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask))
    (pad 35 thru_hole circle (at 0 -43.18 180) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask))
    (pad 34 thru_hole circle (at -2.54 -40.64 180) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask))
    (pad 33 thru_hole circle (at 0 -40.64 180) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask))
    (pad 32 thru_hole circle (at -2.54 -38.1 180) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask))
    (pad 31 thru_hole circle (at 0 -38.1 180) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask))
    (pad 30 thru_hole circle (at -2.54 -35.56 180) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 29 thru_hole circle (at 0 -35.56 180) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask))
    (pad 28 thru_hole circle (at -2.54 -33.02 180) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask)
      (net 17 /R2))
    (pad 27 thru_hole circle (at 0 -33.02 180) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask))
    (pad 26 thru_hole circle (at -2.54 -30.48 180) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask)
      (net 18 /R1))
    (pad 25 thru_hole circle (at 0 -30.48 180) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask))
    (pad 24 thru_hole circle (at -2.54 -27.94 180) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask)
      (net 19 /R0))
    (pad 23 thru_hole circle (at 0 -27.94 180) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask))
    (pad 22 thru_hole circle (at -2.54 -25.4 180) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask)
      (net 20 /G2))
    (pad 21 thru_hole circle (at 0 -25.4 180) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask))
    (pad 20 thru_hole circle (at -2.54 -22.86 180) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask)
      (net 21 /G1))
    (pad 19 thru_hole circle (at 0 -22.86 180) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask))
    (pad 18 thru_hole circle (at -2.54 -20.32 180) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask)
      (net 22 /G0))
    (pad 17 thru_hole circle (at 0 -20.32 180) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask))
    (pad 16 thru_hole circle (at -2.54 -17.78 180) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask)
      (net 24 /B2))
    (pad 15 thru_hole circle (at 0 -17.78 180) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask)
      (net 25 /B0))
    (pad 14 thru_hole circle (at -2.54 -15.24 180) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask)
      (net 23 /B1))
    (pad 13 thru_hole circle (at 0 -15.24 180) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask))
    (pad 12 thru_hole circle (at -2.54 -12.7 180) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 11 thru_hole circle (at 0 -12.7 180) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask))
    (pad 10 thru_hole circle (at -2.54 -10.16 180) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask)
      (net 26 /HS))
    (pad 9 thru_hole circle (at 0 -10.16 180) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at -2.54 -7.62 180) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask)
      (net 27 /VS))
    (pad 7 thru_hole circle (at 0 -7.62 180) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at -2.54 -5.08 180) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at 0 -5.08 180) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at -2.54 -2.54 180) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 0 -2.54 180) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -2.54 0 180) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask))
    (pad 1 thru_hole roundrect (at 0 0 180) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask) (roundrect_rratio 0.1))
    (model ${KIPRJMOD}/000_LOCAL.pretty/3dshapes/PinSocket_2x20_P2.54mm_Vertical.step_
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/3dshapes/SFH11-PBPC-D20-ST-BK--3DModel-STEP-1.STEP
      (offset (xyz -1.27 -24.127 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -90))
    )
  )
  (module 000_LOCAL:PinSocket_2x20_P2.54mm_Vertical (layer Bottom) (tedit 61876BA9)
    (at 123.19 125.095)
    (descr "Through hole straight socket strip, 2x20, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 2x20 2.54mm double row")
    (fp_text reference J1 (at 0 2.159 -90 unlocked) (layer B.SilkS))
    (fp_text value GPIO_0 (at -5.715 0 -90 unlocked) (layer B.SilkS))
    (fp_text user %R (at 2.54 -3.048 90) (layer B.Fab))
    (pad 40 thru_hole circle (at -2.54 -48.26) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask)
      (net 7 /DIFFB))
    (pad 39 thru_hole circle (at 0 -48.26) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask)
      (net 4 /DIFFG))
    (pad 38 thru_hole circle (at -2.54 -45.72) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask)
      (net 9 /DIFF_N))
    (pad 37 thru_hole circle (at 0 -45.72) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask)
      (net 9 /DIFF_N))
    (pad 36 thru_hole circle (at -2.54 -43.18) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask))
    (pad 35 thru_hole circle (at 0 -43.18) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask))
    (pad 34 thru_hole circle (at -2.54 -40.64) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask))
    (pad 33 thru_hole circle (at 0 -40.64) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask))
    (pad 32 thru_hole circle (at -2.54 -38.1) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask)
      (net 8 /DIFFR))
    (pad 31 thru_hole circle (at 0 -38.1) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask)
      (net 9 /DIFF_N))
    (pad 30 thru_hole circle (at -2.54 -35.56) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 29 thru_hole circle (at 0 -35.56) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask))
    (pad 28 thru_hole circle (at -2.54 -33.02) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask))
    (pad 27 thru_hole circle (at 0 -33.02) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask)
      (net 36 "Net-(J1-Pad27)"))
    (pad 26 thru_hole circle (at -2.54 -30.48) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask))
    (pad 25 thru_hole circle (at 0 -30.48) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask)
      (net 37 "Net-(J1-Pad25)"))
    (pad 24 thru_hole circle (at -2.54 -27.94) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask))
    (pad 23 thru_hole circle (at 0 -27.94) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask)
      (net 38 "Net-(J1-Pad23)"))
    (pad 22 thru_hole circle (at -2.54 -25.4) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask))
    (pad 21 thru_hole circle (at 0 -25.4) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask)
      (net 39 "Net-(J1-Pad21)"))
    (pad 20 thru_hole circle (at -2.54 -22.86) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask))
    (pad 19 thru_hole circle (at 0 -22.86) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask)
      (net 40 "Net-(J1-Pad19)"))
    (pad 18 thru_hole circle (at -2.54 -20.32) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask))
    (pad 17 thru_hole circle (at 0 -20.32) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask)
      (net 41 "Net-(J1-Pad17)"))
    (pad 16 thru_hole circle (at -2.54 -17.78) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask))
    (pad 15 thru_hole circle (at 0 -17.78) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask)
      (net 42 "Net-(J1-Pad15)"))
    (pad 14 thru_hole circle (at -2.54 -15.24) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask))
    (pad 13 thru_hole circle (at 0 -15.24) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask)
      (net 43 "Net-(J1-Pad13)"))
    (pad 12 thru_hole circle (at -2.54 -12.7) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 11 thru_hole circle (at 0 -12.7) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask)
      (net 10 +5V))
    (pad 10 thru_hole circle (at -2.54 -10.16) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask))
    (pad 9 thru_hole circle (at 0 -10.16) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at -2.54 -7.62) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask)
      (net 11 /_BRIGHT))
    (pad 7 thru_hole circle (at 0 -7.62) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at -2.54 -5.08) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask)
      (net 12 /D0))
    (pad 5 thru_hole circle (at 0 -5.08) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at -2.54 -2.54) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask)
      (net 13 /D1))
    (pad 3 thru_hole circle (at 0 -2.54) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask)
      (net 14 /_VSYNC))
    (pad 2 thru_hole circle (at -2.54 0) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask)
      (net 15 /D2))
    (pad 1 thru_hole roundrect (at 0 0) (size 1.524 1.524) (drill 0.9398) (layers *.Cu *.Mask) (roundrect_rratio 0.1)
      (net 16 /_HSYNC))
    (model ${KIPRJMOD}/000_LOCAL.pretty/3dshapes/PinSocket_2x20_P2.54mm_Vertical.step_
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/3dshapes/SFH11-PBPC-D20-ST-BK--3DModel-STEP-1.STEP
      (offset (xyz -1.27 -24.127 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -90))
    )
  )
  (module 000_LOCAL:SOIC-8_4x5 (layer Top) (tedit 6183C035)
    (at 157.353 106.045 270)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference U1 (at -0.635 1.016) (layer F.SilkS))
    (fp_text value LM1881 (at 0.635 0) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 8 smd roundrect (at 2.475 -1.905 270) (size 1.95 0.6) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 +5V))
    (pad 7 smd roundrect (at 2.475 -0.635 270) (size 1.95 0.6) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 6 smd roundrect (at 2.475 0.635 270) (size 1.95 0.6) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /RSET))
    (pad 5 smd roundrect (at 2.475 1.905 270) (size 1.95 0.6) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 4 smd roundrect (at -2.475 1.905 270) (size 1.95 0.6) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 3 smd roundrect (at -2.475 0.635 270) (size 1.95 0.6) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 "Net-(JP3-Pad1)"))
    (pad 2 smd roundrect (at -2.475 -0.635 270) (size 1.95 0.6) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 46 "Net-(C1-Pad2)"))
    (pad 1 smd roundrect (at -2.475 -1.905 270) (size 1.95 0.6) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 "Net-(JP2-Pad1)"))
    (model ${KIPRJMOD}/000_LOCAL.pretty/3dshapes/SOIC-8_4x5.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000_LOCAL:SW_DIP_SPSTx08_Slide_9.78x22.5mm_W7.62mm_P2.54mm (layer Top) (tedit 6183B7CA)
    (at 127 92.075)
    (descr "8x-dip-switch SPST , Slide, row spacing 7.62 mm (300 mils), body size 9.78x22.5mm (see e.g. https://www.ctscorp.com/wp-content/uploads/206-208.pdf)")
    (tags "DIP Switch SPST Slide 7.62mm 300mil")
    (fp_text reference SW1 (at 3.81 -3.42) (layer F.SilkS))
    (fp_text value SW_DIP_x08 (at 3.81 21.2) (layer F.Fab))
    (fp_text user on (at 5.365 -1.4975) (layer F.Fab))
    (fp_text user %R (at 7.27 8.89 90) (layer F.Fab))
    (pad 16 thru_hole circle (at 7.62 0) (size 1.397 1.397) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 8 thru_hole circle (at 0 17.78) (size 1.397 1.397) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 "Net-(J1-Pad13)"))
    (pad 15 thru_hole circle (at 7.62 2.54) (size 1.397 1.397) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole circle (at 0 15.24) (size 1.397 1.397) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 "Net-(J1-Pad15)"))
    (pad 14 thru_hole circle (at 7.62 5.08) (size 1.397 1.397) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole circle (at 0 12.7) (size 1.397 1.397) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 "Net-(J1-Pad17)"))
    (pad 13 thru_hole circle (at 7.62 7.62) (size 1.397 1.397) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole circle (at 0 10.16) (size 1.397 1.397) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 "Net-(J1-Pad19)"))
    (pad 12 thru_hole circle (at 7.62 10.16) (size 1.397 1.397) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole circle (at 0 7.62) (size 1.397 1.397) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 "Net-(J1-Pad21)"))
    (pad 11 thru_hole circle (at 7.62 12.7) (size 1.397 1.397) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at 0 5.08) (size 1.397 1.397) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 "Net-(J1-Pad23)"))
    (pad 10 thru_hole circle (at 7.62 15.24) (size 1.397 1.397) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 0 2.54) (size 1.397 1.397) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 "Net-(J1-Pad25)"))
    (pad 9 thru_hole circle (at 7.62 17.78) (size 1.397 1.397) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole roundrect (at 0 0) (size 1.397 1.397) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.1)
      (net 36 "Net-(J1-Pad27)"))
    (model ${KIPRJMOD}/000_LOCAL.pretty/3dshapes/SW_DIP_SPSTx08_Slide_9.78x22.5mm_W7.62mm_P2.54mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module 000_LOCAL:PT-10 (layer Top) (tedit 6183E41E)
    (at 142.875 120.65)
    (descr "<b>Trimm Potentiometer</b>")
    (fp_text reference R24 (at 0 5.588 unlocked) (layer F.SilkS))
    (fp_text value 10K (at 0 -2 unlocked) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 -5.08) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 3 thru_hole circle (at 2.54 5.08) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at -2.54 5.08) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 /DIFF_N) (solder_mask_margin 0.1016))
    (model ${KIPRJMOD}/000_LOCAL.pretty/3dshapes/PT10LV10.step
      (offset (xyz 0 0 5.6))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module 000_LOCAL:JP (layer Top) (tedit 6183B972)
    (at 143.51 86.995 90)
    (descr "pin header 01x02 2.54mm ")
    (fp_text reference JP3 (at 0.635 -2.54 unlocked) (layer F.SilkS))
    (fp_text value Jumper_2_Open (at -2.7 -2.5) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 -1.27 90) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 14 /_VSYNC) (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at 0 1.27 90) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 29 "Net-(JP3-Pad1)") (solder_mask_margin 0.1016))
    (model ${KIPRJMOD}/000_LOCAL.pretty/3dshapes/PinHeader_1x02_P2.54mm_Vertical.step
      (offset (xyz 0 1.27 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000_LOCAL:JP (layer Top) (tedit 6183B972)
    (at 143.51 81.915 90)
    (descr "pin header 01x02 2.54mm ")
    (fp_text reference JP2 (at 0.635 -2.54 unlocked) (layer F.SilkS))
    (fp_text value Jumper_2_Open (at -2.7 -2.5) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 -1.27 90) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 16 /_HSYNC) (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at 0 1.27 90) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 28 "Net-(JP2-Pad1)") (solder_mask_margin 0.1016))
    (model ${KIPRJMOD}/000_LOCAL.pretty/3dshapes/PinHeader_1x02_P2.54mm_Vertical.step
      (offset (xyz 0 1.27 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000_LOCAL:JP (layer Top) (tedit 6183B972)
    (at 143.51 76.835 270)
    (descr "pin header 01x02 2.54mm ")
    (fp_text reference JP1 (at -0.635 2.54 unlocked) (layer F.SilkS))
    (fp_text value Jumper_2_Open (at -2.7 -2.5) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 -1.27 270) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 2 /CSYNC) (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at 0 1.27 270) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 4 /DIFFG) (solder_mask_margin 0.1016))
    (model ${KIPRJMOD}/000_LOCAL.pretty/3dshapes/PinHeader_1x02_P2.54mm_Vertical.step
      (offset (xyz 0 1.27 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000_LOCAL:RCA (layer Top) (tedit 6186C09A)
    (at 111.125 120.015 180)
    (fp_text reference J4 (at 0.02 -2.55 180 unlocked) (layer F.SilkS) hide)
    (fp_text value C_VIDEO_IN (at -10.795 -6.985 unlocked) (layer F.SilkS))
    (fp_text user REF** (at 0 -1.94) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.413 2.413) (drill 1.7018) (layers *.Cu *.Mask)
      (net 4 /DIFFG) (solder_mask_margin 0.1016))
    (pad 2 thru_hole circle (at 0 -4.4958 180) (size 3.556 3.556) (drill 2.5908) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 2 thru_hole circle (at 5.0038 0 180) (size 3.556 3.556) (drill 2.5908) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 2 thru_hole circle (at -5.0038 0 180) (size 3.556 3.556) (drill 2.5908) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (model ${KIPRJMOD}/000_LOCAL.pretty/3dshapes/CUI_DEVICES_RCJ-014.step
      (offset (xyz -0 -1.2446 6.604))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -90))
    )
  )
  (gr_text GND (at 107.569 80.391 -90) (layer B.SilkS))
  (gr_text G (at 110.109 75.565 -90) (layer B.SilkS))
  (gr_text PB3 (at 117.729 75.692 -90) (layer B.SilkS))
  (gr_text GND (at 107.569 75.692 -90) (layer B.SilkS))
  (gr_text R (at 110.109 80.391 -90) (layer B.SilkS))
  (gr_text B (at 112.649 80.391 -90) (layer B.SilkS))
  (gr_text AUDIO (at 115.189 80.391 -90) (layer B.SilkS))
  (gr_text H (at 115.189 75.565 -90) (layer B.SilkS))
  (gr_text V (at 117.729 80.391 -90) (layer B.SilkS))
  (gr_text "github.com/bkw777/rgb2vga - v003" (at 139.7 100.965 -90) (layer B.SilkS))
  (gr_arc (start 105.537 125.73) (end 102.362 125.73) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 173.99 125.73) (end 173.99 128.905) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 105.537 76.2) (end 105.537 73.025) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 173.99 76.2) (end 177.165 76.2) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 177.165 125.73) (end 177.165 76.2) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 105.537 128.905) (end 173.99 128.905) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 173.99 73.025) (end 105.537 73.025) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 102.362 76.2) (end 102.362 125.73) (layer Edge.Cuts) (width 0.05))
  (gr_text "DE0-NANO RGB2VGA" (at 115.57 100.965 90) (layer F.SilkS))
  (gr_text SCANLINE (at 136.525 110.49) (layer F.SilkS))
  (gr_text "SYNC LEVEL" (at 136.525 107.95) (layer F.SilkS))
  (gr_text ARTIFACT (at 136.525 105.41) (layer F.SilkS))
  (gr_text "ART. INV." (at 136.525 102.8536) (layer F.SilkS))
  (gr_text DEINTERLACE (at 136.525 97.79) (layer F.SilkS))
  (gr_text SHRINK (at 136.525 92.6936) (layer F.SilkS))
  (gr_text VOLTAGE (at 142.875 114.3) (layer F.SilkS))
  (gr_text MSX (at 136.525 95.25) (layer F.SilkS))
  (gr_text "JP1: C_VIDEO" (at 142.494 74.8665) (layer F.SilkS))
  (gr_text "JP2+JP3: CSYNC" (at 141.7955 84.963) (layer F.SilkS))
  (gr_text "APPLE ][" (at 136.525 100.33) (layer F.SilkS))
  (gr_text "Based on FPGA RGB2VGA by Luis Antoniosi" (at 137.16 100.965 -90) (layer B.SilkS))
  (zone (net 1) (net_name GND) (layer Top) (hatch edge 0.508)
    (priority 6)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.2) (thermal_bridge_width 0.4) (smoothing fillet) (radius 0.1))
    (polygon
      (pts
        (xy 177.165 128.905) (xy 102.362 128.905) (xy 102.362 73.025) (xy 177.165 73.025)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer Bottom) (hatch edge 0.508)
    (priority 6)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.2) (thermal_bridge_width 0.4) (smoothing fillet) (radius 0.1))
    (polygon
      (pts
        (xy 177.165 128.905) (xy 102.362 128.905) (xy 102.362 73.025) (xy 177.165 73.025)
      )
    )
  )
)
