(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 13)
    (no_connects 0)
    (area 121.715 99.2 142.875 106.9)
    (thickness 1.6)
    (drawings 12)
    (tracks 21)
    (zones 0)
    (modules 4)
    (nets 4)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 1.5)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.99898 1.99898)
    (pad_drill 0.8001)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (grid_origin 117.5 93.5)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x31cf0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerber/))
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad1)")
  (net 2 VCC)
  (net 3 GND)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 1.5)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (net_class high ""
    (clearance 0.2)
    (trace_width 1.5)
    (via_dia 1.5)
    (via_drill 1)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(D1-Pad1)")
    (add_net VCC)
  )
  (module LEDs:LED_RGB_PLCC-6 (layer F.Cu) (tedit 589BF9C3)
    (at 139 103 90)
    (descr "RGB LED PLCC-6")
    (tags "RGB LED PLCC-6")
    (attr smd)
    (fp_text reference D1 (at 0 0 360) (layer F.SilkS))
    (fp_text value LED_RGB (at 0 2.8 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.55 -1.1 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at -1.55 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 3 smd rect (at -1.55 1.1 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 4 smd rect (at 1.55 1.1 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 5 smd rect (at 1.55 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 6 smd rect (at 1.55 -1.1 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
  )
  (module LEDs:LED_RGB_PLCC-6 (layer F.Cu) (tedit 589BF9C8)
    (at 134 103 90)
    (descr "RGB LED PLCC-6")
    (tags "RGB LED PLCC-6")
    (attr smd)
    (fp_text reference D2 (at 0 0 360) (layer F.SilkS))
    (fp_text value LED_RGB (at 0 2.8 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.55 -1.1 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at -1.55 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 3 smd rect (at -1.55 1.1 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 4 smd rect (at 1.55 1.1 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 5 smd rect (at 1.55 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 6 smd rect (at 1.55 -1.1 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
  )
  (module Resistors_SMD:R_2010 (layer F.Cu) (tedit 589BF9DA)
    (at 129.5 103 90)
    (descr "Resistor SMD 2010, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 2010")
    (attr smd)
    (fp_text reference R1 (at 0 0 90) (layer F.SilkS))
    (fp_text value 470 (at 0 2.7 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -2.45 0 90) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 2.45 0 90) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model Resistors_SMD.3dshapes/R_2010.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wire_Pads:SolderWirePad_2x_0-8mmDrill (layer F.Cu) (tedit 589CD98D)
    (at 126.5 103 90)
    (fp_text reference REF** (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value "" (at 0.635 2.54 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -1.905 0 90) (size 1.99898 1.99898) (drill 0.8001) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 2 thru_hole circle (at 1.905 0 90) (size 1.99898 1.99898) (drill 0.8001) (layers *.Cu *.Mask)
      (net 3 GND))
  )
  (gr_text - (at 136.5 106) (layer F.SilkS))
  (gr_text + (at 136.5 100) (layer F.SilkS))
  (gr_text - (at 128.5 101) (layer B.SilkS))
  (gr_text + (at 128.5 105) (layer B.SilkS))
  (gr_text - (at 125.5 102) (layer F.SilkS))
  (gr_text + (at 125.5 104) (layer F.SilkS))
  (gr_line (start 125 106.5) (end 125.5 106.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 125 99.5) (end 125 106.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 125.5 99.5) (end 125 99.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 141.5 106.5) (end 125.5 106.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 141.5 99.5) (end 141.5 106.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 125.5 99.5) (end 141.5 99.5) (angle 90) (layer Edge.Cuts) (width 0.15))
)
