(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 65)
    (no_connects 2)
    (area 116.764999 57.074999 177.875001 124.535001)
    (thickness 1.6)
    (drawings 45)
    (tracks 243)
    (zones 0)
    (modules 10)
    (nets 89)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.7272 1.7272)
    (pad_drill 1.016)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (grid_origin 193.04 86.36)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 P7.7)
  (net 2 P6.7)
  (net 3 P7.6)
  (net 4 P6.6)
  (net 5 P7.5)
  (net 6 P6.5)
  (net 7 P7.4)
  (net 8 P6.4)
  (net 9 P7.3)
  (net 10 P6.3)
  (net 11 P7.2)
  (net 12 P6.2)
  (net 13 P7.1)
  (net 14 P6.1)
  (net 15 P7.0)
  (net 16 P6.0)
  (net 17 P5.7)
  (net 18 P4.7)
  (net 19 P5.6)
  (net 20 P4.6)
  (net 21 P5.5)
  (net 22 P4.5)
  (net 23 P5.4)
  (net 24 P4.4)
  (net 25 P5.3)
  (net 26 P4.3)
  (net 27 P5.2)
  (net 28 P4.2)
  (net 29 P5.1)
  (net 30 P4.1)
  (net 31 P5.0)
  (net 32 P4.0)
  (net 33 GND)
  (net 34 +3V3)
  (net 35 ANI0.7)
  (net 36 ANI0.6)
  (net 37 CPO+)
  (net 38 ANI0.5)
  (net 39 CPO-)
  (net 40 ANI0.4)
  (net 41 CPI+)
  (net 42 ANI0.3)
  (net 43 CPI-)
  (net 44 ANI0.2)
  (net 45 DAC1)
  (net 46 ANI0.1)
  (net 47 DAC0)
  (net 48 ANI0.0)
  (net 49 VREF1)
  (net 50 VREF)
  (net 51 VREF0)
  (net 52 VREFD)
  (net 53 +5V)
  (net 54 P3.0)
  (net 55 P0.0)
  (net 56 P3.1)
  (net 57 P0.1)
  (net 58 P3.2)
  (net 59 P0.2)
  (net 60 P3.3)
  (net 61 P0.3)
  (net 62 P3.4)
  (net 63 P0.4)
  (net 64 P3.5)
  (net 65 P0.5)
  (net 66 P3.6)
  (net 67 P0.6)
  (net 68 P3.7)
  (net 69 P0.7)
  (net 70 P1.0)
  (net 71 P2.0)
  (net 72 P1.1)
  (net 73 P2.1)
  (net 74 P1.2)
  (net 75 P2.2)
  (net 76 P1.3)
  (net 77 P2.3)
  (net 78 P1.4)
  (net 79 P2.4)
  (net 80 P1.5)
  (net 81 P2.5)
  (net 82 P1.6)
  (net 83 P2.6)
  (net 84 P1.7)
  (net 85 P2.7)
  (net 86 "Net-(P6-Pad1)")
  (net 87 "Net-(P6-Pad4)")
  (net 88 "Net-(P6-Pad5)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net ANI0.0)
    (add_net ANI0.1)
    (add_net ANI0.2)
    (add_net ANI0.3)
    (add_net ANI0.4)
    (add_net ANI0.5)
    (add_net ANI0.6)
    (add_net ANI0.7)
    (add_net CPI+)
    (add_net CPI-)
    (add_net CPO+)
    (add_net CPO-)
    (add_net DAC0)
    (add_net DAC1)
    (add_net GND)
    (add_net "Net-(P6-Pad1)")
    (add_net "Net-(P6-Pad4)")
    (add_net "Net-(P6-Pad5)")
    (add_net P0.0)
    (add_net P0.1)
    (add_net P0.2)
    (add_net P0.3)
    (add_net P0.4)
    (add_net P0.5)
    (add_net P0.6)
    (add_net P0.7)
    (add_net P1.0)
    (add_net P1.1)
    (add_net P1.2)
    (add_net P1.3)
    (add_net P1.4)
    (add_net P1.5)
    (add_net P1.6)
    (add_net P1.7)
    (add_net P2.0)
    (add_net P2.1)
    (add_net P2.2)
    (add_net P2.3)
    (add_net P2.4)
    (add_net P2.5)
    (add_net P2.6)
    (add_net P2.7)
    (add_net P3.0)
    (add_net P3.1)
    (add_net P3.2)
    (add_net P3.3)
    (add_net P3.4)
    (add_net P3.5)
    (add_net P3.6)
    (add_net P3.7)
    (add_net P4.0)
    (add_net P4.1)
    (add_net P4.2)
    (add_net P4.3)
    (add_net P4.4)
    (add_net P4.5)
    (add_net P4.6)
    (add_net P4.7)
    (add_net P5.0)
    (add_net P5.1)
    (add_net P5.2)
    (add_net P5.3)
    (add_net P5.4)
    (add_net P5.5)
    (add_net P5.6)
    (add_net P5.7)
    (add_net P6.0)
    (add_net P6.1)
    (add_net P6.2)
    (add_net P6.3)
    (add_net P6.4)
    (add_net P6.5)
    (add_net P6.6)
    (add_net P6.7)
    (add_net P7.0)
    (add_net P7.1)
    (add_net P7.2)
    (add_net P7.3)
    (add_net P7.4)
    (add_net P7.5)
    (add_net P7.6)
    (add_net P7.7)
    (add_net VREF)
    (add_net VREF0)
    (add_net VREF1)
    (add_net VREFD)
  )
  (net_class Medium ""
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (net_class Wide ""
    (clearance 0.2)
    (trace_width 0.75)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module Housings_DIP:DIP-32_W15.24mm_LongPads (layer F.Cu) (tedit 58631955)
    (at 121.92 95.25 90)
    (descr "32-lead dip package, row spacing 15.24 mm (600 mils), longer pads")
    (tags "dil dip 2.54 600")
    (fp_text reference U1 (at 8.89 -2.54 90) (layer F.SilkS))
    (fp_text value HM628512BFP-5 (at 7.62 19.05 180) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 P4.3))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 P4.2))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 P6.7))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 P6.5))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 P6.3))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 P6.1))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 P5.7))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 P5.5))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 P5.4))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 P5.2))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 P5.1))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 P5.0))
    (pad 13 thru_hole oval (at 0 30.48 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 P7.6))
    (pad 14 thru_hole oval (at 0 33.02 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 P7.4))
    (pad 15 thru_hole oval (at 0 35.56 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 P7.2))
    (pad 16 thru_hole oval (at 0 38.1 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 GND))
    (pad 17 thru_hole oval (at 15.24 38.1 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 P7.0))
    (pad 18 thru_hole oval (at 15.24 35.56 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 P7.1))
    (pad 19 thru_hole oval (at 15.24 33.02 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 P7.3))
    (pad 20 thru_hole oval (at 15.24 30.48 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 P7.5))
    (pad 21 thru_hole oval (at 15.24 27.94 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 P7.7))
    (pad 22 thru_hole oval (at 15.24 25.4 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 P4.5))
    (pad 23 thru_hole oval (at 15.24 22.86 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 P5.3))
    (pad 24 thru_hole oval (at 15.24 20.32 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 P4.6))
    (pad 25 thru_hole oval (at 15.24 17.78 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 P5.6))
    (pad 26 thru_hole oval (at 15.24 15.24 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 P6.0))
    (pad 27 thru_hole oval (at 15.24 12.7 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 P6.2))
    (pad 28 thru_hole oval (at 15.24 10.16 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 P6.4))
    (pad 29 thru_hole oval (at 15.24 7.62 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 P4.7))
    (pad 30 thru_hole oval (at 15.24 5.08 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 P4.4))
    (pad 31 thru_hole oval (at 15.24 2.54 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 P6.6))
    (pad 32 thru_hole oval (at 15.24 0 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 +3V3))
    (model Housings_DIP.3dshapes/DIP-32_W15.24mm_LongPads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x04 (layer F.Cu) (tedit 58631924)
    (at 121.92 67.31 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P4 (at 1.27 -2.54 90) (layer F.SilkS))
    (fp_text value "" (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 33 GND))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 53 +5V))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 33 GND))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 53 +5V))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 33 GND))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 53 +5V))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 33 GND))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 53 +5V))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x04.wrl
      (at (xyz 0.05 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 586318A2)
    (at 160.02 59.69 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P7 (at 0 -2.54 90) (layer F.SilkS))
    (fp_text value "" (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 70 P1.0))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 72 P1.1))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 33 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x16 (layer F.Cu) (tedit 58631933)
    (at 137.16 120.65 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at 1.27 -2.54 90) (layer F.SilkS))
    (fp_text value "" (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 P7.7))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 P6.7))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 P7.6))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 P6.6))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 P7.5))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 P6.5))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 P7.4))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 P6.4))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 P7.3))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 P6.3))
    (pad 11 thru_hole oval (at 0 12.7 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 P7.2))
    (pad 12 thru_hole oval (at 2.54 12.7 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 P6.2))
    (pad 13 thru_hole oval (at 0 15.24 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 P7.1))
    (pad 14 thru_hole oval (at 2.54 15.24 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 14 P6.1))
    (pad 15 thru_hole oval (at 0 17.78 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 P7.0))
    (pad 16 thru_hole oval (at 2.54 17.78 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 16 P6.0))
    (pad 17 thru_hole oval (at 0 20.32 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 P5.7))
    (pad 18 thru_hole oval (at 2.54 20.32 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 P4.7))
    (pad 19 thru_hole oval (at 0 22.86 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 P5.6))
    (pad 20 thru_hole oval (at 2.54 22.86 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 P4.6))
    (pad 21 thru_hole oval (at 0 25.4 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 P5.5))
    (pad 22 thru_hole oval (at 2.54 25.4 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 22 P4.5))
    (pad 23 thru_hole oval (at 0 27.94 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 P5.4))
    (pad 24 thru_hole oval (at 2.54 27.94 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 24 P4.4))
    (pad 25 thru_hole oval (at 0 30.48 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 25 P5.3))
    (pad 26 thru_hole oval (at 2.54 30.48 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 P4.3))
    (pad 27 thru_hole oval (at 0 33.02 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 27 P5.2))
    (pad 28 thru_hole oval (at 2.54 33.02 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 28 P4.2))
    (pad 29 thru_hole oval (at 0 35.56 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 29 P5.1))
    (pad 30 thru_hole oval (at 2.54 35.56 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 30 P4.1))
    (pad 31 thru_hole oval (at 0 38.1 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 31 P5.0))
    (pad 32 thru_hole oval (at 2.54 38.1 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 32 P4.0))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x16.wrl
      (at (xyz 0.05 -0.75 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x04 (layer F.Cu) (tedit 58631916)
    (at 121.92 74.93 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at 1.27 -2.54 90) (layer F.SilkS))
    (fp_text value "" (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 33 GND))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 34 +3V3))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 33 GND))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 34 +3V3))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 33 GND))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 34 +3V3))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 33 GND))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 34 +3V3))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x04.wrl
      (at (xyz 0.05 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x11 (layer F.Cu) (tedit 5863300D)
    (at 167.64 80.01)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P3 (at 1.27 -2.54) (layer F.SilkS))
    (fp_text value "" (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 33 GND))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 35 ANI0.7))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 34 +3V3))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 36 ANI0.6))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 37 CPO+))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 38 ANI0.5))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 39 CPO-))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 40 ANI0.4))
    (pad 9 thru_hole oval (at 0 10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 41 CPI+))
    (pad 10 thru_hole oval (at 2.54 10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 42 ANI0.3))
    (pad 11 thru_hole oval (at 0 12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 43 CPI-))
    (pad 12 thru_hole oval (at 2.54 12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 44 ANI0.2))
    (pad 13 thru_hole oval (at 0 15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 45 DAC1))
    (pad 14 thru_hole oval (at 2.54 15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 46 ANI0.1))
    (pad 15 thru_hole oval (at 0 17.78) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 47 DAC0))
    (pad 16 thru_hole oval (at 2.54 17.78) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 48 ANI0.0))
    (pad 17 thru_hole oval (at 0 20.32) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 49 VREF1))
    (pad 18 thru_hole oval (at 2.54 20.32) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 50 VREF))
    (pad 19 thru_hole oval (at 0 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 51 VREF0))
    (pad 20 thru_hole oval (at 2.54 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 50 VREF))
    (pad 21 thru_hole oval (at 0 25.4) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 52 VREFD))
    (pad 22 thru_hole oval (at 2.54 25.4) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 50 VREF))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x11.wrl
      (at (xyz 0.05 -0.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x16 (layer F.Cu) (tedit 586318CE)
    (at 137.16 67.31 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P5 (at 1.27 -2.54 90) (layer F.SilkS))
    (fp_text value "" (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 54 P3.0))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 55 P0.0))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 56 P3.1))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 57 P0.1))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 58 P3.2))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 59 P0.2))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 60 P3.3))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 61 P0.3))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 62 P3.4))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 63 P0.4))
    (pad 11 thru_hole oval (at 0 12.7 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 64 P3.5))
    (pad 12 thru_hole oval (at 2.54 12.7 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 65 P0.5))
    (pad 13 thru_hole oval (at 0 15.24 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 66 P3.6))
    (pad 14 thru_hole oval (at 2.54 15.24 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 67 P0.6))
    (pad 15 thru_hole oval (at 0 17.78 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 68 P3.7))
    (pad 16 thru_hole oval (at 2.54 17.78 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 69 P0.7))
    (pad 17 thru_hole oval (at 0 20.32 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 70 P1.0))
    (pad 18 thru_hole oval (at 2.54 20.32 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 71 P2.0))
    (pad 19 thru_hole oval (at 0 22.86 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 72 P1.1))
    (pad 20 thru_hole oval (at 2.54 22.86 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 73 P2.1))
    (pad 21 thru_hole oval (at 0 25.4 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 74 P1.2))
    (pad 22 thru_hole oval (at 2.54 25.4 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 75 P2.2))
    (pad 23 thru_hole oval (at 0 27.94 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 76 P1.3))
    (pad 24 thru_hole oval (at 2.54 27.94 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 77 P2.3))
    (pad 25 thru_hole oval (at 0 30.48 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 78 P1.4))
    (pad 26 thru_hole oval (at 2.54 30.48 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 79 P2.4))
    (pad 27 thru_hole oval (at 0 33.02 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 80 P1.5))
    (pad 28 thru_hole oval (at 2.54 33.02 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 81 P2.5))
    (pad 29 thru_hole oval (at 0 35.56 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 82 P1.6))
    (pad 30 thru_hole oval (at 2.54 35.56 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 83 P2.6))
    (pad 31 thru_hole oval (at 0 38.1 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 84 P1.7))
    (pad 32 thru_hole oval (at 2.54 38.1 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 85 P2.7))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x16.wrl
      (at (xyz 0.05 -0.75 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x06 (layer F.Cu) (tedit 586318DD)
    (at 137.16 72.39 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P6 (at 0 -2.54 90) (layer F.SilkS))
    (fp_text value "" (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 86 "Net-(P6-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 55 P0.0))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 57 P0.1))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 87 "Net-(P6-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 88 "Net-(P6-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 33 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x06.wrl
      (at (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x05 (layer F.Cu) (tedit 586318AB)
    (at 160.02 72.39 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P8 (at 0 -2.54 90) (layer F.SilkS))
    (fp_text value "" (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 78 P1.4))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 74 P1.2))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 76 P1.3))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 33 GND))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 34 +3V3))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x05.wrl
      (at (xyz 0 -0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x05 (layer F.Cu) (tedit 586318B6)
    (at 142.24 59.69 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P9 (at 0 -2.54 90) (layer F.SilkS))
    (fp_text value "" (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 59 P0.2))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 61 P0.3))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 63 P0.4))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 65 P0.5))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 33 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x05.wrl
      (at (xyz 0 -0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (gr_text "Memory Expansion\nEX-F02x-Q100\n\nBitBanger" (at 144.78 109.9) (layer F.SilkS))
  (gr_text "Version 1.0  12/27/16\n" (at 143.51 111) (layer B.SilkS))
  (gr_line (start 134.62 62.23) (end 116.84 62.23) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 135.89 60.96) (end 134.62 62.23) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 139.7 57.15) (end 135.89 60.96) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 167.64 57.15) (end 139.7 57.15) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 172.72 62.23) (end 167.64 57.15) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 171.45 60.96) (end 172.72 62.23) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 167.64 57.15) (end 171.45 60.96) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 177.8 62.23) (end 172.72 62.23) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 177.8 124.46) (end 177.8 62.23) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 116.84 124.46) (end 177.8 124.46) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 116.84 62.23) (end 116.84 124.46) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 33) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 172.72 62.23) (xy 177.8 62.23) (xy 177.8 124.46) (xy 116.84 124.46) (xy 116.84 62.23)
        (xy 134.62 62.23) (xy 139.7 57.15) (xy 167.64 57.15)
      )
    )
  )
  (zone (net 34) (net_name +3V3) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 172.72 62.23) (xy 177.8 62.23) (xy 177.8 124.46) (xy 116.84 124.46) (xy 116.84 62.23)
        (xy 134.62 62.23) (xy 139.7 57.15) (xy 167.64 57.15)
      )
    )
  )
)
