(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 60)
    (no_connects 0)
    (area 46.924999 56.924999 157.075001 138.075001)
    (thickness 1.6)
    (drawings 4)
    (tracks 138)
    (zones 0)
    (modules 41)
    (nets 30)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 Row1)
  (net 2 "Net-(D1-Pad1)")
  (net 3 Row2)
  (net 4 "Net-(D2-Pad1)")
  (net 5 Row3)
  (net 6 "Net-(D3-Pad1)")
  (net 7 Row4)
  (net 8 "Net-(D4-Pad1)")
  (net 9 "Net-(D5-Pad1)")
  (net 10 "Net-(D6-Pad1)")
  (net 11 "Net-(D7-Pad1)")
  (net 12 "Net-(D8-Pad1)")
  (net 13 "Net-(D9-Pad1)")
  (net 14 "Net-(D10-Pad1)")
  (net 15 "Net-(D11-Pad1)")
  (net 16 "Net-(D12-Pad1)")
  (net 17 "Net-(D13-Pad1)")
  (net 18 "Net-(D14-Pad1)")
  (net 19 "Net-(D15-Pad1)")
  (net 20 "Net-(D16-Pad1)")
  (net 21 "Net-(D17-Pad1)")
  (net 22 "Net-(D18-Pad1)")
  (net 23 "Net-(D19-Pad1)")
  (net 24 "Net-(D20-Pad1)")
  (net 25 Col1)
  (net 26 Col2)
  (net 27 Col3)
  (net 28 Col4)
  (net 29 Col5)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net Col1)
    (add_net Col2)
    (add_net Col3)
    (add_net Col4)
    (add_net Col5)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D10-Pad1)")
    (add_net "Net-(D11-Pad1)")
    (add_net "Net-(D12-Pad1)")
    (add_net "Net-(D13-Pad1)")
    (add_net "Net-(D14-Pad1)")
    (add_net "Net-(D15-Pad1)")
    (add_net "Net-(D16-Pad1)")
    (add_net "Net-(D17-Pad1)")
    (add_net "Net-(D18-Pad1)")
    (add_net "Net-(D19-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D20-Pad1)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(D5-Pad1)")
    (add_net "Net-(D6-Pad1)")
    (add_net "Net-(D7-Pad1)")
    (add_net "Net-(D8-Pad1)")
    (add_net "Net-(D9-Pad1)")
    (add_net Row1)
    (add_net Row2)
    (add_net Row3)
    (add_net Row4)
  )
  (module prettylib:SOT123-DIODE (layer B.Cu) (tedit 55C2C69D)
    (at 67 69)
    (descr DIODE)
    (tags DIODE)
    (fp_text reference D1 (at 0 3.81 270) (layer B.SilkS))
    (fp_text value DIODE (at 2.032 0 270) (layer B.SilkS) hide)
    (pad 2 smd rect (at 0 1.7526 90) (size 1.00076 0.8509) (layers B.Cu B.Paste B.Mask)
      (net 1 Row1))
    (pad 1 smd rect (at 0 -1.74752 90) (size 1.00076 0.8509) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(D1-Pad1)"))
  )
  (module prettylib:SOT123-DIODE (layer B.Cu) (tedit 55C2C69D)
    (at 67 88)
    (descr DIODE)
    (tags DIODE)
    (fp_text reference D2 (at 0 3.81 270) (layer B.SilkS))
    (fp_text value DIODE (at 2.032 0 270) (layer B.SilkS) hide)
    (pad 2 smd rect (at 0 1.7526 90) (size 1.00076 0.8509) (layers B.Cu B.Paste B.Mask)
      (net 3 Row2))
    (pad 1 smd rect (at 0 -1.74752 90) (size 1.00076 0.8509) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(D2-Pad1)"))
  )
  (module prettylib:SOT123-DIODE (layer B.Cu) (tedit 55C2C69D)
    (at 67 107)
    (descr DIODE)
    (tags DIODE)
    (fp_text reference D3 (at 0 3.81 270) (layer B.SilkS))
    (fp_text value DIODE (at 2.032 0 270) (layer B.SilkS) hide)
    (pad 2 smd rect (at 0 1.7526 90) (size 1.00076 0.8509) (layers B.Cu B.Paste B.Mask)
      (net 5 Row3))
    (pad 1 smd rect (at 0 -1.74752 90) (size 1.00076 0.8509) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(D3-Pad1)"))
  )
  (module prettylib:SOT123-DIODE (layer B.Cu) (tedit 55C2C69D)
    (at 67 126)
    (descr DIODE)
    (tags DIODE)
    (fp_text reference D4 (at 0 3.81 270) (layer B.SilkS))
    (fp_text value DIODE (at 2.032 0 270) (layer B.SilkS) hide)
    (pad 2 smd rect (at 0 1.7526 90) (size 1.00076 0.8509) (layers B.Cu B.Paste B.Mask)
      (net 7 Row4))
    (pad 1 smd rect (at 0 -1.74752 90) (size 1.00076 0.8509) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(D4-Pad1)"))
  )
  (module prettylib:SOT123-DIODE (layer B.Cu) (tedit 55C2C69D)
    (at 86 69)
    (descr DIODE)
    (tags DIODE)
    (fp_text reference D5 (at 0 3.81 270) (layer B.SilkS))
    (fp_text value DIODE (at 2.032 0 270) (layer B.SilkS) hide)
    (pad 2 smd rect (at 0 1.7526 90) (size 1.00076 0.8509) (layers B.Cu B.Paste B.Mask)
      (net 1 Row1))
    (pad 1 smd rect (at 0 -1.74752 90) (size 1.00076 0.8509) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(D5-Pad1)"))
  )
  (module prettylib:SOT123-DIODE (layer B.Cu) (tedit 55C2C69D)
    (at 86 88)
    (descr DIODE)
    (tags DIODE)
    (fp_text reference D6 (at 0 3.81 270) (layer B.SilkS))
    (fp_text value DIODE (at 2.032 0 270) (layer B.SilkS) hide)
    (pad 2 smd rect (at 0 1.7526 90) (size 1.00076 0.8509) (layers B.Cu B.Paste B.Mask)
      (net 3 Row2))
    (pad 1 smd rect (at 0 -1.74752 90) (size 1.00076 0.8509) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(D6-Pad1)"))
  )
  (module prettylib:SOT123-DIODE (layer B.Cu) (tedit 55C2C69D)
    (at 86 107)
    (descr DIODE)
    (tags DIODE)
    (fp_text reference D7 (at 0 3.81 270) (layer B.SilkS))
    (fp_text value DIODE (at 2.032 0 270) (layer B.SilkS) hide)
    (pad 2 smd rect (at 0 1.7526 90) (size 1.00076 0.8509) (layers B.Cu B.Paste B.Mask)
      (net 5 Row3))
    (pad 1 smd rect (at 0 -1.74752 90) (size 1.00076 0.8509) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(D7-Pad1)"))
  )
  (module prettylib:SOT123-DIODE (layer B.Cu) (tedit 55C2C69D)
    (at 86 126)
    (descr DIODE)
    (tags DIODE)
    (fp_text reference D8 (at 0 3.81 270) (layer B.SilkS))
    (fp_text value DIODE (at 2.032 0 270) (layer B.SilkS) hide)
    (pad 2 smd rect (at 0 1.7526 90) (size 1.00076 0.8509) (layers B.Cu B.Paste B.Mask)
      (net 7 Row4))
    (pad 1 smd rect (at 0 -1.74752 90) (size 1.00076 0.8509) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(D8-Pad1)"))
  )
  (module prettylib:SOT123-DIODE (layer B.Cu) (tedit 55C2C69D)
    (at 105 69)
    (descr DIODE)
    (tags DIODE)
    (fp_text reference D9 (at 0 3.81 270) (layer B.SilkS))
    (fp_text value DIODE (at 2.032 0 270) (layer B.SilkS) hide)
    (pad 2 smd rect (at 0 1.7526 90) (size 1.00076 0.8509) (layers B.Cu B.Paste B.Mask)
      (net 1 Row1))
    (pad 1 smd rect (at 0 -1.74752 90) (size 1.00076 0.8509) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(D9-Pad1)"))
  )
  (module prettylib:SOT123-DIODE (layer B.Cu) (tedit 55C2C69D)
    (at 105 88)
    (descr DIODE)
    (tags DIODE)
    (fp_text reference D10 (at 0 3.81 270) (layer B.SilkS))
    (fp_text value DIODE (at 2.032 0 270) (layer B.SilkS) hide)
    (pad 2 smd rect (at 0 1.7526 90) (size 1.00076 0.8509) (layers B.Cu B.Paste B.Mask)
      (net 3 Row2))
    (pad 1 smd rect (at 0 -1.74752 90) (size 1.00076 0.8509) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(D10-Pad1)"))
  )
  (module prettylib:SOT123-DIODE (layer B.Cu) (tedit 55C2C69D)
    (at 105 107)
    (descr DIODE)
    (tags DIODE)
    (fp_text reference D11 (at 0 3.81 270) (layer B.SilkS))
    (fp_text value DIODE (at 2.032 0 270) (layer B.SilkS) hide)
    (pad 2 smd rect (at 0 1.7526 90) (size 1.00076 0.8509) (layers B.Cu B.Paste B.Mask)
      (net 5 Row3))
    (pad 1 smd rect (at 0 -1.74752 90) (size 1.00076 0.8509) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(D11-Pad1)"))
  )
  (module prettylib:SOT123-DIODE (layer B.Cu) (tedit 55C2C69D)
    (at 105 126)
    (descr DIODE)
    (tags DIODE)
    (fp_text reference D12 (at 0 3.81 270) (layer B.SilkS))
    (fp_text value DIODE (at 2.032 0 270) (layer B.SilkS) hide)
    (pad 2 smd rect (at 0 1.7526 90) (size 1.00076 0.8509) (layers B.Cu B.Paste B.Mask)
      (net 7 Row4))
    (pad 1 smd rect (at 0 -1.74752 90) (size 1.00076 0.8509) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(D12-Pad1)"))
  )
  (module prettylib:SOT123-DIODE (layer B.Cu) (tedit 55C2C69D)
    (at 124 69)
    (descr DIODE)
    (tags DIODE)
    (fp_text reference D13 (at 0 3.81 270) (layer B.SilkS))
    (fp_text value DIODE (at 2.032 0 270) (layer B.SilkS) hide)
    (pad 2 smd rect (at 0 1.7526 90) (size 1.00076 0.8509) (layers B.Cu B.Paste B.Mask)
      (net 1 Row1))
    (pad 1 smd rect (at 0 -1.74752 90) (size 1.00076 0.8509) (layers B.Cu B.Paste B.Mask)
      (net 17 "Net-(D13-Pad1)"))
  )
  (module prettylib:SOT123-DIODE (layer B.Cu) (tedit 55C2C69D)
    (at 124 88)
    (descr DIODE)
    (tags DIODE)
    (fp_text reference D14 (at 0 3.81 270) (layer B.SilkS))
    (fp_text value DIODE (at 2.032 0 270) (layer B.SilkS) hide)
    (pad 2 smd rect (at 0 1.7526 90) (size 1.00076 0.8509) (layers B.Cu B.Paste B.Mask)
      (net 3 Row2))
    (pad 1 smd rect (at 0 -1.74752 90) (size 1.00076 0.8509) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(D14-Pad1)"))
  )
  (module prettylib:SOT123-DIODE (layer B.Cu) (tedit 55C2C69D)
    (at 124 107)
    (descr DIODE)
    (tags DIODE)
    (fp_text reference D15 (at 0 3.81 270) (layer B.SilkS))
    (fp_text value DIODE (at 2.032 0 270) (layer B.SilkS) hide)
    (pad 2 smd rect (at 0 1.7526 90) (size 1.00076 0.8509) (layers B.Cu B.Paste B.Mask)
      (net 5 Row3))
    (pad 1 smd rect (at 0 -1.74752 90) (size 1.00076 0.8509) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(D15-Pad1)"))
  )
  (module prettylib:SOT123-DIODE (layer B.Cu) (tedit 55C2C69D)
    (at 124 126)
    (descr DIODE)
    (tags DIODE)
    (fp_text reference D16 (at 0 3.81 270) (layer B.SilkS))
    (fp_text value DIODE (at 2.032 0 270) (layer B.SilkS) hide)
    (pad 2 smd rect (at 0 1.7526 90) (size 1.00076 0.8509) (layers B.Cu B.Paste B.Mask)
      (net 7 Row4))
    (pad 1 smd rect (at 0 -1.74752 90) (size 1.00076 0.8509) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(D16-Pad1)"))
  )
  (module prettylib:SOT123-DIODE (layer B.Cu) (tedit 55C2C69D)
    (at 143 69)
    (descr DIODE)
    (tags DIODE)
    (fp_text reference D17 (at 0 3.81 270) (layer B.SilkS))
    (fp_text value DIODE (at 2.032 0 270) (layer B.SilkS) hide)
    (pad 2 smd rect (at 0 1.7526 90) (size 1.00076 0.8509) (layers B.Cu B.Paste B.Mask)
      (net 1 Row1))
    (pad 1 smd rect (at 0 -1.74752 90) (size 1.00076 0.8509) (layers B.Cu B.Paste B.Mask)
      (net 21 "Net-(D17-Pad1)"))
  )
  (module prettylib:SOT123-DIODE (layer B.Cu) (tedit 55C2C69D)
    (at 143 88)
    (descr DIODE)
    (tags DIODE)
    (fp_text reference D18 (at 0 3.81 270) (layer B.SilkS))
    (fp_text value DIODE (at 2.032 0 270) (layer B.SilkS) hide)
    (pad 2 smd rect (at 0 1.7526 90) (size 1.00076 0.8509) (layers B.Cu B.Paste B.Mask)
      (net 3 Row2))
    (pad 1 smd rect (at 0 -1.74752 90) (size 1.00076 0.8509) (layers B.Cu B.Paste B.Mask)
      (net 22 "Net-(D18-Pad1)"))
  )
  (module prettylib:SOT123-DIODE (layer B.Cu) (tedit 55C2C69D)
    (at 143 107)
    (descr DIODE)
    (tags DIODE)
    (fp_text reference D19 (at 0 3.81 270) (layer B.SilkS))
    (fp_text value DIODE (at 2.032 0 270) (layer B.SilkS) hide)
    (pad 2 smd rect (at 0 1.7526 90) (size 1.00076 0.8509) (layers B.Cu B.Paste B.Mask)
      (net 5 Row3))
    (pad 1 smd rect (at 0 -1.74752 90) (size 1.00076 0.8509) (layers B.Cu B.Paste B.Mask)
      (net 23 "Net-(D19-Pad1)"))
  )
  (module prettylib:SOT123-DIODE (layer B.Cu) (tedit 55C2C69D)
    (at 143 126)
    (descr DIODE)
    (tags DIODE)
    (fp_text reference D20 (at 0 3.81 270) (layer B.SilkS))
    (fp_text value DIODE (at 2.032 0 270) (layer B.SilkS) hide)
    (pad 2 smd rect (at 0 1.7526 90) (size 1.00076 0.8509) (layers B.Cu B.Paste B.Mask)
      (net 7 Row4))
    (pad 1 smd rect (at 0 -1.74752 90) (size 1.00076 0.8509) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(D20-Pad1)"))
  )
  (module Pin_Headers:Pin_Header_Angled_1x09_Pitch2.54mm (layer B.Cu) (tedit 59650532)
    (at 152 132.16)
    (descr "Through hole angled pin header, 1x09, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x09 2.54mm single row")
    (fp_text reference J1 (at 4.385 2.27) (layer B.SilkS))
    (fp_text value Conn_01x09_Male (at 4.385 -22.59) (layer B.Fab))
    (fp_text user %R (at 2.77 -10.16 270) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 Col1))
    (pad 2 thru_hole oval (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 Col2))
    (pad 3 thru_hole oval (at 0 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 Col3))
    (pad 4 thru_hole oval (at 0 -7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 Col4))
    (pad 5 thru_hole oval (at 0 -10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 Col5))
    (pad 6 thru_hole oval (at 0 -12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 Row4))
    (pad 7 thru_hole oval (at 0 -15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 Row3))
    (pad 8 thru_hole oval (at 0 -17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 Row2))
    (pad 9 thru_hole oval (at 0 -20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 Row1))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Angled_1x09_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module prettylib:MXALPS (layer F.Cu) (tedit 55C2C681)
    (at 64 69)
    (descr MXALPS)
    (tags MXALPS)
    (fp_text reference S1 (at 0 3.048) (layer B.SilkS))
    (fp_text value MXALPS (at -3.5 9) (layer B.SilkS) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3.98781 3.98781) (drill 3.9878) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.1524))
    (pad "" np_thru_hole circle (at -5.08 0) (size 1.70181 1.70181) (drill 1.7018) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.1524))
    (pad "" np_thru_hole circle (at 5.08 0) (size 1.70181 1.70181) (drill 1.7018) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.1524))
    (pad 1 thru_hole oval (at -3.405 -3.27 330.95) (size 2.5 4.17) (drill oval 1.5 3.17) (layers *.Cu *.Mask F.SilkS)
      (net 25 Col1))
    (pad 2 thru_hole oval (at 2.52 -4.79 356.1) (size 2.5 3.08) (drill oval 1.5 2.08) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(D1-Pad1)"))
  )
  (module prettylib:MXALPS (layer F.Cu) (tedit 55C2C681)
    (at 64 88)
    (descr MXALPS)
    (tags MXALPS)
    (fp_text reference S2 (at 0 3.048) (layer B.SilkS))
    (fp_text value MXALPS (at -3.5 9) (layer B.SilkS) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3.98781 3.98781) (drill 3.9878) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.1524))
    (pad "" np_thru_hole circle (at -5.08 0) (size 1.70181 1.70181) (drill 1.7018) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.1524))
    (pad "" np_thru_hole circle (at 5.08 0) (size 1.70181 1.70181) (drill 1.7018) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.1524))
    (pad 1 thru_hole oval (at -3.405 -3.27 330.95) (size 2.5 4.17) (drill oval 1.5 3.17) (layers *.Cu *.Mask F.SilkS)
      (net 25 Col1))
    (pad 2 thru_hole oval (at 2.52 -4.79 356.1) (size 2.5 3.08) (drill oval 1.5 2.08) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(D2-Pad1)"))
  )
  (module prettylib:MXALPS (layer F.Cu) (tedit 55C2C681)
    (at 64 107)
    (descr MXALPS)
    (tags MXALPS)
    (fp_text reference S3 (at 0 3.048) (layer B.SilkS))
    (fp_text value MXALPS (at -3.5 9) (layer B.SilkS) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3.98781 3.98781) (drill 3.9878) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.1524))
    (pad "" np_thru_hole circle (at -5.08 0) (size 1.70181 1.70181) (drill 1.7018) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.1524))
    (pad "" np_thru_hole circle (at 5.08 0) (size 1.70181 1.70181) (drill 1.7018) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.1524))
    (pad 1 thru_hole oval (at -3.405 -3.27 330.95) (size 2.5 4.17) (drill oval 1.5 3.17) (layers *.Cu *.Mask F.SilkS)
      (net 25 Col1))
    (pad 2 thru_hole oval (at 2.52 -4.79 356.1) (size 2.5 3.08) (drill oval 1.5 2.08) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(D3-Pad1)"))
  )
  (module prettylib:MXALPS (layer F.Cu) (tedit 55C2C681)
    (at 64 126)
    (descr MXALPS)
    (tags MXALPS)
    (fp_text reference S4 (at 0 3.048) (layer B.SilkS))
    (fp_text value MXALPS (at -3.5 9) (layer B.SilkS) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3.98781 3.98781) (drill 3.9878) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.1524))
    (pad "" np_thru_hole circle (at -5.08 0) (size 1.70181 1.70181) (drill 1.7018) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.1524))
    (pad "" np_thru_hole circle (at 5.08 0) (size 1.70181 1.70181) (drill 1.7018) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.1524))
    (pad 1 thru_hole oval (at -3.405 -3.27 330.95) (size 2.5 4.17) (drill oval 1.5 3.17) (layers *.Cu *.Mask F.SilkS)
      (net 25 Col1))
    (pad 2 thru_hole oval (at 2.52 -4.79 356.1) (size 2.5 3.08) (drill oval 1.5 2.08) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(D4-Pad1)"))
  )
  (module prettylib:MXALPS (layer F.Cu) (tedit 55C2C681)
    (at 83 69)
    (descr MXALPS)
    (tags MXALPS)
    (fp_text reference S5 (at 0 3.048) (layer B.SilkS))
    (fp_text value MXALPS (at -3.5 9) (layer B.SilkS) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3.98781 3.98781) (drill 3.9878) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.1524))
    (pad "" np_thru_hole circle (at -5.08 0) (size 1.70181 1.70181) (drill 1.7018) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.1524))
    (pad "" np_thru_hole circle (at 5.08 0) (size 1.70181 1.70181) (drill 1.7018) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.1524))
    (pad 1 thru_hole oval (at -3.405 -3.27 330.95) (size 2.5 4.17) (drill oval 1.5 3.17) (layers *.Cu *.Mask F.SilkS)
      (net 26 Col2))
    (pad 2 thru_hole oval (at 2.52 -4.79 356.1) (size 2.5 3.08) (drill oval 1.5 2.08) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(D5-Pad1)"))
  )
  (module prettylib:MXALPS (layer F.Cu) (tedit 55C2C681)
    (at 83 88)
    (descr MXALPS)
    (tags MXALPS)
    (fp_text reference S6 (at 0 3.048) (layer B.SilkS))
    (fp_text value MXALPS (at -3.5 9) (layer B.SilkS) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3.98781 3.98781) (drill 3.9878) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.1524))
    (pad "" np_thru_hole circle (at -5.08 0) (size 1.70181 1.70181) (drill 1.7018) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.1524))
    (pad "" np_thru_hole circle (at 5.08 0) (size 1.70181 1.70181) (drill 1.7018) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.1524))
    (pad 1 thru_hole oval (at -3.405 -3.27 330.95) (size 2.5 4.17) (drill oval 1.5 3.17) (layers *.Cu *.Mask F.SilkS)
      (net 26 Col2))
    (pad 2 thru_hole oval (at 2.52 -4.79 356.1) (size 2.5 3.08) (drill oval 1.5 2.08) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(D6-Pad1)"))
  )
  (module prettylib:MXALPS (layer F.Cu) (tedit 55C2C681)
    (at 83 107)
    (descr MXALPS)
    (tags MXALPS)
    (fp_text reference S7 (at 0 3.048) (layer B.SilkS))
    (fp_text value MXALPS (at -3.5 9) (layer B.SilkS) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3.98781 3.98781) (drill 3.9878) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.1524))
    (pad "" np_thru_hole circle (at -5.08 0) (size 1.70181 1.70181) (drill 1.7018) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.1524))
    (pad "" np_thru_hole circle (at 5.08 0) (size 1.70181 1.70181) (drill 1.7018) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.1524))
    (pad 1 thru_hole oval (at -3.405 -3.27 330.95) (size 2.5 4.17) (drill oval 1.5 3.17) (layers *.Cu *.Mask F.SilkS)
      (net 26 Col2))
    (pad 2 thru_hole oval (at 2.52 -4.79 356.1) (size 2.5 3.08) (drill oval 1.5 2.08) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(D7-Pad1)"))
  )
  (module prettylib:MXALPS (layer F.Cu) (tedit 55C2C681)
    (at 83 126)
    (descr MXALPS)
    (tags MXALPS)
    (fp_text reference S8 (at 0 3.048) (layer B.SilkS))
    (fp_text value MXALPS (at -3.5 9) (layer B.SilkS) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3.98781 3.98781) (drill 3.9878) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.1524))
    (pad "" np_thru_hole circle (at -5.08 0) (size 1.70181 1.70181) (drill 1.7018) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.1524))
    (pad "" np_thru_hole circle (at 5.08 0) (size 1.70181 1.70181) (drill 1.7018) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.1524))
    (pad 1 thru_hole oval (at -3.405 -3.27 330.95) (size 2.5 4.17) (drill oval 1.5 3.17) (layers *.Cu *.Mask F.SilkS)
      (net 26 Col2))
    (pad 2 thru_hole oval (at 2.52 -4.79 356.1) (size 2.5 3.08) (drill oval 1.5 2.08) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(D8-Pad1)"))
  )
  (module prettylib:MXALPS (layer F.Cu) (tedit 55C2C681)
    (at 102 69)
    (descr MXALPS)
    (tags MXALPS)
    (fp_text reference S9 (at 0 3.048) (layer B.SilkS))
    (fp_text value MXALPS (at -3.5 9) (layer B.SilkS) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3.98781 3.98781) (drill 3.9878) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.1524))
    (pad "" np_thru_hole circle (at -5.08 0) (size 1.70181 1.70181) (drill 1.7018) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.1524))
    (pad "" np_thru_hole circle (at 5.08 0) (size 1.70181 1.70181) (drill 1.7018) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.1524))
    (pad 1 thru_hole oval (at -3.405 -3.27 330.95) (size 2.5 4.17) (drill oval 1.5 3.17) (layers *.Cu *.Mask F.SilkS)
      (net 27 Col3))
    (pad 2 thru_hole oval (at 2.52 -4.79 356.1) (size 2.5 3.08) (drill oval 1.5 2.08) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(D9-Pad1)"))
  )
  (module prettylib:MXALPS (layer F.Cu) (tedit 55C2C681)
    (at 102 88)
    (descr MXALPS)
    (tags MXALPS)
    (fp_text reference S10 (at 0 3.048) (layer B.SilkS))
    (fp_text value MXALPS (at -3.5 9) (layer B.SilkS) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3.98781 3.98781) (drill 3.9878) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.1524))
    (pad "" np_thru_hole circle (at -5.08 0) (size 1.70181 1.70181) (drill 1.7018) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.1524))
    (pad "" np_thru_hole circle (at 5.08 0) (size 1.70181 1.70181) (drill 1.7018) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.1524))
    (pad 1 thru_hole oval (at -3.405 -3.27 330.95) (size 2.5 4.17) (drill oval 1.5 3.17) (layers *.Cu *.Mask F.SilkS)
      (net 27 Col3))
    (pad 2 thru_hole oval (at 2.52 -4.79 356.1) (size 2.5 3.08) (drill oval 1.5 2.08) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(D10-Pad1)"))
  )
  (module prettylib:MXALPS (layer F.Cu) (tedit 55C2C681)
    (at 102 106.68)
    (descr MXALPS)
    (tags MXALPS)
    (fp_text reference S11 (at 0 3.048) (layer B.SilkS))
    (fp_text value MXALPS (at -3.5 9) (layer B.SilkS) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3.98781 3.98781) (drill 3.9878) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.1524))
    (pad "" np_thru_hole circle (at -5.08 0) (size 1.70181 1.70181) (drill 1.7018) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.1524))
    (pad "" np_thru_hole circle (at 5.08 0) (size 1.70181 1.70181) (drill 1.7018) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.1524))
    (pad 1 thru_hole oval (at -3.405 -3.27 330.95) (size 2.5 4.17) (drill oval 1.5 3.17) (layers *.Cu *.Mask F.SilkS)
      (net 27 Col3))
    (pad 2 thru_hole oval (at 2.52 -4.79 356.1) (size 2.5 3.08) (drill oval 1.5 2.08) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(D11-Pad1)"))
  )
  (module prettylib:MXALPS (layer F.Cu) (tedit 55C2C681)
    (at 102 126)
    (descr MXALPS)
    (tags MXALPS)
    (fp_text reference S12 (at 0 3.048) (layer B.SilkS))
    (fp_text value MXALPS (at -3.5 9) (layer B.SilkS) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3.98781 3.98781) (drill 3.9878) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.1524))
    (pad "" np_thru_hole circle (at -5.08 0) (size 1.70181 1.70181) (drill 1.7018) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.1524))
    (pad "" np_thru_hole circle (at 5.08 0) (size 1.70181 1.70181) (drill 1.7018) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.1524))
    (pad 1 thru_hole oval (at -3.405 -3.27 330.95) (size 2.5 4.17) (drill oval 1.5 3.17) (layers *.Cu *.Mask F.SilkS)
      (net 27 Col3))
    (pad 2 thru_hole oval (at 2.52 -4.79 356.1) (size 2.5 3.08) (drill oval 1.5 2.08) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(D12-Pad1)"))
  )
  (module prettylib:MXALPS (layer F.Cu) (tedit 55C2C681)
    (at 121 69)
    (descr MXALPS)
    (tags MXALPS)
    (fp_text reference S13 (at 0 3.048) (layer B.SilkS))
    (fp_text value MXALPS (at -3.5 9) (layer B.SilkS) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3.98781 3.98781) (drill 3.9878) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.1524))
    (pad "" np_thru_hole circle (at -5.08 0) (size 1.70181 1.70181) (drill 1.7018) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.1524))
    (pad "" np_thru_hole circle (at 5.08 0) (size 1.70181 1.70181) (drill 1.7018) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.1524))
    (pad 1 thru_hole oval (at -3.405 -3.27 330.95) (size 2.5 4.17) (drill oval 1.5 3.17) (layers *.Cu *.Mask F.SilkS)
      (net 28 Col4))
    (pad 2 thru_hole oval (at 2.52 -4.79 356.1) (size 2.5 3.08) (drill oval 1.5 2.08) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(D13-Pad1)"))
  )
  (module prettylib:MXALPS (layer F.Cu) (tedit 55C2C681)
    (at 121 88)
    (descr MXALPS)
    (tags MXALPS)
    (fp_text reference S14 (at 0 3.048) (layer B.SilkS))
    (fp_text value MXALPS (at -3.5 9) (layer B.SilkS) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3.98781 3.98781) (drill 3.9878) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.1524))
    (pad "" np_thru_hole circle (at -5.08 0) (size 1.70181 1.70181) (drill 1.7018) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.1524))
    (pad "" np_thru_hole circle (at 5.08 0) (size 1.70181 1.70181) (drill 1.7018) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.1524))
    (pad 1 thru_hole oval (at -3.405 -3.27 330.95) (size 2.5 4.17) (drill oval 1.5 3.17) (layers *.Cu *.Mask F.SilkS)
      (net 28 Col4))
    (pad 2 thru_hole oval (at 2.52 -4.79 356.1) (size 2.5 3.08) (drill oval 1.5 2.08) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(D14-Pad1)"))
  )
  (module prettylib:MXALPS (layer F.Cu) (tedit 55C2C681)
    (at 121.08 107)
    (descr MXALPS)
    (tags MXALPS)
    (fp_text reference S15 (at 0 3.048) (layer B.SilkS))
    (fp_text value MXALPS (at -3.5 9) (layer B.SilkS) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3.98781 3.98781) (drill 3.9878) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.1524))
    (pad "" np_thru_hole circle (at -5.08 0) (size 1.70181 1.70181) (drill 1.7018) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.1524))
    (pad "" np_thru_hole circle (at 5.08 0) (size 1.70181 1.70181) (drill 1.7018) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.1524))
    (pad 1 thru_hole oval (at -3.405 -3.27 330.95) (size 2.5 4.17) (drill oval 1.5 3.17) (layers *.Cu *.Mask F.SilkS)
      (net 28 Col4))
    (pad 2 thru_hole oval (at 2.52 -4.79 356.1) (size 2.5 3.08) (drill oval 1.5 2.08) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(D15-Pad1)"))
  )
  (module prettylib:MXALPS (layer F.Cu) (tedit 55C2C681)
    (at 121 126)
    (descr MXALPS)
    (tags MXALPS)
    (fp_text reference S16 (at 0 3.048) (layer B.SilkS))
    (fp_text value MXALPS (at -3.5 9) (layer B.SilkS) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3.98781 3.98781) (drill 3.9878) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.1524))
    (pad "" np_thru_hole circle (at -5.08 0) (size 1.70181 1.70181) (drill 1.7018) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.1524))
    (pad "" np_thru_hole circle (at 5.08 0) (size 1.70181 1.70181) (drill 1.7018) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.1524))
    (pad 1 thru_hole oval (at -3.405 -3.27 330.95) (size 2.5 4.17) (drill oval 1.5 3.17) (layers *.Cu *.Mask F.SilkS)
      (net 28 Col4))
    (pad 2 thru_hole oval (at 2.52 -4.79 356.1) (size 2.5 3.08) (drill oval 1.5 2.08) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(D16-Pad1)"))
  )
  (module prettylib:MXALPS (layer F.Cu) (tedit 55C2C681)
    (at 140 69)
    (descr MXALPS)
    (tags MXALPS)
    (fp_text reference S17 (at 0 3.048) (layer B.SilkS))
    (fp_text value MXALPS (at -3.5 9) (layer B.SilkS) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3.98781 3.98781) (drill 3.9878) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.1524))
    (pad "" np_thru_hole circle (at -5.08 0) (size 1.70181 1.70181) (drill 1.7018) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.1524))
    (pad "" np_thru_hole circle (at 5.08 0) (size 1.70181 1.70181) (drill 1.7018) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.1524))
    (pad 1 thru_hole oval (at -3.405 -3.27 330.95) (size 2.5 4.17) (drill oval 1.5 3.17) (layers *.Cu *.Mask F.SilkS)
      (net 29 Col5))
    (pad 2 thru_hole oval (at 2.52 -4.79 356.1) (size 2.5 3.08) (drill oval 1.5 2.08) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(D17-Pad1)"))
  )
  (module prettylib:MXALPS (layer F.Cu) (tedit 55C2C681)
    (at 140 88)
    (descr MXALPS)
    (tags MXALPS)
    (fp_text reference S18 (at 0 3.048) (layer B.SilkS))
    (fp_text value MXALPS (at -3.5 9) (layer B.SilkS) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3.98781 3.98781) (drill 3.9878) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.1524))
    (pad "" np_thru_hole circle (at -5.08 0) (size 1.70181 1.70181) (drill 1.7018) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.1524))
    (pad "" np_thru_hole circle (at 5.08 0) (size 1.70181 1.70181) (drill 1.7018) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.1524))
    (pad 1 thru_hole oval (at -3.405 -3.27 330.95) (size 2.5 4.17) (drill oval 1.5 3.17) (layers *.Cu *.Mask F.SilkS)
      (net 29 Col5))
    (pad 2 thru_hole oval (at 2.52 -4.79 356.1) (size 2.5 3.08) (drill oval 1.5 2.08) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(D18-Pad1)"))
  )
  (module prettylib:MXALPS (layer F.Cu) (tedit 55C2C681)
    (at 140 107)
    (descr MXALPS)
    (tags MXALPS)
    (fp_text reference S19 (at 0 3.048) (layer B.SilkS))
    (fp_text value MXALPS (at -3.5 9) (layer B.SilkS) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3.98781 3.98781) (drill 3.9878) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.1524))
    (pad "" np_thru_hole circle (at -5.08 0) (size 1.70181 1.70181) (drill 1.7018) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.1524))
    (pad "" np_thru_hole circle (at 5.08 0) (size 1.70181 1.70181) (drill 1.7018) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.1524))
    (pad 1 thru_hole oval (at -3.405 -3.27 330.95) (size 2.5 4.17) (drill oval 1.5 3.17) (layers *.Cu *.Mask F.SilkS)
      (net 29 Col5))
    (pad 2 thru_hole oval (at 2.52 -4.79 356.1) (size 2.5 3.08) (drill oval 1.5 2.08) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(D19-Pad1)"))
  )
  (module prettylib:MXALPS (layer F.Cu) (tedit 55C2C681)
    (at 140 126)
    (descr MXALPS)
    (tags MXALPS)
    (fp_text reference S20 (at 0 3.048) (layer B.SilkS))
    (fp_text value MXALPS (at -3.5 9) (layer B.SilkS) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3.98781 3.98781) (drill 3.9878) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.1524))
    (pad "" np_thru_hole circle (at -5.08 0) (size 1.70181 1.70181) (drill 1.7018) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.1524))
    (pad "" np_thru_hole circle (at 5.08 0) (size 1.70181 1.70181) (drill 1.7018) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.1524))
    (pad 1 thru_hole oval (at -3.405 -3.27 330.95) (size 2.5 4.17) (drill oval 1.5 3.17) (layers *.Cu *.Mask F.SilkS)
      (net 29 Col5))
    (pad 2 thru_hole oval (at 2.52 -4.79 356.1) (size 2.5 3.08) (drill oval 1.5 2.08) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(D20-Pad1)"))
  )
  (gr_line (start 47 138) (end 157 138) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 157 57) (end 47 57) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 157 57) (end 157 138) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 47 138) (end 47 57) (layer Edge.Cuts) (width 0.15))
)
