(kicad_pcb (version 4) (host pcbnew 4.0.2+e4-6225~38~ubuntu14.04.1-stable)
  (general
    (links 20)
    (no_connects 3)
    (area 64.924999 69.924999 215.075001 120.075001)
    (thickness 1.6)
    (drawings 13)
    (tracks 41)
    (zones 0)
    (modules 8)
    (nets 10)
  )
  (page USLetter)
  (title_block
    (title "Cobwebb Junction Box With RF Choke")
    (date 2016-06-11)
    (rev 0.0.1)
    (company "K7FOS & W7BFF")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 2.2)
    (trace_clearance 0.3)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3.5 3.5)
    (pad_drill 3)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_ffffffff)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory export/))
  )
  (net 0 "")
  (net 1 "Net-(P1-Pad1)")
  (net 2 "Net-(P1-Pad2)")
  (net 3 "Net-(U1-Pad1)")
  (net 4 "Net-(U1-Pad10)")
  (net 5 "Net-(U1-Pad3)")
  (net 6 "Net-(U1-Pad5)")
  (net 7 "Net-(U1-Pad7)")
  (net 8 "Net-(U1-Pad9)")
  (net 9 "Net-(U2-Pad4)")
  (net_class Default "This is the default net class."
    (clearance 0.3)
    (trace_width 2.2)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(P1-Pad1)")
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(U1-Pad9)")
    (add_net "Net-(U2-Pad4)")
  )
  (module 60-clock:1pin (layer F.Cu) (tedit 575C6FB4)
    (at 70 75)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF**1111 (at 5 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 5 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3) (layers *.Cu *.Mask))
  )
  (module 60-clock:1pin (layer F.Cu) (tedit 575C6FC8)
    (at 210 115)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF**1122 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3) (layers *.Cu *.Mask))
  )
  (module 60-clock:1pin (layer F.Cu) (tedit 575C6FBA)
    (at 70 115)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF**1112 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3) (layers *.Cu *.Mask))
  )
  (module 60-clock:1pin (layer F.Cu) (tedit 575C6FC2)
    (at 210 75)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF**1121 (at -5 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3) (layers *.Cu *.Mask))
  )
  (module CobwebbJunctionBox:Terminal_Block_10_Pin (layer F.Cu) (tedit 575BBCC4)
    (at 199.25 80 180)
    (fp_text reference U1 (at 37.25 -4.75 180) (layer F.SilkS))
    (fp_text value Terminal_Block_10_Pin (at 36.25 -6.75 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 3.2 3.2) (drill 1.8) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(U1-Pad1)"))
    (pad 2 thru_hole circle (at 8.25 0 180) (size 3.2 3.2) (drill 1.8) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(U1-Pad10)"))
    (pad 3 thru_hole circle (at 16.5 0 180) (size 3.2 3.2) (drill 1.8) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(U1-Pad3)"))
    (pad 4 thru_hole circle (at 24.75 0 180) (size 3.2 3.2) (drill 1.8) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(U1-Pad10)"))
    (pad 5 thru_hole circle (at 33 0 180) (size 3.2 3.2) (drill 1.8) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(U1-Pad5)"))
    (pad 6 thru_hole circle (at 41.25 0 180) (size 3.2 3.2) (drill 1.8) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(U1-Pad10)"))
    (pad 7 thru_hole circle (at 49.5 0 180) (size 3.2 3.2) (drill 1.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(U1-Pad7)"))
    (pad 8 thru_hole circle (at 57.75 0 180) (size 3.2 3.2) (drill 1.8) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(U1-Pad10)"))
    (pad 9 thru_hole circle (at 66 0 180) (size 3.2 3.2) (drill 1.8) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(U1-Pad9)"))
    (pad 10 thru_hole circle (at 74.25 0 180) (size 3.2 3.2) (drill 1.8) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(U1-Pad10)"))
  )
  (module CobwebbJunctionBox:RF_Choke_T106-2 (layer F.Cu) (tedit 575C6FE0)
    (at 100 95)
    (fp_text reference U2 (at 0 10) (layer F.SilkS))
    (fp_text value RF_Choke (at 0 -11) (layer F.Fab))
    (fp_text user - (at -20 -10) (layer F.SilkS))
    (fp_text user + (at -20 -14) (layer F.SilkS))
    (fp_text user + (at -20 10) (layer F.SilkS))
    (fp_text user - (at -20 14) (layer F.SilkS))
    (pad "" thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole circle (at -23 -14) (size 3 3) (drill 2) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(P1-Pad2)"))
    (pad 2 thru_hole circle (at -23 -10) (size 3 3) (drill 2) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(P1-Pad1)"))
    (pad 3 thru_hole circle (at -23 10) (size 3 3) (drill 2) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(U1-Pad10)"))
    (pad 4 thru_hole circle (at -23 14) (size 3 3) (drill 2) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(U2-Pad4)"))
  )
  (module CobwebbJunctionBox:Terminal_Block_10_Pin (layer F.Cu) (tedit 575BBCC4)
    (at 125 110)
    (fp_text reference U3 (at 37.25 -4.75) (layer F.SilkS))
    (fp_text value Terminal_Block_10_Pin (at 36.25 -6.75) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.2 3.2) (drill 1.8) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(U2-Pad4)"))
    (pad 2 thru_hole circle (at 8.25 0) (size 3.2 3.2) (drill 1.8) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(U1-Pad9)"))
    (pad 3 thru_hole circle (at 16.5 0) (size 3.2 3.2) (drill 1.8) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(U2-Pad4)"))
    (pad 4 thru_hole circle (at 24.75 0) (size 3.2 3.2) (drill 1.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(U1-Pad7)"))
    (pad 5 thru_hole circle (at 33 0) (size 3.2 3.2) (drill 1.8) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(U2-Pad4)"))
    (pad 6 thru_hole circle (at 41.25 0) (size 3.2 3.2) (drill 1.8) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(U1-Pad5)"))
    (pad 7 thru_hole circle (at 49.5 0) (size 3.2 3.2) (drill 1.8) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(U2-Pad4)"))
    (pad 8 thru_hole circle (at 57.75 0) (size 3.2 3.2) (drill 1.8) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(U1-Pad3)"))
    (pad 9 thru_hole circle (at 66 0) (size 3.2 3.2) (drill 1.8) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(U2-Pad4)"))
    (pad 10 thru_hole circle (at 74.25 0) (size 3.2 3.2) (drill 1.8) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(U1-Pad1)"))
  )
  (module CobwebbJunctionBox:BNC_Connector (layer F.Cu) (tedit 575BD102)
    (at 73 95 270)
    (fp_text reference P1 (at 0 7 270) (layer F.SilkS))
    (fp_text value BNC (at 0 -7 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 0 270) (size 1.9 1.9) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(P1-Pad2)"))
    (pad 1 thru_hole circle (at -3.3 -3.3 270) (size 1.9 1.9) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(P1-Pad1)"))
    (pad 1 thru_hole circle (at 3.3 -3.3 270) (size 1.9 1.9) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(P1-Pad1)"))
    (pad 1 thru_hole circle (at -3.3 3.3 270) (size 1.9 1.9) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(P1-Pad1)"))
    (pad 1 thru_hole circle (at 3.3 3.3 270) (size 1.9 1.9) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(P1-Pad1)"))
  )
  (gr_text https://github.com/efosmark/cobwebb-junction-box (at 199.39 73.66) (layer B.SilkS))
  (gr_text "REV 1.1.0\nJune 10, 2016" (at 210 80 90) (layer F.SilkS))
  (gr_text "W7BFF - Charles Parker II\nK7FOS - Evan Fosmark" (at 84.5 116) (layer F.SilkS))
  (gr_text "JUNCTION BOX WITH\nBUILT-IN RF CHOKE" (at 179.5 95) (layer F.SilkS))
  (gr_text "Cobwebb Antenna" (at 147.5 95) (layer F.SilkS))
  (gr_arc (start 210 75) (end 210 70) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 210 115) (end 215 115) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 70 115) (end 70 120) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 70 75) (end 65 75) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 210 70) (end 70 70) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 215 115) (end 215 75) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 70 120) (end 210 120) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 65 75) (end 65 115) (layer Edge.Cuts) (width 0.15))
)
