(kicad_pcb (version 20170123) (host pcbnew no-vcs-found-1a33efa~58~ubuntu16.04.1)
  (general
    (links 237)
    (no_connects 1)
    (area 47.772599 39.899999 137.649001 123.600001)
    (thickness 1.6002)
    (drawings 11)
    (tracks 803)
    (zones 0)
    (modules 90)
    (nets 71)
  )
  (page USLetter)
  (title_block
    (title GeoCentinela)
    (date "sáb 15 nov 2014")
    (rev 4.0)
    (company timining)
    (comment 1 "Luis Saavedra")
  )
  (layers
    (0 Top jumper)
    (31 Bottom signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.254)
    (user_trace_width 0.508)
    (user_trace_width 1.016)
    (trace_clearance 0.1524)
    (zone_clearance 0.381)
    (zone_45_only yes)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.0254)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.508)
    (via_min_drill 0.127)
    (user_via 0.508 0.254)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.16)
    (mod_text_size 0.5 0.5)
    (mod_text_width 0.125)
    (pad_size 0.8 0.75)
    (pad_drill 0)
    (pad_to_mask_clearance 0)
    (pad_to_paste_clearance_ratio -0.1)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +3.3V)
  (net 2 +3.3VP)
  (net 3 +5V)
  (net 4 +5VA)
  (net 5 AGND)
  (net 6 GND)
  (net 7 VCC)
  (net 8 "Net-(C3-Pad2)")
  (net 9 "Net-(C10-Pad2)")
  (net 10 "Net-(C10-Pad1)")
  (net 11 "Net-(C11-Pad2)")
  (net 12 "Net-(C11-Pad1)")
  (net 13 "Net-(D1-Pad2)")
  (net 14 GNDPWR)
  (net 15 "Net-(SW1-Pad1)")
  (net 16 "Net-(U2-Pad7)")
  (net 17 "Net-(U3-Pad7)")
  (net 18 "Net-(U4-Pad7)")
  (net 19 "/Signal Conditioning/+Ch0")
  (net 20 "/Signal Conditioning/-Ch0")
  (net 21 "/Signal Conditioning/+Ch1")
  (net 22 "/Signal Conditioning/-Ch1")
  (net 23 "/Signal Conditioning/+Ch2")
  (net 24 "/Signal Conditioning/-Ch2")
  (net 25 /SD_CS)
  (net 26 +12VA)
  (net 27 /XBEE_Sleep_RQ)
  (net 28 /BAT)
  (net 29 /XBEE_TX)
  (net 30 /XBEE_RX)
  (net 31 /SPI_MOSI)
  (net 32 /SPI_CLK)
  (net 33 /SPI_MISO)
  (net 34 "Net-(R18-Pad2)")
  (net 35 /vbat)
  (net 36 /ch2)
  (net 37 /~CS)
  (net 38 /A0)
  (net 39 /A1)
  (net 40 /A2)
  (net 41 /ch0)
  (net 42 /ch1)
  (net 43 /EXT)
  (net 44 /SDX)
  (net 45 /PGA)
  (net 46 GNDREF)
  (net 47 Vbias)
  (net 48 Vref)
  (net 49 "Net-(C40-Pad2)")
  (net 50 "Net-(JP1-Pad1)")
  (net 51 "Net-(D2-Pad1)")
  (net 52 /Wp)
  (net 53 "Net-(C4-Pad2)")
  (net 54 "Net-(C48-Pad1)")
  (net 55 "Net-(C49-Pad2)")
  (net 56 "Net-(C52-Pad1)")
  (net 57 "Net-(C53-Pad2)")
  (net 58 "Net-(D1-Pad4)")
  (net 59 "Net-(D1-Pad1)")
  (net 60 /XBEE_~RESET)
  (net 61 /XBEE_ON_~SLEEP)
  (net 62 /XBEE_~CTS)
  (net 63 /MCU_RX1)
  (net 64 /MCU_TX1)
  (net 65 /XBEE_~RTS)
  (net 66 /PPS)
  (net 67 /Tx)
  (net 68 /Rx)
  (net 69 "Net-(RN1-Pad8)")
  (net 70 "Net-(RN1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net +12VA)
    (add_net +3.3V)
    (add_net +3.3VP)
    (add_net +5V)
    (add_net +5VA)
    (add_net /A0)
    (add_net /A1)
    (add_net /A2)
    (add_net /BAT)
    (add_net /EXT)
    (add_net /MCU_RX1)
    (add_net /MCU_TX1)
    (add_net /PGA)
    (add_net /PPS)
    (add_net /Rx)
    (add_net /SDX)
    (add_net /SD_CS)
    (add_net /SPI_CLK)
    (add_net /SPI_MISO)
    (add_net /SPI_MOSI)
    (add_net "/Signal Conditioning/+Ch0")
    (add_net "/Signal Conditioning/+Ch1")
    (add_net "/Signal Conditioning/+Ch2")
    (add_net "/Signal Conditioning/-Ch0")
    (add_net "/Signal Conditioning/-Ch1")
    (add_net "/Signal Conditioning/-Ch2")
    (add_net /Tx)
    (add_net /Wp)
    (add_net /XBEE_ON_~SLEEP)
    (add_net /XBEE_RX)
    (add_net /XBEE_Sleep_RQ)
    (add_net /XBEE_TX)
    (add_net /XBEE_~CTS)
    (add_net /XBEE_~RESET)
    (add_net /XBEE_~RTS)
    (add_net /ch0)
    (add_net /ch1)
    (add_net /ch2)
    (add_net /vbat)
    (add_net /~CS)
    (add_net AGND)
    (add_net GND)
    (add_net GNDPWR)
    (add_net GNDREF)
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C10-Pad2)")
    (add_net "Net-(C11-Pad1)")
    (add_net "Net-(C11-Pad2)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C4-Pad2)")
    (add_net "Net-(C40-Pad2)")
    (add_net "Net-(C48-Pad1)")
    (add_net "Net-(C49-Pad2)")
    (add_net "Net-(C52-Pad1)")
    (add_net "Net-(C53-Pad2)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D1-Pad4)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(JP1-Pad1)")
    (add_net "Net-(R18-Pad2)")
    (add_net "Net-(RN1-Pad1)")
    (add_net "Net-(RN1-Pad8)")
    (add_net "Net-(SW1-Pad1)")
    (add_net "Net-(U2-Pad7)")
    (add_net "Net-(U3-Pad7)")
    (add_net "Net-(U4-Pad7)")
    (add_net VCC)
    (add_net Vbias)
    (add_net Vref)
  )
  (module geocentinela:CP-16-4 (layer Top) (tedit 591F72AF)
    (at 66 54.95)
    (fp_text reference U3 (at -1.7 -2.45) (layer F.SilkS))
    (fp_text value AD8231 (at 0 -0.95) (layer B.SilkS))
    (pad 11 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 5 AGND) (zone_connect 2))
    (pad 11 smd rect (at 0 0) (size 1.233288 1.233288) (layers Bottom F.Paste B.Mask)
      (net 5 AGND))
    (pad 11 smd rect (at 0 0) (size 1.95 1.95) (layers Top F.Mask)
      (net 5 AGND) (clearance 0.105))
    (pad 16 smd rect (at -0.975 -1.7653) (size 0.3556 1.0668) (layers Top F.Paste F.Mask)
      (net 40 /A2) (clearance 0.07))
    (pad 15 smd rect (at -0.325 -1.7653) (size 0.3556 1.0668) (layers Top F.Paste F.Mask)
      (net 39 /A1) (clearance 0.07))
    (pad 14 smd rect (at 0.325 -1.7653) (size 0.3556 1.0668) (layers Top F.Paste F.Mask)
      (net 38 /A0) (clearance 0.07))
    (pad 13 smd rect (at 0.975 -1.7653) (size 0.3556 1.0668) (layers Top F.Paste F.Mask)
      (net 37 /~CS) (clearance 0.07))
    (pad 12 smd rect (at 1.7653 -0.975) (size 1.0668 0.3556) (layers Top F.Paste F.Mask)
      (net 4 +5VA) (clearance 0.07))
    (pad 11 smd rect (at 1.7653 -0.325) (size 1.0668 0.3556) (layers Top F.Paste F.Mask)
      (net 5 AGND) (clearance 0.07))
    (pad 10 smd rect (at 1.7653 0.325) (size 1.0668 0.3556) (layers Top F.Paste F.Mask)
      (net 41 /ch0) (clearance 0.07))
    (pad 9 smd rect (at 1.7653 0.975) (size 1.0668 0.3556) (layers Top F.Paste F.Mask)
      (net 17 "Net-(U3-Pad7)") (clearance 0.07))
    (pad 8 smd rect (at 0.975 1.7653) (size 0.3556 1.0668) (layers Top F.Paste F.Mask)
      (net 17 "Net-(U3-Pad7)") (clearance 0.07))
    (pad 7 smd rect (at 0.325 1.7653) (size 0.3556 1.0668) (layers Top F.Paste F.Mask)
      (net 17 "Net-(U3-Pad7)") (clearance 0.07))
    (pad 6 smd rect (at -0.325 1.7653) (size 0.3556 1.0668) (layers Top F.Paste F.Mask)
      (net 47 Vbias) (clearance 0.07))
    (pad 5 smd rect (at -0.975 1.7653) (size 0.3556 1.0668) (layers Top F.Paste F.Mask)
      (net 4 +5VA) (clearance 0.07))
    (pad 4 smd rect (at -1.7653 0.975) (size 1.0668 0.3556) (layers Top F.Paste F.Mask)
      (clearance 0.07))
    (pad 3 smd rect (at -1.7653 0.325) (size 1.0668 0.3556) (layers Top F.Paste F.Mask)
      (net 9 "Net-(C10-Pad2)") (clearance 0.07))
    (pad 2 smd rect (at -1.7653 -0.325) (size 1.0668 0.3556) (layers Top F.Paste F.Mask)
      (net 10 "Net-(C10-Pad1)") (clearance 0.07))
    (pad 1 smd rect (at -1.7653 -0.975) (size 1.0668 0.3556) (layers Top F.Paste F.Mask)
      (clearance 0.07))
    (model GeoCentinela.3dshapes/AD8231.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module geocentinela:SLP3-150-100-F (layer Top) (tedit 592A2647)
    (at 127.4 112.6 90)
    (fp_text reference U6 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value "Led's Pipe" (at 0 2.159 90) (layer B.SilkS))
    (fp_text user D=118mils (at 0 4.445 90) (layer F.Fab))
    (fp_text user H=h+60mils (at 0 3.175 90) (layer F.Fab))
    (fp_text user h=150mils (at 0 3.81 90) (layer F.Fab))
    (pad "" thru_hole circle (at 1.27 -2.6924 90) (size 1.4224 1.4224) (drill 1.1684) (layers *.Cu))
    (pad "" thru_hole circle (at -1.27 -2.6924 90) (size 1.4224 1.4224) (drill 1.1684) (layers *.Cu))
  )
  (module geocentinela:KFC-A36-06 (layer Top) (tedit 592A221D)
    (at 127.2 105.5 270)
    (fp_text reference SW1 (at 0 0.5 270) (layer F.SilkS))
    (fp_text value Commissioning (at 0 1.5 270) (layer F.Fab))
    (fp_text user w=1.7mm (at 0 -5 270) (layer F.Fab))
    (fp_text user hc=2.6mm (at 0 -4.4 270) (layer F.Fab))
    (fp_text user H=4.4mm (at 0 3.1 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 2.5 0 270) (size 1.6002 1.6002) (drill 0.8382) (layers *.Cu *.Mask)
      (net 15 "Net-(SW1-Pad1)"))
    (pad 2 thru_hole circle (at -2.5 0 270) (size 1.6002 1.6002) (drill 0.8382) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 3 thru_hole circle (at 3.5 2.5 270) (size 1.6002 1.6002) (drill 1.3462) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at -3.5 2.5 270) (size 1.6002 1.6002) (drill 1.3462) (layers *.Cu *.Mask))
  )
  (module geocentinela:XBee (layer Top) (tedit 59215FDE)
    (at 113.2 100.5 270)
    (fp_text reference XB1 (at 0 0 270) (layer F.SilkS))
    (fp_text value XBEE (at 0 0 270) (layer B.SilkS))
    (fp_text user D=8mm (at -3.81 -19.685 270) (layer F.Fab))
    (fp_text user h=4.4mm (at -3.81 -21.59 270) (layer F.Fab))
    (pad 11 thru_hole circle (at 11 9 270) (size 1.0668 1.0668) (drill 0.635) (layers *.Cu *.Mask F.SilkS)
      (net 31 /SPI_MOSI))
    (pad 10 thru_hole circle (at -11 9 270) (size 1.0668 1.0668) (drill 0.635) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (pad 20 thru_hole circle (at 11 -9 270) (size 1.0668 1.0668) (drill 0.635) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(SW1-Pad1)"))
    (pad 19 thru_hole circle (at 11 -7 270) (size 1.0668 1.0668) (drill 0.635) (layers *.Cu *.Mask F.SilkS))
    (pad 18 thru_hole circle (at 11 -5 270) (size 1.0668 1.0668) (drill 0.635) (layers *.Cu *.Mask F.SilkS)
      (net 32 /SPI_CLK))
    (pad 17 thru_hole circle (at 11 -3 270) (size 1.0668 1.0668) (drill 0.635) (layers *.Cu *.Mask F.SilkS)
      (net 34 "Net-(R18-Pad2)"))
    (pad 16 thru_hole circle (at 11 -1 270) (size 1.0668 1.0668) (drill 0.635) (layers *.Cu *.Mask F.SilkS)
      (net 65 /XBEE_~RTS))
    (pad 15 thru_hole circle (at 11 1 270) (size 1.0668 1.0668) (drill 0.635) (layers *.Cu *.Mask F.SilkS)
      (net 59 "Net-(D1-Pad1)"))
    (pad 14 thru_hole circle (at 11 3 270) (size 1.0668 1.0668) (drill 0.635) (layers *.Cu *.Mask F.SilkS))
    (pad 13 thru_hole circle (at 11 5 270) (size 1.0668 1.0668) (drill 0.635) (layers *.Cu *.Mask F.SilkS)
      (net 61 /XBEE_ON_~SLEEP))
    (pad 12 thru_hole circle (at 11 7 270) (size 1.0668 1.0668) (drill 0.635) (layers *.Cu *.Mask F.SilkS)
      (net 62 /XBEE_~CTS))
    (pad 9 thru_hole circle (at -11 7 270) (size 1.0668 1.0668) (drill 0.635) (layers *.Cu *.Mask F.SilkS)
      (net 27 /XBEE_Sleep_RQ))
    (pad 8 thru_hole circle (at -11 5 270) (size 1.0668 1.0668) (drill 0.635) (layers *.Cu *.Mask F.SilkS))
    (pad 7 thru_hole circle (at -11 3 270) (size 1.0668 1.0668) (drill 0.635) (layers *.Cu *.Mask F.SilkS)
      (net 25 /SD_CS))
    (pad 6 thru_hole circle (at -11 1 270) (size 1.0668 1.0668) (drill 0.635) (layers *.Cu *.Mask F.SilkS))
    (pad 5 thru_hole circle (at -11 -1 270) (size 1.0668 1.0668) (drill 0.635) (layers *.Cu *.Mask F.SilkS)
      (net 60 /XBEE_~RESET))
    (pad 4 thru_hole circle (at -11 -3 270) (size 1.0668 1.0668) (drill 0.635) (layers *.Cu *.Mask F.SilkS)
      (net 33 /SPI_MISO))
    (pad 3 thru_hole circle (at -11 -5 270) (size 1.0668 1.0668) (drill 0.635) (layers *.Cu *.Mask F.SilkS)
      (net 30 /XBEE_RX))
    (pad 2 thru_hole circle (at -11 -7 270) (size 1.0668 1.0668) (drill 0.635) (layers *.Cu *.Mask F.SilkS)
      (net 29 /XBEE_TX))
    (pad 1 thru_hole circle (at -11 -9 270) (size 1.0668 1.0668) (drill 0.635) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3.3V))
  )
  (module geocentinela:15EDGRC-3.5-9P (layer Top) (tedit 59246057)
    (at 56 67.2 90)
    (fp_text reference P1 (at 0 -4 90) (layer F.SilkS))
    (fp_text value "Geophone Array" (at 0 -4 90) (layer B.SilkS))
    (pad 9 thru_hole circle (at -14 0 90) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 14 GNDPWR))
    (pad 8 thru_hole circle (at -10.5 0 90) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 24 "/Signal Conditioning/-Ch2"))
    (pad 7 thru_hole circle (at -7 0 90) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 23 "/Signal Conditioning/+Ch2"))
    (pad 6 thru_hole circle (at -3.5 0 90) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 14 GNDPWR))
    (pad 5 thru_hole circle (at 0 0 90) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 22 "/Signal Conditioning/-Ch1"))
    (pad 4 thru_hole circle (at 3.5 0 90) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 21 "/Signal Conditioning/+Ch1"))
    (pad 3 thru_hole circle (at 7 0 90) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 14 GNDPWR))
    (pad 2 thru_hole circle (at 10.5 0 90) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 20 "/Signal Conditioning/-Ch0"))
    (pad 1 thru_hole rect (at 14 0 90) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 19 "/Signal Conditioning/+Ch0"))
  )
  (module geocentinela:SD-DM1AA-SF-PEJ (layer Top) (tedit 59243836)
    (at 98 75.7 90)
    (fp_text reference SD1 (at 27.65 -1.2 180) (layer F.SilkS))
    (fp_text value SD (at 14 10.7 90) (layer B.SilkS))
    (pad CD smd rect (at -2.2 9.2 90) (size 2 1) (layers Top F.Paste F.Mask))
    (pad WP smd rect (at -2.2 18.15 90) (size 2 1) (layers Top F.Paste F.Mask))
    (pad CMD smd rect (at -2.2 20.75 90) (size 2 1) (layers Top F.Paste F.Mask))
    (pad "" smd rect (at 26.4 23.2 90) (size 2 2) (layers Top F.Paste F.Mask))
    (pad "" smd rect (at -2.6 23.2 90) (size 2 2) (layers Top F.Paste F.Mask))
    (pad "" smd rect (at 26.4 4.55 90) (size 2 2) (layers Top F.Paste F.Mask))
    (pad "" smd rect (at -2.6 4.55 90) (size 2 2) (layers Top F.Paste F.Mask))
    (pad "" thru_hole circle (at 22.4 0 90) (size 1.554 1.554) (drill 1.3) (layers *.Cu))
    (pad "" thru_hole circle (at 0 0 90) (size 1.554 1.554) (drill 1.3) (layers *.Cu))
    (pad 9 smd rect (at 20.475 -2.2 90) (size 1 2) (layers Top F.Paste F.Mask))
    (pad 8 smd rect (at 1.35 -2.2 90) (size 1 2) (layers Top F.Paste F.Mask))
    (pad 7 smd rect (at 3.05 -2.2 90) (size 1 2) (layers Top F.Paste F.Mask)
      (net 33 /SPI_MISO))
    (pad 6 smd rect (at 5.475 -2.2 90) (size 1 2) (layers Top F.Paste F.Mask)
      (net 6 GND))
    (pad 5 smd rect (at 7.975 -2.2 90) (size 1 2) (layers Top F.Paste F.Mask)
      (net 32 /SPI_CLK))
    (pad 4 smd rect (at 10.475 -2.2 90) (size 1 2) (layers Top F.Paste F.Mask)
      (net 49 "Net-(C40-Pad2)"))
    (pad 3 smd rect (at 12.975 -2.2 90) (size 1 2) (layers Top F.Paste F.Mask)
      (net 6 GND))
    (pad 2 smd rect (at 15.475 -2.2 90) (size 1 2) (layers Top F.Paste F.Mask)
      (net 31 /SPI_MOSI))
    (pad 1 smd rect (at 17.975 -2.2 90) (size 1 2) (layers Top F.Paste F.Mask)
      (net 25 /SD_CS))
  )
  (module geocentinela:TEENSY3 (layer Top) (tedit 54670AB2)
    (at 79.4 67.035 180)
    (fp_text reference U10 (at 0 0 180) (layer F.SilkS))
    (fp_text value Teensy3.2 (at 0 0 180) (layer B.SilkS))
    (pad 34 thru_hole circle (at 5.08 -3.81 180) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask F.SilkS)
      (net 47 Vbias))
    (pad 35 thru_hole circle (at 5.08 -6.35 180) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask F.SilkS)
      (net 36 /ch2))
    (pad 36 thru_hole circle (at 5.08 -8.89 180) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask F.SilkS)
      (net 48 Vref))
    (pad 37 thru_hole circle (at 5.08 -13.97 180) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask F.SilkS)
      (net 70 "Net-(RN1-Pad1)"))
    (pad 33 thru_hole circle (at 7.62 -16.51 180) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask F.SilkS)
      (net 3 +5V))
    (pad 32 thru_hole circle (at 7.62 -13.97 180) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask F.SilkS)
      (net 5 AGND))
    (pad 31 thru_hole circle (at 7.62 -11.43 180) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask F.SilkS))
    (pad 30 thru_hole circle (at 7.62 -8.89 180) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask F.SilkS)
      (net 45 /PGA))
    (pad 29 thru_hole circle (at 7.62 -6.35 180) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask F.SilkS)
      (net 35 /vbat))
    (pad 28 thru_hole circle (at 7.62 -3.81 180) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask F.SilkS)
      (net 43 /EXT))
    (pad 27 thru_hole circle (at 7.62 -1.27 180) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask F.SilkS)
      (net 44 /SDX))
    (pad 26 thru_hole circle (at 7.62 1.27 180) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask F.SilkS)
      (net 37 /~CS))
    (pad 25 thru_hole circle (at 7.62 3.81 180) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask F.SilkS)
      (net 38 /A0))
    (pad 24 thru_hole circle (at 7.62 6.35 180) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask F.SilkS)
      (net 42 /ch1))
    (pad 23 thru_hole circle (at 7.62 8.89 180) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask F.SilkS)
      (net 41 /ch0))
    (pad 22 thru_hole circle (at 7.62 11.43 180) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask F.SilkS)
      (net 40 /A2))
    (pad 21 thru_hole circle (at 7.62 13.97 180) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask F.SilkS)
      (net 39 /A1))
    (pad 20 thru_hole circle (at 7.62 16.51 180) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask F.SilkS)
      (net 32 /SPI_CLK))
    (pad 19 thru_hole circle (at 5.08 16.51 180) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask F.SilkS))
    (pad 18 thru_hole circle (at 2.54 16.51 180) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask F.SilkS))
    (pad 17 thru_hole circle (at 0 16.51 180) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask F.SilkS))
    (pad 16 thru_hole circle (at -2.54 16.51 180) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask F.SilkS)
      (net 50 "Net-(JP1-Pad1)"))
    (pad 15 thru_hole circle (at -5.08 16.51 180) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask F.SilkS)
      (net 28 /BAT))
    (pad 14 thru_hole circle (at -7.62 16.51 180) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask F.SilkS)
      (net 33 /SPI_MISO))
    (pad 13 thru_hole circle (at -7.62 13.97 180) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask F.SilkS)
      (net 31 /SPI_MOSI))
    (pad 12 thru_hole circle (at -7.62 11.43 180) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask F.SilkS)
      (net 25 /SD_CS))
    (pad 11 thru_hole circle (at -7.62 8.89 180) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask F.SilkS)
      (net 66 /PPS))
    (pad 10 thru_hole circle (at -7.62 6.35 180) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask F.SilkS)
      (net 67 /Tx))
    (pad 9 thru_hole circle (at -7.62 3.81 180) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask F.SilkS)
      (net 68 /Rx))
    (pad 8 thru_hole circle (at -7.62 1.27 180) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask F.SilkS)
      (net 65 /XBEE_~RTS))
    (pad 7 thru_hole circle (at -7.62 -1.27 180) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask F.SilkS)
      (net 61 /XBEE_ON_~SLEEP))
    (pad 6 thru_hole circle (at -7.62 -3.81 180) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask F.SilkS)
      (net 62 /XBEE_~CTS))
    (pad 5 thru_hole circle (at -7.62 -6.35 180) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask F.SilkS)
      (net 27 /XBEE_Sleep_RQ))
    (pad 4 thru_hole circle (at -7.62 -8.89 180) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask F.SilkS)
      (net 52 /Wp))
    (pad 3 thru_hole circle (at -7.62 -11.43 180) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask F.SilkS)
      (net 64 /MCU_TX1))
    (pad 2 thru_hole circle (at -7.62 -13.97 180) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask F.SilkS)
      (net 63 /MCU_RX1))
    (pad 1 thru_hole circle (at -7.62 -16.51 180) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND) (die_length 1))
  )
  (module Capacitors_SMD:C_0603 (layer Top) (tedit 5927A087)
    (at 69.1 83 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C49 (at 1.6 0 180) (layer F.SilkS))
    (fp_text value 103K (at 0 0 270) (layer B.SilkS))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers Top F.Paste F.Mask)
      (net 55 "Net-(C49-Pad2)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers Top F.Paste F.Mask)
      (net 4 +5VA))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module geocentinela:LED_RGB_0605 (layer Top) (tedit 56C38BBE)
    (at 127.4 112.6 270)
    (descr "LED 0605 dual 0603 smd package")
    (tags "LED 0605 SMD RGB")
    (attr smd)
    (fp_text reference D1 (at 2.7 0) (layer F.SilkS))
    (fp_text value Associate/SCLK (at 0 0 270) (layer F.Fab))
    (pad 4 smd rect (at 0.775 0.5 90) (size 0.75 0.5) (layers Top F.Paste F.Mask)
      (net 58 "Net-(D1-Pad4)"))
    (pad 3 smd rect (at 0.775 -0.5 90) (size 0.75 0.5) (layers Top F.Paste F.Mask)
      (net 32 /SPI_CLK))
    (pad 1 smd rect (at -0.775 -0.5 90) (size 0.75 0.5) (layers Top F.Paste F.Mask)
      (net 59 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at -0.75 0.5 90) (size 0.75 0.5) (layers Top F.Paste F.Mask)
      (net 13 "Net-(D1-Pad2)"))
  )
  (module geocentinela:RJ12 (layer Top) (tedit 5922CB3D)
    (at 54 104 90)
    (fp_text reference RJ12 (at 0 0.5 90) (layer F.SilkS))
    (fp_text value GPS (at 0 -0.5 90) (layer B.SilkS))
    (pad 6 thru_hole circle (at -2.55 4.84 90) (size 1.044 1.044) (drill 0.79) (layers *.Cu *.Mask)
      (net 2 +3.3VP))
    (pad 5 thru_hole circle (at -1.53 2.3 90) (size 1.044 1.044) (drill 0.79) (layers *.Cu *.Mask)
      (net 28 /BAT))
    (pad 4 thru_hole circle (at -0.51 4.84 90) (size 1.044 1.044) (drill 0.79) (layers *.Cu *.Mask)
      (net 66 /PPS))
    (pad 3 thru_hole circle (at 0.51 2.3 90) (size 1.044 1.044) (drill 0.79) (layers *.Cu *.Mask)
      (net 67 /Tx))
    (pad 2 thru_hole circle (at 1.53 4.84 90) (size 1.044 1.044) (drill 0.79) (layers *.Cu *.Mask)
      (net 68 /Rx))
    (pad 1 thru_hole circle (at 2.55 2.3 90) (size 1.044 1.044) (drill 0.79) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad "" thru_hole circle (at -6 0 90) (size 2.554 2.554) (drill 2.3) (layers *.Cu))
    (pad "" thru_hole circle (at 6 0 90) (size 2.554 2.554) (drill 2.3) (layers *.Cu))
  )
  (module geocentinela:TestPoint_TH (layer Top) (tedit 59221A3D)
    (at 75.1 88.1 90)
    (fp_text reference TP1 (at 0 1.1 180) (layer F.SilkS))
    (fp_text value 5V (at 0 0.9 180) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 3 +5V) (zone_connect 2))
  )
  (module geocentinela:TestPoint_TH (layer Top) (tedit 59221A9E)
    (at 122.2 87 90)
    (fp_text reference TP2 (at 0 -1.1 180) (layer F.SilkS))
    (fp_text value 3.3V (at 0 -1.2 180) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 1 +3.3V) (zone_connect 2))
  )
  (module geocentinela:TestPoint_TH (layer Top) (tedit 59221B43)
    (at 69.8 71 90)
    (fp_text reference TP3 (at 0 -1.1 180) (layer F.SilkS))
    (fp_text value 5Va (at 0 -1.1 180) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 4 +5VA) (zone_connect 2))
  )
  (module geocentinela:TestPoint_TH (layer Top) (tedit 59221A76)
    (at 64.8 100.7 90)
    (fp_text reference TP4 (at 0 -1.1 180) (layer F.SilkS))
    (fp_text value 3.3Vp (at 0 -1.4 180) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 2 +3.3VP) (zone_connect 2))
  )
  (module geocentinela:TestPoint_TH (layer Top) (tedit 59221B48)
    (at 69.8 72.8 90)
    (fp_text reference TP5 (at 0 -1.1 180) (layer F.SilkS))
    (fp_text value Vref (at 0 -1.1 180) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 48 Vref) (zone_connect 2))
  )
  (module geocentinela:TestPoint_TH (layer Top) (tedit 59221B4B)
    (at 69.8 69 90)
    (fp_text reference TP6 (at 0 -1.1 180) (layer F.SilkS))
    (fp_text value Vbias (at 0 -1.4 180) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 47 Vbias) (zone_connect 2))
  )
  (module geocentinela:TestPoint_TH (layer Top) (tedit 592219DD)
    (at 62 71 90)
    (fp_text reference TP7 (at 0 -1.1 180) (layer F.SilkS))
    (fp_text value VGND (at 0 -1.4 180) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 46 GNDREF) (zone_connect 2))
  )
  (module geocentinela:TestPoint_TH (layer Top) (tedit 592219A6)
    (at 69.8 55.8 90)
    (fp_text reference TP8 (at -1.1 0 270) (layer F.SilkS))
    (fp_text value ch0 (at -1.1 0 270) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 41 /ch0) (zone_connect 2))
  )
  (module geocentinela:TestPoint_TH (layer Top) (tedit 592219B1)
    (at 69.8 66.3 90)
    (fp_text reference TP9 (at -1.1 0 270) (layer F.SilkS))
    (fp_text value ch1 (at -1.1 0 270) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 42 /ch1) (zone_connect 2))
  )
  (module geocentinela:TestPoint_TH (layer Top) (tedit 592219BD)
    (at 69.8 76.8 90)
    (fp_text reference TP10 (at -1.3 0 270) (layer F.SilkS))
    (fp_text value ch2 (at -1.1 0 270) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (net 36 /ch2) (zone_connect 2))
  )
  (module geocentinela:BAT-HLD-001 (layer Top) (tedit 59221C2F)
    (at 74.8 108.1 180)
    (fp_text reference BT1 (at -11.4 -3.1 180) (layer F.SilkS))
    (fp_text value CR2032 (at 0 0) (layer B.SilkS))
    (pad 1 smd rect (at 11.43 0 180) (size 2.54 5.08) (layers Top F.Paste F.Mask)
      (net 28 /BAT))
    (pad 1 smd rect (at -11.43 0 180) (size 2.54 5.08) (layers Top F.Paste F.Mask)
      (net 28 /BAT))
    (pad 2 smd circle (at 0 0 180) (size 17.78 17.78) (layers Top F.Paste F.Mask)
      (net 6 GND) (solder_paste_margin_ratio -0.4))
  )
  (module geocentinela:CP-16-4 (layer Top) (tedit 591F72AF)
    (at 66 75.95)
    (fp_text reference U2 (at -1.7 -2.45) (layer F.SilkS))
    (fp_text value AD8231 (at 0 -0.95) (layer B.SilkS))
    (pad 11 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 5 AGND) (zone_connect 2))
    (pad 11 smd rect (at 0 0) (size 1.233288 1.233288) (layers Bottom F.Paste B.Mask)
      (net 5 AGND))
    (pad 11 smd rect (at 0 0) (size 1.95 1.95) (layers Top F.Mask)
      (net 5 AGND) (clearance 0.105))
    (pad 16 smd rect (at -0.975 -1.7653) (size 0.3556 1.0668) (layers Top F.Paste F.Mask)
      (net 40 /A2) (clearance 0.07))
    (pad 15 smd rect (at -0.325 -1.7653) (size 0.3556 1.0668) (layers Top F.Paste F.Mask)
      (net 39 /A1) (clearance 0.07))
    (pad 14 smd rect (at 0.325 -1.7653) (size 0.3556 1.0668) (layers Top F.Paste F.Mask)
      (net 38 /A0) (clearance 0.07))
    (pad 13 smd rect (at 0.975 -1.7653) (size 0.3556 1.0668) (layers Top F.Paste F.Mask)
      (net 37 /~CS) (clearance 0.07))
    (pad 12 smd rect (at 1.7653 -0.975) (size 1.0668 0.3556) (layers Top F.Paste F.Mask)
      (net 4 +5VA) (clearance 0.07))
    (pad 11 smd rect (at 1.7653 -0.325) (size 1.0668 0.3556) (layers Top F.Paste F.Mask)
      (net 5 AGND) (clearance 0.07))
    (pad 10 smd rect (at 1.7653 0.325) (size 1.0668 0.3556) (layers Top F.Paste F.Mask)
      (net 36 /ch2) (clearance 0.07))
    (pad 9 smd rect (at 1.7653 0.975) (size 1.0668 0.3556) (layers Top F.Paste F.Mask)
      (net 16 "Net-(U2-Pad7)") (clearance 0.07))
    (pad 8 smd rect (at 0.975 1.7653) (size 0.3556 1.0668) (layers Top F.Paste F.Mask)
      (net 16 "Net-(U2-Pad7)") (clearance 0.07))
    (pad 7 smd rect (at 0.325 1.7653) (size 0.3556 1.0668) (layers Top F.Paste F.Mask)
      (net 16 "Net-(U2-Pad7)") (clearance 0.07))
    (pad 6 smd rect (at -0.325 1.7653) (size 0.3556 1.0668) (layers Top F.Paste F.Mask)
      (net 47 Vbias) (clearance 0.07))
    (pad 5 smd rect (at -0.975 1.7653) (size 0.3556 1.0668) (layers Top F.Paste F.Mask)
      (net 4 +5VA) (clearance 0.07))
    (pad 4 smd rect (at -1.7653 0.975) (size 1.0668 0.3556) (layers Top F.Paste F.Mask)
      (clearance 0.07))
    (pad 3 smd rect (at -1.7653 0.325) (size 1.0668 0.3556) (layers Top F.Paste F.Mask)
      (net 53 "Net-(C4-Pad2)") (clearance 0.07))
    (pad 2 smd rect (at -1.7653 -0.325) (size 1.0668 0.3556) (layers Top F.Paste F.Mask)
      (net 8 "Net-(C3-Pad2)") (clearance 0.07))
    (pad 1 smd rect (at -1.7653 -0.975) (size 1.0668 0.3556) (layers Top F.Paste F.Mask)
      (clearance 0.07))
    (model GeoCentinela.3dshapes/AD8231.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module geocentinela:CP-16-4 (layer Top) (tedit 591F72AF)
    (at 66 65.45)
    (fp_text reference U4 (at -1.7 -2.45) (layer F.SilkS))
    (fp_text value AD8231 (at 0 -0.95) (layer B.SilkS))
    (pad 11 thru_hole circle (at 0 0) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 5 AGND) (zone_connect 2))
    (pad 11 smd rect (at 0 0) (size 1.233288 1.233288) (layers Bottom F.Paste B.Mask)
      (net 5 AGND))
    (pad 11 smd rect (at 0 0) (size 1.95 1.95) (layers Top F.Mask)
      (net 5 AGND) (clearance 0.105))
    (pad 16 smd rect (at -0.975 -1.7653) (size 0.3556 1.0668) (layers Top F.Paste F.Mask)
      (net 40 /A2) (clearance 0.07))
    (pad 15 smd rect (at -0.325 -1.7653) (size 0.3556 1.0668) (layers Top F.Paste F.Mask)
      (net 39 /A1) (clearance 0.07))
    (pad 14 smd rect (at 0.325 -1.7653) (size 0.3556 1.0668) (layers Top F.Paste F.Mask)
      (net 38 /A0) (clearance 0.07))
    (pad 13 smd rect (at 0.975 -1.7653) (size 0.3556 1.0668) (layers Top F.Paste F.Mask)
      (net 37 /~CS) (clearance 0.07))
    (pad 12 smd rect (at 1.7653 -0.975) (size 1.0668 0.3556) (layers Top F.Paste F.Mask)
      (net 4 +5VA) (clearance 0.07))
    (pad 11 smd rect (at 1.7653 -0.325) (size 1.0668 0.3556) (layers Top F.Paste F.Mask)
      (net 5 AGND) (clearance 0.07))
    (pad 10 smd rect (at 1.7653 0.325) (size 1.0668 0.3556) (layers Top F.Paste F.Mask)
      (net 42 /ch1) (clearance 0.07))
    (pad 9 smd rect (at 1.7653 0.975) (size 1.0668 0.3556) (layers Top F.Paste F.Mask)
      (net 18 "Net-(U4-Pad7)") (clearance 0.07))
    (pad 8 smd rect (at 0.975 1.7653) (size 0.3556 1.0668) (layers Top F.Paste F.Mask)
      (net 18 "Net-(U4-Pad7)") (clearance 0.07))
    (pad 7 smd rect (at 0.325 1.7653) (size 0.3556 1.0668) (layers Top F.Paste F.Mask)
      (net 18 "Net-(U4-Pad7)") (clearance 0.07))
    (pad 6 smd rect (at -0.325 1.7653) (size 0.3556 1.0668) (layers Top F.Paste F.Mask)
      (net 47 Vbias) (clearance 0.07))
    (pad 5 smd rect (at -0.975 1.7653) (size 0.3556 1.0668) (layers Top F.Paste F.Mask)
      (net 4 +5VA) (clearance 0.07))
    (pad 4 smd rect (at -1.7653 0.975) (size 1.0668 0.3556) (layers Top F.Paste F.Mask)
      (clearance 0.07))
    (pad 3 smd rect (at -1.7653 0.325) (size 1.0668 0.3556) (layers Top F.Paste F.Mask)
      (net 11 "Net-(C11-Pad2)") (clearance 0.07))
    (pad 2 smd rect (at -1.7653 -0.325) (size 1.0668 0.3556) (layers Top F.Paste F.Mask)
      (net 12 "Net-(C11-Pad1)") (clearance 0.07))
    (pad 1 smd rect (at -1.7653 -0.975) (size 1.0668 0.3556) (layers Top F.Paste F.Mask)
      (clearance 0.07))
    (model GeoCentinela.3dshapes/AD8231.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module geocentinela:SO8 (layer Top) (tedit 591EDF8A)
    (at 70 90.4 180)
    (fp_text reference U9 (at 3.1 1.5 180) (layer F.SilkS))
    (fp_text value LT1763-5 (at 0 0 180) (layer B.SilkS))
    (pad 8 smd rect (at -1.905 -2.57175 180) (size 0.762 1.143) (layers Top F.Paste F.Mask)
      (net 7 VCC))
    (pad 7 smd rect (at -0.635 -2.57175 180) (size 0.762 1.143) (layers Top F.Paste F.Mask)
      (net 6 GND))
    (pad 6 smd rect (at 0.635 -2.57175 180) (size 0.762 1.143) (layers Top F.Paste F.Mask)
      (net 6 GND))
    (pad 5 smd rect (at 1.905 -2.57175 180) (size 0.762 1.143) (layers Top F.Paste F.Mask)
      (net 7 VCC))
    (pad 4 smd rect (at 1.905 2.57175 180) (size 0.762 1.143) (layers Top F.Paste F.Mask)
      (net 54 "Net-(C48-Pad1)"))
    (pad 3 smd rect (at 0.635 2.57175 180) (size 0.762 1.143) (layers Top F.Paste F.Mask)
      (net 6 GND))
    (pad 2 smd rect (at -0.635 2.57175 180) (size 0.762 1.143) (layers Top F.Paste F.Mask)
      (net 3 +5V))
    (pad 1 smd rect (at -1.905 2.57175 180) (size 0.762 1.143) (layers Top F.Paste F.Mask)
      (net 3 +5V))
  )
  (module geocentinela:SO8 (layer Top) (tedit 591EDF8A)
    (at 118.6 95.7 180)
    (fp_text reference U12 (at 3.3 1.5 180) (layer F.SilkS))
    (fp_text value LT1763-3.3 (at 0 0 180) (layer B.SilkS))
    (pad 8 smd rect (at -1.905 -2.57175 180) (size 0.762 1.143) (layers Top F.Paste F.Mask)
      (net 7 VCC))
    (pad 7 smd rect (at -0.635 -2.57175 180) (size 0.762 1.143) (layers Top F.Paste F.Mask)
      (net 6 GND))
    (pad 6 smd rect (at 0.635 -2.57175 180) (size 0.762 1.143) (layers Top F.Paste F.Mask)
      (net 6 GND))
    (pad 5 smd rect (at 1.905 -2.57175 180) (size 0.762 1.143) (layers Top F.Paste F.Mask)
      (net 44 /SDX))
    (pad 4 smd rect (at 1.905 2.57175 180) (size 0.762 1.143) (layers Top F.Paste F.Mask)
      (net 56 "Net-(C52-Pad1)"))
    (pad 3 smd rect (at 0.635 2.57175 180) (size 0.762 1.143) (layers Top F.Paste F.Mask)
      (net 6 GND))
    (pad 2 smd rect (at -0.635 2.57175 180) (size 0.762 1.143) (layers Top F.Paste F.Mask)
      (net 1 +3.3V))
    (pad 1 smd rect (at -1.905 2.57175 180) (size 0.762 1.143) (layers Top F.Paste F.Mask)
      (net 1 +3.3V))
  )
  (module geocentinela:Jumper_2 (layer Top) (tedit 59221B6B)
    (at 63.7 90 90)
    (fp_text reference P2 (at 0 -1.778 90) (layer B.SilkS))
    (fp_text value Pow (at 0.1 -1.8 90) (layer F.SilkS))
    (pad 2 thru_hole circle (at 1.27 0 90) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (pad 1 thru_hole rect (at -1.27 0 90) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask F.SilkS)
      (net 7 VCC))
  )
  (module geocentinela:Jumper_3 (layer Top) (tedit 591ECF39)
    (at 92.3 56.9 270)
    (fp_text reference JP1 (at -4.3 0) (layer F.SilkS))
    (fp_text value PWSD (at 0 1.7 270) (layer B.SilkS))
    (pad 3 thru_hole circle (at 2.54 0 270) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3.3V))
    (pad 2 thru_hole circle (at 0 0 270) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask F.SilkS)
      (net 49 "Net-(C40-Pad2)"))
    (pad 1 thru_hole rect (at -2.54 0 270) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask F.SilkS)
      (net 50 "Net-(JP1-Pad1)"))
  )
  (module Resistors_SMD:R_0603 (layer Top) (tedit 5927A220)
    (at 58.3 53.6 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at -1.5 0 180) (layer F.SilkS))
    (fp_text value 202F (at 0 0 90) (layer B.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers Top F.Paste F.Mask)
      (net 10 "Net-(C10-Pad1)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers Top F.Paste F.Mask)
      (net 19 "/Signal Conditioning/+Ch0"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer Top) (tedit 5927A20D)
    (at 58.3 56.3 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at -1.5 0) (layer F.SilkS))
    (fp_text value 202F (at 0 0 90) (layer B.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers Top F.Paste F.Mask)
      (net 9 "Net-(C10-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers Top F.Paste F.Mask)
      (net 20 "/Signal Conditioning/-Ch0"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer Top) (tedit 58AA844E)
    (at 65.1 68.7 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C15 (at -1.6 0 270) (layer F.SilkS))
    (fp_text value 104M (at 0 0 180) (layer B.SilkS))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers Top F.Paste F.Mask)
      (net 5 AGND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers Top F.Paste F.Mask)
      (net 47 Vbias))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer Top) (tedit 591ECBE8)
    (at 73.6 88.9 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C50 (at -2 0) (layer F.SilkS))
    (fp_text value 106M (at 0 0 270) (layer B.SilkS))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers Top F.Paste F.Mask)
      (net 6 GND))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers Top F.Paste F.Mask)
      (net 3 +5V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer Top) (tedit 591ECCD1)
    (at 122.2 94.2 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C54 (at 0 -1.3 90) (layer F.SilkS))
    (fp_text value 106M (at 0 0 270) (layer B.SilkS))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers Top F.Paste F.Mask)
      (net 6 GND))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers Top F.Paste F.Mask)
      (net 1 +3.3V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer Top) (tedit 5927A232)
    (at 59.9 86.5 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R26 (at -1.5 0) (layer F.SilkS))
    (fp_text value 104F (at 0 0 270) (layer B.SilkS))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers Top F.Paste F.Mask)
      (net 6 GND))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers Top F.Paste F.Mask)
      (net 35 /vbat))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer Top) (tedit 5927A2D1)
    (at 59.1 90 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C25 (at 0 1.3 270) (layer F.SilkS))
    (fp_text value 106M (at 0 0 270) (layer B.SilkS))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers Top F.Paste F.Mask)
      (net 7 VCC))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers Top F.Paste F.Mask)
      (net 6 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer Top) (tedit 58AA844E)
    (at 65.1 79.2 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C13 (at -1.6 0 270) (layer F.SilkS))
    (fp_text value 104M (at 0 0 180) (layer B.SilkS))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers Top F.Paste F.Mask)
      (net 5 AGND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers Top F.Paste F.Mask)
      (net 47 Vbias))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer Top) (tedit 58AA844E)
    (at 65.1 58.2 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C14 (at -1.6 0 270) (layer F.SilkS))
    (fp_text value 104M (at 0 0 180) (layer B.SilkS))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers Top F.Paste F.Mask)
      (net 5 AGND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers Top F.Paste F.Mask)
      (net 47 Vbias))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer Top) (tedit 5927A211)
    (at 59.9 56.3 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R10 (at -1.5 0 -180) (layer F.SilkS))
    (fp_text value 106J (at 0 0 90) (layer B.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers Top F.Paste F.Mask)
      (net 9 "Net-(C10-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers Top F.Paste F.Mask)
      (net 46 GNDREF))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer Top) (tedit 58AA844E)
    (at 62.8 54.95 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C10 (at -1.6 0) (layer F.SilkS))
    (fp_text value 333J (at 0 0 270) (layer B.SilkS))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers Top F.Paste F.Mask)
      (net 9 "Net-(C10-Pad2)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers Top F.Paste F.Mask)
      (net 10 "Net-(C10-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer Top) (tedit 58AA844E)
    (at 61.4 74.6 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at -1.6 0) (layer F.SilkS))
    (fp_text value 332J (at 0 0 270) (layer B.SilkS))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers Top F.Paste F.Mask)
      (net 8 "Net-(C3-Pad2)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers Top F.Paste F.Mask)
      (net 46 GNDREF))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer Top) (tedit 5927A01C)
    (at 61.4 77.3 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at -1.6 0) (layer F.SilkS))
    (fp_text value 332J (at 0 0 90) (layer B.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers Top F.Paste F.Mask)
      (net 53 "Net-(C4-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers Top F.Paste F.Mask)
      (net 46 GNDREF))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer Top) (tedit 58AA844E)
    (at 61.4 53.6 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at -1.6 0) (layer F.SilkS))
    (fp_text value 332J (at 0 0 270) (layer B.SilkS))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers Top F.Paste F.Mask)
      (net 10 "Net-(C10-Pad1)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers Top F.Paste F.Mask)
      (net 46 GNDREF))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer Top) (tedit 58AA844E)
    (at 61.4 56.3 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C6 (at -1.6 0 -180) (layer F.SilkS))
    (fp_text value 332J (at 0 0 90) (layer B.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers Top F.Paste F.Mask)
      (net 9 "Net-(C10-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers Top F.Paste F.Mask)
      (net 46 GNDREF))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer Top) (tedit 58AA844E)
    (at 61.4 64.1 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C7 (at -1.6 0) (layer F.SilkS))
    (fp_text value 332J (at 0 0 270) (layer B.SilkS))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers Top F.Paste F.Mask)
      (net 12 "Net-(C11-Pad1)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers Top F.Paste F.Mask)
      (net 46 GNDREF))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer Top) (tedit 5927A034)
    (at 61.4 66.8 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C8 (at -1.6 0) (layer F.SilkS))
    (fp_text value 332J (at 0 0 90) (layer B.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers Top F.Paste F.Mask)
      (net 11 "Net-(C11-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers Top F.Paste F.Mask)
      (net 46 GNDREF))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer Top) (tedit 5927A02C)
    (at 62.8 75.95 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C9 (at -1.6 0 180) (layer F.SilkS))
    (fp_text value 333J (at 0 0 270) (layer B.SilkS))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers Top F.Paste F.Mask)
      (net 53 "Net-(C4-Pad2)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers Top F.Paste F.Mask)
      (net 8 "Net-(C3-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer Top) (tedit 5927A03A)
    (at 62.8 65.45 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C11 (at -1.6 0 180) (layer F.SilkS))
    (fp_text value 333J (at 0 0 270) (layer B.SilkS))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers Top F.Paste F.Mask)
      (net 11 "Net-(C11-Pad2)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers Top F.Paste F.Mask)
      (net 12 "Net-(C11-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer Top) (tedit 5927A2A5)
    (at 66.6 92.3 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C42 (at -1.6 0 180) (layer F.SilkS))
    (fp_text value 105M (at 0 0 270) (layer B.SilkS))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers Top F.Paste F.Mask)
      (net 7 VCC))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers Top F.Paste F.Mask)
      (net 6 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer Top) (tedit 59239503)
    (at 65.3 80.8)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C43 (at -1.6 0.6 90) (layer F.SilkS))
    (fp_text value 105M (at 0 0 180) (layer B.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers Top F.Paste F.Mask)
      (net 5 AGND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers Top F.Paste F.Mask)
      (net 7 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer Top) (tedit 591ECD13)
    (at 123 91.6)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C44 (at -1.6 0 90) (layer F.SilkS))
    (fp_text value 105M (at 0 0) (layer B.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers Top F.Paste F.Mask)
      (net 6 GND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers Top F.Paste F.Mask)
      (net 1 +3.3V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer Top) (tedit 5924393A)
    (at 124.4 89.5 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C45 (at 0 -1.1 90) (layer F.SilkS))
    (fp_text value 470M (at 0 0 270) (layer B.SilkS))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers Top F.Paste F.Mask)
      (net 6 GND))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers Top F.Paste F.Mask)
      (net 1 +3.3V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer Top) (tedit 58AA844E)
    (at 115.2 97.6 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C46 (at -1.6 0) (layer F.SilkS))
    (fp_text value 105M (at 0 0 270) (layer B.SilkS))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers Top F.Paste F.Mask)
      (net 7 VCC))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers Top F.Paste F.Mask)
      (net 6 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer Top) (tedit 58AA844E)
    (at 68 96.7 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C47 (at -1.6 0 180) (layer F.SilkS))
    (fp_text value 105M (at 0 0 90) (layer B.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers Top F.Paste F.Mask)
      (net 6 GND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers Top F.Paste F.Mask)
      (net 7 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer Top) (tedit 591ECA84)
    (at 70 86.3)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C48 (at -1.6 0 90) (layer F.SilkS))
    (fp_text value 103K (at 0 0) (layer B.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers Top F.Paste F.Mask)
      (net 3 +5V))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers Top F.Paste F.Mask)
      (net 54 "Net-(C48-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer Top) (tedit 591ECF9B)
    (at 118.6 91.6)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C52 (at -1.6 0 90) (layer F.SilkS))
    (fp_text value 103K (at 0 0) (layer B.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers Top F.Paste F.Mask)
      (net 1 +3.3V))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers Top F.Paste F.Mask)
      (net 56 "Net-(C52-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer Top) (tedit 5927A1E2)
    (at 58.3 74.6 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at -1.5 0 180) (layer F.SilkS))
    (fp_text value 202F (at 0 0 270) (layer B.SilkS))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers Top F.Paste F.Mask)
      (net 8 "Net-(C3-Pad2)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers Top F.Paste F.Mask)
      (net 23 "/Signal Conditioning/+Ch2"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer Top) (tedit 58AAD9CA)
    (at 58.3 77.3 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at -1.5 0 -180) (layer F.SilkS))
    (fp_text value 202F (at 0 0 90) (layer B.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers Top F.Paste F.Mask)
      (net 53 "Net-(C4-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers Top F.Paste F.Mask)
      (net 24 "/Signal Conditioning/-Ch2"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer Top) (tedit 5927A1FF)
    (at 58.3 64.1 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at -1.5 0) (layer F.SilkS))
    (fp_text value 202F (at 0 0 270) (layer B.SilkS))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers Top F.Paste F.Mask)
      (net 12 "Net-(C11-Pad1)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers Top F.Paste F.Mask)
      (net 21 "/Signal Conditioning/+Ch1"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer Top) (tedit 5927A1EB)
    (at 58.3 66.8 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at -1.5 0 -180) (layer F.SilkS))
    (fp_text value 202F (at 0 0 90) (layer B.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers Top F.Paste F.Mask)
      (net 11 "Net-(C11-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers Top F.Paste F.Mask)
      (net 22 "/Signal Conditioning/-Ch1"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer Top) (tedit 5927A1E5)
    (at 59.9 74.6 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at -1.5 0 180) (layer F.SilkS))
    (fp_text value 106J (at 0 0 270) (layer B.SilkS))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers Top F.Paste F.Mask)
      (net 8 "Net-(C3-Pad2)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers Top F.Paste F.Mask)
      (net 46 GNDREF))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer Top) (tedit 58AAD9CA)
    (at 59.9 77.3 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at -1.5 0 -180) (layer F.SilkS))
    (fp_text value 106J (at 0 0 90) (layer B.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers Top F.Paste F.Mask)
      (net 53 "Net-(C4-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers Top F.Paste F.Mask)
      (net 46 GNDREF))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer Top) (tedit 5927A224)
    (at 59.9 53.6 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R9 (at -1.5 0 180) (layer F.SilkS))
    (fp_text value 106J (at 0 0 270) (layer B.SilkS))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers Top F.Paste F.Mask)
      (net 10 "Net-(C10-Pad1)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers Top F.Paste F.Mask)
      (net 46 GNDREF))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer Top) (tedit 5927A1F9)
    (at 59.9 64.1 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R11 (at -1.5 0) (layer F.SilkS))
    (fp_text value 106J (at 0 0 270) (layer B.SilkS))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers Top F.Paste F.Mask)
      (net 12 "Net-(C11-Pad1)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers Top F.Paste F.Mask)
      (net 46 GNDREF))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer Top) (tedit 5927A1F3)
    (at 59.9 66.8 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R12 (at -1.5 0) (layer F.SilkS))
    (fp_text value 106J (at 0 0 90) (layer B.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers Top F.Paste F.Mask)
      (net 11 "Net-(C11-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers Top F.Paste F.Mask)
      (net 46 GNDREF))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer Top) (tedit 5927A22F)
    (at 58.3 86.5 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R25 (at -1.5 0) (layer F.SilkS))
    (fp_text value 205F (at 0 0 270) (layer B.SilkS))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers Top F.Paste F.Mask)
      (net 35 /vbat))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers Top F.Paste F.Mask)
      (net 26 +12VA))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer Top) (tedit 592109BB)
    (at 62.2 96.2 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C53 (at -1.6 0 180) (layer F.SilkS))
    (fp_text value 103K (at 0 0 90) (layer B.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers Top F.Paste F.Mask)
      (net 57 "Net-(C53-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers Top F.Paste F.Mask)
      (net 2 +3.3VP))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer Top) (tedit 58AA844E)
    (at 61.4 86.5 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C26 (at -1.6 0) (layer F.SilkS))
    (fp_text value 105M (at 0 0 270) (layer B.SilkS))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers Top F.Paste F.Mask)
      (net 6 GND))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers Top F.Paste F.Mask)
      (net 35 /vbat))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer Top) (tedit 591ECFD1)
    (at 91.9 63.8 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C41 (at -2 0) (layer F.SilkS))
    (fp_text value 106M (at 0 0 270) (layer B.SilkS))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers Top F.Paste F.Mask)
      (net 49 "Net-(C40-Pad2)"))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers Top F.Paste F.Mask)
      (net 6 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer Top) (tedit 5927A1B8)
    (at 68.6 80.5)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C51 (at 0 -1.3 180) (layer F.SilkS))
    (fp_text value 106M (at 0 0) (layer B.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers Top F.Paste F.Mask)
      (net 5 AGND))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers Top F.Paste F.Mask)
      (net 4 +5VA))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer Top) (tedit 591ECC3C)
    (at 65.2 98.9)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C55 (at -2 0 -270) (layer F.SilkS))
    (fp_text value 106M (at 0 0) (layer B.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers Top F.Paste F.Mask)
      (net 6 GND))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers Top F.Paste F.Mask)
      (net 2 +3.3VP))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer Top) (tedit 59239514)
    (at 63.1 79.4 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 1.6 0 -180) (layer F.SilkS))
    (fp_text value 104M (at 0 0 90) (layer B.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers Top F.Paste F.Mask)
      (net 5 AGND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers Top F.Paste F.Mask)
      (net 4 +5VA))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer Top) (tedit 58AA844E)
    (at 69.2 75.1 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C17 (at -1.6 0) (layer F.SilkS))
    (fp_text value 104M (at 0 0 270) (layer B.SilkS))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers Top F.Paste F.Mask)
      (net 5 AGND))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers Top F.Paste F.Mask)
      (net 4 +5VA))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer Top) (tedit 58AA844E)
    (at 69.2 54.1 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C18 (at -1.6 0) (layer F.SilkS))
    (fp_text value 104M (at 0 0 270) (layer B.SilkS))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers Top F.Paste F.Mask)
      (net 5 AGND))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers Top F.Paste F.Mask)
      (net 4 +5VA))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer Top) (tedit 58AA844E)
    (at 69.2 64.6 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C19 (at -1.6 0) (layer F.SilkS))
    (fp_text value 104M (at 0 0 270) (layer B.SilkS))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers Top F.Paste F.Mask)
      (net 5 AGND))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers Top F.Paste F.Mask)
      (net 4 +5VA))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer Top) (tedit 5927A275)
    (at 80.9 74 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C20 (at -1.6 0 180) (layer F.SilkS))
    (fp_text value 104M (at 0 0 270) (layer B.SilkS))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers Top F.Paste F.Mask)
      (net 5 AGND))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers Top F.Paste F.Mask)
      (net 4 +5VA))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer Top) (tedit 58AA844E)
    (at 93.6 63.8 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C40 (at -1.6 0) (layer F.SilkS))
    (fp_text value 104M (at 0 0 270) (layer B.SilkS))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers Top F.Paste F.Mask)
      (net 49 "Net-(C40-Pad2)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers Top F.Paste F.Mask)
      (net 6 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer Top) (tedit 5927A250)
    (at 122.2 98.5 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R18 (at 1.5 0 180) (layer F.SilkS))
    (fp_text value 103J (at 0 0 90) (layer B.SilkS))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers Top F.Paste F.Mask)
      (net 34 "Net-(R18-Pad2)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers Top F.Paste F.Mask)
      (net 1 +3.3V))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module geocentinela:TSOT-23_S5 (layer Top) (tedit 591ED530)
    (at 65.1 96.2 90)
    (fp_text reference U13 (at 0 0 270) (layer F.SilkS))
    (fp_text value LT1761-3.3 (at 1.8 0 180) (layer B.SilkS))
    (pad 3 smd rect (at 0.95 1.31 90) (size 0.6 1.22) (layers Top F.Paste F.Mask)
      (net 43 /EXT) (clearance 0.15))
    (pad 2 smd rect (at 0 1.31 90) (size 0.6 1.22) (layers Top F.Paste F.Mask)
      (net 6 GND) (clearance 0.15))
    (pad 1 smd rect (at -0.95 1.31 90) (size 0.6 1.22) (layers Top F.Paste F.Mask)
      (net 7 VCC) (clearance 0.15))
    (pad 4 smd rect (at 0.95 -1.31 90) (size 0.6 1.22) (layers Top F.Paste F.Mask)
      (net 57 "Net-(C53-Pad2)") (clearance 0.15))
    (pad 5 smd rect (at -0.95 -1.31 90) (size 0.6 1.22) (layers Top F.Paste F.Mask)
      (net 2 +3.3VP) (clearance 0.15))
  )
  (module geocentinela:TSOT-23_S5 (layer Top) (tedit 59238954)
    (at 66.2 83.1 270)
    (fp_text reference U11 (at 1.9 0 180) (layer F.SilkS))
    (fp_text value LT1761-5 (at 0 0 270) (layer B.SilkS))
    (pad 3 smd rect (at 0.95 1.31 270) (size 0.6 1.22) (layers Top F.Paste F.Mask)
      (net 45 /PGA) (clearance 0.15))
    (pad 2 smd rect (at 0 1.31 270) (size 0.6 1.22) (layers Top F.Paste F.Mask)
      (net 5 AGND) (clearance 0.15))
    (pad 1 smd rect (at -0.95 1.31 270) (size 0.6 1.22) (layers Top F.Paste F.Mask)
      (net 7 VCC) (clearance 0.15))
    (pad 4 smd rect (at 0.95 -1.31 270) (size 0.6 1.22) (layers Top F.Paste F.Mask)
      (net 55 "Net-(C49-Pad2)") (clearance 0.15))
    (pad 5 smd rect (at -0.95 -1.31 270) (size 0.6 1.22) (layers Top F.Paste F.Mask)
      (net 4 +5VA) (clearance 0.15))
  )
  (module Capacitors_SMD:C_0603 (layer Top) (tedit 5927A27C)
    (at 77.4 70.9 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C22 (at -1.6 0 270) (layer F.SilkS))
    (fp_text value 104M (at 0 0 180) (layer B.SilkS))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers Top F.Paste F.Mask)
      (net 47 Vbias))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers Top F.Paste F.Mask)
      (net 5 AGND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer Top) (tedit 5927A787)
    (at 60.6 83.3)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C12 (at 1.6 0 90) (layer F.SilkS))
    (fp_text value 105M (at 0 0) (layer B.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers Top F.Paste F.Mask)
      (net 5 AGND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers Top F.Paste F.Mask)
      (net 46 GNDREF))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer Top) (tedit 5927A26D)
    (at 82.3 74 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C16 (at 1.6 0 180) (layer F.SilkS))
    (fp_text value 105M (at 0 0 270) (layer B.SilkS))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers Top F.Paste F.Mask)
      (net 5 AGND))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers Top F.Paste F.Mask)
      (net 4 +5VA))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_0603 (layer Top) (tedit 59244E25)
    (at 87 85.8 180)
    (descr "Diode SMD in 0603 package")
    (tags "smd diode")
    (attr smd)
    (fp_text reference D2 (at 0 -1) (layer F.SilkS))
    (fp_text value 1N4148 (at 0 0 180) (layer B.SilkS))
    (pad 2 smd rect (at 0.85 0 180) (size 0.6 0.8) (layers Top F.Paste F.Mask)
      (net 3 +5V))
    (pad 1 smd rect (at -0.85 0 180) (size 0.6 0.8) (layers Top F.Paste F.Mask)
      (net 51 "Net-(D2-Pad1)"))
  )
  (module Resistors_SMD:R_Array_Concave_4x0603 (layer Top) (tedit 59221D10)
    (at 108.9 92.9)
    (descr "Thick Film Chip Resistor Array, Wave soldering, Vishay CRA06P (see cra06p.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN1 (at -1.9 0 90) (layer F.SilkS))
    (fp_text value 331J (at 0 0 90) (layer B.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 5 smd rect (at 0.85 1.2) (size 0.9 0.4) (layers Top F.Paste F.Mask)
      (net 29 /XBEE_TX))
    (pad 6 smd rect (at 0.85 0.4) (size 0.9 0.4) (layers Top F.Paste F.Mask)
      (net 30 /XBEE_RX))
    (pad 7 smd rect (at 0.85 -0.4) (size 0.9 0.4) (layers Top F.Paste F.Mask)
      (net 60 /XBEE_~RESET))
    (pad 8 smd rect (at 0.85 -1.2) (size 0.9 0.4) (layers Top F.Paste F.Mask)
      (net 69 "Net-(RN1-Pad8)"))
    (pad 4 smd rect (at -0.85 1.2) (size 0.9 0.4) (layers Top F.Paste F.Mask)
      (net 63 /MCU_RX1))
    (pad 1 smd rect (at -0.85 -1.2) (size 0.9 0.4) (layers Top F.Paste F.Mask)
      (net 70 "Net-(RN1-Pad1)"))
    (pad 3 smd rect (at -0.85 0.4) (size 0.9 0.4) (layers Top F.Paste F.Mask)
      (net 64 /MCU_TX1))
    (pad 2 smd rect (at -0.85 -0.4) (size 0.9 0.4) (layers Top F.Paste F.Mask)
      (net 52 /Wp))
    (model Resistors_SMD.3dshapes/R_Array_Concave_4x0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module geocentinela:timining (layer Top) (tedit 5921697F)
    (at 58.1 115.6)
    (fp_text reference GeoCentinelaV4.0 (at 55.1 3.4) (layer F.SilkS))
    (fp_text value www.timining.cl (at 55.1 -1.5) (layer F.SilkS))
  )
  (module geocentinela:SOT-23-5 (layer Top) (tedit 59222282)
    (at 78 74.5 180)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U5 (at 0 2 180) (layer F.SilkS))
    (fp_text value REF2030 (at 0 0 270) (layer B.SilkS))
    (pad 5 smd rect (at 1.35 -0.95 180) (size 1.24 0.74) (layers Top F.Paste F.Mask)
      (net 48 Vref))
    (pad 4 smd rect (at 1.35 0.95 180) (size 1.24 0.74) (layers Top F.Paste F.Mask)
      (net 4 +5VA))
    (pad 3 smd rect (at -1.35 0.95 180) (size 1.24 0.74) (layers Top F.Paste F.Mask)
      (net 4 +5VA))
    (pad 2 smd rect (at -1.35 0 180) (size 1.24 0.74) (layers Top F.Paste F.Mask)
      (net 5 AGND))
    (pad 1 smd rect (at -1.35 -0.95 180) (size 1.24 0.74) (layers Top F.Paste F.Mask)
      (net 47 Vbias))
    (model GeoCentinela.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_Array_Concave_2x0603 (layer Top) (tedit 59221ADE)
    (at 121.8 114.3 180)
    (descr "Thick Film Chip Resistor Array, Wave soldering, Vishay CRA06P (see cra06p.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN2 (at -0.1 -1.4 180) (layer F.SilkS))
    (fp_text value 471J (at 0 0 270) (layer B.SilkS))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.85 -0.4 180) (size 0.9 0.4) (layers Top F.Paste F.Mask)
      (net 58 "Net-(D1-Pad4)"))
    (pad 2 smd rect (at -0.85 0.4 180) (size 0.9 0.4) (layers Top F.Paste F.Mask)
      (net 13 "Net-(D1-Pad2)"))
    (pad 3 smd rect (at 0.85 0.4 180) (size 0.9 0.4) (layers Top F.Paste F.Mask)
      (net 6 GND))
    (pad 4 smd rect (at 0.85 -0.4 180) (size 0.9 0.4) (layers Top F.Paste F.Mask)
      (net 6 GND))
    (model Resistors_SMD.3dshapes/R_Array_Concave_2x0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module geocentinela:15EDGRC-3.5-3P (layer Top) (tedit 59246072)
    (at 56 90 90)
    (fp_text reference P7 (at 0 -4 90) (layer F.SilkS))
    (fp_text value Vin (at 0 -4 90) (layer B.SilkS))
    (pad 1 thru_hole rect (at 3.5 0 90) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 2 thru_hole circle (at 0 0 90) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 26 +12VA))
    (pad 3 thru_hole circle (at -3.5 0 90) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 7 VCC))
  )
  (module Capacitors_SMD:C_0603 (layer Top) (tedit 5927A574)
    (at 61.1 80.1 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 1.6 0 270) (layer F.SilkS))
    (fp_text value 105M (at 0 0 180) (layer B.SilkS))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers Top F.Paste F.Mask)
      (net 4 +5VA))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers Top F.Paste F.Mask)
      (net 46 GNDREF))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module geocentinela:LP3 (layer Top) (tedit 5927A79A)
    (at 62.5 81.7 180)
    (descr LP3)
    (fp_text reference U1 (at -0.2 -2.1 180) (layer B.SilkS))
    (fp_text value TLE2426 (at 3.7 0 270) (layer F.SilkS))
    (pad 3 thru_hole oval (at 2.54 0 180) (size 1 1.5) (drill 0.746) (layers *.Cu *.Mask)
      (net 46 GNDREF))
    (pad 2 thru_hole oval (at 1.27 0 180) (size 1 1.5) (drill 0.746) (layers *.Cu *.Mask)
      (net 5 AGND))
    (pad 1 thru_hole rect (at 0 0 180) (size 1 1.5) (drill 0.746) (layers *.Cu *.Mask)
      (net 4 +5VA))
  )
  (module geocentinela:SK-12D07 (layer Top) (tedit 59283379)
    (at 126.8 83.5 90)
    (fp_text reference SW2 (at 0 -1.27 90) (layer F.SilkS))
    (fp_text value "Eject SD" (at 0 -1.27 90) (layer B.SilkS))
    (fp_text user H=4.7mm (at 0 1.7 90) (layer F.Fab))
    (fp_text user hc=2.6mm (at 0 5.7 90) (layer F.Fab))
    (fp_text user w=2mm (at 0 4.9 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -2 0 90) (size 1.25 1.25) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 51 "Net-(D2-Pad1)"))
    (pad 2 thru_hole circle (at 0 0 90) (size 1.25 1.25) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 69 "Net-(RN1-Pad8)"))
    (pad 3 thru_hole circle (at 2 0 90) (size 1.25 1.25) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
    (pad "" thru_hole circle (at -4.1 0 90) (size 1.704 1.704) (drill 1.45) (layers *.Cu *.Mask F.SilkS))
    (pad "" thru_hole circle (at 4.1 0 90) (size 1.704 1.704) (drill 1.45) (layers *.Cu *.Mask F.SilkS))
  )
  (gr_text FAST (at 53.7 47) (layer F.SilkS))
  (gr_line (start 130 40) (end 130 123.5) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 50 40) (end 50 123.5) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 50 123.5) (end 130 123.5) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 50 40) (end 130 40) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (zone (net 14) (net_name GNDPWR) (layer Bottom) (hatch edge 0.508)
    (connect_pads (clearance 0.381))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 130 46) (xy 58.3 46) (xy 58.3 85.1) (xy 54.1 85.1) (xy 54.1 117.5)
        (xy 130 117.5) (xy 130 123.5) (xy 50 123.5) (xy 50 40) (xy 130 40)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 130 40) (xy 130 43) (xy 50 43) (xy 50 40)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 50 43) (xy 50 40) (xy 130 40) (xy 130 43)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 50 123.5) (xy 50 120.5) (xy 130 120.5) (xy 130 123.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 130 123.5) (xy 130 120.5) (xy 50 120.5) (xy 50 123.5)
      )
    )
  )
  (zone (net 14) (net_name GNDPWR) (layer Top) (hatch edge 0.508)
    (connect_pads (clearance 0.381))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 54.1 85.1) (xy 54.1 117.5) (xy 130 117.5) (xy 130 123.5) (xy 50 123.5)
        (xy 50 40) (xy 130 40) (xy 130 46) (xy 58.3 46) (xy 58.3 85.1)
      )
    )
  )
  (zone (net 6) (net_name GND) (layer Bottom) (hatch edge 0.508)
    (connect_pads (clearance 0.381))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 130 117.1) (xy 54.5 117.1) (xy 54.5 94.9) (xy 62.4 94.9) (xy 62.4 85.6)
        (xy 82.2 85.6) (xy 85.7 82.1) (xy 85.7 46.4) (xy 130 46.4)
      )
    )
  )
  (zone (net 46) (net_name GNDREF) (layer Bottom) (hatch edge 0.508)
    (connect_pads (clearance 0.381))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 63.2 52.2) (xy 58.9 52.2) (xy 58.9 83.2) (xy 60.4 83.2) (xy 60.4 78.7)
        (xy 63.2 78.7)
      )
    )
  )
  (zone (net 5) (net_name AGND) (layer Bottom) (hatch edge 0.508)
    (connect_pads (clearance 0.381))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 74.9 69.9) (xy 80.6 69.9) (xy 83.4 72.7) (xy 83.4 75.3) (xy 74 84.7)
        (xy 64.1 84.7) (xy 64.1 82.6) (xy 60.8 82.6) (xy 60.8 79.1) (xy 63.6 79.1)
        (xy 63.6 52.4) (xy 74.9 52.4)
      )
    )
  )
)
