(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 71)
    (no_connects 0)
    (area 103.556999 81.712999 140.283001 140.283001)
    (thickness 1.6)
    (drawings 25)
    (tracks 347)
    (zones 0)
    (modules 25)
    (nets 51)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.5)
    (user_trace_width 0.75)
    (user_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.7 1.7)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFEFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 RAW)
  (net 2 GND)
  (net 3 "Net-(C3-Pad1)")
  (net 4 "Net-(C4-Pad1)")
  (net 5 VCC)
  (net 6 MC_RX)
  (net 7 MC_TX)
  (net 8 SCL)
  (net 9 SDA)
  (net 10 A0)
  (net 11 A1)
  (net 12 A2)
  (net 13 A3)
  (net 14 INT)
  (net 15 "Net-(R1-Pad2)")
  (net 16 CAN_TXD)
  (net 17 CAN_RXD)
  (net 18 SCK)
  (net 19 MOSI)
  (net 20 CS)
  (net 21 RES)
  (net 22 "Net-(U3-Pad5)")
  (net 23 CANL)
  (net 24 CANH)
  (net 25 "Net-(uC1-Pad2)")
  (net 26 "Net-(uC1-Pad3)")
  (net 27 "Net-(R2-Pad2)")
  (net 28 "Net-(R3-Pad1)")
  (net 29 A7)
  (net 30 A6)
  (net 31 "Net-(U1-Pad3)")
  (net 32 "Net-(U1-Pad4)")
  (net 33 "Net-(U1-Pad5)")
  (net 34 "Net-(U1-Pad6)")
  (net 35 "Net-(U1-Pad10)")
  (net 36 "Net-(U1-Pad11)")
  (net 37 "Net-(J5-Pad1)")
  (net 38 "Net-(J5-Pad2)")
  (net 39 D3)
  (net 40 D4)
  (net 41 D5)
  (net 42 D6)
  (net 43 D7)
  (net 44 D8)
  (net 45 D9)
  (net 46 MISO)
  (net 47 "Net-(J1-Pad1)")
  (net 48 "Net-(J7-Pad1)")
  (net 49 "Net-(J8-Pad1)")
  (net 50 "Net-(J9-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net A0)
    (add_net A1)
    (add_net A2)
    (add_net A3)
    (add_net A6)
    (add_net A7)
    (add_net CANH)
    (add_net CANL)
    (add_net CAN_RXD)
    (add_net CAN_TXD)
    (add_net CS)
    (add_net D3)
    (add_net D4)
    (add_net D5)
    (add_net D6)
    (add_net D7)
    (add_net D8)
    (add_net D9)
    (add_net GND)
    (add_net INT)
    (add_net MC_RX)
    (add_net MC_TX)
    (add_net MISO)
    (add_net MOSI)
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J5-Pad1)")
    (add_net "Net-(J5-Pad2)")
    (add_net "Net-(J7-Pad1)")
    (add_net "Net-(J8-Pad1)")
    (add_net "Net-(J9-Pad1)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad11)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U3-Pad5)")
    (add_net "Net-(uC1-Pad2)")
    (add_net "Net-(uC1-Pad3)")
    (add_net RAW)
    (add_net RES)
    (add_net SCK)
    (add_net SCL)
    (add_net SDA)
    (add_net VCC)
  )
  (module FootPrints:ARDUINO_NANO (layer F.Cu) (tedit 5A662E28)
    (at 125.222 118.364 90)
    (fp_text reference uC1 (at -17.4625 0.1905 180) (layer F.SilkS))
    (fp_text value NANO (at 0 0 90) (layer F.Fab))
    (pad 30 thru_hole oval (at -17.78 -7.62 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 MISO))
    (pad 1 thru_hole oval (at -17.78 7.62 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 SCK))
    (pad 29 thru_hole oval (at -15.24 -7.62 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 MOSI))
    (pad 2 thru_hole oval (at -15.24 7.62 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(uC1-Pad2)"))
    (pad 28 thru_hole oval (at -12.7 -7.62 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 CS))
    (pad 3 thru_hole oval (at -12.7 7.62 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(uC1-Pad3)"))
    (pad 27 thru_hole oval (at -10.16 -7.62 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 D9))
    (pad 4 thru_hole oval (at -10.16 7.62 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 A0))
    (pad 26 thru_hole oval (at -7.62 -7.62 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 D8))
    (pad 5 thru_hole oval (at -7.62 7.62 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 A1))
    (pad 25 thru_hole oval (at -5.08 -7.62 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 D7))
    (pad 6 thru_hole oval (at -5.08 7.62 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 A2))
    (pad 24 thru_hole oval (at -2.54 -7.62 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 D6))
    (pad 7 thru_hole oval (at -2.54 7.62 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 A3))
    (pad 23 thru_hole oval (at 0 -7.62 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 D5))
    (pad 8 thru_hole oval (at 0 7.62 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 SDA))
    (pad 22 thru_hole oval (at 2.54 -7.62 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 D4))
    (pad 9 thru_hole oval (at 2.54 7.62 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 SCL))
    (pad 21 thru_hole oval (at 5.08 -7.62 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 D3))
    (pad 10 thru_hole oval (at 5.08 7.62 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 A6))
    (pad 20 thru_hole oval (at 7.62 -7.62 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 INT))
    (pad 11 thru_hole oval (at 7.62 7.62 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 A7))
    (pad 19 thru_hole oval (at 10.16 -7.62 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 12 thru_hole oval (at 10.16 7.62 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 VCC))
    (pad 18 thru_hole oval (at 12.7 -7.62 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 RES))
    (pad 13 thru_hole oval (at 12.7 7.62 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 RES))
    (pad 17 thru_hole oval (at 15.24 -7.62 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 MC_RX))
    (pad 14 thru_hole oval (at 15.24 7.62 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 16 thru_hole oval (at 17.78 -7.62 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 MC_TX))
    (pad 15 thru_hole oval (at 17.78 7.62 90) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 RAW))
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5A6638DE)
    (at 128.6764 100.9904 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C6 (at 0.1524 1.1684 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 VCC))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58AA848B)
    (at 125.1585 120.142)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C7 (at 0 -1.25) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 -1.25) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 VCC))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58AA848B)
    (at 136.5504 113.2332)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C9 (at 0 -1.25) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 -1.25) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 VCC))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 137.8585 115.824)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33) (layer F.SilkS))
    (fp_text value I2C (at 0 9.95) (layer F.Fab))
    (fp_text user %R (at 0 3.81 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 VCC))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 SCL))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 SDA))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 137.922 132.334 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33 180) (layer F.SilkS))
    (fp_text value CAN (at 0 7.41 180) (layer F.Fab))
    (fp_text user %R (at 0 2.54 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 CANH))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 CANL))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5A6638D6)
    (at 115.062 113.284 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 3.048 0 360) (layer F.SilkS))
    (fp_text value Rs (at 0 1.55 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(R3-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C4-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-18W_7.5x11.6mm_Pitch1.27mm (layer F.Cu) (tedit 5A662E43)
    (at 125.222 107.95)
    (descr "18-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1 (at 0.127 6.7945) (layer F.SilkS))
    (fp_text value MCP2515-SOIC (at 0 6.875) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -4.7 -5.08) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 CAN_TXD))
    (pad 2 smd rect (at -4.7 -3.81) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 CAN_RXD))
    (pad 3 smd rect (at -4.7 -2.54) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(U1-Pad3)"))
    (pad 4 smd rect (at -4.7 -1.27) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(U1-Pad4)"))
    (pad 5 smd rect (at -4.7 0) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(U1-Pad5)"))
    (pad 6 smd rect (at -4.7 1.27) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(U1-Pad6)"))
    (pad 7 smd rect (at -4.7 2.54) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (pad 8 smd rect (at -4.7 3.81) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(R3-Pad1)"))
    (pad 9 smd rect (at -4.7 5.08) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 10 smd rect (at 4.7 5.08) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(U1-Pad10)"))
    (pad 11 smd rect (at 4.7 3.81) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(U1-Pad11)"))
    (pad 12 smd rect (at 4.7 2.54) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 INT))
    (pad 13 smd rect (at 4.7 1.27) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 18 SCK))
    (pad 14 smd rect (at 4.7 0) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 19 MOSI))
    (pad 15 smd rect (at 4.7 -1.27) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 46 MISO))
    (pad 16 smd rect (at 4.7 -2.54) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 20 CS))
    (pad 17 smd rect (at 4.7 -3.81) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(R2-Pad2)"))
    (pad 18 smd rect (at 4.7 -5.08) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 VCC))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-18W_7.5x11.6mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 5A662E24)
    (at 125.095 124.714 270)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U3 (at -2.794 -3.429 270) (layer F.SilkS))
    (fp_text value MCP2551-I/SN (at 0 3.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 CAN_TXD))
    (pad 2 smd rect (at -2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 VCC))
    (pad 4 smd rect (at -2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 CAN_RXD))
    (pad 5 smd rect (at 2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(U3-Pad5)"))
    (pad 6 smd rect (at 2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 23 CANL))
    (pad 7 smd rect (at 2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 24 CANH))
    (pad 8 smd rect (at 2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R1-Pad2)"))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystals:Crystal_SMD_HC49-SD (layer F.Cu) (tedit 5A662BA1)
    (at 111.506 110.744 270)
    (descr "SMD Crystal HC-49-SD http://cdn-reichelt.de/documents/datenblatt/B400/xxx-HC49-SMD.pdf, 11.4x4.7mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference Y3 (at -3.048 3.556 360) (layer F.SilkS))
    (fp_text value 8MHz (at 0 3.55 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -4.25 0 270) (size 4.5 2) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 4.25 0 270) (size 4.5 2) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C4-Pad1)"))
    (model ${KISYS3DMOD}/Crystals.3dshapes/Crystal_SMD_HC49-SD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58AA848B)
    (at 136.525 108.204)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 0 -1.25) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 -1.25) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 VCC))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 128.651 126.4285 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 0 -1.45 270) (layer F.SilkS))
    (fp_text value 4K7 (at 0 1.55 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5A6638E3)
    (at 124.1044 100.9904)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 0.1016 -1.1684) (layer F.SilkS))
    (fp_text value 4K7 (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 VCC))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(R2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 58AA84B8)
    (at 113.03 102.743)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C3 (at 0 -1.75) (layer F.SilkS))
    (fp_text value 22pFF (at 0 2) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 5A6638D3)
    (at 113.03 118.745)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C4 (at -3.556 0.127) (layer F.SilkS))
    (fp_text value 22pF (at 0 2) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 5B563B47)
    (at 105.156 96.52 180)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J4 (at 0.508 9.652 180) (layer F.SilkS))
    (fp_text value UART (at 0 9.95 180) (layer F.Fab))
    (fp_text user %R (at 0 3.81 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 VCC))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 MC_TX))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 MC_RX))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_NV_B02P-NV_2x5.00mm_Vertical (layer F.Cu) (tedit 59DBB535)
    (at 124.206 85.09 180)
    (descr "JST NV series connector, B02P-NV, 5.00mm pitch, top entry type, through hole")
    (tags "connector jst nv vertical")
    (fp_text reference J5 (at 2.5 -4.8 180) (layer F.SilkS))
    (fp_text value PWR (at 2.5 6 180) (layer F.Fab))
    (fp_text user %R (at 2.5 2.5 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.35 3) (drill 1.65) (layers *.Cu *.Mask)
      (net 37 "Net-(J5-Pad1)"))
    (pad 2 thru_hole oval (at 5 0 180) (size 2.35 3) (drill 1.65) (layers *.Cu *.Mask)
      (net 38 "Net-(J5-Pad2)"))
    (model ${KISYS3DMOD}/Connectors_JST.3dshapes/JST_NV_B02P-NV_2x5.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x16_Pitch2.54mm (layer F.Cu) (tedit 5B563947)
    (at 105.156 100.584)
    (descr "Through hole straight pin header, 1x16, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x16 2.54mm single row")
    (fp_text reference J6 (at 2.54 -1.016) (layer F.SilkS))
    (fp_text value Breakout (at 0 40.43) (layer F.Fab))
    (fp_text user %R (at 0 19.05 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 MC_TX))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 MC_RX))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 RES))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 INT))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 D3))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 D4))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 D5))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 D6))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 D7))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 D8))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 D9))
    (pad 13 thru_hole oval (at 0 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 CS))
    (pad 14 thru_hole oval (at 0 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 MOSI))
    (pad 15 thru_hole oval (at 0 35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 MISO))
    (pad 16 thru_hole oval (at 0 38.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 VCC))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x16_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module FootPrints:3A_mini_buck (layer F.Cu) (tedit 59970938)
    (at 122.936 85.598 180)
    (fp_text reference U2 (at 0 2.54 180) (layer F.SilkS))
    (fp_text value 3A_BUCK (at 0 -9.525 180) (layer F.Fab))
    (pad 1 thru_hole rect (at -8.255 -10.795 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole rect (at -8.255 -8.255 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole rect (at -8.255 0 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 VCC))
    (pad 4 thru_hole rect (at -8.255 2.54 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 VCC))
    (pad 5 thru_hole rect (at 10.16 2.54 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 37 "Net-(J5-Pad1)"))
    (pad 6 thru_hole rect (at 10.16 0 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 37 "Net-(J5-Pad1)"))
    (pad 7 thru_hole rect (at 10.16 -8.255 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 38 "Net-(J5-Pad2)"))
    (pad 8 thru_hole rect (at 10.16 -10.795 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 38 "Net-(J5-Pad2)"))
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 128.524 130.302 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R4 (at 0 1.85 90) (layer B.SilkS))
    (fp_text value 120R (at 0 -1.9 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 24 CANH))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 23 CANL))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D16.0mm_P7.50mm (layer B.Cu) (tedit 597BC7C2)
    (at 118.364 89.916)
    (descr "CP, Radial series, Radial, pin pitch=7.50mm, , diameter=16mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 7.50mm  diameter 16mm Electrolytic Capacitor")
    (fp_text reference C1 (at 3.75 9.31) (layer B.SilkS))
    (fp_text value 1000uF (at 3.75 -9.31) (layer B.Fab))
    (fp_text user %R (at 3.75 0) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 5 VCC))
    (pad 2 thru_hole circle (at 7.5 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D16.0mm_P7.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_Pad (layer F.Cu) (tedit 5B563677)
    (at 136.652 143.256)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference J1 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value Conn_01x01 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 47 "Net-(J1-Pad1)"))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_Pad (layer F.Cu) (tedit 5B56367C)
    (at 107.188 143.256)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference J7 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value Conn_01x01 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 48 "Net-(J7-Pad1)"))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_Pad (layer F.Cu) (tedit 5B563670)
    (at 136.652 83.566)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference J8 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value Conn_01x01 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 49 "Net-(J8-Pad1)"))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_Pad (layer F.Cu) (tedit 5B56366C)
    (at 107.188 83.566)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference J9 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value Conn_01x01 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 50 "Net-(J9-Pad1)"))
  )
  (gr_line (start 103.632 80.01) (end 103.632 140.208) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 140.208 140.208) (end 140.208 80.01) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "CAN TERM" (at 126.238 129.794 90) (layer B.SilkS))
  (gr_text GJS (at 122.174 144.78) (layer B.SilkS))
  (gr_text Tigercat (at 122.174 141.224) (layer B.SilkS))
  (gr_text Tigercat (at 121.666 141.224) (layer F.SilkS))
  (gr_text "HOLES 1.16\" x 2.35\" SPACING" (at 121.666 145.796) (layer F.SilkS))
  (gr_line (start 103.632 80.01) (end 140.208 80.01) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 103.632 146.812) (end 103.632 140.208) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 140.208 146.812) (end 103.632 146.812) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 140.208 140.208) (end 140.208 146.812) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "HOLES 1.16\" x 2.35\" SPACING" (at 121.666 80.772) (layer B.SilkS))
  (gr_text "H\n" (at 135.382 132.334) (layer F.SilkS))
  (gr_text L (at 135.382 127.254) (layer F.SilkS))
  (gr_text 5V (at 108.204 96.774) (layer F.SilkS))
  (gr_text "GND\n" (at 108.966 93.98) (layer F.SilkS))
  (gr_text RX (at 108.204 91.44) (layer F.SilkS))
  (gr_text TX (at 107.95 88.9) (layer F.SilkS))
  (gr_text GND (at 114.046 81.28) (layer F.SilkS))
  (gr_text PWR (at 129.54 81.28) (layer F.SilkS))
  (gr_text CANH (at 137.414 135.382) (layer B.SilkS))
  (gr_text GND (at 135.382 115.824 90) (layer B.SilkS))
  (gr_text "SDA\n" (at 135.382 123.698 90) (layer B.SilkS))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 140.208 137.668) (xy 140.208 98.806) (xy 107.188 98.806) (xy 107.188 137.668) (xy 139.954 137.668)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 140.208 137.668) (xy 140.208 98.806) (xy 107.188 98.806) (xy 107.188 137.668) (xy 139.954 137.668)
      )
    )
  )
)
