(kicad_pcb (version 4) (host pcbnew 4.0.2-stable)
  (general
    (links 53)
    (no_connects 6)
    (area 120.694029 101.8026 156.165972 131.7574)
    (thickness 1.6)
    (drawings 81)
    (tracks 164)
    (zones 0)
    (modules 22)
    (nets 22)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.1524)
    (user_trace_width 0.2032)
    (user_trace_width 0.254)
    (trace_clearance 0.1524)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.1524)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (user_via 0.6858 0.3302)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0.6858)
    (uvia_min_drill 0.3302)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.032 2.032)
    (pad_drill 1.016)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VDD)
  (net 2 GND)
  (net 3 "Net-(C3-Pad1)")
  (net 4 "Net-(C5-Pad1)")
  (net 5 "Net-(JP1-Pad1)")
  (net 6 "Net-(JP1-Pad3)")
  (net 7 "Net-(JP2-Pad1)")
  (net 8 "Net-(JP2-Pad3)")
  (net 9 "Net-(JP3-Pad1)")
  (net 10 "Net-(JP3-Pad3)")
  (net 11 SDA)
  (net 12 SCL)
  (net 13 SDO_A/G)
  (net 14 SDO_M)
  (net 15 CS_A/G)
  (net 16 CS_M)
  (net 17 DRDY_M)
  (net 18 INT_M)
  (net 19 INT1_A/G)
  (net 20 INT2_A/G)
  (net 21 DEN_A/G)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net CS_A/G)
    (add_net CS_M)
    (add_net DEN_A/G)
    (add_net DRDY_M)
    (add_net GND)
    (add_net INT1_A/G)
    (add_net INT2_A/G)
    (add_net INT_M)
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(JP1-Pad1)")
    (add_net "Net-(JP1-Pad3)")
    (add_net "Net-(JP2-Pad1)")
    (add_net "Net-(JP2-Pad3)")
    (add_net "Net-(JP3-Pad1)")
    (add_net "Net-(JP3-Pad3)")
    (add_net SCL)
    (add_net SDA)
    (add_net SDO_A/G)
    (add_net SDO_M)
    (add_net VDD)
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 (layer B.Cu) (tedit 57C10736)
    (at 128.27 113.03 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at 0 5.1 180) (layer B.SilkS) hide)
    (fp_text value CONN_01X04 (at 0 3.1 180) (layer B.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 1 VDD))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 11 SDA))
    (pad 4 thru_hole oval (at 0 -7.62 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 12 SCL))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57C12770)
    (at 133.35 119.38 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 0 -1.9 180) (layer F.SilkS) hide)
    (fp_text value 0.1u (at 0 1.9 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57C12768)
    (at 133.35 116.84 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 0 -1.9 180) (layer F.SilkS) hide)
    (fp_text value 0.1u (at 0 1.9 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57C1276C)
    (at 133.35 118.11 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at 0 -1.9 180) (layer F.SilkS) hide)
    (fp_text value 0.1u (at 0 1.9 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57C12763)
    (at 133.35 115.57 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at 0 -1.9 180) (layer F.SilkS) hide)
    (fp_text value 10u (at 0 1.9 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57C1275D)
    (at 133.35 114.3 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at 0 -1.9 180) (layer F.SilkS) hide)
    (fp_text value 10n (at 0 1.9 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x09 (layer B.Cu) (tedit 57C10B64)
    (at 148.59 125.73)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at 0 5.1) (layer B.SilkS) hide)
    (fp_text value CONN_01X09 (at 0 3.1) (layer B.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 13 SDO_A/G))
    (pad 2 thru_hole oval (at 0 -2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 14 SDO_M))
    (pad 3 thru_hole oval (at 0 -5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 15 CS_A/G))
    (pad 4 thru_hole oval (at 0 -7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 16 CS_M))
    (pad 5 thru_hole oval (at 0 -10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 17 DRDY_M))
    (pad 6 thru_hole oval (at 0 -12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 18 INT_M))
    (pad 7 thru_hole oval (at 0 -15.24) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 19 INT1_A/G))
    (pad 8 thru_hole oval (at 0 -17.78) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 20 INT2_A/G))
    (pad 9 thru_hole oval (at 0 -20.32) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 21 DEN_A/G))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x09.wrl
      (at (xyz 0 -0.4 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57C12799)
    (at 144.78 115.57 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 0 -1.9 270) (layer F.SilkS) hide)
    (fp_text value 10k (at 0 1.9 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(JP1-Pad3)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 CS_A/G))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57C12790)
    (at 144.78 119.38 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 0 -1.9 270) (layer F.SilkS) hide)
    (fp_text value 10k (at 0 1.9 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(JP2-Pad3)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 SDO_A/G))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57C12780)
    (at 137.16 121.92 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 0 -1.9 90) (layer F.SilkS) hide)
    (fp_text value 10k (at 0 1.9 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(JP3-Pad3)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 12 SCL))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57C12794)
    (at 143.51 115.57 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 0 -1.9 90) (layer F.SilkS) hide)
    (fp_text value 10k (at 0 1.9 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(JP1-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 16 CS_M))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57C1278C)
    (at 143.51 119.38 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at 0 -1.9 90) (layer F.SilkS) hide)
    (fp_text value 10k (at 0 1.9 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(JP2-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 SDO_M))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57C12785)
    (at 138.43 121.92 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at 0 -1.9 90) (layer F.SilkS) hide)
    (fp_text value 10k (at 0 1.9 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(JP3-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 SDA))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lsm9ds1_breakout:LGA-24-3.5X3X1mm (layer F.Cu) (tedit 57C106AC)
    (at 138.43 115.57 90)
    (fp_text reference U1 (at 0 6.35 90) (layer F.SilkS) hide)
    (fp_text value LSM9DS1 (at 0 -6.858 90) (layer F.Fab) hide)
    (pad 18 smd rect (at 1.505 -1.25 90) (size 0.28 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 19 smd rect (at 1.075 -1.25 90) (size 0.28 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 20 smd rect (at 0.645 -1.25 90) (size 0.28 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 21 smd rect (at 0.215 -1.25 90) (size 0.28 0.4) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C5-Pad1)"))
    (pad 1 smd rect (at -1.505 -1.25 90) (size 0.28 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 24 smd rect (at -1.075 -1.25 90) (size 0.28 0.4) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (pad 23 smd rect (at -0.645 -1.25 90) (size 0.28 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 22 smd rect (at -0.215 -1.25 90) (size 0.28 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -1.5 -0.645 90) (size 0.4 0.28) (layers F.Cu F.Paste F.Mask)
      (net 12 SCL))
    (pad 3 smd rect (at -1.5 -0.215 90) (size 0.4 0.28) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 4 smd rect (at -1.5 0.215 90) (size 0.4 0.28) (layers F.Cu F.Paste F.Mask)
      (net 11 SDA))
    (pad 5 smd rect (at -1.5 0.645 90) (size 0.4 0.28) (layers F.Cu F.Paste F.Mask)
      (net 13 SDO_A/G))
    (pad 6 smd rect (at -1.505 1.25 90) (size 0.28 0.4) (layers F.Cu F.Paste F.Mask)
      (net 14 SDO_M))
    (pad 7 smd rect (at -1.075 1.25 90) (size 0.28 0.4) (layers F.Cu F.Paste F.Mask)
      (net 15 CS_A/G))
    (pad 8 smd rect (at -0.645 1.25 90) (size 0.28 0.4) (layers F.Cu F.Paste F.Mask)
      (net 16 CS_M))
    (pad 9 smd rect (at -0.215 1.25 90) (size 0.28 0.4) (layers F.Cu F.Paste F.Mask)
      (net 17 DRDY_M))
    (pad 10 smd rect (at 0.215 1.25 90) (size 0.28 0.4) (layers F.Cu F.Paste F.Mask)
      (net 18 INT_M))
    (pad 11 smd rect (at 0.645 1.25 90) (size 0.28 0.4) (layers F.Cu F.Paste F.Mask)
      (net 19 INT1_A/G))
    (pad 12 smd rect (at 1.075 1.25 90) (size 0.28 0.4) (layers F.Cu F.Paste F.Mask)
      (net 20 INT2_A/G))
    (pad 13 smd rect (at 1.505 1.25 90) (size 0.28 0.4) (layers F.Cu F.Paste F.Mask)
      (net 21 DEN_A/G))
    (pad 14 smd rect (at 1.5 0.645 90) (size 0.4 0.28) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 15 smd rect (at 1.5 0.215 90) (size 0.4 0.28) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 16 smd rect (at 1.5 -0.215 90) (size 0.4 0.28) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 17 smd rect (at 1.5 -0.645 90) (size 0.4 0.28) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module lsm9ds1_breakout:jumper (layer B.Cu) (tedit 57C12498)
    (at 143.51 118.11)
    (fp_text reference JP1 (at 0 -1.524) (layer B.SilkS) hide)
    (fp_text value JUMPER3 (at 0.254 3.302) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.8255 0) (size 0.635 1.27) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(JP1-Pad1)"))
    (pad 2 smd rect (at 0 0) (size 0.635 1.27) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 3 smd rect (at 0.8255 0) (size 0.635 1.27) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(JP1-Pad3)"))
    (pad 3 smd rect (at 0.41275 0) (size 0.1905 0.1905) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(JP1-Pad3)"))
    (pad 1 smd rect (at -0.41275 0) (size 0.1905 0.1905) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(JP1-Pad1)"))
  )
  (module lsm9ds1_breakout:jumper (layer B.Cu) (tedit 57C124A0)
    (at 143.51 120.65)
    (fp_text reference JP2 (at 0 -1.524) (layer B.SilkS) hide)
    (fp_text value JUMPER3 (at 0.254 3.302) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.8255 0) (size 0.635 1.27) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(JP2-Pad1)"))
    (pad 2 smd rect (at 0 0) (size 0.635 1.27) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 3 smd rect (at 0.8255 0) (size 0.635 1.27) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(JP2-Pad3)"))
    (pad 3 smd rect (at 0.41275 0) (size 0.1905 0.1905) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(JP2-Pad3)"))
    (pad 1 smd rect (at -0.41275 0) (size 0.1905 0.1905) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(JP2-Pad1)"))
  )
  (module lsm9ds1_breakout:jumper (layer B.Cu) (tedit 57C3995E)
    (at 138.43 121.92 180)
    (fp_text reference JP3 (at 0 -1.524 180) (layer B.SilkS) hide)
    (fp_text value JUMPER3 (at 0.254 3.302 180) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.8255 0 180) (size 0.635 1.27) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(JP3-Pad1)"))
    (pad 2 smd rect (at 0 0 180) (size 0.635 1.27) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 3 smd rect (at 0.8255 0 180) (size 0.635 1.27) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(JP3-Pad3)"))
    (pad 3 smd rect (at 0.41275 0 180) (size 0.1905 0.1905) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(JP3-Pad3)"))
    (pad 1 smd rect (at -0.41275 0 180) (size 0.1905 0.1905) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(JP3-Pad1)"))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_DIN965 (layer F.Cu) (tedit 57C11A18)
    (at 133.35 124.46)
    (descr "Mounting Hole 3.2mm, no annular, M3, DIN965")
    (tags "mounting hole 3.2mm no annular m3 din965")
    (fp_text reference REF** (at 0 -3.8) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_DIN965 (at 0 3.8) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask F.SilkS))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_DIN965 (layer F.Cu) (tedit 57C11A5B)
    (at 143.51 124.46)
    (descr "Mounting Hole 3.2mm, no annular, M3, DIN965")
    (tags "mounting hole 3.2mm no annular m3 din965")
    (fp_text reference REF** (at 0 -3.8) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_DIN965 (at 0 3.8) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask F.SilkS))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_DIN965 (layer F.Cu) (tedit 57C11AD5)
    (at 133.35 106.68)
    (descr "Mounting Hole 3.2mm, no annular, M3, DIN965")
    (tags "mounting hole 3.2mm no annular m3 din965")
    (fp_text reference REF** (at 0 -3.8) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_DIN965 (at 0 3.8) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask F.SilkS))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_DIN965 (layer F.Cu) (tedit 57C11AF2)
    (at 143.51 106.68)
    (descr "Mounting Hole 3.2mm, no annular, M3, DIN965")
    (tags "mounting hole 3.2mm no annular m3 din965")
    (fp_text reference REF** (at 0 -3.8) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_DIN965 (at 0 3.8) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask F.SilkS))
  )
  (module Symbols:OSHW-Symbol_6.7x6mm_SilkScreen (layer F.Cu) (tedit 57C12723)
    (at 138.43 110.49)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference REF*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value OSHW-Symbol_6.7x6mm_SilkScreen (at 0.75 0) (layer F.Fab) hide)
  )
  (gr_text "LSM9DS1\nBreakout" (at 138.43 105.918) (layer F.SilkS))
  (gr_text DEN (at 146.177 105.41) (layer B.SilkS))
  (gr_text INT2 (at 146.05 107.95) (layer B.SilkS))
  (gr_text INT1 (at 146.05 110.49) (layer B.SilkS))
  (gr_text INTM (at 145.923 113.03) (layer B.SilkS))
  (gr_text RDY (at 146.177 115.57) (layer B.SilkS))
  (gr_text "CS\nM" (at 147.193 118.11) (layer B.SilkS))
  (gr_text "CS\nAG" (at 145.669 120.65) (layer B.SilkS))
  (gr_text "SDO\nM" (at 147.193 123.317) (layer B.SilkS))
  (gr_text "SDO\n AG" (at 147.32 125.73) (layer B.SilkS))
  (gr_text SCL (at 130.81 120.65) (layer B.SilkS))
  (gr_text SDA (at 130.81 118.11) (layer B.SilkS))
  (gr_text VDD (at 130.683 115.57) (layer B.SilkS))
  (gr_text GND (at 131.191 113.03) (layer B.SilkS))
  (gr_text AG (at 144.399 116.459) (layer B.SilkS))
  (gr_text M (at 142.621 116.459) (layer B.SilkS))
  (gr_text CS (at 141.351 118.11 270) (layer B.SilkS))
  (gr_text SDO (at 141.351 120.65 270) (layer B.SilkS))
  (gr_text PU (at 137.922 124.46) (layer B.SilkS))
  (gr_text 2 (at 139.319 124.079) (layer B.SilkS))
  (gr_text "I C" (at 139.954 124.46) (layer B.SilkS))
  (gr_text "SDO\nAG" (at 147.32 125.73) (layer F.SilkS))
  (gr_text "SDO\nM" (at 147.32 123.19) (layer F.SilkS))
  (gr_text "CS\nAG" (at 147.32 120.65) (layer F.SilkS))
  (gr_text "CS\nM" (at 147.32 118.11) (layer F.SilkS))
  (gr_text RDY (at 146.558 115.57) (layer F.SilkS))
  (gr_text INTM (at 146.05 113.03) (layer F.SilkS))
  (gr_text INT1 (at 146.05 110.49) (layer F.SilkS))
  (gr_text INT2 (at 146.05 107.95) (layer F.SilkS))
  (gr_text DEN (at 146.177 105.41) (layer F.SilkS))
  (gr_text SCL (at 130.683 120.65) (layer F.SilkS))
  (gr_text SDA (at 130.683 118.11) (layer F.SilkS))
  (gr_text VDD (at 130.683 115.57) (layer F.SilkS))
  (gr_text GND (at 130.683 113.03) (layer F.SilkS))
  (gr_text X (at 132.461 110.617) (layer F.SilkS))
  (gr_text Y (at 133.9088 112.1918) (layer F.SilkS))
  (gr_text Z (at 134.239 110.6678) (layer F.SilkS))
  (gr_line (start 127 104.14) (end 127 127) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 149.86 104.14) (end 127 104.14) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 149.86 127) (end 149.86 104.14) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 127 127) (end 149.86 127) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.3048) (smoothing fillet))
    (polygon
      (pts
        (xy 149.86 127) (xy 127 127) (xy 127 104.14) (xy 149.86 104.14) (xy 149.86 127)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 16) (thermal_gap 0.1524) (thermal_bridge_width 0.254) (smoothing fillet))
    (polygon
      (pts
        (xy 149.86 127) (xy 127 127) (xy 127 104.14) (xy 149.86 104.14) (xy 149.86 127)
      )
    )
  )
)
