(kicad_pcb (version 20171130) (host pcbnew "(5.1.5)-3")
  (general
    (thickness 1.6)
    (drawings 17)
    (tracks 622)
    (zones 0)
    (modules 83)
    (nets 51)
  )
  (page USLetter)
  (title_block
    (title TIAPreamp2)
    (date 2020-02-08)
    (company "UT Austin")
  )
  (layers
    (0 AFRONT signal)
    (1 GND power)
    (2 DSIG signal)
    (31 ABACK signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.25)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x3ffff_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Gerbers/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(C1-Pad1)")
  (net 3 "Net-(C2-Pad1)")
  (net 4 Tip)
  (net 5 "Net-(C7-Pad1)")
  (net 6 "Net-(C12-Pad1)")
  (net 7 VDD)
  (net 8 "Net-(C18-Pad1)")
  (net 9 "Net-(C21-Pad1)")
  (net 10 "Net-(C23-Pad2)")
  (net 11 "Net-(C24-Pad1)")
  (net 12 "Net-(C26-Pad1)")
  (net 13 "Net-(C27-Pad1)")
  (net 14 "Net-(C28-Pad1)")
  (net 15 "Net-(C29-Pad1)")
  (net 16 "Net-(C30-Pad2)")
  (net 17 "Net-(C31-Pad1)")
  (net 18 "Net-(C33-Pad1)")
  (net 19 "Net-(C35-Pad1)")
  (net 20 "Net-(C37-Pad1)")
  (net 21 "Net-(C40-Pad1)")
  (net 22 "Net-(D1-Pad1)")
  (net 23 "Net-(D1-Pad2)")
  (net 24 "Net-(IC1-Pad1)")
  (net 25 "Net-(IC1-Pad10)")
  (net 26 "Net-(IC1-Pad3)")
  (net 27 "Net-(IC1-Pad12)")
  (net 28 "Net-(IC1-Pad7)")
  (net 29 "Net-(IC1-Pad8)")
  (net 30 "Net-(IC1-Pad11)")
  (net 31 "Net-(IC1-Pad14)")
  (net 32 "Net-(IC1-Pad15)")
  (net 33 "Net-(IC1-Pad16)")
  (net 34 "Net-(IC2-Pad1)")
  (net 35 "Net-(IC2-Pad3)")
  (net 36 "Net-(IC3-Pad1)")
  (net 37 "Net-(IC3-Pad2)")
  (net 38 "Net-(IC3-Pad3)")
  (net 39 "Net-(IC3-Pad5)")
  (net 40 "Net-(IC3-Pad8)")
  (net 41 "Net-(J1-Pad1)")
  (net 42 "Net-(J7-Pad1)")
  (net 43 A1)
  (net 44 A2)
  (net 45 A0)
  (net 46 "Net-(J16-Pad1)")
  (net 47 "Net-(R25-Pad2)")
  (net 48 "Net-(S4-PadA1)")
  (net 49 "Net-(S4-PadA2)")
  (net 50 "Net-(U1-Pad7)")
  (net_class Default "This is the default net class."
    (clearance 0.25)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net A0)
    (add_net A1)
    (add_net A2)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C12-Pad1)")
    (add_net "Net-(C18-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C21-Pad1)")
    (add_net "Net-(C23-Pad2)")
    (add_net "Net-(C24-Pad1)")
    (add_net "Net-(C26-Pad1)")
    (add_net "Net-(C27-Pad1)")
    (add_net "Net-(C28-Pad1)")
    (add_net "Net-(C29-Pad1)")
    (add_net "Net-(C30-Pad2)")
    (add_net "Net-(C31-Pad1)")
    (add_net "Net-(C33-Pad1)")
    (add_net "Net-(C35-Pad1)")
    (add_net "Net-(C37-Pad1)")
    (add_net "Net-(C40-Pad1)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(IC1-Pad1)")
    (add_net "Net-(IC1-Pad10)")
    (add_net "Net-(IC1-Pad11)")
    (add_net "Net-(IC1-Pad12)")
    (add_net "Net-(IC1-Pad14)")
    (add_net "Net-(IC1-Pad15)")
    (add_net "Net-(IC1-Pad16)")
    (add_net "Net-(IC1-Pad3)")
    (add_net "Net-(IC1-Pad7)")
    (add_net "Net-(IC1-Pad8)")
    (add_net "Net-(IC2-Pad1)")
    (add_net "Net-(IC2-Pad3)")
    (add_net "Net-(IC3-Pad1)")
    (add_net "Net-(IC3-Pad2)")
    (add_net "Net-(IC3-Pad3)")
    (add_net "Net-(IC3-Pad5)")
    (add_net "Net-(IC3-Pad8)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J16-Pad1)")
    (add_net "Net-(J7-Pad1)")
    (add_net "Net-(R25-Pad2)")
    (add_net "Net-(S4-PadA1)")
    (add_net "Net-(S4-PadA2)")
    (add_net "Net-(U1-Pad7)")
    (add_net Tip)
    (add_net VDD)
  )
  (module TestPoint:TestPoint_2Pads_Pitch2.54mm_Drill0.8mm (layer AFRONT) (tedit 5A0F774F)
    (at 137.16 61.976 90)
    (descr "Test point with 2 pins, pitch 2.54mm, drill diameter 0.8mm")
    (tags "CONN DEV")
    (attr virtual)
    (fp_text reference TP5 (at 1.3 -2 90) (layer F.SilkS))
    (fp_text value TestPoint_2Pole (at 1.27 2 90) (layer F.Fab))
    (fp_text user %R (at 1.3 -2 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 "Net-(IC3-Pad3)"))
  )
  (module TestPoint:TestPoint_2Pads_Pitch2.54mm_Drill0.8mm (layer AFRONT) (tedit 5A0F774F)
    (at 142.748 74.168 270)
    (descr "Test point with 2 pins, pitch 2.54mm, drill diameter 0.8mm")
    (tags "CONN DEV")
    (attr virtual)
    (fp_text reference TP4 (at 1.3 -2 90) (layer F.SilkS))
    (fp_text value TestPoint_2Pole (at 1.27 2 90) (layer F.Fab))
    (fp_text user %R (at 1.3 -2 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 "Net-(J1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(C24-Pad1)"))
  )
  (module SamacSys_Parts:0316575 (layer AFRONT) (tedit 5E4C9737)
    (at 121.92 51.308 90)
    (descr 031-6575-1)
    (tags Connector)
    (fp_text reference J21 (at 17.05 -2.54 90) (layer F.SilkS))
    (fp_text value Conn_Coaxial_x2 (at 17.05 -2.54 90) (layer F.SilkS) hide)
    (pad 6 thru_hole circle (at 8.89 2.54 180) (size 3.015 3.015) (drill 2.01) (layers *.Cu *.Mask F.SilkS))
    (pad 5 thru_hole circle (at 8.89 -7.62 180) (size 3.015 3.015) (drill 2.01) (layers *.Cu *.Mask F.SilkS))
    (pad 4 thru_hole circle (at 2.54 -2.54 180) (size 1.446 1.446) (drill 0.89) (layers *.Cu *.Mask F.SilkS))
    (pad 3 thru_hole circle (at 0 -5.08 180) (size 1.446 1.446) (drill 0.89) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole circle (at 0 -2.54 180) (size 1.446 1.446) (drill 0.89) (layers *.Cu *.Mask F.SilkS)
      (net 45 A0))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.446 1.446) (drill 0.89) (layers *.Cu *.Mask F.SilkS)
      (net 43 A1))
  )
  (module SamacSys_Parts:0316575 (layer AFRONT) (tedit 5E4C9737)
    (at 101.092 51.308 90)
    (descr 031-6575-1)
    (tags Connector)
    (fp_text reference J20 (at 17.05 -2.54 90) (layer F.SilkS))
    (fp_text value Conn_Coaxial_x2 (at 17.05 -2.54 90) (layer F.SilkS) hide)
    (pad 6 thru_hole circle (at 8.89 2.54 180) (size 3.015 3.015) (drill 2.01) (layers *.Cu *.Mask F.SilkS))
    (pad 5 thru_hole circle (at 8.89 -7.62 180) (size 3.015 3.015) (drill 2.01) (layers *.Cu *.Mask F.SilkS))
    (pad 4 thru_hole circle (at 2.54 -2.54 180) (size 1.446 1.446) (drill 0.89) (layers *.Cu *.Mask F.SilkS))
    (pad 3 thru_hole circle (at 0 -5.08 180) (size 1.446 1.446) (drill 0.89) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole circle (at 0 -2.54 180) (size 1.446 1.446) (drill 0.89) (layers *.Cu *.Mask F.SilkS)
      (net 44 A2))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.446 1.446) (drill 0.89) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(IC1-Pad1)"))
  )
  (module Connector_Coaxial:BNC_Amphenol_B6252HB-NPP3G-50_Horizontal (layer AFRONT) (tedit 5C13907B)
    (at 185.928 49.276)
    (descr http://www.farnell.com/datasheets/612848.pdf)
    (tags "BNC Amphenol Horizontal")
    (fp_text reference J19 (at 0 4) (layer F.SilkS))
    (fp_text value Conn_Coaxial (at 0 6 180) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 thru_hole oval (at -2.54 0) (size 1.6 2.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole oval (at 0 0) (size 1.6 2.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 14 "Net-(C28-Pad1)"))
    (pad 2 thru_hole oval (at 5.08 -5.08) (size 3.5 7) (drill 2.01) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at -5.08 -5.08) (size 3.5 7) (drill 2.01) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_Coaxial.3dshapes/BNC_Amphenol_B6252HB-NPP3G-50_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer AFRONT) (tedit 5B36C52B)
    (at 173.482 63.373 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R11 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value "5.1k, 1/8W" (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(C28-Pad1)"))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 "Net-(IC1-Pad11)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:TSSOP-16_4.4x5mm_P0.65mm (layer ABACK) (tedit 5A02F25C)
    (at 115.824 84.328 180)
    (descr "16-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference S2 (at 0 3.55) (layer B.SilkS))
    (fp_text value MUX36S08IPWR (at 0 -3.55) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -2.95 2.275 180) (size 1.5 0.45) (layers ABACK B.Paste B.Mask)
      (net 45 A0))
    (pad 2 smd rect (at -2.95 1.625 180) (size 1.5 0.45) (layers ABACK B.Paste B.Mask)
      (net 7 VDD))
    (pad 3 smd rect (at -2.95 0.975 180) (size 1.5 0.45) (layers ABACK B.Paste B.Mask)
      (net 10 "Net-(C23-Pad2)"))
    (pad 4 smd rect (at -2.95 0.325 180) (size 1.5 0.45) (layers ABACK B.Paste B.Mask)
      (net 11 "Net-(C24-Pad1)"))
    (pad 5 smd rect (at -2.95 -0.325 180) (size 1.5 0.45) (layers ABACK B.Paste B.Mask)
      (net 12 "Net-(C26-Pad1)"))
    (pad 6 smd rect (at -2.95 -0.975 180) (size 1.5 0.45) (layers ABACK B.Paste B.Mask)
      (net 13 "Net-(C27-Pad1)"))
    (pad 7 smd rect (at -2.95 -1.625 180) (size 1.5 0.45) (layers ABACK B.Paste B.Mask)
      (net 15 "Net-(C29-Pad1)"))
    (pad 8 smd rect (at -2.95 -2.275 180) (size 1.5 0.45) (layers ABACK B.Paste B.Mask)
      (net 11 "Net-(C24-Pad1)"))
    (pad 9 smd rect (at 2.95 -2.275 180) (size 1.5 0.45) (layers ABACK B.Paste B.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 10 smd rect (at 2.95 -1.625 180) (size 1.5 0.45) (layers ABACK B.Paste B.Mask)
      (net 5 "Net-(C7-Pad1)"))
    (pad 11 smd rect (at 2.95 -0.975 180) (size 1.5 0.45) (layers ABACK B.Paste B.Mask)
      (net 6 "Net-(C12-Pad1)"))
    (pad 12 smd rect (at 2.95 -0.325 180) (size 1.5 0.45) (layers ABACK B.Paste B.Mask)
      (net 8 "Net-(C18-Pad1)"))
    (pad 13 smd rect (at 2.95 0.325 180) (size 1.5 0.45) (layers ABACK B.Paste B.Mask)
      (net 7 VDD))
    (pad 14 smd rect (at 2.95 0.975 180) (size 1.5 0.45) (layers ABACK B.Paste B.Mask)
      (net 1 GND))
    (pad 15 smd rect (at 2.95 1.625 180) (size 1.5 0.45) (layers ABACK B.Paste B.Mask)
      (net 44 A2))
    (pad 16 smd rect (at 2.95 2.275 180) (size 1.5 0.45) (layers ABACK B.Paste B.Mask)
      (net 43 A1))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TSSOP-16_4.4x5mm_P0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:TSSOP-16_4.4x5mm_P0.65mm (layer AFRONT) (tedit 5A02F25C)
    (at 116.078 90.17 180)
    (descr "16-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference S1 (at 0 -3.55) (layer F.SilkS))
    (fp_text value MUX36S08IPWR (at 0 3.55) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2.95 -2.275 180) (size 1.5 0.45) (layers AFRONT F.Paste F.Mask)
      (net 45 A0))
    (pad 2 smd rect (at -2.95 -1.625 180) (size 1.5 0.45) (layers AFRONT F.Paste F.Mask)
      (net 7 VDD))
    (pad 3 smd rect (at -2.95 -0.975 180) (size 1.5 0.45) (layers AFRONT F.Paste F.Mask)
      (net 10 "Net-(C23-Pad2)"))
    (pad 4 smd rect (at -2.95 -0.325 180) (size 1.5 0.45) (layers AFRONT F.Paste F.Mask)
      (net 11 "Net-(C24-Pad1)"))
    (pad 5 smd rect (at -2.95 0.325 180) (size 1.5 0.45) (layers AFRONT F.Paste F.Mask)
      (net 12 "Net-(C26-Pad1)"))
    (pad 6 smd rect (at -2.95 0.975 180) (size 1.5 0.45) (layers AFRONT F.Paste F.Mask)
      (net 13 "Net-(C27-Pad1)"))
    (pad 7 smd rect (at -2.95 1.625 180) (size 1.5 0.45) (layers AFRONT F.Paste F.Mask)
      (net 15 "Net-(C29-Pad1)"))
    (pad 8 smd rect (at -2.95 2.275 180) (size 1.5 0.45) (layers AFRONT F.Paste F.Mask)
      (net 34 "Net-(IC2-Pad1)"))
    (pad 9 smd rect (at 2.95 2.275 180) (size 1.5 0.45) (layers AFRONT F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 10 smd rect (at 2.95 1.625 180) (size 1.5 0.45) (layers AFRONT F.Paste F.Mask)
      (net 5 "Net-(C7-Pad1)"))
    (pad 11 smd rect (at 2.95 0.975 180) (size 1.5 0.45) (layers AFRONT F.Paste F.Mask)
      (net 6 "Net-(C12-Pad1)"))
    (pad 12 smd rect (at 2.95 0.325 180) (size 1.5 0.45) (layers AFRONT F.Paste F.Mask)
      (net 8 "Net-(C18-Pad1)"))
    (pad 13 smd rect (at 2.95 -0.325 180) (size 1.5 0.45) (layers AFRONT F.Paste F.Mask)
      (net 7 VDD))
    (pad 14 smd rect (at 2.95 -0.975 180) (size 1.5 0.45) (layers AFRONT F.Paste F.Mask)
      (net 1 GND))
    (pad 15 smd rect (at 2.95 -1.625 180) (size 1.5 0.45) (layers AFRONT F.Paste F.Mask)
      (net 44 A2))
    (pad 16 smd rect (at 2.95 -2.275 180) (size 1.5 0.45) (layers AFRONT F.Paste F.Mask)
      (net 43 A1))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TSSOP-16_4.4x5mm_P0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_Tantalum_SMD:CP_EIA-3528-21_Kemet-B (layer AFRONT) (tedit 5B342532)
    (at 112.268 108.204)
    (descr "Tantalum Capacitor SMD Kemet-B (3528-21 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (attr smd)
    (fp_text reference C23 (at -0.508 2.54) (layer F.SilkS))
    (fp_text value 10u (at 0 2.35) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.5375 0) (size 1.325 2.35) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.188679)
      (net 10 "Net-(C23-Pad2)"))
    (pad 1 smd roundrect (at -1.5375 0) (size 1.325 2.35) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.188679)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-3528-21_Kemet-B.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_Tantalum_SMD:CP_EIA-3528-21_Kemet-B (layer AFRONT) (tedit 5B342532)
    (at 112.268 103.124)
    (descr "Tantalum Capacitor SMD Kemet-B (3528-21 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (attr smd)
    (fp_text reference C17 (at 0 2.54) (layer F.SilkS))
    (fp_text value 10u (at 0 2.35) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.5375 0) (size 1.325 2.35) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.188679)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.5375 0) (size 1.325 2.35) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.188679)
      (net 7 VDD))
    (model ${KISYS3DMOD}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-3528-21_Kemet-B.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Pad_4.0x4.0mm (layer AFRONT) (tedit 5A0F774F)
    (at 192.659 90.932 180)
    (descr "SMD rectangular pad as test Point, square 4.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference TP2 (at 0 -2.898) (layer F.SilkS))
    (fp_text value TestPoint (at 0 3.1) (layer F.Fab))
    (fp_text user %R (at 0 -2.9) (layer F.Fab))
    (pad 1 smd rect (at 0 0 180) (size 4 4) (layers AFRONT F.Mask)
      (net 9 "Net-(C21-Pad1)"))
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer AFRONT) (tedit 5B301BBE)
    (at 141.732 65.532 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value 6.8p (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(C1-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer AFRONT) (tedit 5B301BBE)
    (at 114.808 84.328 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at 0 -1.17 90) (layer F.SilkS))
    (fp_text value 0.3p (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 Tip))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer AFRONT) (tedit 5B301BBE)
    (at 109.22 84.328 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C7 (at 0 -1.17 90) (layer F.SilkS))
    (fp_text value 0.3p (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 Tip))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(C7-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer AFRONT) (tedit 5B301BBE)
    (at 104.648 84.328 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C12 (at 0 -1.17 90) (layer F.SilkS))
    (fp_text value 0.3p (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(C12-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 Tip))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer AFRONT) (tedit 5B301BBE)
    (at 99.568 84.328 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C18 (at 0 -1.17 90) (layer F.SilkS))
    (fp_text value 0.75p (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 Tip))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 "Net-(C18-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer AFRONT) (tedit 5B301BBE)
    (at 110.236 99.568 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C20 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value 100p (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 VDD))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer AFRONT) (tedit 5B301BBE)
    (at 157.607 56.388 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C21 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value 100p (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 "Net-(C21-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_Tantalum_SMD:CP_EIA-3528-21_Kemet-B (layer AFRONT) (tedit 5B342532)
    (at 153.797 57.023 90)
    (descr "Tantalum Capacitor SMD Kemet-B (3528-21 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (attr smd)
    (fp_text reference C22 (at 0 -2.35 90) (layer F.SilkS))
    (fp_text value 6.8u (at 0 2.35 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.5375 0 90) (size 1.325 2.35) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.188679)
      (net 1 GND))
    (pad 2 smd roundrect (at 1.5375 0 90) (size 1.325 2.35) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.188679)
      (net 9 "Net-(C21-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-3528-21_Kemet-B.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer AFRONT) (tedit 5B301BBE)
    (at 118.872 66.04 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C24 (at -3.048 0) (layer F.SilkS))
    (fp_text value 1.5p (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(C24-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 Tip))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer AFRONT) (tedit 5B301BBE)
    (at 114.3 99.568 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C25 (at 0 1.27 90) (layer F.SilkS))
    (fp_text value 100p (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(C23-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer AFRONT) (tedit 5B301BBE)
    (at 118.618 76.708 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C26 (at -2.794 0) (layer F.SilkS))
    (fp_text value 1.5p (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(C26-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 Tip))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer AFRONT) (tedit 5B301BBE)
    (at 118.745 80.772 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C27 (at -2.667 -0.508) (layer F.SilkS))
    (fp_text value 1.5p (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 Tip))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(C27-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer AFRONT) (tedit 5B301BBE)
    (at 173.482 58.293 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C28 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value 6.8p (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(C28-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer AFRONT) (tedit 5B301BBE)
    (at 120.015 84.836 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C29 (at 2.54 0) (layer F.SilkS))
    (fp_text value 2.2p (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 Tip))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 "Net-(C29-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer AFRONT) (tedit 5B301BBE)
    (at 171.577 51.308 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C30 (at -3.81 0) (layer F.SilkS))
    (fp_text value 100p (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 "Net-(C30-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer AFRONT) (tedit 5B301BBE)
    (at 131.064 105.029)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C31 (at 0 1.27) (layer F.SilkS))
    (fp_text value 0.3p (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 "Net-(C31-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_Tantalum_SMD:CP_EIA-3528-21_Kemet-B (layer AFRONT) (tedit 5B342532)
    (at 172.847 48.133)
    (descr "Tantalum Capacitor SMD Kemet-B (3528-21 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (attr smd)
    (fp_text reference C32 (at 0 -2.35) (layer F.SilkS))
    (fp_text value 6.8u (at 0 2.35) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.5375 0) (size 1.325 2.35) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.188679)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.5375 0) (size 1.325 2.35) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.188679)
      (net 16 "Net-(C30-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-3528-21_Kemet-B.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer AFRONT) (tedit 5B301BBE)
    (at 127.889 105.664 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C33 (at 0 -1.17 90) (layer F.SilkS))
    (fp_text value 1.5p (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 "Net-(C33-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer AFRONT) (tedit 5B301BBE)
    (at 125.349 105.664 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C35 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value 2.2n (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 "Net-(C35-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer AFRONT) (tedit 5B301BBE)
    (at 134.747 98.425)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C37 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 68p (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 "Net-(C37-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer AFRONT) (tedit 5B36C52B)
    (at 134.747 101.6)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C40 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 75p (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 "Net-(C40-Pad1)"))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_0603_1608Metric (layer AFRONT) (tedit 5B301BBE)
    (at 153.162 90.043 270)
    (descr "Diode SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D1 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value "3V, 10mA" (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 "Net-(D1-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SamacSys_Parts:SOP65P640X120-16N (layer AFRONT) (tedit 5E3CD6D5)
    (at 165.608 68.58)
    (descr "PW (R-PDSO-G16)")
    (tags "Integrated Circuit")
    (attr smd)
    (fp_text reference IC1 (at 0 0) (layer F.SilkS))
    (fp_text value TMUX6136PWR (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.938 -2.275 90) (size 0.45 1.475) (layers AFRONT F.Paste F.Mask)
      (net 24 "Net-(IC1-Pad1)"))
    (pad 2 smd rect (at -2.938 -1.625 90) (size 0.45 1.475) (layers AFRONT F.Paste F.Mask)
      (net 25 "Net-(IC1-Pad10)"))
    (pad 3 smd rect (at -2.938 -0.975 90) (size 0.45 1.475) (layers AFRONT F.Paste F.Mask)
      (net 26 "Net-(IC1-Pad3)"))
    (pad 4 smd rect (at -2.938 -0.325 90) (size 0.45 1.475) (layers AFRONT F.Paste F.Mask)
      (net 27 "Net-(IC1-Pad12)"))
    (pad 5 smd rect (at -2.938 0.325 90) (size 0.45 1.475) (layers AFRONT F.Paste F.Mask)
      (net 9 "Net-(C21-Pad1)"))
    (pad 6 smd rect (at -2.938 0.975 90) (size 0.45 1.475) (layers AFRONT F.Paste F.Mask)
      (net 1 GND))
    (pad 7 smd rect (at -2.938 1.625 90) (size 0.45 1.475) (layers AFRONT F.Paste F.Mask)
      (net 28 "Net-(IC1-Pad7)"))
    (pad 8 smd rect (at -2.938 2.275 90) (size 0.45 1.475) (layers AFRONT F.Paste F.Mask)
      (net 29 "Net-(IC1-Pad8)"))
    (pad 9 smd rect (at 2.938 2.275 90) (size 0.45 1.475) (layers AFRONT F.Paste F.Mask)
      (net 24 "Net-(IC1-Pad1)"))
    (pad 10 smd rect (at 2.938 1.625 90) (size 0.45 1.475) (layers AFRONT F.Paste F.Mask)
      (net 25 "Net-(IC1-Pad10)"))
    (pad 11 smd rect (at 2.938 0.975 90) (size 0.45 1.475) (layers AFRONT F.Paste F.Mask)
      (net 30 "Net-(IC1-Pad11)"))
    (pad 12 smd rect (at 2.938 0.325 90) (size 0.45 1.475) (layers AFRONT F.Paste F.Mask)
      (net 27 "Net-(IC1-Pad12)"))
    (pad 13 smd rect (at 2.938 -0.325 90) (size 0.45 1.475) (layers AFRONT F.Paste F.Mask)
      (net 16 "Net-(C30-Pad2)"))
    (pad 14 smd rect (at 2.938 -0.975 90) (size 0.45 1.475) (layers AFRONT F.Paste F.Mask)
      (net 31 "Net-(IC1-Pad14)"))
    (pad 15 smd rect (at 2.938 -1.625 90) (size 0.45 1.475) (layers AFRONT F.Paste F.Mask)
      (net 32 "Net-(IC1-Pad15)"))
    (pad 16 smd rect (at 2.938 -2.275 90) (size 0.45 1.475) (layers AFRONT F.Paste F.Mask)
      (net 33 "Net-(IC1-Pad16)"))
  )
  (module SamacSys_Parts:SOT95P280X145-5N (layer AFRONT) (tedit 5E387FBF)
    (at 112.522 95.885 180)
    (descr "SOT23 RJ-5")
    (tags "Integrated Circuit")
    (attr smd)
    (fp_text reference IC2 (at 0 0) (layer F.SilkS))
    (fp_text value AD8067ARTZ-R2 (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.25 -0.95 270) (size 0.6 1.2) (layers AFRONT F.Paste F.Mask)
      (net 34 "Net-(IC2-Pad1)"))
    (pad 2 smd rect (at -1.25 0 270) (size 0.6 1.2) (layers AFRONT F.Paste F.Mask)
      (net 10 "Net-(C23-Pad2)"))
    (pad 3 smd rect (at -1.25 0.95 270) (size 0.6 1.2) (layers AFRONT F.Paste F.Mask)
      (net 35 "Net-(IC2-Pad3)"))
    (pad 4 smd rect (at 1.25 0.95 270) (size 0.6 1.2) (layers AFRONT F.Paste F.Mask)
      (net 4 Tip))
    (pad 5 smd rect (at 1.25 -0.95 270) (size 0.6 1.2) (layers AFRONT F.Paste F.Mask)
      (net 7 VDD))
  )
  (module SamacSys_Parts:SOIC127P600X175-8N (layer AFRONT) (tedit 5E39BB6B)
    (at 163.957 53.213)
    (descr D0008A)
    (tags "Integrated Circuit")
    (attr smd)
    (fp_text reference IC3 (at 0 0) (layer F.SilkS))
    (fp_text value THS4021ID (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.711 -1.905 90) (size 0.65 1.528) (layers AFRONT F.Paste F.Mask)
      (net 36 "Net-(IC3-Pad1)"))
    (pad 2 smd rect (at -2.711 -0.635 90) (size 0.65 1.528) (layers AFRONT F.Paste F.Mask)
      (net 37 "Net-(IC3-Pad2)"))
    (pad 3 smd rect (at -2.711 0.635 90) (size 0.65 1.528) (layers AFRONT F.Paste F.Mask)
      (net 38 "Net-(IC3-Pad3)"))
    (pad 4 smd rect (at -2.711 1.905 90) (size 0.65 1.528) (layers AFRONT F.Paste F.Mask)
      (net 9 "Net-(C21-Pad1)"))
    (pad 5 smd rect (at 2.711 1.905 90) (size 0.65 1.528) (layers AFRONT F.Paste F.Mask)
      (net 39 "Net-(IC3-Pad5)"))
    (pad 6 smd rect (at 2.711 0.635 90) (size 0.65 1.528) (layers AFRONT F.Paste F.Mask)
      (net 26 "Net-(IC1-Pad3)"))
    (pad 7 smd rect (at 2.711 -0.635 90) (size 0.65 1.528) (layers AFRONT F.Paste F.Mask)
      (net 16 "Net-(C30-Pad2)"))
    (pad 8 smd rect (at 2.711 -1.905 90) (size 0.65 1.528) (layers AFRONT F.Paste F.Mask)
      (net 40 "Net-(IC3-Pad8)"))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical (layer AFRONT) (tedit 59FED5CC)
    (at 128.524 70.104 90)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value Conn_01x05_Male (at 0 12.49 90) (layer F.Fab))
    (fp_text user %R (at 0 5.08) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 "Net-(J1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 "Net-(J1-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 "Net-(J1-Pad1)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 "Net-(J1-Pad1)"))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical (layer AFRONT) (tedit 59FED5CC)
    (at 128.524 66.04 90)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value Conn_01x05_Male (at 0 12.49 90) (layer F.Fab))
    (fp_text user %R (at 0 5.08) (layer F.Fab))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Coaxial:BNC_Amphenol_B6252HB-NPP3G-50_Horizontal (layer AFRONT) (tedit 5C13907B)
    (at 103.505 95.631 90)
    (descr http://www.farnell.com/datasheets/612848.pdf)
    (tags "BNC Amphenol Horizontal")
    (fp_text reference J3 (at 0 4 90) (layer F.SilkS))
    (fp_text value Conn_Coaxial (at 0 6 270) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at -5.08 -5.08 90) (size 3.5 7) (drill 2.01) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 5.08 -5.08 90) (size 3.5 7) (drill 2.01) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole oval (at 0 0 90) (size 1.6 2.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 4 Tip))
    (pad 2 thru_hole oval (at -2.54 0 90) (size 1.6 2.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_Coaxial.3dshapes/BNC_Amphenol_B6252HB-NPP3G-50_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical (layer AFRONT) (tedit 59FED5CC)
    (at 106.807 111.379 270)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference J4 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value Conn_01x05_Male (at 0 12.49 90) (layer F.Fab))
    (fp_text user %R (at 0 5.08) (layer F.Fab))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 VDD))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 VDD))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 VDD))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 VDD))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 VDD))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical (layer AFRONT) (tedit 59FED5CC)
    (at 142.367 48.133)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference J5 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x05_Male (at 0 12.49) (layer F.Fab))
    (fp_text user %R (at 0 5.08 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(IC3-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(IC3-Pad3)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(IC3-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(IC3-Pad3)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(IC3-Pad3)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical (layer AFRONT) (tedit 59FED5CC)
    (at 147.32 62.992 90)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference J6 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value Conn_01x05_Male (at 0 12.49 90) (layer F.Fab))
    (fp_text user %R (at 0 5.08) (layer F.Fab))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(IC1-Pad1)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(IC1-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(IC1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(IC1-Pad1)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(IC1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical (layer AFRONT) (tedit 59FED5CC)
    (at 146.812 44.958 90)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference J7 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value Conn_01x05_Male (at 0 12.49 90) (layer F.Fab))
    (fp_text user %R (at 0 5.08) (layer F.Fab))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 "Net-(J7-Pad1)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 "Net-(J7-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 "Net-(J7-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 "Net-(J7-Pad1)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 "Net-(J7-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical (layer AFRONT) (tedit 59FED5CC)
    (at 135.636 82.296)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference J8 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x05_Male (at 0 12.49) (layer F.Fab))
    (fp_text user %R (at 0 5.08 90) (layer F.Fab))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 A1))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 A1))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 A1))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 A1))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 A1))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical (layer AFRONT) (tedit 59FED5CC)
    (at 117.602 99.06)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference J9 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x05_Male (at 0 12.49) (layer F.Fab))
    (fp_text user %R (at 0 5.08 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(C23-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(C23-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(C23-Pad2)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(C23-Pad2)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(C23-Pad2)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical (layer AFRONT) (tedit 59FED5CC)
    (at 131.445 82.296)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference J10 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x05_Male (at 0 12.49) (layer F.Fab))
    (fp_text user %R (at 0 5.08 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 A2))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 A2))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 A2))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 A2))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 A2))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical (layer AFRONT) (tedit 59FED5CC)
    (at 127.508 82.296)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference J11 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x05_Male (at 0 12.49) (layer F.Fab))
    (fp_text user %R (at 0 5.08 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 A0))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 A0))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 A0))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 A0))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 A0))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical (layer AFRONT) (tedit 59FED5CC)
    (at 137.668 77.216 270)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference J12 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value Conn_01x05_Male (at 0 12.49 90) (layer F.Fab))
    (fp_text user %R (at 0 5.08) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(C24-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(C24-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(C24-Pad1)"))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(C24-Pad1)"))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(C24-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical (layer AFRONT) (tedit 59FED5CC)
    (at 106.68 107.188 270)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference J13 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value Conn_01x05_Male (at 0 12.49 90) (layer F.Fab))
    (fp_text user %R (at 0 5.08) (layer F.Fab))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(IC2-Pad1)"))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(IC2-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(IC2-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(IC2-Pad1)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(IC2-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical (layer AFRONT) (tedit 59FED5CC)
    (at 177.8 59.436)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference J14 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x05_Male (at 0 12.49) (layer F.Fab))
    (fp_text user %R (at 0 5.08 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(C28-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(C28-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(C28-Pad1)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(C28-Pad1)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(C28-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical (layer AFRONT) (tedit 59FED5CC)
    (at 171.577 54.356 90)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference J15 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value Conn_01x05_Male (at 0 12.49 90) (layer F.Fab))
    (fp_text user %R (at 0 5.08) (layer F.Fab))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(IC1-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(IC1-Pad3)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(IC1-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(IC1-Pad3)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(IC1-Pad3)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SamacSys_Parts:CONSOCJ2155 (layer AFRONT) (tedit 5E02F6A8)
    (at 180.34 106.426 90)
    (descr CON-SOCJ-2155_1)
    (tags Connector)
    (fp_text reference J16 (at -5.925 1.425 90) (layer F.SilkS))
    (fp_text value CON-SOCJ-2155 (at -5.925 1.425 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 180) (size 5.3 5.3) (drill 3.6401) (layers *.Cu *.Mask F.SilkS)
      (net 46 "Net-(J16-Pad1)"))
    (pad 2 thru_hole circle (at -6 0 180) (size 5 5) (drill 3.1623) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3 thru_hole circle (at -3 4.7 180) (size 5.3 5.3) (drill 3.6401) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical (layer AFRONT) (tedit 59FED5CC)
    (at 164.846 117.348 180)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference J17 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x05_Male (at 0 12.49) (layer F.Fab))
    (fp_text user %R (at 0 5.08 90) (layer F.Fab))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical (layer AFRONT) (tedit 59FED5CC)
    (at 153.416 117.348 180)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference J18 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x05_Male (at 0 12.49) (layer F.Fab))
    (fp_text user %R (at 0 5.08 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer AFRONT) (tedit 5B36C52B)
    (at 141.854 70.429 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value "5.1k, 1/8W" (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(C1-Pad1)"))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 41 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer AFRONT) (tedit 5B301BBD)
    (at 111.76 82.804 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at 4.064 0 90) (layer F.SilkS))
    (fp_text value 100M (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 4 Tip))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer AFRONT) (tedit 5B36C52B)
    (at 106.172 83.312 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at 3.048 0 90) (layer F.SilkS))
    (fp_text value 10M (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(C7-Pad1)"))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 Tip))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer AFRONT) (tedit 5B36C52B)
    (at 101.6 83.82 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at 3.048 0 90) (layer F.SilkS))
    (fp_text value 1M (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 Tip))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(C12-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer AFRONT) (tedit 5B301BBD)
    (at 96.012 81.788 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 100k (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 4 Tip))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 8 "Net-(C18-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer AFRONT) (tedit 5B36C52B)
    (at 147.447 52.578 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R6 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 2k (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 "Net-(R25-Pad2)"))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 38 "Net-(IC3-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer AFRONT) (tedit 5B301BBD)
    (at 147.447 57.023 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R7 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 1k (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 38 "Net-(IC3-Pad3)"))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer AFRONT) (tedit 5B36C52B)
    (at 163.957 58.928 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R8 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value "5.1k, 1/8W" (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 37 "Net-(IC3-Pad2)"))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 "Net-(IC1-Pad10)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_2512_6332Metric (layer AFRONT) (tedit 5B301BBD)
    (at 154.432 50.673)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R9 (at 0 -2.62) (layer F.SilkS))
    (fp_text value 10 (at 0 2.62) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -2.9 0) (size 1.35 3.35) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.185185)
      (net 1 GND))
    (pad 2 smd roundrect (at 2.9 0) (size 1.35 3.35) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.185185)
      (net 37 "Net-(IC3-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_2010_5025Metric (layer AFRONT) (tedit 5B301BBD)
    (at 167.767 59.563 270)
    (descr "Resistor SMD 2010 (5025 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R10 (at 0 -2.28 90) (layer F.SilkS))
    (fp_text value "510, 1/4W" (at 0 2.28 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -2.25 0 270) (size 1.35 2.65) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.185185)
      (net 37 "Net-(IC3-Pad2)"))
    (pad 2 smd roundrect (at 2.25 0 270) (size 1.35 2.65) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.185185)
      (net 27 "Net-(IC1-Pad12)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_2010_5025Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer AFRONT) (tedit 5B36C52B)
    (at 118.872 68.58 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R12 (at -3.556 0) (layer F.SilkS))
    (fp_text value 10 (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 Tip))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(C24-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_2512_6332Metric (layer AFRONT) (tedit 5B301BBD)
    (at 120.904 73.66 180)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R13 (at -5.08 -0.508) (layer F.SilkS))
    (fp_text value 100 (at 0 2.62) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 2.9 0 180) (size 1.35 3.35) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.185185)
      (net 4 Tip))
    (pad 1 smd roundrect (at -2.9 0 180) (size 1.35 3.35) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.185185)
      (net 12 "Net-(C26-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer AFRONT) (tedit 5B301BBD)
    (at 119.888 78.74 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R14 (at -4.191 -0.127) (layer F.SilkS))
    (fp_text value 1k (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 13 "Net-(C27-Pad1)"))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 4 Tip))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer AFRONT) (tedit 5B301BBD)
    (at 118.745 82.931 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R15 (at -3.683 -0.381 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 4 Tip))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 15 "Net-(C29-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_2512_6332Metric (layer AFRONT) (tedit 5B301BBD)
    (at 129.159 111.379 270)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R16 (at 0 -2.62 90) (layer F.SilkS))
    (fp_text value 10 (at 0 2.62 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -2.9 0 270) (size 1.35 3.35) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.185185)
      (net 18 "Net-(C33-Pad1)"))
    (pad 2 smd roundrect (at 2.9 0 270) (size 1.35 3.35) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.185185)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_2512_6332Metric (layer AFRONT) (tedit 5B301BBD)
    (at 123.952 111.379 270)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R17 (at 0 -2.62 90) (layer F.SilkS))
    (fp_text value 10 (at 0 2.62 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 2.9 0 270) (size 1.35 3.35) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.185185)
      (net 1 GND))
    (pad 1 smd roundrect (at -2.9 0 270) (size 1.35 3.35) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.185185)
      (net 19 "Net-(C35-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_2512_6332Metric (layer AFRONT) (tedit 5B301BBD)
    (at 144.272 94.107)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R18 (at 0 -2.62) (layer F.SilkS))
    (fp_text value 10 (at 0 2.62) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -2.9 0) (size 1.35 3.35) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.185185)
      (net 20 "Net-(C37-Pad1)"))
    (pad 2 smd roundrect (at 2.9 0) (size 1.35 3.35) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.185185)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer AFRONT) (tedit 5B301BBD)
    (at 153.162 98.298 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R19 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 1k (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 23 "Net-(D1-Pad2)"))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 16 "Net-(C30-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_2512_6332Metric (layer AFRONT) (tedit 5B301BBD)
    (at 141.097 99.695)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R20 (at 0 -2.62) (layer F.SilkS))
    (fp_text value 10 (at 0 2.62) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -2.9 0) (size 1.35 3.35) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.185185)
      (net 21 "Net-(C40-Pad1)"))
    (pad 2 smd roundrect (at 2.9 0) (size 1.35 3.35) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.185185)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer AFRONT) (tedit 5B36C52B)
    (at 151.257 93.853)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R21 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 2k (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_2512_6332Metric (layer AFRONT) (tedit 5B301BBD)
    (at 134.874 111.379 270)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R22 (at 0 -2.62 90) (layer F.SilkS))
    (fp_text value 10 (at 0 2.62 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 2.9 0 270) (size 1.35 3.35) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.185185)
      (net 1 GND))
    (pad 1 smd roundrect (at -2.9 0 270) (size 1.35 3.35) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.185185)
      (net 17 "Net-(C31-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer AFRONT) (tedit 5B36C52B)
    (at 151.257 86.233)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R23 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 220 (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 "Net-(D1-Pad1)"))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SamacSys_Parts:3306F1103 (layer AFRONT) (tedit 5E3E93CC)
    (at 163.957 43.688)
    (descr 3306F)
    (tags Resistor)
    (fp_text reference R24 (at 0 0) (layer F.SilkS))
    (fp_text value 3306F-1-103 (at 0 0) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -2.5 2.5 90) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 36 "Net-(IC3-Pad1)"))
    (pad 2 thru_hole circle (at 0 -2.5 90) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(C21-Pad1)"))
    (pad 3 thru_hole circle (at 2.5 2.5 90) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 40 "Net-(IC3-Pad8)"))
  )
  (module Resistor_SMD:R_0805_2012Metric (layer AFRONT) (tedit 5B36C52B)
    (at 147.447 48.768 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R25 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 2k (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 "Net-(R25-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers AFRONT F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 42 "Net-(J7-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SamacSys_Parts:15522602 (layer AFRONT) (tedit 5E3E904A)
    (at 178.816 77.724 180)
    (descr 1552.2602-2)
    (tags Switch)
    (fp_text reference S4 (at 6 -2.55) (layer F.SilkS))
    (fp_text value 1552.2602 (at 6 -2.55) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 270) (size 2.55 2.55) (drill 1.7) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(C21-Pad1)"))
    (pad 2 thru_hole circle (at 12 0 270) (size 2.55 2.55) (drill 1.7) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(C30-Pad2)"))
    (pad A1 thru_hole circle (at 0 -6 270) (size 2.55 2.55) (drill 1.7) (layers *.Cu *.Mask F.SilkS)
      (net 48 "Net-(S4-PadA1)"))
    (pad A2 thru_hole circle (at 12 -6 270) (size 2.55 2.55) (drill 1.7) (layers *.Cu *.Mask F.SilkS)
      (net 49 "Net-(S4-PadA2)"))
  )
  (module TestPoint:TestPoint_Pad_4.0x4.0mm (layer AFRONT) (tedit 5A0F774F)
    (at 193.04 106.172 180)
    (descr "SMD rectangular pad as test Point, square 4.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference TP1 (at 0 -2.898) (layer F.SilkS))
    (fp_text value TestPoint (at 0 3.1) (layer F.Fab))
    (fp_text user %R (at 0 -2.9) (layer F.Fab))
    (pad 1 smd rect (at 0 0 180) (size 4 4) (layers AFRONT F.Mask)
      (net 46 "Net-(J16-Pad1)"))
  )
  (module TestPoint:TestPoint_Pad_4.0x4.0mm (layer AFRONT) (tedit 5A0F774F)
    (at 159.004 93.472)
    (descr "SMD rectangular pad as test Point, square 4.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference TP3 (at 0 -2.898) (layer F.SilkS))
    (fp_text value TestPoint (at 0 3.1) (layer F.Fab))
    (fp_text user %R (at 0 -2.9) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 4 4) (layers AFRONT F.Mask)
      (net 16 "Net-(C30-Pad2)"))
  )
  (module Package_DIP:DIP-14_W7.62mm (layer AFRONT) (tedit 5A02E8C5)
    (at 165.1 100.076 90)
    (descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U1 (at 3.81 -2.33 90) (layer F.SilkS))
    (fp_text value NMH2409SC (at 3.81 17.57 90) (layer F.Fab))
    (fp_text user %R (at 3.81 7.62 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 8 thru_hole oval (at 7.62 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 9 thru_hole oval (at 7.62 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 "Net-(S4-PadA2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 10 thru_hole oval (at 7.62 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 11 thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 "Net-(S4-PadA1)"))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 12 thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 13 thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 "Net-(U1-Pad7)"))
    (pad 14 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 "Net-(J16-Pad1)"))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-14_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:TSSOP-16_4.4x5mm_P0.65mm (layer AFRONT) (tedit 5A02F25C)
    (at 125.857 98.679)
    (descr "16-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference S3 (at 0 -3.55) (layer F.SilkS))
    (fp_text value MUX36S08IPWR (at 0 3.55) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 16 smd rect (at 2.95 -2.275) (size 1.5 0.45) (layers AFRONT F.Paste F.Mask)
      (net 43 A1))
    (pad 15 smd rect (at 2.95 -1.625) (size 1.5 0.45) (layers AFRONT F.Paste F.Mask)
      (net 44 A2))
    (pad 14 smd rect (at 2.95 -0.975) (size 1.5 0.45) (layers AFRONT F.Paste F.Mask)
      (net 1 GND))
    (pad 13 smd rect (at 2.95 -0.325) (size 1.5 0.45) (layers AFRONT F.Paste F.Mask)
      (net 7 VDD))
    (pad 12 smd rect (at 2.95 0.325) (size 1.5 0.45) (layers AFRONT F.Paste F.Mask)
      (net 20 "Net-(C37-Pad1)"))
    (pad 11 smd rect (at 2.95 0.975) (size 1.5 0.45) (layers AFRONT F.Paste F.Mask)
      (net 21 "Net-(C40-Pad1)"))
    (pad 10 smd rect (at 2.95 1.625) (size 1.5 0.45) (layers AFRONT F.Paste F.Mask)
      (net 17 "Net-(C31-Pad1)"))
    (pad 9 smd rect (at 2.95 2.275) (size 1.5 0.45) (layers AFRONT F.Paste F.Mask)
      (net 17 "Net-(C31-Pad1)"))
    (pad 8 smd rect (at -2.95 2.275) (size 1.5 0.45) (layers AFRONT F.Paste F.Mask)
      (net 35 "Net-(IC2-Pad3)"))
    (pad 7 smd rect (at -2.95 1.625) (size 1.5 0.45) (layers AFRONT F.Paste F.Mask)
      (net 19 "Net-(C35-Pad1)"))
    (pad 6 smd rect (at -2.95 0.975) (size 1.5 0.45) (layers AFRONT F.Paste F.Mask)
      (net 18 "Net-(C33-Pad1)"))
    (pad 5 smd rect (at -2.95 0.325) (size 1.5 0.45) (layers AFRONT F.Paste F.Mask)
      (net 18 "Net-(C33-Pad1)"))
    (pad 4 smd rect (at -2.95 -0.325) (size 1.5 0.45) (layers AFRONT F.Paste F.Mask)
      (net 18 "Net-(C33-Pad1)"))
    (pad 3 smd rect (at -2.95 -0.975) (size 1.5 0.45) (layers AFRONT F.Paste F.Mask)
      (net 10 "Net-(C23-Pad2)"))
    (pad 2 smd rect (at -2.95 -1.625) (size 1.5 0.45) (layers AFRONT F.Paste F.Mask)
      (net 7 VDD))
    (pad 1 smd rect (at -2.95 -2.275) (size 1.5 0.45) (layers AFRONT F.Paste F.Mask)
      (net 45 A0))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TSSOP-16_4.4x5mm_P0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text Filter-Out (at 133.604 59.436 90) (layer F.SilkS))
  (gr_text Filter-In (at 146.304 75.692 90) (layer F.SilkS))
  (gr_line (start 199.644 35.052) (end 88.9 35.052) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 199.644 123.952) (end 199.644 35.052) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 88.9 123.952) (end 199.644 123.952) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 88.9 35.052) (end 88.9 123.952) (layer Edge.Cuts) (width 0.05))
  (gr_text GND (at 159.004 111.76 180) (layer F.SilkS))
  (gr_text Vout (at 93.472 107.188 270) (layer F.SilkS))
  (gr_text V+ (at 93.472 111.76 270) (layer F.SilkS))
  (gr_text V- (at 117.856 112.776) (layer F.SilkS))
  (gr_text Gain-select (at 138.684 86.36 90) (layer F.SilkS))
  (gr_text "TIA Output" (at 134.62 73.66) (layer F.SilkS))
  (gr_text "Post-amp\nInput" (at 137.668 52.324 90) (layer F.SilkS))
  (gr_text "V-divider\nInput" (at 152.527 41.148) (layer F.SilkS))
  (gr_text "Gain Select\n0 = 50x\n1 = 500x" (at 153.416 67.564) (layer F.SilkS))
  (gr_text "Post-amp Filtered\nOutput" (at 181.737 64.643 90) (layer F.SilkS))
  (gr_text "Post-amp\nOutput" (at 187.452 56.896) (layer F.SilkS))
  (zone (net 1) (net_name GND) (layer GND) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 197.104 122.428) (xy 90.424 122.428) (xy 90.424 38.1) (xy 197.104 38.1)
      )
    )
  )
)
