(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (title_block
    (title "Gain Stage Split-Stage Amp V2.1 (Larger MDM Foot)")
    (date "2023-06-02")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 6)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "Net-(Q22-G)")
  (net 2 "Net-(Q22-D)")
  (net 3 "Net-(Q22-S)")
  (net 4 "Net-(Q12-G)")
  (net 5 "Net-(Q12-D)")
  (net 6 "Net-(Q12-S)")
  (net 7 "Net-(Cf2221-Pad2)")
  (net 8 "/6")
  (net 9 "Net-(Cf1718-Pad2)")
  (net 10 "Net-(Cf2221-Pad1)")
  (net 11 "Net-(Cf1718-Pad1)")
  (net 12 "Net-(Cf821-Pad2)")
  (net 13 "Net-(Cf518-Pad2)")
  (net 14 "Net-(Cf1023-Pad1)")
  (net 15 "Net-(Cc22-Pad1)")
  (net 16 "Net-(Cf316-Pad1)")
  (net 17 "Net-(Cc12-Pad1)")
  (net 18 "/14")
  (net 19 "Net-(Cf1225-Pad2)")
  (net 20 "/15")
  (net 21 "Net-(J24-A)")
  (net 22 "/16")
  (net 23 "/17")
  (net 24 "/18")
  (net 25 "Net-(J2-A)")
  (net 26 "Net-(J2-B)")
  (net 27 "Net-(J11-A)")
  (net 28 "/19")
  (net 29 "/5")
  (net 30 "/1")
  (net 31 "Net-(Cf114-Pad1)")
  (net 32 "/2")
  (net 33 "/3")
  (net 34 "Net-(Cf316-Pad2)")
  (net 35 "/4")
  (net 36 "Net-(Cf416-Pad1)")
  (net 37 "Net-(Cf923-Pad1)")
  (net 38 "Net-(Cf1023-Pad2)")
  (net 39 "Net-(Cf1225-Pad1)")
  (net 40 "Net-(Cf114-Pad2)")
  (net 41 "unconnected-(D4K1-Pad13)")
  (net 42 "unconnected-(D4K2-Pad5)")
  (net 43 "unconnected-(D4K2-Pad6)")
  (net 44 "unconnected-(D4K2-Pad7)")
  (net 45 "unconnected-(D4K2-Pad8)")
  (net 46 "unconnected-(D4K2-Pad13)")
  (net 47 "unconnected-(D4K2-Pad17)")
  (net 48 "unconnected-(D4K2-Pad18)")
  (net 49 "unconnected-(D4K2-Pad19)")
  (net 50 "unconnected-(D4K2-Pad20)")
  (net 51 "unconnected-(D4K2-Pad21)")
  (net 52 "unconnected-(D4K2-Pad22)")
  (net 53 "/12")
  (net 54 "/25")
  (net 55 "/24")
  (net 56 "/23")
  (net 57 "/22")
  (net 58 "/21")
  (net 59 "/20")
  (net 60 "/7")
  (net 61 "/8")
  (net 62 "/9")
  (net 63 "/10")
  (net 64 "/11")
  (net 65 "Net-(J11-B)")
  (net 66 "Net-(J15-A)")
  (net 67 "Net-(J15-B)")
  (net 68 "Net-(J24-B)")
  (net 69 "unconnected-(D4K1-PadMH1)")
  (net 70 "unconnected-(D4K1-PadMH2)")
  (net 71 "unconnected-(D4K2-PadMH1)")
  (net 72 "unconnected-(D4K2-PadMH2)")
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 123.36 65.51 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "Rf6" (at 0 -1.82 90) (layer "F.SilkS"))
    (fp_text value "R=" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 8 "/6") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 5 "Net-(Q12-D)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 150.78 65.597167 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "Rf11" (at 0 -1.82 90) (layer "F.SilkS"))
    (fp_text value "R=" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 64 "/11") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 27 "Net-(J11-A)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad" (layer "F.Cu")
    (at 95.25 107.95)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "M3" (at 0 -3.8) (layer "F.SilkS"))
    (fp_text value "MountingHole_3.2mm_M3_DIN965_Pad" (at 0 3.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Capacitor_SMD:C_1812_4532Metric_Pad1.57x3.40mm_HandSolder" (layer "F.Cu")
    (at 153.55 79.04 180)
    (descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "Cf1225" (at 0 -2.65) (layer "F.SilkS"))
    (fp_text value "C=" (at 0 2.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.1375 0 180) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15873)
      (net 39 "Net-(Cf1225-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 2.1375 0 180) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15873)
      (net 19 "Net-(Cf1225-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1812_4532Metric_Pad1.57x3.40mm_HandSolder" (layer "F.Cu")
    (at 119.3 78.9575 -90)
    (descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "Csc1" (at 0 -2.65 90) (layer "F.SilkS"))
    (fp_text value "C=  " (at 0 2.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.1375 0 270) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15873)
      (net 9 "Net-(Cf1718-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 2.1375 0 270) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15873)
      (net 6 "Net-(Q12-S)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1812_4532Metric_Pad1.57x3.40mm_HandSolder" (layer "F.Cu")
    (at 144.72 72.49)
    (descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "Cf923" (at 0 -2.65) (layer "F.SilkS"))
    (fp_text value "C=" (at 0 2.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.1375 0) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15873)
      (net 37 "Net-(Cf923-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 2.1375 0) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15873)
      (net 14 "Net-(Cf1023-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Dsub:MDM25SBSP" (layer "F.Cu")
    (at 111.35 55.5 180)
    (descr "MDM-25SBSP-4")
    (tags "Connector")
    (property "Arrow Part Number" "MDM-25SBSP")
    (property "Arrow Price/Stock" "https://www.arrow.com/en/products/mdm-25sbsp/itt-corporation?region=nac")
    (property "Height" "14.1")
    (property "Manufacturer_Name" "ITT CANNON")
    (property "Manufacturer_Part_Number" "MDM-25SBSP")
    (property "Mouser Part Number" "965-MDM-25SBSP")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/ITT-Cannon/MDM-25SBSP?qs=%2FPVulymFwT26Zeyn0PUvAA%3D%3D")
    (property "Sheetfile" "SplitStage-4K-V2.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "D-Sub Micro-D Connectors")
    (attr through_hole)
    (fp_text reference "D4K1-F" (at -15.09 7.25) (layer "F.SilkS"))
    (fp_text value "MDM-25-F-BSP" (at -15.24 0.95) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at -15.24 0.95) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 30 "/1") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.54 0 180) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 32 "/2") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at -5.08 0 180) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 33 "/3") (pinfunction "3") (pintype "passive"))
    (pad "4" thru_hole circle (at -7.62 0 180) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 35 "/4") (pinfunction "4") (pintype "passive"))
    (pad "5" thru_hole circle (at -10.16 0 180) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 29 "/5") (pinfunction "5") (pintype "passive"))
    (pad "6" thru_hole circle (at -12.7 0 180) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 8 "/6") (pinfunction "6") (pintype "passive"))
    (pad "7" thru_hole circle (at -15.24 0 180) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 60 "/7") (pinfunction "7") (pintype "passive"))
    (pad "8" thru_hole circle (at -17.78 0 180) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 61 "/8") (pinfunction "8") (pintype "passive"))
    (pad "9" thru_hole circle (at -20.32 0 180) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 62 "/9") (pinfunction "9") (pintype "passive"))
    (pad "10" thru_hole circle (at -22.86 0 180) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 63 "/10") (pinfunction "10") (pintype "passive"))
    (pad "11" thru_hole circle (at -25.4 0 180) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 64 "/11") (pinfunction "11") (pintype "passive"))
    (pad "12" thru_hole circle (at -27.94 0 180) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 53 "/12") (pinfunction "12") (pintype "passive"))
    (pad "13" thru_hole circle (at -30.48 0 180) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 41 "unconnected-(D4K1-Pad13)") (pinfunction "13") (pintype "passive"))
    (pad "14" thru_hole circle (at -1.27 2.54 180) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 18 "/14") (pinfunction "14") (pintype "passive"))
    (pad "15" thru_hole circle (at -3.81 2.54 180) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 20 "/15") (pinfunction "15") (pintype "passive"))
    (pad "16" thru_hole circle (at -6.35 2.54 180) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 22 "/16") (pinfunction "16") (pintype "passive"))
    (pad "17" thru_hole circle (at -8.89 2.54 180) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 23 "/17") (pinfunction "17") (pintype "passive"))
    (pad "18" thru_hole circle (at -11.43 2.54 180) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 24 "/18") (pinfunction "18") (pintype "passive"))
    (pad "19" thru_hole circle (at -13.97 2.54 180) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 28 "/19") (pinfunction "19") (pintype "passive"))
    (pad "20" thru_hole circle (at -16.51 2.54 180) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 59 "/20") (pinfunction "20") (pintype "passive"))
    (pad "21" thru_hole circle (at -19.05 2.54 180) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 58 "/21") (pinfunction "21") (pintype "passive"))
    (pad "22" thru_hole circle (at -21.59 2.54 180) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 57 "/22") (pinfunction "22") (pintype "passive"))
    (pad "23" thru_hole circle (at -24.13 2.54 180) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 56 "/23") (pinfunction "23") (pintype "passive"))
    (pad "24" thru_hole circle (at -26.67 2.54 180) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 55 "/24") (pinfunction "24") (pintype "passive"))
    (pad "25" thru_hole circle (at -29.21 2.54 180) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 54 "/25") (pinfunction "25") (pintype "passive"))
    (pad "MH1" thru_hole circle (at 3.81 1.27 180) (size 4.155 4.155) (drill 2.77) (layers "*.Cu" "*.Mask")
      (net 69 "unconnected-(D4K1-PadMH1)") (pinfunction "MH1") (pintype "passive"))
    (pad "MH2" thru_hole circle (at -34.29 1.27 180) (size 4.155 4.155) (drill 2.77) (layers "*.Cu" "*.Mask")
      (net 70 "unconnected-(D4K1-PadMH2)") (pinfunction "MH2") (pintype "passive"))
    (model "MDM-25SBSP.stp"
      (offset (xyz -15.23999954 -1.299999933 6.760000127))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 130.56 78.75 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "Rsc2" (at 0 -1.82 90) (layer "F.SilkS"))
    (fp_text value "R=  " (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 7 "Net-(Cf2221-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 3 "Net-(Q22-S)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 135.239364 65.597167 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "Rf8" (at 0 -1.82 90) (layer "F.SilkS"))
    (fp_text value "R=" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 61 "/8") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 12 "Net-(Cf821-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 140.419964 65.612167 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "Rf9" (at 0 -1.82 90) (layer "F.SilkS"))
    (fp_text value "R=" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 62 "/9") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 37 "Net-(Cf923-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 113.09 65.52 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "Rf4" (at 0 -1.82 90) (layer "F.SilkS"))
    (fp_text value "R=" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 35 "/4") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 36 "Net-(Cf416-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1812_4532Metric_Pad1.57x3.40mm_HandSolder" (layer "F.Cu")
    (at 100.11 78.8775)
    (descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "Cf114" (at -0.01 2.6625) (layer "F.SilkS"))
    (fp_text value "C=" (at 0 2.65) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.1375 0) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15873)
      (net 31 "Net-(Cf114-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 2.1375 0) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15873)
      (net 40 "Net-(Cf114-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 139.63 78.92 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "Rgn2" (at 0 -1.82 90) (layer "F.SilkS"))
    (fp_text value "R=" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 12 "Net-(Cf821-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 2 "Net-(Q22-D)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1812_4532Metric_Pad1.57x3.40mm_HandSolder" (layer "F.Cu")
    (at 103.4 72.53 180)
    (descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "Cf316" (at -0.0547 2.606) (layer "F.SilkS"))
    (fp_text value "C=" (at 0.2653 -2.754) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.1375 0 180) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15873)
      (net 16 "Net-(Cf316-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 2.1375 0 180) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15873)
      (net 34 "Net-(Cf316-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1812_4532Metric_Pad1.57x3.40mm_HandSolder" (layer "F.Cu")
    (at 135.05 79.0275 -90)
    (descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "Csc2" (at 0 -2.65 90) (layer "F.SilkS"))
    (fp_text value "C=  " (at 0 2.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.1375 0 270) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15873)
      (net 7 "Net-(Cf2221-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 2.1375 0 270) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15873)
      (net 3 "Net-(Q22-S)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1812_4532Metric_Pad1.57x3.40mm_HandSolder" (layer "F.Cu")
    (at 110.07 72.54 180)
    (descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "Cf416" (at 0.0485 2.576) (layer "F.SilkS"))
    (fp_text value "C=" (at 0.0185 -2.754) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.1375 0 180) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15873)
      (net 36 "Net-(Cf416-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 2.1375 0 180) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15873)
      (net 16 "Net-(Cf316-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1812_4532Metric_Pad1.57x3.40mm_HandSolder" (layer "F.Cu")
    (at 141.72 85.67 180)
    (descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "Cc22" (at 0 -2.65) (layer "F.SilkS"))
    (fp_text value "C=" (at 0 2.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.1375 0 180) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15873)
      (net 15 "Net-(Cc22-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 2.1375 0 180) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15873)
      (net 1 "Net-(Q22-G)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad" (layer "F.Cu")
    (at 158.75 107.95)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "M3" (at 0 -3.8) (layer "F.SilkS"))
    (fp_text value "MountingHole_3.2mm_M3_DIN965_Pad" (at 0 3.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Transistor_Power_Module:CryoHEMTTransistor" (layer "F.Cu")
    (at 115.69 85.5425 90)
    (property "Sheetfile" "SplitStage-4K-V2.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "N-JFET transistor, gate/drain/source")
    (property "ki_keywords" "transistor NJFET N-JFET")
    (attr smd)
    (fp_text reference "Q12" (at 0.605 3.69 90 unlocked) (layer "F.SilkS"))
    (fp_text value "200pF" (at 0.425 -1.77 90 unlocked) (layer "F.Fab"))
    (fp_text user "G" (at -2.475 -0.32 90) (layer "F.SilkS"))
    (fp_text user "D" (at -2.475 2.22 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0.7 0.95) (layer "F.Fab"))
    (pad "1" smd rect (at -0.65 0 90) (size 1.65 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "Net-(Q12-G)") (pinfunction "G") (pintype "input"))
    (pad "2" smd rect (at -0.65 1.9 90) (size 1.65 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "Net-(Q12-D)") (pinfunction "D") (pintype "passive"))
    (pad "3" smd rect (at 2.06 0.95 90) (size 1.65 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "Net-(Q12-S)") (pinfunction "S") (pintype "passive"))
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad" (layer "F.Cu")
    (at 158.75 44.45)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "M3" (at 0.01 3.94) (layer "F.SilkS"))
    (fp_text value "MountingHole_3.2mm_M3_DIN965_Pad" (at 0 3.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 130.054764 65.612167 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "Rf7" (at 0 -1.82 90) (layer "F.SilkS"))
    (fp_text value "R=" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 60 "/7") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 2 "Net-(Q22-D)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1812_4532Metric_Pad1.57x3.40mm_HandSolder" (layer "F.Cu")
    (at 123.5175 72.58)
    (descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "Cf619" (at 0 -2.65) (layer "F.SilkS"))
    (fp_text value "C=" (at 0 2.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.1375 0) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15873)
      (net 5 "Net-(Q12-D)") (pintype "passive"))
    (pad "2" smd roundrect (at 2.1375 0) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15873)
      (net 6 "Net-(Q12-S)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1812_4532Metric_Pad1.57x3.40mm_HandSolder" (layer "F.Cu")
    (at 108.9625 84.82)
    (descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "Cc12" (at 0 -2.65) (layer "F.SilkS"))
    (fp_text value "C=" (at 0 2.65) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.1375 0) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15873)
      (net 17 "Net-(Cc12-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 2.1375 0) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15873)
      (net 4 "Net-(Q12-G)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 123.87 78.9075 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "Rsc1" (at 0 -1.82 90) (layer "F.SilkS"))
    (fp_text value "R=  " (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 9 "Net-(Cf1718-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 6 "Net-(Q12-S)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1812_4532Metric_Pad1.57x3.40mm_HandSolder" (layer "F.Cu")
    (at 116.8 72.59)
    (descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "Cf518" (at 0 -2.65) (layer "F.SilkS"))
    (fp_text value "C=" (at 0 2.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.1375 0) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15873)
      (net 9 "Net-(Cf1718-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 2.1375 0) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15873)
      (net 13 "Net-(Cf518-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 155.940764 65.600746 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "Rf12" (at 0 -1.82 90) (layer "F.SilkS"))
    (fp_text value "R=" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 53 "/12") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 39 "Net-(Cf1225-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad" (layer "F.Cu")
    (at 95.25 44.45)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "M3" (at -0.03 3.97) (layer "F.SilkS"))
    (fp_text value "MountingHole_3.2mm_M3_DIN965_Pad" (at 0 3.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 156.32 72.67 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Jumper, 2-pole, closed/bridged")
    (property "ki_keywords" "Jumper SPST")
    (attr smd)
    (fp_text reference "J11" (at 0 -1.82 90) (layer "F.SilkS"))
    (fp_text value "R=" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 27 "Net-(J11-A)") (pinfunction "A") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 65 "Net-(J11-B)") (pinfunction "B") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 107.77 65.56 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "Rf3" (at 0 -1.82 90) (layer "F.SilkS"))
    (fp_text value "R=" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 33 "/3") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 34 "Net-(Cf316-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 97.36 65.61 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "Rf1" (at 0 -1.82 90) (layer "F.SilkS"))
    (fp_text value "R=" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 30 "/1") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 31 "Net-(Cf114-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 97.6075 72.57 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Jumper, 2-pole, closed/bridged")
    (property "ki_keywords" "Jumper SPST")
    (attr smd)
    (fp_text reference "J2" (at 0 -1.82 90) (layer "F.SilkS"))
    (fp_text value "R=" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 25 "Net-(J2-A)") (pinfunction "A") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 26 "Net-(J2-B)") (pinfunction "B") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Transistor_Power_Module:CryoHEMTTransistor" (layer "F.Cu")
    (at 135.6 86.77 180)
    (property "Sheetfile" "SplitStage-4K-V2.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "N-JFET transistor, gate/drain/source")
    (property "ki_keywords" "transistor NJFET N-JFET")
    (attr smd)
    (fp_text reference "Q22" (at 0.63 -1.84 unlocked) (layer "F.SilkS"))
    (fp_text value "200pF" (at 0.45 3.6 unlocked) (layer "F.Fab"))
    (fp_text user "G" (at -2.475 -0.32) (layer "F.SilkS"))
    (fp_text user "D" (at -2.475 2.22) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0.7 0.95 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.65 0 180) (size 1.65 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "Net-(Q22-G)") (pinfunction "G") (pintype "input"))
    (pad "2" smd rect (at -0.65 1.9 180) (size 1.65 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "Net-(Q22-D)") (pinfunction "D") (pintype "passive"))
    (pad "3" smd rect (at 2.06 0.95 180) (size 1.65 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "Net-(Q22-S)") (pinfunction "S") (pintype "passive"))
  )
  (footprint "Capacitor_SMD:C_1812_4532Metric_Pad1.57x3.40mm_HandSolder" (layer "F.Cu")
    (at 138.0525 72.49 180)
    (descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "Cf821" (at 0.0945 2.636) (layer "F.SilkS"))
    (fp_text value "C=" (at -0.0755 -2.754) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.1375 0 180) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15873)
      (net 7 "Net-(Cf2221-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 2.1375 0 180) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15873)
      (net 12 "Net-(Cf821-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 106.94 78.9375 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "Rfol1" (at 0 -1.82 90) (layer "F.SilkS"))
    (fp_text value "R=" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 16 "Net-(Cf316-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 17 "Net-(Cc12-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 102.61 65.56 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "Rf2" (at 0 -1.82 90) (layer "F.SilkS"))
    (fp_text value "R=" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 32 "/2") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 25 "Net-(J2-A)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Dsub:MDM25PBSP" (layer "F.Cu")
    (at 111.35 96.78)
    (descr "MDM-25PBSP-1")
    (tags "Connector")
    (property "Height" "13.74")
    (property "Manufacturer_Name" "ITT CANNON")
    (property "Manufacturer_Part_Number" "MDM-25PBSP")
    (property "Mouser Part Number" "965-MDM-25PBSP")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/ITT-Cannon/MDM-25PBSP?qs=%2FPVulymFwT3mrCwbZuIR5w%3D%3D")
    (property "Sheetfile" "SplitStage-4K-V2.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "D-Sub Micro-D Connectors MICRO 25 M PC JACKP")
    (attr through_hole)
    (fp_text reference "D4K2-M" (at 15.77 -4.84) (layer "F.SilkS"))
    (fp_text value "MDM-25-F-BSP" (at 15.24 1.27) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 15.24 1.27) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 31 "Net-(Cf114-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 26 "Net-(J2-B)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at 5.08 0) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 34 "Net-(Cf316-Pad2)") (pinfunction "3") (pintype "passive"))
    (pad "4" thru_hole circle (at 7.62 0) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 36 "Net-(Cf416-Pad1)") (pinfunction "4") (pintype "passive"))
    (pad "5" thru_hole circle (at 10.16 0) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 42 "unconnected-(D4K2-Pad5)") (pinfunction "5") (pintype "passive"))
    (pad "6" thru_hole circle (at 12.7 0) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 43 "unconnected-(D4K2-Pad6)") (pinfunction "6") (pintype "passive"))
    (pad "7" thru_hole circle (at 15.24 0) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 44 "unconnected-(D4K2-Pad7)") (pinfunction "7") (pintype "passive"))
    (pad "8" thru_hole circle (at 17.78 0) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 45 "unconnected-(D4K2-Pad8)") (pinfunction "8") (pintype "passive"))
    (pad "9" thru_hole circle (at 20.32 0) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 37 "Net-(Cf923-Pad1)") (pinfunction "9") (pintype "passive"))
    (pad "10" thru_hole circle (at 22.86 0) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 38 "Net-(Cf1023-Pad2)") (pinfunction "10") (pintype "passive"))
    (pad "11" thru_hole circle (at 25.4 0) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 65 "Net-(J11-B)") (pinfunction "11") (pintype "passive"))
    (pad "12" thru_hole circle (at 27.94 0) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 39 "Net-(Cf1225-Pad1)") (pinfunction "12") (pintype "passive"))
    (pad "13" thru_hole circle (at 30.48 0) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 46 "unconnected-(D4K2-Pad13)") (pinfunction "13") (pintype "passive"))
    (pad "14" thru_hole circle (at 1.27 2.54) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 40 "Net-(Cf114-Pad2)") (pinfunction "14") (pintype "passive"))
    (pad "15" thru_hole circle (at 3.81 2.54) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 67 "Net-(J15-B)") (pinfunction "15") (pintype "passive"))
    (pad "16" thru_hole circle (at 6.35 2.54) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 17 "Net-(Cc12-Pad1)") (pinfunction "16") (pintype "passive"))
    (pad "17" thru_hole circle (at 8.89 2.54) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 47 "unconnected-(D4K2-Pad17)") (pinfunction "17") (pintype "passive"))
    (pad "18" thru_hole circle (at 11.43 2.54) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 48 "unconnected-(D4K2-Pad18)") (pinfunction "18") (pintype "passive"))
    (pad "19" thru_hole circle (at 13.97 2.54) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 49 "unconnected-(D4K2-Pad19)") (pinfunction "19") (pintype "passive"))
    (pad "20" thru_hole circle (at 16.51 2.54) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 50 "unconnected-(D4K2-Pad20)") (pinfunction "20") (pintype "passive"))
    (pad "21" thru_hole circle (at 19.05 2.54) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 51 "unconnected-(D4K2-Pad21)") (pinfunction "21") (pintype "passive"))
    (pad "22" thru_hole circle (at 21.59 2.54) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 52 "unconnected-(D4K2-Pad22)") (pinfunction "22") (pintype "passive"))
    (pad "23" thru_hole circle (at 24.13 2.54) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 15 "Net-(Cc22-Pad1)") (pinfunction "23") (pintype "passive"))
    (pad "24" thru_hole circle (at 26.67 2.54) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 68 "Net-(J24-B)") (pinfunction "24") (pintype "passive"))
    (pad "25" thru_hole circle (at 29.21 2.54) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 19 "Net-(Cf1225-Pad2)") (pinfunction "25") (pintype "passive"))
    (pad "MH1" thru_hole circle (at -3.81 1.27) (size 3.96 3.96) (drill 2.64) (layers "*.Cu" "*.Mask")
      (net 71 "unconnected-(D4K2-PadMH1)") (pinfunction "MH1") (pintype "passive"))
    (pad "MH2" thru_hole circle (at 34.29 1.27) (size 3.96 3.96) (drill 2.64) (layers "*.Cu" "*.Mask")
      (net 72 "unconnected-(D4K2-PadMH2)") (pinfunction "MH2") (pintype "passive"))
    (model "MDM-25PBSP.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1812_4532Metric_Pad1.57x3.40mm_HandSolder" (layer "F.Cu")
    (at 151.41 72.52)
    (descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "Cf1023" (at 0 -2.65) (layer "F.SilkS"))
    (fp_text value "C=" (at 0 2.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.1375 0) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15873)
      (net 14 "Net-(Cf1023-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 2.1375 0) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15873)
      (net 38 "Net-(Cf1023-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1812_4532Metric_Pad1.57x3.40mm_HandSolder" (layer "F.Cu")
    (at 131.35 72.53 180)
    (descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "Cf720" (at 0 -2.65) (layer "F.SilkS"))
    (fp_text value "C=" (at 0 2.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.1375 0 180) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15873)
      (net 2 "Net-(Q22-D)") (pintype "passive"))
    (pad "2" smd roundrect (at 2.1375 0 180) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15873)
      (net 3 "Net-(Q22-S)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 147.44 79 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "Rfol2" (at 0 -1.82 90) (layer "F.SilkS"))
    (fp_text value "R=" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 14 "Net-(Cf1023-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 15 "Net-(Cc22-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 143.54 78.94 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "Rgt2" (at 0 -1.82 90) (layer "F.SilkS"))
    (fp_text value "R=" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 10 "Net-(Cf2221-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 1 "Net-(Q22-G)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 145.612564 65.597167 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "Rf10" (at 0 -1.82 90) (layer "F.SilkS"))
    (fp_text value "R=" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 63 "/10") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 38 "Net-(Cf1023-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 110.5 78.8975 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "Rgt1" (at 0 -1.82 90) (layer "F.SilkS"))
    (fp_text value "R=" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 11 "Net-(Cf1718-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 4 "Net-(Q12-G)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 118.14 65.54 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "Rf5" (at 0 -1.82 90) (layer "F.SilkS"))
    (fp_text value "R=" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 29 "/5") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 13 "Net-(Cf518-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 114.46 78.8975 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "Rgn1" (at 0 -1.82 90) (layer "F.SilkS"))
    (fp_text value "R=" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 13 "Net-(Cf518-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 5 "Net-(Q12-D)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "B.Cu")
    (at 123.36 65.51 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "Rf19" (at 0 1.82 90) (layer "B.SilkS"))
    (fp_text value "R=" (at 0 -1.82 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.192308)
      (net 28 "/19") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.192308)
      (net 6 "Net-(Q12-S)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "B.Cu")
    (at 102.61 65.56 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "Rf15" (at 0 1.82 90) (layer "B.SilkS"))
    (fp_text value "R=" (at 0 -1.82 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.192308)
      (net 20 "/15") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.192308)
      (net 66 "Net-(J15-A)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "B.Cu")
    (at 145.61 65.6 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "Rf23" (at 0 1.82 90) (layer "B.SilkS"))
    (fp_text value "R=" (at 0 -1.82 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.192308)
      (net 56 "/23") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.192308)
      (net 14 "Net-(Cf1023-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "B.Cu")
    (at 97.36 65.61 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "Rf14" (at 0 1.82 90) (layer "B.SilkS"))
    (fp_text value "R=" (at 0 -1.82 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.192308)
      (net 18 "/14") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.192308)
      (net 40 "Net-(Cf114-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "B.Cu")
    (at 97.6075 72.54 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Jumper, 2-pole, closed/bridged")
    (property "ki_keywords" "Jumper SPST")
    (attr smd)
    (fp_text reference "J15" (at 0 1.82 90) (layer "B.SilkS"))
    (fp_text value "R=" (at 0 -1.82 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.192308)
      (net 66 "Net-(J15-A)") (pinfunction "A") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.192308)
      (net 67 "Net-(J15-B)") (pinfunction "B") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "B.Cu")
    (at 113.09 65.52 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "Rf17" (at 0 1.82 90) (layer "B.SilkS"))
    (fp_text value "R=" (at 0 -1.82 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.192308)
      (net 23 "/17") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.192308)
      (net 11 "Net-(Cf1718-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "B.Cu")
    (at 107.77 65.56 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "Rf16" (at 0 1.82 90) (layer "B.SilkS"))
    (fp_text value "R=" (at 0 -1.82 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.192308)
      (net 22 "/16") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.192308)
      (net 16 "Net-(Cf316-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "B.Cu")
    (at 140.42 65.6 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "Rf22" (at 0 1.82 90) (layer "B.SilkS"))
    (fp_text value "R=" (at 0 -1.82 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.192308)
      (net 57 "/22") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.192308)
      (net 10 "Net-(Cf2221-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "B.Cu")
    (at 150.77 65.59 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "Rf24" (at 0 1.82 90) (layer "B.SilkS"))
    (fp_text value "R=" (at 0 -1.82 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.192308)
      (net 55 "/24") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.192308)
      (net 21 "Net-(J24-A)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "B.Cu")
    (at 130.05 65.62 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "Rf20" (at 0 1.82 90) (layer "B.SilkS"))
    (fp_text value "R=" (at 0 -1.82 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.192308)
      (net 59 "/20") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.192308)
      (net 3 "Net-(Q22-S)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1812_4532Metric_Pad1.57x3.40mm_HandSolder" (layer "B.Cu")
    (at 144.72 72.5)
    (descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "Cf2221" (at -0.0177 -2.636) (layer "B.SilkS"))
    (fp_text value "C=" (at 0.0823 2.784) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -2.1375 0) (size 1.575 3.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.15873)
      (net 10 "Net-(Cf2221-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 2.1375 0) (size 1.575 3.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.15873)
      (net 7 "Net-(Cf2221-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "B.Cu")
    (at 135.24 65.6 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "Rf21" (at 0 1.82 90) (layer "B.SilkS"))
    (fp_text value "R=" (at 0 -1.82 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.192308)
      (net 58 "/21") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.192308)
      (net 7 "Net-(Cf2221-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "B.Cu")
    (at 118.14 65.54 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "Rf18" (at 0 1.82 90) (layer "B.SilkS"))
    (fp_text value "R=" (at 0 -1.82 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.192308)
      (net 24 "/18") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.192308)
      (net 9 "Net-(Cf1718-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1812_4532Metric_Pad1.57x3.40mm_HandSolder" (layer "B.Cu")
    (at 110.0825 72.56)
    (descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "Cf1718" (at -0.0017 -2.666) (layer "B.SilkS"))
    (fp_text value "C=" (at -0.0317 2.724) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -2.1375 0) (size 1.575 3.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.15873)
      (net 11 "Net-(Cf1718-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 2.1375 0) (size 1.575 3.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.15873)
      (net 9 "Net-(Cf1718-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "B.Cu")
    (at 156.31 72.67 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Jumper, 2-pole, closed/bridged")
    (property "ki_keywords" "Jumper SPST")
    (attr smd)
    (fp_text reference "J24" (at 0 1.82 90) (layer "B.SilkS"))
    (fp_text value "R=" (at 0 -1.82 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.192308)
      (net 21 "Net-(J24-A)") (pinfunction "A") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.192308)
      (net 68 "Net-(J24-B)") (pinfunction "B") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "B.Cu")
    (at 155.94 65.61 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "Rf25" (at 0 1.82 90) (layer "B.SilkS"))
    (fp_text value "R=" (at 0 -1.82 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.192308)
      (net 54 "/25") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.192308)
      (net 19 "Net-(Cf1225-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_rect (start 89.94 39.95) (end 164.05 112.72)
    (fill none) (layer "Edge.Cuts"))
  (gr_text "Amp 2" (at 157.04 61.37) (layer "F.SilkS"))
  (gr_text "Amp 1\n" (at 92.68 61.11) (layer "F.SilkS"))
  (gr_text "SPLENDOR Split-Stage Amplifier\n4K Gain Stage V2.1\nAnczarski 2023-06-02" (at 130.5 109.88) (layer "F.SilkS"))
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.508))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 9.999999))
    (polygon
      (pts
        (xy 89.94 39.95)
        (xy 89.94 112.72)
        (xy 164.05 112.72)
        (xy 164.05 39.95)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.5)
    (priority 1)
    (connect_pads (clearance 0.508))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 9.999999))
    (polygon
      (pts
        (xy 103.54 48.3)
        (xy 149.7 48.37)
        (xy 159.06 62.05)
        (xy 159.04 92.96)
        (xy 149.69 103.89)
        (xy 103.5 103.94)
        (xy 94.99 93.01)
        (xy 94.8 60.85)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.5)
    (priority 1)
    (connect_pads (clearance 0.508))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 9.999998))
    (polygon
      (pts
        (xy 103.540108 48.292924)
        (xy 149.700108 48.362924)
        (xy 159.060108 62.042924)
        (xy 159.040108 92.952924)
        (xy 149.690108 103.882924)
        (xy 103.500108 103.932924)
        (xy 94.990108 93.002924)
        (xy 94.800108 60.842924)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.508))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 9.999998))
    (polygon
      (pts
        (xy 89.94 39.95)
        (xy 89.94 112.72)
        (xy 164.05 112.72)
        (xy 164.05 39.95)
      )
    )
  )
)
