(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 20)
    (no_connects 0)
    (area 131.750999 97.968999 147.141001 119.455001)
    (thickness 1.6)
    (drawings 17)
    (tracks 113)
    (zones 0)
    (modules 6)
    (nets 9)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VCC)
  (net 2 GND)
  (net 3 "Net-(IC1-Pad1)")
  (net 4 "Net-(IC1-Pad2)")
  (net 5 "Net-(IC1-Pad3)")
  (net 6 "Net-(IC1-Pad5)")
  (net 7 "Net-(IC1-Pad6)")
  (net 8 "Net-(IC1-Pad7)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(IC1-Pad1)")
    (add_net "Net-(IC1-Pad2)")
    (add_net "Net-(IC1-Pad3)")
    (add_net "Net-(IC1-Pad5)")
    (add_net "Net-(IC1-Pad6)")
    (add_net "Net-(IC1-Pad7)")
    (add_net VCC)
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5A6ABFB7)
    (at 138.684 103.632 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at -1.778 1.524 180) (layer F.SilkS))
    (fp_text value 10k (at 0.254 15.24 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(IC1-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5A6A3DF7)
    (at 144.78 103.632 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0.762 1.524 180) (layer F.SilkS))
    (fp_text value 0.1u (at -2.54 15.24 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIJ-8_5.3x5.3mm_Pitch1.27mm (layer F.Cu) (tedit 5A6AC00A)
    (at 141.732 108.966)
    (descr "8-Lead Plastic Small Outline (SM) - Medium, 5.28 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference IC1 (at 0 -3.68) (layer F.SilkS))
    (fp_text value ATTINY85-S (at -0.762 -12.446) (layer F.Fab))
    (pad 1 smd rect (at -3.65 -1.905) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(IC1-Pad1)"))
    (pad 2 smd rect (at -3.65 -0.635) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(IC1-Pad2)"))
    (pad 3 smd rect (at -3.65 0.635) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(IC1-Pad3)"))
    (pad 4 smd rect (at -3.65 1.905) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 3.65 1.905) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(IC1-Pad5)"))
    (pad 6 smd rect (at 3.65 0.635) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(IC1-Pad6)"))
    (pad 7 smd rect (at 3.65 -0.635) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(IC1-Pad7)"))
    (pad 8 smd rect (at 3.65 -1.905) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (model Housings_SOIC.3dshapes/SOIJ-8_5.3x5.3mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03 (layer F.Cu) (tedit 57FE94F2)
    (at 138.684 117.602 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference ISP1 (at 0 7.366 90) (layer F.SilkS))
    (fp_text value ISP (at -3.81 -0.762 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(IC1-Pad6)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(IC1-Pad7)"))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(IC1-Pad5)"))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(IC1-Pad1)"))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x03.wrl
      (at (xyz 0.05 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x08_Pitch2.54mm (layer F.Cu) (tedit 5A6A3F3D)
    (at 133.35 99.822)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference J1 (at -1.016 -4.318) (layer F.SilkS) hide)
    (fp_text value CONN_01X08 (at -4.318 22.86) (layer F.Fab))
    (fp_text user %R (at -2.794 9.144 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(IC1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(IC1-Pad3)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(IC1-Pad2)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(IC1-Pad7)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(IC1-Pad6)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(IC1-Pad5)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x08_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_SMD:SW_DIP_x1_W7.62mm_Slide_Copal_CHS-B (layer F.Cu) (tedit 5A6A45D5)
    (at 141.986 99.822)
    (descr "1x-dip-switch, Slide, row spacing 7.62 mm (300 mils), Copal_CHS-B")
    (tags "DIP Switch Slide 7.62mm 300mil Copal_CHS-B")
    (attr smd)
    (fp_text reference SW1 (at 0.254 0) (layer F.SilkS))
    (fp_text value SW_Push (at 8.636 -3.302) (layer F.Fab))
    (fp_text user %R (at 2.1 0 90) (layer F.Fab))
    (pad 1 smd rect (at -3.81 0) (size 1.6 0.76) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(IC1-Pad1)"))
    (pad 2 smd rect (at 3.81 0) (size 1.6 0.76) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Buttons_Switches_SMD.3dshapes/SW_DIP_x1_W7.62mm_Slide_Copal_CHS-B.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (dimension 21.336 (width 0.3) (layer Dwgs.User)
    (gr_text "21,336 mm" (at 153.242 108.712 90) (layer Dwgs.User))
    (feature1 (pts (xy 147.828 98.044) (xy 154.592 98.044)))
    (feature2 (pts (xy 147.828 119.38) (xy 154.592 119.38)))
    (crossbar (pts (xy 151.892 119.38) (xy 151.892 98.044)))
    (arrow1a (pts (xy 151.892 98.044) (xy 152.478421 99.170504)))
    (arrow1b (pts (xy 151.892 98.044) (xy 151.305579 99.170504)))
    (arrow2a (pts (xy 151.892 119.38) (xy 152.478421 118.253496)))
    (arrow2b (pts (xy 151.892 119.38) (xy 151.305579 118.253496)))
  )
  (gr_text RES (at 134.62 100.076) (layer F.SilkS))
  (gr_text GN (at 145.034 114.3) (layer F.SilkS))
  (gr_text GND (at 143.51 113.03 180) (layer B.SilkS))
  (gr_text "www.arduinoslovakia.eu\n2018/01\nATtiny85 board" (at 138.176 101.092 90) (layer B.SilkS))
  (dimension 15.24 (width 0.3) (layer Dwgs.User)
    (gr_text "15,240 mm" (at 139.446 126.572) (layer Dwgs.User))
    (feature1 (pts (xy 147.066 120.396) (xy 147.066 127.922)))
    (feature2 (pts (xy 131.826 120.396) (xy 131.826 127.922)))
    (crossbar (pts (xy 131.826 125.222) (xy 147.066 125.222)))
    (arrow1a (pts (xy 147.066 125.222) (xy 145.939496 125.808421)))
    (arrow1b (pts (xy 147.066 125.222) (xy 145.939496 124.635579)))
    (arrow2a (pts (xy 131.826 125.222) (xy 132.952504 125.808421)))
    (arrow2b (pts (xy 131.826 125.222) (xy 132.952504 124.635579)))
  )
  (gr_text 4 (at 135.128 107.442) (layer F.SilkS))
  (gr_text 3 (at 135.128 109.982) (layer F.SilkS))
  (gr_text 2 (at 135.128 112.522) (layer F.SilkS))
  (gr_text 1 (at 135.128 115.062) (layer F.SilkS))
  (gr_text 0 (at 135.128 117.602) (layer F.SilkS))
  (gr_text GND (at 134.62 104.902) (layer F.SilkS))
  (gr_text VCC (at 134.62 102.362) (layer F.SilkS))
  (gr_line (start 147.066 98.044) (end 131.826 98.044) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 147.066 119.38) (end 147.066 98.044) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 131.826 119.38) (end 147.066 119.38) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 131.826 98.044) (end 131.826 119.38) (angle 90) (layer Edge.Cuts) (width 0.15))
)
