(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 30)
    (no_connects 0)
    (area 113.5826 82.804266 156.260001 112.775733)
    (thickness 1.6002)
    (drawings 35)
    (tracks 185)
    (zones 0)
    (modules 3)
    (nets 31)
  )
  (page A4)
  (layers
    (0 Top signal)
    (31 Bottom signal)
    (33 F.Adhes user)
    (35 F.Paste user)
    (37 F.SilkS user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (47 F.CrtYd user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.1 1.1)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010a8_ffffffff)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory plots))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad1)")
  (net 2 "Net-(J1-Pad3)")
  (net 3 "Net-(J1-Pad5)")
  (net 4 "Net-(J1-Pad7)")
  (net 5 "Net-(J1-Pad9)")
  (net 6 "Net-(J1-Pad11)")
  (net 7 "Net-(J1-Pad13)")
  (net 8 "Net-(J1-Pad15)")
  (net 9 "Net-(J1-Pad17)")
  (net 10 "Net-(J1-Pad19)")
  (net 11 "Net-(J1-Pad21)")
  (net 12 "Net-(J1-Pad23)")
  (net 13 "Net-(J1-Pad25)")
  (net 14 "Net-(J1-Pad27)")
  (net 15 "Net-(J1-Pad29)")
  (net 16 "Net-(J1-Pad2)")
  (net 17 "Net-(J1-Pad4)")
  (net 18 "Net-(J1-Pad6)")
  (net 19 "Net-(J1-Pad8)")
  (net 20 "Net-(J1-Pad10)")
  (net 21 "Net-(J1-Pad12)")
  (net 22 "Net-(J1-Pad14)")
  (net 23 "Net-(J1-Pad16)")
  (net 24 "Net-(J1-Pad18)")
  (net 25 "Net-(J1-Pad20)")
  (net 26 "Net-(J1-Pad22)")
  (net 27 "Net-(J1-Pad24)")
  (net 28 "Net-(J1-Pad26)")
  (net 29 "Net-(J1-Pad28)")
  (net 30 "Net-(J1-Pad30)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad11)")
    (add_net "Net-(J1-Pad12)")
    (add_net "Net-(J1-Pad13)")
    (add_net "Net-(J1-Pad14)")
    (add_net "Net-(J1-Pad15)")
    (add_net "Net-(J1-Pad16)")
    (add_net "Net-(J1-Pad17)")
    (add_net "Net-(J1-Pad18)")
    (add_net "Net-(J1-Pad19)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad20)")
    (add_net "Net-(J1-Pad21)")
    (add_net "Net-(J1-Pad22)")
    (add_net "Net-(J1-Pad23)")
    (add_net "Net-(J1-Pad24)")
    (add_net "Net-(J1-Pad25)")
    (add_net "Net-(J1-Pad26)")
    (add_net "Net-(J1-Pad27)")
    (add_net "Net-(J1-Pad28)")
    (add_net "Net-(J1-Pad29)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad30)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J1-Pad9)")
  )
  (module Pin_Headers:Pin_Header_Straight_1x15_Pitch2.54mm locked placed (layer Top) (tedit 58CD4EC2)
    (at 152.4 107.79 270)
    (descr "Through hole straight pin header, 1x15, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x15 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33 270) (layer F.SilkS))
    (fp_text value CONN_01X15 (at 0 37.89 270) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad3)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad5)"))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad7)"))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad9)"))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad11)"))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad13)"))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad15)"))
    (pad 9 thru_hole oval (at 0 20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad17)"))
    (pad 10 thru_hole oval (at 0 22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad19)"))
    (pad 11 thru_hole oval (at 0 25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad21)"))
    (pad 12 thru_hole oval (at 0 27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad23)"))
    (pad 13 thru_hole oval (at 0 30.48 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-Pad25)"))
    (pad 14 thru_hole oval (at 0 33.02 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-Pad27)"))
    (pad 15 thru_hole oval (at 0 35.56 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad29)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x15_Pitch2.54mm.wrl
      (at (xyz 0 -0.7 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x15_Pitch2.54mm locked placed (layer Top) (tedit 58CD4EC2)
    (at 152.4 87.79 270)
    (descr "Through hole straight pin header, 1x15, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x15 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33 270) (layer F.SilkS))
    (fp_text value CONN_01X15 (at 0 37.89 270) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J1-Pad4)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J1-Pad6)"))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J1-Pad8)"))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(J1-Pad10)"))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(J1-Pad12)"))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(J1-Pad14)"))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(J1-Pad16)"))
    (pad 9 thru_hole oval (at 0 20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(J1-Pad18)"))
    (pad 10 thru_hole oval (at 0 22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(J1-Pad20)"))
    (pad 11 thru_hole oval (at 0 25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(J1-Pad22)"))
    (pad 12 thru_hole oval (at 0 27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(J1-Pad24)"))
    (pad 13 thru_hole oval (at 0 30.48 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(J1-Pad26)"))
    (pad 14 thru_hole oval (at 0 33.02 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(J1-Pad28)"))
    (pad 15 thru_hole oval (at 0 35.56 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(J1-Pad30)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x15_Pitch2.54mm.wrl
      (at (xyz 0 -0.7 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Molex500913-0402:Molex_SlimStack_Plug_2x15_Pitch0.5mm_501920-3001 placed (layer Top) (tedit 590981CF)
    (at 147.32 97.79 270)
    (descr "Molex SlimStack plug, 02x15 contacts 0.5mm pitch 4mm height, http://www.molex.com/pdm_docs/sd/5019204001_sd.pdf")
    (tags "connector molex slimstack 501920-3001")
    (attr smd)
    (fp_text reference J1 (at 0 -3.5 270) (layer F.SilkS))
    (fp_text value CONN_02X15 (at 0 3.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad x smd rect (at 3.64 1.8 270) (size 1 1) (layers Top F.Paste F.Mask))
    (pad x smd rect (at -3.64 1.8 270) (size 1 1) (layers Top F.Paste F.Mask))
    (pad x smd rect (at 3.64 -1.8 270) (size 1 1) (layers Top F.Paste F.Mask))
    (pad 1 smd rect (at -2.8 -1.8 270) (size 0.22 1) (layers Top F.Paste F.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 3 smd rect (at -2.4 -1.8 270) (size 0.22 1) (layers Top F.Paste F.Mask)
      (net 2 "Net-(J1-Pad3)"))
    (pad 5 smd rect (at -2 -1.8 270) (size 0.22 1) (layers Top F.Paste F.Mask)
      (net 3 "Net-(J1-Pad5)"))
    (pad 7 smd rect (at -1.6 -1.8 270) (size 0.22 1) (layers Top F.Paste F.Mask)
      (net 4 "Net-(J1-Pad7)"))
    (pad 9 smd rect (at -1.2 -1.8 270) (size 0.22 1) (layers Top F.Paste F.Mask)
      (net 5 "Net-(J1-Pad9)"))
    (pad 11 smd rect (at -0.8 -1.8 270) (size 0.22 1) (layers Top F.Paste F.Mask)
      (net 6 "Net-(J1-Pad11)"))
    (pad 13 smd rect (at -0.4 -1.8 270) (size 0.22 1) (layers Top F.Paste F.Mask)
      (net 7 "Net-(J1-Pad13)"))
    (pad 15 smd rect (at 0 -1.8 270) (size 0.22 1) (layers Top F.Paste F.Mask)
      (net 8 "Net-(J1-Pad15)"))
    (pad 17 smd rect (at 0.4 -1.8 270) (size 0.22 1) (layers Top F.Paste F.Mask)
      (net 9 "Net-(J1-Pad17)"))
    (pad 19 smd rect (at 0.8 -1.8 270) (size 0.22 1) (layers Top F.Paste F.Mask)
      (net 10 "Net-(J1-Pad19)"))
    (pad 21 smd rect (at 1.2 -1.8 270) (size 0.22 1) (layers Top F.Paste F.Mask)
      (net 11 "Net-(J1-Pad21)"))
    (pad 23 smd rect (at 1.6 -1.8 270) (size 0.22 1) (layers Top F.Paste F.Mask)
      (net 12 "Net-(J1-Pad23)"))
    (pad 25 smd rect (at 2 -1.8 270) (size 0.22 1) (layers Top F.Paste F.Mask)
      (net 13 "Net-(J1-Pad25)"))
    (pad 27 smd rect (at 2.4 -1.8 270) (size 0.22 1) (layers Top F.Paste F.Mask)
      (net 14 "Net-(J1-Pad27)"))
    (pad 29 smd rect (at 2.8 -1.8 270) (size 0.22 1) (layers Top F.Paste F.Mask)
      (net 15 "Net-(J1-Pad29)"))
    (pad 2 smd rect (at -2.8 1.8 270) (size 0.22 1) (layers Top F.Paste F.Mask)
      (net 16 "Net-(J1-Pad2)"))
    (pad 4 smd rect (at -2.4 1.8 270) (size 0.22 1) (layers Top F.Paste F.Mask)
      (net 17 "Net-(J1-Pad4)"))
    (pad 6 smd rect (at -2 1.8 270) (size 0.22 1) (layers Top F.Paste F.Mask)
      (net 18 "Net-(J1-Pad6)"))
    (pad 8 smd rect (at -1.6 1.8 270) (size 0.22 1) (layers Top F.Paste F.Mask)
      (net 19 "Net-(J1-Pad8)"))
    (pad 10 smd rect (at -1.2 1.8 270) (size 0.22 1) (layers Top F.Paste F.Mask)
      (net 20 "Net-(J1-Pad10)"))
    (pad 12 smd rect (at -0.8 1.8 270) (size 0.22 1) (layers Top F.Paste F.Mask)
      (net 21 "Net-(J1-Pad12)"))
    (pad 14 smd rect (at -0.4 1.8 270) (size 0.22 1) (layers Top F.Paste F.Mask)
      (net 22 "Net-(J1-Pad14)"))
    (pad 16 smd rect (at 0 1.8 270) (size 0.22 1) (layers Top F.Paste F.Mask)
      (net 23 "Net-(J1-Pad16)"))
    (pad 18 smd rect (at 0.4 1.8 270) (size 0.22 1) (layers Top F.Paste F.Mask)
      (net 24 "Net-(J1-Pad18)"))
    (pad 20 smd rect (at 0.8 1.8 270) (size 0.22 1) (layers Top F.Paste F.Mask)
      (net 25 "Net-(J1-Pad20)"))
    (pad 22 smd rect (at 1.2 1.8 270) (size 0.22 1) (layers Top F.Paste F.Mask)
      (net 26 "Net-(J1-Pad22)"))
    (pad 24 smd rect (at 1.6 1.8 270) (size 0.22 1) (layers Top F.Paste F.Mask)
      (net 27 "Net-(J1-Pad24)"))
    (pad 26 smd rect (at 2 1.8 270) (size 0.22 1) (layers Top F.Paste F.Mask)
      (net 28 "Net-(J1-Pad26)"))
    (pad 28 smd rect (at 2.4 1.8 270) (size 0.22 1) (layers Top F.Paste F.Mask)
      (net 29 "Net-(J1-Pad28)"))
    (pad 30 smd rect (at 2.8 1.8 270) (size 0.22 1) (layers Top F.Paste F.Mask)
      (net 30 "Net-(J1-Pad30)"))
    (pad x smd rect (at -3.64 -1.8 270) (size 1 1) (layers Top F.Paste F.Mask))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_SlimStack_Plug_2x15_Pitch0.5mm_501920-3001.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model C:/Users/ggira/Desktop/5009130302.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz -90 0 0))
    )
  )
  (gr_line (start 114.3 83.82) (end 114.3 83.82) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 156.21 83.82) (end 114.3 83.82) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 156.21 111.76) (end 156.21 83.82) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.3 111.76) (end 156.21 111.76) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.3 83.82) (end 114.3 111.76) (layer Edge.Cuts) (width 0.1))
  (gr_text 28 (at 119.3546 85.09) (layer F.SilkS))
  (gr_text 26 (at 121.92 84.836) (layer F.SilkS))
  (gr_text 24 (at 124.4346 85.09) (layer F.SilkS))
  (gr_text 22 (at 127 84.836) (layer F.SilkS))
  (gr_text "20\n" (at 129.5146 85.09) (layer F.SilkS))
  (gr_text 18 (at 132.08 84.836) (layer F.SilkS))
  (gr_text 16 (at 134.5946 85.09) (layer F.SilkS))
  (gr_text 14 (at 137.033 84.836) (layer F.SilkS))
  (gr_text 12 (at 139.6746 85.09) (layer F.SilkS))
  (gr_text 10 (at 142.24 84.836) (layer F.SilkS))
  (gr_text 8 (at 144.6784 85.0646) (layer F.SilkS))
  (gr_text 6 (at 147.2946 85.09) (layer F.SilkS))
  (gr_text 4 (at 149.8346 85.0392) (layer F.SilkS))
  (gr_text 2 (at 152.527 84.963) (layer F.SilkS))
  (gr_text 30 (at 116.84 84.836) (layer F.SilkS))
  (gr_text 29 (at 116.8146 110.6932) (layer F.SilkS))
  (gr_text 27 (at 119.3292 110.5154) (layer F.SilkS))
  (gr_text 25 (at 121.8946 110.8202) (layer F.SilkS))
  (gr_text 23 (at 124.4092 110.6424) (layer F.SilkS))
  (gr_text 21 (at 126.9746 110.8202) (layer F.SilkS))
  (gr_text 19 (at 129.3622 110.6424) (layer F.SilkS))
  (gr_text 17 (at 132.0546 110.9472) (layer F.SilkS))
  (gr_text 15 (at 134.5692 110.7694) (layer F.SilkS))
  (gr_text 13 (at 137.2616 110.8202) (layer F.SilkS))
  (gr_text 11 (at 139.6492 110.7694) (layer F.SilkS))
  (gr_text 9 (at 142.2146 110.6932) (layer F.SilkS))
  (gr_text 7 (at 144.7292 110.6424) (layer F.SilkS))
  (gr_text 5 (at 147.2946 110.6932) (layer F.SilkS))
  (gr_text 3 (at 149.8092 110.7694) (layer F.SilkS))
  (gr_text 1 (at 152.3746 110.6932) (layer F.SilkS))
)
