(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (grid_origin 158.11 54.44)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "Net-(Jr1-B)")
  (net 2 "Net-(Cc11-Pad2)")
  (net 3 "Net-(Jr2-B)")
  (net 4 "Net-(Cc21-Pad2)")
  (net 5 "Net-(D1-Pad1)")
  (net 6 "Net-(Qr1-D)")
  (net 7 "Net-(Q11-D)")
  (net 8 "Net-(D1-Pad4)")
  (net 9 "unconnected-(D1-Pad5)")
  (net 10 "unconnected-(D1-Pad6)")
  (net 11 "unconnected-(D1-Pad7)")
  (net 12 "unconnected-(D1-Pad8)")
  (net 13 "Net-(D1-Pad9)")
  (net 14 "Net-(Q21-D)")
  (net 15 "Net-(Qr2-D)")
  (net 16 "Net-(D1-Pad12)")
  (net 17 "unconnected-(D1-Pad13)")
  (net 18 "Net-(D1-P14)")
  (net 19 "Net-(D1-P15)")
  (net 20 "Net-(D1-P16)")
  (net 21 "unconnected-(D1-P17-Pad17)")
  (net 22 "unconnected-(D1-P18-Pad18)")
  (net 23 "unconnected-(D1-P19-Pad19)")
  (net 24 "unconnected-(D1-P20-Pad20)")
  (net 25 "unconnected-(D1-P21-Pad21)")
  (net 26 "unconnected-(D1-P22-Pad22)")
  (net 27 "Net-(D1-P23)")
  (net 28 "Net-(D1-P24)")
  (net 29 "Net-(D1-P25)")
  (net 30 "Net-(Jr1-A)")
  (net 31 "Net-(Jr2-A)")
  (net 32 "thermal")
  (footprint "charge_amp:Q_NJFET_GDS" (layer "F.Cu")
    (at 152.4 52.47268 180)
    (property "Sheetfile" "SplitStage-base-V2.0.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "N-JFET transistor, gate/drain/source")
    (property "ki_keywords" "transistor NJFET N-JFET")
    (attr smd)
    (fp_text reference "Qr1" (at -3.868735 -4.681268 unlocked) (layer "F.SilkS"))
    (fp_text value "1.8pF" (at 0 1 180 unlocked) (layer "F.Fab") hide)
    (fp_text user "G" (at -2.982 -3.095) (layer "F.SilkS"))
    (fp_text user "S" (at -2.982 -6.27) (layer "F.SilkS"))
    (fp_text user "D" (at 2.733 -3.095) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -5.08) (layer "F.Fab"))
    (pad "1" smd rect (at -0.95 -3.73 270) (size 1.65 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "Net-(D1-P15)") (pinfunction "G") (pintype "input"))
    (pad "2" smd rect (at 0.95 -3.73 270) (size 1.65 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "Net-(Qr1-D)") (pinfunction "D") (pintype "passive"))
    (pad "3" smd rect (at 0 -6.44 270) (size 1.65 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 30 "Net-(Jr1-A)") (pinfunction "S") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 145.817469 67.442852)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SplitStage-base-V2.0.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "Rfb1" (at 0.838651 -1.89545) (layer "F.SilkS"))
    (fp_text value "R=1" (at 0 1.82) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0.8) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 8 "Net-(D1-Pad4)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 1 "Net-(Jr1-B)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder" (layer "F.Cu")
    (at 151.199257 68.015201 -90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "SplitStage-base-V2.0.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "Cc11" (at -0.263931 -2.86561 -180) (layer "F.SilkS"))
    (fp_text value "C=1" (at 0 1.16 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.5675 0 270) (size 0.735 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "Net-(Jr1-B)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.5675 0 270) (size 0.735 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "Net-(Cc11-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2_DIN965_Pad" (layer "F.Cu")
    (at 172.25867 55.142453)
    (descr "Mounting Hole 2.2mm, M2, DIN965")
    (tags "mounting hole 2.2mm m2 din965")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -2.9) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_2.2mm_M2_DIN965_Pad" (at 0 2.9) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 3.8 3.8) (drill 2.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder" (layer "F.Cu")
    (at 165.886769 67.65566 -90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "SplitStage-base-V2.0.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "Cc21" (at -0.46708 -2.432903 -180) (layer "F.SilkS"))
    (fp_text value "C=1" (at 0 1.16 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.5675 0 270) (size 0.735 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(Jr2-B)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.5675 0 270) (size 0.735 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(Cc21-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2_DIN965_Pad" (layer "F.Cu")
    (at 143.606561 79.983355)
    (descr "Mounting Hole 2.2mm, M2, DIN965")
    (tags "mounting hole 2.2mm m2 din965")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -2.9) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_2.2mm_M2_DIN965_Pad" (at 0 2.9) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 3.8 3.8) (drill 2.2) (layers "*.Cu" "*.Mask")
      (net 32 "thermal"))
  )
  (footprint "" (layer "F.Cu")
    (at 172.25867 55.142453)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at 0 0) (size 3.8 3.8) (drill 2.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "" (layer "F.Cu")
    (at 143.703831 55.203356)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at 0 0) (size 3.8 3.8) (drill 2.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 170.701343 69.732755 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SplitStage-base-V2.0.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "Rbs2" (at -3.457849 1.13514 180) (layer "F.SilkS"))
    (fp_text value "R=1" (at 0 1.82 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 90) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 16 "Net-(D1-Pad12)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 90) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 4 "Net-(Cc21-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2_DIN965_Pad" (layer "F.Cu")
    (at 172.667013 79.84724)
    (descr "Mounting Hole 2.2mm, M2, DIN965")
    (tags "mounting hole 2.2mm m2 din965")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -2.9) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_2.2mm_M2_DIN965_Pad" (at 0 2.9) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 3.8 3.8) (drill 2.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "charge_amp:Q_NJFET_GDS" (layer "F.Cu")
    (at 152.4 69.131541)
    (property "Sheetfile" "SplitStage-base-V2.0.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "N-JFET transistor, gate/drain/source")
    (property "ki_keywords" "transistor NJFET N-JFET")
    (attr smd)
    (fp_text reference "Q11" (at 3.821844 -4.990863 unlocked) (layer "F.SilkS"))
    (fp_text value "1.8pF" (at -5.08 -4.94 unlocked) (layer "F.Fab") hide)
    (fp_text user "S" (at -2.982 -6.27 180) (layer "F.SilkS"))
    (fp_text user "G" (at -2.982 -3.095 180) (layer "F.SilkS"))
    (fp_text user "D" (at 2.733 -3.095 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -5.08) (layer "F.Fab"))
    (pad "1" smd rect (at -0.95 -3.73 90) (size 1.65 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "Net-(Jr1-B)") (pinfunction "G") (pintype "input"))
    (pad "2" smd rect (at 0.95 -3.73 90) (size 1.65 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "Net-(Q11-D)") (pinfunction "D") (pintype "passive"))
    (pad "3" smd rect (at 0 -6.44 90) (size 1.65 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "Net-(D1-P16)") (pinfunction "S") (pintype "passive"))
  )
  (footprint "charge_amp:Q_NJFET_GDS" (layer "F.Cu")
    (at 165.824748 52.056097 180)
    (property "Sheetfile" "SplitStage-base-V2.0.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "N-JFET transistor, gate/drain/source")
    (property "ki_keywords" "transistor NJFET N-JFET")
    (attr smd)
    (fp_text reference "Qr2" (at 3.976007 -4.769615 unlocked) (layer "F.SilkS"))
    (fp_text value "1.8pF" (at 0 1 180 unlocked) (layer "F.Fab") hide)
    (fp_text user "S" (at -2.982 -6.27) (layer "F.SilkS"))
    (fp_text user "G" (at -2.982 -3.095) (layer "F.SilkS"))
    (fp_text user "D" (at 2.733 -3.095) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -5.08) (layer "F.Fab"))
    (pad "1" smd rect (at -0.95 -3.73 270) (size 1.65 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 28 "Net-(D1-P24)") (pinfunction "G") (pintype "input"))
    (pad "2" smd rect (at 0.95 -3.73 270) (size 1.65 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "Net-(Qr2-D)") (pinfunction "D") (pintype "passive"))
    (pad "3" smd rect (at 0 -6.44 270) (size 1.65 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "Net-(Jr2-A)") (pinfunction "S") (pintype "passive"))
  )
  (footprint "charge_amp:detector" (layer "F.Cu")
    (at 159 71.12 90)
    (property "Sheetfile" "SplitStage-base-V2.0.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "Detector1" (at -3.1534 -5.033096 unlocked) (layer "F.SilkS"))
    (fp_text value "C=1" (at -3.55233 -4.893171 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 -5.08 90) (size 1 1) (drill 1) (layers "F&B.Cu" "*.Mask"))
    (pad "1" smd roundrect (at 0 -7.62 90) (size 1.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "Net-(Cc11-Pad2)") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at 0 -2.54 90) (size 1.5 1.5) (layers "B.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "Net-(D1-P14)") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2_DIN965_Pad" (layer "F.Cu")
    (at 143.703831 55.203356)
    (descr "Mounting Hole 2.2mm, M2, DIN965")
    (tags "mounting hole 2.2mm m2 din965")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -2.9) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_2.2mm_M2_DIN965_Pad" (at 0 2.9) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 3.8 3.8) (drill 2.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 144.78 72.67 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SplitStage-base-V2.0.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "Rbs1" (at -3.53 0 180) (layer "F.SilkS"))
    (fp_text value "R=1" (at 0 1.82 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 90) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 5 "Net-(D1-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 90) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 2 "Net-(Cc11-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "charge_amp:Q_NJFET_GDS" (layer "F.Cu")
    (at 166.849952 68.50529)
    (property "Sheetfile" "SplitStage-base-V2.0.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "N-JFET transistor, gate/drain/source")
    (property "ki_keywords" "transistor NJFET N-JFET")
    (attr smd)
    (fp_text reference "Q21" (at 3.330048 -5.00529 unlocked) (layer "F.SilkS"))
    (fp_text value "1.8pF" (at 5.870048 -6.04529 unlocked) (layer "F.Fab") hide)
    (fp_text user "S" (at -1.749952 -6.27) (layer "F.SilkS"))
    (fp_text user "D" (at 2.733 -3.095) (layer "F.SilkS"))
    (fp_text user "G" (at -2.982 -3.095) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -5.08) (layer "F.Fab"))
    (pad "1" smd rect (at -0.95 -3.73 90) (size 1.65 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "Net-(Jr2-B)") (pinfunction "G") (pintype "input"))
    (pad "2" smd rect (at 0.95 -3.73 90) (size 1.65 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "Net-(Q21-D)") (pinfunction "D") (pintype "passive"))
    (pad "3" smd rect (at 0 -6.44 90) (size 1.65 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "Net-(D1-P23)") (pinfunction "S") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 161.12645 67.091847)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SplitStage-base-V2.0.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "Rfb2" (at 0 -1.82) (layer "F.SilkS"))
    (fp_text value "R=1" (at 0 1.82) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 13 "Net-(D1-Pad9)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 3 "Net-(Jr2-B)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "charge_amp:detector" (layer "F.Cu")
    (at 157.48 71.12 -90)
    (property "Sheetfile" "SplitStage-base-V2.0.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "Detector2" (at 3.1534 -5.594314 unlocked) (layer "F.SilkS"))
    (fp_text value "C=1" (at 3.58 -7.62 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 -5.08 270) (size 1 1) (drill 1) (layers "F&B.Cu" "*.Mask"))
    (pad "1" smd roundrect (at 0 -7.62 270) (size 1.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(Cc21-Pad2)") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at 0 -2.54 270) (size 1.5 1.5) (layers "B.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "Net-(D1-P25)") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 162.709579 61.256013 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SplitStage-base-V2.0.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Jumper, 2-pole, closed/bridged")
    (property "ki_keywords" "Jumper SPST")
    (attr smd)
    (fp_text reference "Jr2" (at 0.034234 1.89787 90) (layer "F.SilkS"))
    (fp_text value "R=0" (at 0 1.82 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 31 "Net-(Jr2-A)") (pinfunction "A") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 3 "Net-(Jr2-B)") (pinfunction "B") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "charge_amp:MDM_25_F" (layer "F.Cu")
    (at 158.11 54.44)
    (property "Sheetfile" "SplitStage-base-V2.0.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "25-pin female D-SUB connector")
    (property "ki_keywords" "female D-SUB connector")
    (attr smd)
    (fp_text reference "D1" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "MDM25_FEMALE" (at 0 1 unlocked) (layer "F.Fab") hide)
    (fp_text user "1" (at -8.255 -5.73) (layer "F.SilkS"))
    (fp_text user "14" (at -8.255 -10.81) (layer "F.SilkS"))
    (fp_text user "25" (at 8.89 -10.81) (layer "F.SilkS"))
    (fp_text user "13" (at 8.255 -5.73) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -7.932) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -7.62 -7.62 180) (size 1.05 1.05) (drill 0.61) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(D1-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at -6.35 -7.62 180) (size 1.05 1.05) (drill 0.61) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(Qr1-D)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at -5.08 -7.62 180) (size 1.05 1.05) (drill 0.61) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(Q11-D)") (pinfunction "3") (pintype "passive"))
    (pad "4" thru_hole circle (at -3.81 -7.62 180) (size 1.05 1.05) (drill 0.61) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(D1-Pad4)") (pinfunction "4") (pintype "passive"))
    (pad "5" thru_hole circle (at -2.54 -7.62 180) (size 1.05 1.05) (drill 0.61) (layers "*.Cu" "*.Mask")
      (net 9 "unconnected-(D1-Pad5)") (pinfunction "5") (pintype "passive"))
    (pad "6" thru_hole circle (at -1.27 -7.62 180) (size 1.05 1.05) (drill 0.61) (layers "*.Cu" "*.Mask")
      (net 10 "unconnected-(D1-Pad6)") (pinfunction "6") (pintype "passive"))
    (pad "7" thru_hole circle (at 0 -7.62 180) (size 1.05 1.05) (drill 0.61) (layers "*.Cu" "*.Mask")
      (net 11 "unconnected-(D1-Pad7)") (pinfunction "7") (pintype "passive"))
    (pad "8" thru_hole circle (at 1.27 -7.62 180) (size 1.05 1.05) (drill 0.61) (layers "*.Cu" "*.Mask")
      (net 12 "unconnected-(D1-Pad8)") (pinfunction "8") (pintype "passive"))
    (pad "9" thru_hole circle (at 2.54 -7.62 180) (size 1.05 1.05) (drill 0.61) (layers "*.Cu" "*.Mask")
      (net 13 "Net-(D1-Pad9)") (pinfunction "9") (pintype "passive"))
    (pad "10" thru_hole circle (at 3.81 -7.62 180) (size 1.05 1.05) (drill 0.61) (layers "*.Cu" "*.Mask")
      (net 14 "Net-(Q21-D)") (pinfunction "10") (pintype "passive"))
    (pad "11" thru_hole circle (at 5.08 -7.62 180) (size 1.05 1.05) (drill 0.61) (layers "*.Cu" "*.Mask")
      (net 15 "Net-(Qr2-D)") (pinfunction "11") (pintype "passive"))
    (pad "12" thru_hole circle (at 6.35 -7.62 180) (size 1.05 1.05) (drill 0.61) (layers "*.Cu" "*.Mask")
      (net 16 "Net-(D1-Pad12)") (pinfunction "12") (pintype "passive"))
    (pad "13" thru_hole circle (at 7.62 -7.62 180) (size 1.05 1.05) (drill 0.61) (layers "*.Cu" "*.Mask")
      (net 17 "unconnected-(D1-Pad13)") (pinfunction "13") (pintype "passive"))
    (pad "14" thru_hole circle (at -6.99 -8.72 180) (size 1.05 1.05) (drill 0.61) (layers "*.Cu" "*.Mask")
      (net 18 "Net-(D1-P14)") (pinfunction "P14") (pintype "passive"))
    (pad "15" thru_hole circle (at -5.72 -8.72 180) (size 1.05 1.05) (drill 0.61) (layers "*.Cu" "*.Mask")
      (net 19 "Net-(D1-P15)") (pinfunction "P15") (pintype "passive"))
    (pad "16" thru_hole circle (at -4.45 -8.72 180) (size 1.05 1.05) (drill 0.61) (layers "*.Cu" "*.Mask")
      (net 20 "Net-(D1-P16)") (pinfunction "P16") (pintype "passive"))
    (pad "17" thru_hole circle (at -3.18 -8.72 180) (size 1.05 1.05) (drill 0.61) (layers "*.Cu" "*.Mask")
      (net 21 "unconnected-(D1-P17-Pad17)") (pinfunction "P17") (pintype "passive"))
    (pad "18" thru_hole circle (at -1.91 -8.72 180) (size 1.05 1.05) (drill 0.61) (layers "*.Cu" "*.Mask")
      (net 22 "unconnected-(D1-P18-Pad18)") (pinfunction "P18") (pintype "passive"))
    (pad "19" thru_hole circle (at -0.64 -8.72 180) (size 1.05 1.05) (drill 0.61) (layers "*.Cu" "*.Mask")
      (net 23 "unconnected-(D1-P19-Pad19)") (pinfunction "P19") (pintype "passive"))
    (pad "20" thru_hole circle (at 0.64 -8.72 180) (size 1.05 1.05) (drill 0.61) (layers "*.Cu" "*.Mask")
      (net 24 "unconnected-(D1-P20-Pad20)") (pinfunction "P20") (pintype "passive"))
    (pad "21" thru_hole circle (at 1.91 -8.72 180) (size 1.05 1.05) (drill 0.61) (layers "*.Cu" "*.Mask")
      (net 25 "unconnected-(D1-P21-Pad21)") (pinfunction "P21") (pintype "passive"))
    (pad "22" thru_hole circle (at 3.18 -8.72 180) (size 1.05 1.05) (drill 0.61) (layers "*.Cu" "*.Mask")
      (net 26 "unconnected-(D1-P22-Pad22)") (pinfunction "P22") (pintype "passive"))
    (pad "23" thru_hole circle (at 4.45 -8.72 180) (size 1.05 1.05) (drill 0.61) (layers "*.Cu" "*.Mask")
      (net 27 "Net-(D1-P23)") (pinfunction "P23") (pintype "passive"))
    (pad "24" thru_hole circle (at 5.72 -8.72 180) (size 1.05 1.05) (drill 0.61) (layers "*.Cu" "*.Mask")
      (net 28 "Net-(D1-P24)") (pinfunction "P24") (pintype "passive"))
    (pad "25" thru_hole circle (at 6.99 -8.72 180) (size 1.05 1.05) (drill 0.61) (layers "*.Cu" "*.Mask")
      (net 29 "Net-(D1-P25)") (pinfunction "P25") (pintype "passive"))
    (pad "MH1" thru_hole circle (at 12.275 -8.17 180) (size 4.305 4.305) (drill 2.87) (layers "*.Cu" "*.Mask"))
    (pad "MH2" thru_hole circle (at -12.275 -8.17 180) (size 4.305 4.305) (drill 2.87) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 147.383594 60.511063 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SplitStage-base-V2.0.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Jumper, 2-pole, closed/bridged")
    (property "ki_keywords" "Jumper SPST")
    (attr smd)
    (fp_text reference "Jr1" (at 0.019023 1.946635 90) (layer "F.SilkS"))
    (fp_text value "R=0" (at 0 1.82 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 30 "Net-(Jr1-A)") (pinfunction "A") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 1 "Net-(Jr1-B)") (pinfunction "B") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_rect (start 140.192958 40.286286) (end 176.038121 83.603046)
    (fill none) (layer "Edge.Cuts"))
  (zone (net 32) (net_name "thermal") (layers "F&B.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 137.79 39.2)
        (xy 137.79 84.92)
        (xy 178.43 84.92)
        (xy 178.43 77.3)
        (xy 145.41 77.3)
        (xy 145.51 57.79)
        (xy 170.7 57.76)
        (xy 170.72 77.28)
        (xy 178.43 77.3)
        (xy 178.43 39.2)
      )
    )
  )
)
