(kicad_pcb (version 20171130) (host pcbnew 5.1.2-f72e74a~84~ubuntu18.04.1)
  (general
    (thickness 1.6)
    (drawings 5)
    (tracks 7)
    (zones 0)
    (modules 2)
    (nets 6)
  )
  (page USLetter)
  (layers
    (0 F.Cu power)
    (31 B.Cu signal)
    (33 F.Adhes user hide)
    (35 F.Paste user hide)
    (37 F.SilkS user hide)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad4)")
  (net 2 "Net-(J1-Pad2)")
  (net 3 "Net-(J1-Pad1)")
  (net 4 "Net-(J2-Pad2)")
  (net 5 "Net-(J2-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
  )
  (module usb-connectors:CUI_UJ2-AH-4-TH (layer F.Cu) (tedit 5CEB7D50)
    (at 86.05 26.67 180)
    (fp_text reference J1 (at -1.36203 -2.53878) (layer F.SilkS) hide)
    (fp_text value "to vita" (at 3.5 -2.54) (layer F.SilkS))
    (pad SH2 thru_hole circle (at 8.5 2.67 180) (size 3.6 3.6) (drill 2.3) (layers *.Mask B.Cu))
    (pad SH1 thru_hole circle (at -1.5 2.67 180) (size 3.6 3.6) (drill 2.3) (layers *.Mask B.Cu))
    (pad 4 thru_hole circle (at 7 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Mask B.Cu)
      (net 1 "Net-(J1-Pad4)"))
    (pad 3 thru_hole circle (at 4.5 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Mask B.Cu)
      (net 2 "Net-(J1-Pad2)"))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Mask B.Cu)
      (net 2 "Net-(J1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Mask B.Cu)
      (net 3 "Net-(J1-Pad1)"))
  )
  (module usb-connectors:CUI_UP2-AH-1-TH (layer F.Cu) (tedit 5CEB7C1E)
    (at 82.55 36.83)
    (descr http://www.cui.com/product/resource/up2-ah-th.pdf)
    (fp_text reference J2 (at 0 7.62) (layer F.SilkS) hide)
    (fp_text value "To charger" (at 0 -5.08) (layer F.SilkS))
    (pad 1 thru_hole circle (at 3.5 -2.1) (size 1.8 1.8) (drill 1) (layers *.Mask B.Cu)
      (net 3 "Net-(J1-Pad1)"))
    (pad 2 thru_hole circle (at 1 -2.1) (size 1.8 1.8) (drill 1) (layers *.Mask B.Cu)
      (net 4 "Net-(J2-Pad2)"))
    (pad 3 thru_hole circle (at -1 -2.1) (size 1.8 1.8) (drill 1) (layers *.Mask B.Cu)
      (net 5 "Net-(J2-Pad3)"))
    (pad 4 thru_hole circle (at -3.5 -2.1) (size 1.8 1.8) (drill 1) (layers *.Mask B.Cu)
      (net 1 "Net-(J1-Pad4)"))
    (pad SH thru_hole circle (at 2.3 0) (size 2.2 2.2) (drill 1.2) (layers *.Mask B.Cu))
    (pad SH thru_hole circle (at -2.3 0) (size 2.2 2.2) (drill 1.2) (layers *.Mask B.Cu))
    (pad SH thru_hole oval (at 5.85 0) (size 2 3.5) (drill oval 1 2.5) (layers *.Mask B.Cu))
    (pad SH thru_hole oval (at -5.85 0) (size 2 3.5) (drill oval 1 2.5) (layers *.Mask B.Cu))
  )
  (gr_line (start 75.438 19.05) (end 75.438 39.37) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 89.662 19.05) (end 89.662 39.37) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 75.438 19.05) (end 89.662 19.05) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 75.438 39.37) (end 89.662 39.37) (layer Edge.Cuts) (width 0.05))
)
