(kicad_pcb (version 20171130) (host pcbnew "(5.1.10)-1")
  (general
    (thickness 1.6)
    (drawings 14)
    (tracks 25)
    (zones 0)
    (modules 4)
    (nets 5)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.4)
    (user_trace_width 0.4)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.15)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (grid_origin 138.036001 121.496001)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "./Gerber"))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad1)")
  (net 2 "Net-(J1-Pad3)")
  (net 3 "Net-(J1-Pad2)")
  (net 4 "Net-(R1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(R1-Pad1)")
  )
  (module Model_MX1:MXOnly-1U-Hotswap-LED (layer F.Cu) (tedit 617A024D)
    (at 134.036001 113.496001)
    (attr smd)
    (fp_text reference SW1 (at 0 0) (layer B.CrtYd) hide)
    (fp_text value KEYBOARD-SWITCHMX_1U (at 0 -7.9375) (layer Dwgs.User))
    (fp_text user %R (at 0 0) (layer B.SilkS) hide)
    (fp_text user LED (at 0 0) (layer F.SilkS) hide)
    (pad "" np_thru_hole circle (at 2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad S1 smd rect (at -7.085 -2.54) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(J1-Pad3)"))
    (pad S2 smd rect (at 5.842 -5.08) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad C thru_hole rect (at 1.27 5.08) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.SilkS *.Mask)
      (net 4 "Net-(R1-Pad1)"))
    (pad A thru_hole circle (at -1.27 5.08) (size 1.651 1.651) (drill 0.9906) (layers *.Cu *.SilkS *.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (model "E:/m2BACKUP/Desktop/projects/KiCAD Libraries/libraries/3dmodels/qmk components/kailh_socket_mx.stp"
      (offset (xyz -0.65 3.8 -3.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
    (model "E:/m2BACKUP/Desktop/projects/KiCAD Libraries/libraries/3dmodels/mx/asm_mx_asm_PCB.stp"
      (offset (xyz 0.3 0.3 5.25))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 -90))
    )
  )
  (module Model_MX1:R_SMD+THT (layer B.Cu) (tedit 6179FE9F)
    (at 138.036001 121.496001)
    (fp_text reference R1 (at 0 -1.895 180) (layer B.SilkS) hide)
    (fp_text value R (at 0 1.905 180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 1 0) (size 1.2 1.5) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.125)
      (net 1 "Net-(J1-Pad1)") (solder_mask_margin 0.1016))
    (pad 1 smd roundrect (at -1 0) (size 1.2 1.5) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.125)
      (net 4 "Net-(R1-Pad1)") (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at -3.5 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(R1-Pad1)") (solder_mask_margin 0.1016))
    (pad 2 thru_hole circle (at 3.5 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)") (solder_mask_margin 0.1016))
  )
  (module "Model C:USBC_C_Logo" (layer B.Cu) (tedit 0)
    (at 139.306001 117.576001 180)
    (fp_text reference G*** (at 0 0) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer B.SilkS) hide)
  )
  (module TerminalBlock_Phoenix:TerminalBlock_Phoenix_MPT-0,5-3-2.54_1x03_P2.54mm_Horizontal (layer B.Cu) (tedit 6174228D)
    (at 131.536001 121.496001 180)
    (descr "Terminal Block Phoenix MPT-0,5-3-2.54, 3 pins, pitch 2.54mm, size 8.08x6.2mm^2, drill diamater 1.1mm, pad diameter 2.2mm, see http://www.mouser.com/ds/2/324/ItemDetail_1725656-920552.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
    (tags "THT Terminal Block Phoenix MPT-0,5-3-2.54 pitch 2.54mm size 8.08x6.2mm^2 drill 1.1mm pad 2.2mm")
    (fp_text reference J1 (at 2.54 0.62) (layer B.SilkS) hide)
    (fp_text value Terminals (at -1.6 -4.55) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 180) (size 2.1 2.1) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 2.1 2.1) (drill 1.3) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (pad 3 thru_hole circle (at 5.08 0 180) (size 2.1 2.1) (drill 1.3) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad3)"))
    (model ${KISYS3DMOD}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MPT-0,5-3-2.54_1x03_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "MX1 v1" (at 138.036001 123.296001) (layer B.SilkS))
  (gr_text SW (at 126.456001 116.670001 90) (layer B.SilkS))
  (gr_text V+ (at 128.996001 116.670001 90) (layer B.SilkS))
  (gr_text GND (at 131.536001 116.670001 90) (layer B.SilkS))
  (gr_line (start 125.036001 106.446001) (end 125.036001 109.496001) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 143.036001 106.446001) (end 125.036001 106.446001) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 143.036001 124.446001) (end 143.036001 106.446001) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 125.036001 124.446001) (end 143.036001 124.446001) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 125.036001 109.496001) (end 125.036001 124.446001) (layer Edge.Cuts) (width 0.15))
)
