(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (41 "Cmts.User" user "User.Comments")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.25)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "DQ8")
  (net 3 "CTL5")
  (net 4 "B_TXN03")
  (net 5 "CTL4")
  (net 6 "B_TXP03")
  (net 7 "unconnected-(J1-Pad14)")
  (net 8 "B_TXN02")
  (net 9 "unconnected-(J1-Pad16)")
  (net 10 "B_TXN01")
  (net 11 "unconnected-(J1-Pad20)")
  (net 12 "unconnected-(J1-Pad22)")
  (net 13 "B_TXP08")
  (net 14 "unconnected-(J1-Pad26)")
  (net 15 "unconnected-(J1-Pad28)")
  (net 16 "B_TXP01")
  (net 17 "unconnected-(J1-Pad32)")
  (net 18 "B_TXP00")
  (net 19 "unconnected-(J1-Pad34)")
  (net 20 "DQ9")
  (net 21 "unconnected-(J1-Pad38)")
  (net 22 "CTL6")
  (net 23 "unconnected-(J1-Pad40)")
  (net 24 "B_TXP07")
  (net 25 "B_TXN00")
  (net 26 "B_TXN07")
  (net 27 "B_TXN08")
  (net 28 "B_TXP02")
  (net 29 "unconnected-(J2-Pad14)")
  (net 30 "unconnected-(J2-Pad16)")
  (net 31 "unconnected-(J2-Pad20)")
  (net 32 "unconnected-(J2-Pad22)")
  (net 33 "B_TXP04")
  (net 34 "unconnected-(J2-Pad26)")
  (net 35 "B_TXN04")
  (net 36 "unconnected-(J2-Pad28)")
  (net 37 "B_TXP05")
  (net 38 "unconnected-(J2-Pad32)")
  (net 39 "B_TXN05")
  (net 40 "unconnected-(J2-Pad34)")
  (net 41 "B_TXP06")
  (net 42 "unconnected-(J2-Pad38)")
  (net 43 "B_TXN06")
  (net 44 "unconnected-(J2-Pad40)")
  (net 45 "unconnected-(J3-Pad1)")
  (net 46 "unconnected-(J3-Pad2)")
  (net 47 "unconnected-(J3-Pad4)")
  (net 48 "unconnected-(J3-Pad5)")
  (net 49 "DQ31")
  (net 50 "PMODE_2")
  (net 51 "DQ30")
  (net 52 "PMODE_1")
  (net 53 "DQ29")
  (net 54 "PMODE_0")
  (net 55 "DQ28")
  (net 56 "GPIO45")
  (net 57 "DQ27")
  (net 58 "DQ26")
  (net 59 "DQ25")
  (net 60 "DQ24")
  (net 61 "DQ23")
  (net 62 "DQ22")
  (net 63 "DQ21")
  (net 64 "DQ20")
  (net 65 "I2S_WS")
  (net 66 "DQ19")
  (net 67 "I2S_SD")
  (net 68 "DQ18")
  (net 69 "I2S_MCLK")
  (net 70 "DQ17")
  (net 71 "I2S_CLK")
  (net 72 "unconnected-(J4-Pad1)")
  (net 73 "unconnected-(J4-Pad2)")
  (net 74 "unconnected-(J4-Pad3)")
  (net 75 "unconnected-(J4-Pad4)")
  (net 76 "I2C_SDA")
  (net 77 "I2C_SCL")
  (net 78 "unconnected-(J5-Pad14)")
  (net 79 "unconnected-(J5-Pad16)")
  (net 80 "unconnected-(J5-Pad20)")
  (net 81 "unconnected-(J5-Pad22)")
  (net 82 "unconnected-(J5-Pad26)")
  (net 83 "unconnected-(J5-Pad28)")
  (net 84 "unconnected-(J5-Pad32)")
  (net 85 "unconnected-(J5-Pad34)")
  (net 86 "unconnected-(J5-Pad38)")
  (net 87 "unconnected-(J5-Pad40)")
  (net 88 "unconnected-(J6-Pad14)")
  (net 89 "unconnected-(J6-Pad16)")
  (net 90 "unconnected-(J6-Pad20)")
  (net 91 "unconnected-(J6-Pad22)")
  (net 92 "unconnected-(J6-Pad26)")
  (net 93 "unconnected-(J6-Pad28)")
  (net 94 "unconnected-(J6-Pad32)")
  (net 95 "unconnected-(J6-Pad34)")
  (net 96 "unconnected-(J6-Pad38)")
  (net 97 "unconnected-(J6-Pad40)")
  (net 98 "CTL3")
  (net 99 "DQ5")
  (net 100 "CTL2")
  (net 101 "DQ4")
  (net 102 "CTL1")
  (net 103 "DQ3")
  (net 104 "DQ6")
  (net 105 "DQ0")
  (net 106 "DQ1")
  (net 107 "PCLK")
  (net 108 "DQ2")
  (net 109 "CTL0")
  (net 110 "DQ7")
  (footprint "MountingHole:MountingHole_3.2mm_M3" locked (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 84.52125 153.76375)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "AdapterBoard.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H2" (at 0 -4.2) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" locked (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 217.94125 38.15375)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "AdapterBoard.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H3" (at 0 -4.2) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" locked (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 217.94125 87.85375)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "AdapterBoard.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H4" (at 0 -4.2) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" locked (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 84.52125 38.15375)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "AdapterBoard.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H1" (at 0 -4.2) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_2x20_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A433)
    (at 92.53362 55.27362 90)
    (descr "Through hole straight socket strip, 2x20, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 2x20 2.54mm double row")
    (property "Sheetfile" "AdapterBoard.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J4" (at -1.27 -2.77 90) (layer "F.SilkS"))
    (fp_text value "Conn_02x20_Odd_Even" (at -1.27 51.03 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -1.27 24.13) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 72 "unconnected-(J4-Pad1)") (pinfunction "Pin_1") (pintype "passive+no_connect"))
    (pad "2" thru_hole oval locked (at -2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 73 "unconnected-(J4-Pad2)") (pinfunction "Pin_2") (pintype "passive+no_connect"))
    (pad "3" thru_hole oval locked (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 74 "unconnected-(J4-Pad3)") (pinfunction "Pin_3") (pintype "passive+no_connect"))
    (pad "4" thru_hole oval locked (at -2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 75 "unconnected-(J4-Pad4)") (pinfunction "Pin_4") (pintype "passive+no_connect"))
    (pad "5" thru_hole oval locked (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval locked (at -2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval locked (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "B_TXP07") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval locked (at -2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "B_TXP00") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval locked (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "B_TXN07") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval locked (at -2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "B_TXN00") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole oval locked (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "B_TXP08") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole oval locked (at -2.54 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "B_TXP01") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole oval locked (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "B_TXN08") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole oval locked (at -2.54 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "B_TXN01") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" thru_hole oval locked (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "B_TXP02") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" thru_hole oval locked (at -2.54 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "B_TXN02") (pinfunction "Pin_16") (pintype "passive"))
    (pad "17" thru_hole oval locked (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "B_TXP03") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" thru_hole oval locked (at -2.54 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "B_TXN03") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" thru_hole oval locked (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "CTL6") (pinfunction "Pin_19") (pintype "passive"))
    (pad "20" thru_hole oval locked (at -2.54 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "DQ9") (pinfunction "Pin_20") (pintype "passive"))
    (pad "21" thru_hole oval locked (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "CTL5") (pinfunction "Pin_21") (pintype "passive"))
    (pad "22" thru_hole oval locked (at -2.54 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "DQ8") (pinfunction "Pin_22") (pintype "passive"))
    (pad "23" thru_hole oval locked (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "CTL4") (pinfunction "Pin_23") (pintype "passive"))
    (pad "24" thru_hole oval locked (at -2.54 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 110 "DQ7") (pinfunction "Pin_24") (pintype "passive"))
    (pad "25" thru_hole oval locked (at 0 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 98 "CTL3") (pinfunction "Pin_25") (pintype "passive"))
    (pad "26" thru_hole oval locked (at -2.54 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 104 "DQ6") (pinfunction "Pin_26") (pintype "passive"))
    (pad "27" thru_hole oval locked (at 0 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 100 "CTL2") (pinfunction "Pin_27") (pintype "passive"))
    (pad "28" thru_hole oval locked (at -2.54 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 99 "DQ5") (pinfunction "Pin_28") (pintype "passive"))
    (pad "29" thru_hole oval locked (at 0 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 102 "CTL1") (pinfunction "Pin_29") (pintype "passive"))
    (pad "30" thru_hole oval locked (at -2.54 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 101 "DQ4") (pinfunction "Pin_30") (pintype "passive"))
    (pad "31" thru_hole oval locked (at 0 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 109 "CTL0") (pinfunction "Pin_31") (pintype "passive"))
    (pad "32" thru_hole oval locked (at -2.54 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 103 "DQ3") (pinfunction "Pin_32") (pintype "passive"))
    (pad "33" thru_hole oval locked (at 0 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_33") (pintype "passive"))
    (pad "34" thru_hole oval locked (at -2.54 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 108 "DQ2") (pinfunction "Pin_34") (pintype "passive"))
    (pad "35" thru_hole oval locked (at 0 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 107 "PCLK") (pinfunction "Pin_35") (pintype "passive"))
    (pad "36" thru_hole oval locked (at -2.54 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 106 "DQ1") (pinfunction "Pin_36") (pintype "passive"))
    (pad "37" thru_hole oval locked (at 0 45.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_37") (pintype "passive"))
    (pad "38" thru_hole oval locked (at -2.54 45.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 105 "DQ0") (pinfunction "Pin_38") (pintype "passive"))
    (pad "39" thru_hole oval locked (at 0 48.26 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 76 "I2C_SDA") (pinfunction "Pin_39") (pintype "passive"))
    (pad "40" thru_hole oval locked (at -2.54 48.26 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 77 "I2C_SCL") (pinfunction "Pin_40") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x20_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_2x20_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A433)
    (at 160.23362 135.27362 90)
    (descr "Through hole straight socket strip, 2x20, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 2x20 2.54mm double row")
    (property "Sheetfile" "AdapterBoard.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at 3.48 -0.68 90) (layer "F.SilkS"))
    (fp_text value "Conn_02x20_Odd_Even" (at -1.27 51.03 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -1.27 24.13) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "DQ8") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at -2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "DQ9") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval locked (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 104 "DQ6") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval locked (at -2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 110 "DQ7") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval locked (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval locked (at -2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval locked (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 101 "DQ4") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval locked (at -2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 99 "DQ5") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval locked (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 108 "DQ2") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval locked (at -2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 103 "DQ3") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole oval locked (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole oval locked (at -2.54 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole oval locked (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 106 "DQ1") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole oval locked (at -2.54 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "unconnected-(J2-Pad14)") (pinfunction "Pin_14") (pintype "passive+no_connect"))
    (pad "15" thru_hole oval locked (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 105 "DQ0") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" thru_hole oval locked (at -2.54 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "unconnected-(J2-Pad16)") (pinfunction "Pin_16") (pintype "passive+no_connect"))
    (pad "17" thru_hole oval locked (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" thru_hole oval locked (at -2.54 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" thru_hole oval locked (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 107 "PCLK") (pinfunction "Pin_19") (pintype "passive"))
    (pad "20" thru_hole oval locked (at -2.54 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "unconnected-(J2-Pad20)") (pinfunction "Pin_20") (pintype "passive+no_connect"))
    (pad "21" thru_hole oval locked (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 109 "CTL0") (pinfunction "Pin_21") (pintype "passive"))
    (pad "22" thru_hole oval locked (at -2.54 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "unconnected-(J2-Pad22)") (pinfunction "Pin_22") (pintype "passive+no_connect"))
    (pad "23" thru_hole oval locked (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_23") (pintype "passive"))
    (pad "24" thru_hole oval locked (at -2.54 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_24") (pintype "passive"))
    (pad "25" thru_hole oval locked (at 0 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 102 "CTL1") (pinfunction "Pin_25") (pintype "passive"))
    (pad "26" thru_hole oval locked (at -2.54 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "unconnected-(J2-Pad26)") (pinfunction "Pin_26") (pintype "passive+no_connect"))
    (pad "27" thru_hole oval locked (at 0 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 100 "CTL2") (pinfunction "Pin_27") (pintype "passive"))
    (pad "28" thru_hole oval locked (at -2.54 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "unconnected-(J2-Pad28)") (pinfunction "Pin_28") (pintype "passive+no_connect"))
    (pad "29" thru_hole oval locked (at 0 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_29") (pintype "passive"))
    (pad "30" thru_hole oval locked (at -2.54 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_30") (pintype "passive"))
    (pad "31" thru_hole oval locked (at 0 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 98 "CTL3") (pinfunction "Pin_31") (pintype "passive"))
    (pad "32" thru_hole oval locked (at -2.54 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "unconnected-(J2-Pad32)") (pinfunction "Pin_32") (pintype "passive+no_connect"))
    (pad "33" thru_hole oval locked (at 0 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "CTL4") (pinfunction "Pin_33") (pintype "passive"))
    (pad "34" thru_hole oval locked (at -2.54 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 "unconnected-(J2-Pad34)") (pinfunction "Pin_34") (pintype "passive+no_connect"))
    (pad "35" thru_hole oval locked (at 0 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_35") (pintype "passive"))
    (pad "36" thru_hole oval locked (at -2.54 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_36") (pintype "passive"))
    (pad "37" thru_hole oval locked (at 0 45.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "CTL5") (pinfunction "Pin_37") (pintype "passive"))
    (pad "38" thru_hole oval locked (at -2.54 45.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 "unconnected-(J2-Pad38)") (pinfunction "Pin_38") (pintype "passive+no_connect"))
    (pad "39" thru_hole oval locked (at 0 48.26 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "CTL6") (pinfunction "Pin_39") (pintype "passive"))
    (pad "40" thru_hole oval locked (at -2.54 48.26 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 "unconnected-(J2-Pad40)") (pinfunction "Pin_40") (pintype "passive+no_connect"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x20_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_2x20_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A433)
    (at 107.33362 135.27362 90)
    (descr "Through hole straight socket strip, 2x20, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 2x20 2.54mm double row")
    (property "Sheetfile" "AdapterBoard.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at 3.48 -1.12 90) (layer "F.SilkS"))
    (fp_text value "Conn_02x20_Odd_Even" (at -1.27 51.03 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -1.27 24.13) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "B_TXP00") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at -2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "B_TXP07") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval locked (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "B_TXN00") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval locked (at -2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "B_TXN07") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval locked (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval locked (at -2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval locked (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "B_TXP01") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval locked (at -2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "B_TXP08") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval locked (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "B_TXN01") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval locked (at -2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "B_TXN08") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole oval locked (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole oval locked (at -2.54 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole oval locked (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "B_TXP02") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole oval locked (at -2.54 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "unconnected-(J1-Pad14)") (pinfunction "Pin_14") (pintype "passive+no_connect"))
    (pad "15" thru_hole oval locked (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "B_TXN02") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" thru_hole oval locked (at -2.54 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "unconnected-(J1-Pad16)") (pinfunction "Pin_16") (pintype "passive+no_connect"))
    (pad "17" thru_hole oval locked (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" thru_hole oval locked (at -2.54 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" thru_hole oval locked (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "B_TXP03") (pinfunction "Pin_19") (pintype "passive"))
    (pad "20" thru_hole oval locked (at -2.54 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "unconnected-(J1-Pad20)") (pinfunction "Pin_20") (pintype "passive+no_connect"))
    (pad "21" thru_hole oval locked (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "B_TXN03") (pinfunction "Pin_21") (pintype "passive"))
    (pad "22" thru_hole oval locked (at -2.54 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "unconnected-(J1-Pad22)") (pinfunction "Pin_22") (pintype "passive+no_connect"))
    (pad "23" thru_hole oval locked (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_23") (pintype "passive"))
    (pad "24" thru_hole oval locked (at -2.54 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_24") (pintype "passive"))
    (pad "25" thru_hole oval locked (at 0 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "B_TXP04") (pinfunction "Pin_25") (pintype "passive"))
    (pad "26" thru_hole oval locked (at -2.54 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "unconnected-(J1-Pad26)") (pinfunction "Pin_26") (pintype "passive+no_connect"))
    (pad "27" thru_hole oval locked (at 0 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "B_TXN04") (pinfunction "Pin_27") (pintype "passive"))
    (pad "28" thru_hole oval locked (at -2.54 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "unconnected-(J1-Pad28)") (pinfunction "Pin_28") (pintype "passive+no_connect"))
    (pad "29" thru_hole oval locked (at 0 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_29") (pintype "passive"))
    (pad "30" thru_hole oval locked (at -2.54 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_30") (pintype "passive"))
    (pad "31" thru_hole oval locked (at 0 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "B_TXP05") (pinfunction "Pin_31") (pintype "passive"))
    (pad "32" thru_hole oval locked (at -2.54 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "unconnected-(J1-Pad32)") (pinfunction "Pin_32") (pintype "passive+no_connect"))
    (pad "33" thru_hole oval locked (at 0 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 "B_TXN05") (pinfunction "Pin_33") (pintype "passive"))
    (pad "34" thru_hole oval locked (at -2.54 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "unconnected-(J1-Pad34)") (pinfunction "Pin_34") (pintype "passive+no_connect"))
    (pad "35" thru_hole oval locked (at 0 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_35") (pintype "passive"))
    (pad "36" thru_hole oval locked (at -2.54 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_36") (pintype "passive"))
    (pad "37" thru_hole oval locked (at 0 45.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 "B_TXP06") (pinfunction "Pin_37") (pintype "passive"))
    (pad "38" thru_hole oval locked (at -2.54 45.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "unconnected-(J1-Pad38)") (pinfunction "Pin_38") (pintype "passive+no_connect"))
    (pad "39" thru_hole oval locked (at 0 48.26 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 "B_TXN06") (pinfunction "Pin_39") (pintype "passive"))
    (pad "40" thru_hole oval locked (at -2.54 48.26 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "unconnected-(J1-Pad40)") (pinfunction "Pin_40") (pintype "passive+no_connect"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x20_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_2x20_P2.54mm_Horizontal" (layer "F.Cu")
    (tedit 5A19A423)
    (at 107.33362 150.27362 90)
    (descr "Through hole angled socket strip, 2x20, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated")
    (tags "Through hole angled socket strip THT 2x20 2.54mm double row")
    (property "Sheetfile" "AdapterBoard.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J5" (at 3.24 -1.33 90) (layer "F.SilkS"))
    (fp_text value "Conn_02x20_Odd_Even" (at -5.65 51.03 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -8.315 24.13) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "B_TXP00") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at -2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "B_TXP07") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval locked (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "B_TXN00") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval locked (at -2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "B_TXN07") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval locked (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval locked (at -2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval locked (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "B_TXP01") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval locked (at -2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "B_TXP08") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval locked (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "B_TXN01") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval locked (at -2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "B_TXN08") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole oval locked (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole oval locked (at -2.54 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole oval locked (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "B_TXP02") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole oval locked (at -2.54 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 78 "unconnected-(J5-Pad14)") (pinfunction "Pin_14") (pintype "passive+no_connect"))
    (pad "15" thru_hole oval locked (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "B_TXN02") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" thru_hole oval locked (at -2.54 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 79 "unconnected-(J5-Pad16)") (pinfunction "Pin_16") (pintype "passive+no_connect"))
    (pad "17" thru_hole oval locked (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" thru_hole oval locked (at -2.54 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" thru_hole oval locked (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "B_TXP03") (pinfunction "Pin_19") (pintype "passive"))
    (pad "20" thru_hole oval locked (at -2.54 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 80 "unconnected-(J5-Pad20)") (pinfunction "Pin_20") (pintype "passive+no_connect"))
    (pad "21" thru_hole oval locked (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "B_TXN03") (pinfunction "Pin_21") (pintype "passive"))
    (pad "22" thru_hole oval locked (at -2.54 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 81 "unconnected-(J5-Pad22)") (pinfunction "Pin_22") (pintype "passive+no_connect"))
    (pad "23" thru_hole oval locked (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_23") (pintype "passive"))
    (pad "24" thru_hole oval locked (at -2.54 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_24") (pintype "passive"))
    (pad "25" thru_hole oval locked (at 0 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "B_TXP04") (pinfunction "Pin_25") (pintype "passive"))
    (pad "26" thru_hole oval locked (at -2.54 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 82 "unconnected-(J5-Pad26)") (pinfunction "Pin_26") (pintype "passive+no_connect"))
    (pad "27" thru_hole oval locked (at 0 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "B_TXN04") (pinfunction "Pin_27") (pintype "passive"))
    (pad "28" thru_hole oval locked (at -2.54 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 83 "unconnected-(J5-Pad28)") (pinfunction "Pin_28") (pintype "passive+no_connect"))
    (pad "29" thru_hole oval locked (at 0 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_29") (pintype "passive"))
    (pad "30" thru_hole oval locked (at -2.54 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_30") (pintype "passive"))
    (pad "31" thru_hole oval locked (at 0 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "B_TXP05") (pinfunction "Pin_31") (pintype "passive"))
    (pad "32" thru_hole oval locked (at -2.54 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 84 "unconnected-(J5-Pad32)") (pinfunction "Pin_32") (pintype "passive+no_connect"))
    (pad "33" thru_hole oval locked (at 0 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 "B_TXN05") (pinfunction "Pin_33") (pintype "passive"))
    (pad "34" thru_hole oval locked (at -2.54 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 85 "unconnected-(J5-Pad34)") (pinfunction "Pin_34") (pintype "passive+no_connect"))
    (pad "35" thru_hole oval locked (at 0 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_35") (pintype "passive"))
    (pad "36" thru_hole oval locked (at -2.54 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_36") (pintype "passive"))
    (pad "37" thru_hole oval locked (at 0 45.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 "B_TXP06") (pinfunction "Pin_37") (pintype "passive"))
    (pad "38" thru_hole oval locked (at -2.54 45.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 86 "unconnected-(J5-Pad38)") (pinfunction "Pin_38") (pintype "passive+no_connect"))
    (pad "39" thru_hole oval locked (at 0 48.26 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 "B_TXN06") (pinfunction "Pin_39") (pintype "passive"))
    (pad "40" thru_hole oval locked (at -2.54 48.26 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 87 "unconnected-(J5-Pad40)") (pinfunction "Pin_40") (pintype "passive+no_connect"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x20_P2.54mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_2x20_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A433)
    (at 92.53362 96.54862 90)
    (descr "Through hole straight socket strip, 2x20, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 2x20 2.54mm double row")
    (property "Sheetfile" "AdapterBoard.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J3" (at -1.27 -2.77 90) (layer "F.SilkS"))
    (fp_text value "Conn_02x20_Odd_Even" (at -1.27 51.03 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -1.27 24.13) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 "unconnected-(J3-Pad1)") (pinfunction "Pin_1") (pintype "passive+no_connect"))
    (pad "2" thru_hole oval locked (at -2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 "unconnected-(J3-Pad2)") (pinfunction "Pin_2") (pintype "passive+no_connect"))
    (pad "3" thru_hole oval locked (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 "B_TXN06") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval locked (at -2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 "unconnected-(J3-Pad4)") (pinfunction "Pin_4") (pintype "passive+no_connect"))
    (pad "5" thru_hole oval locked (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 "unconnected-(J3-Pad5)") (pinfunction "Pin_5") (pintype "passive+no_connect"))
    (pad "6" thru_hole oval locked (at -2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 "DQ31") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval locked (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 "PMODE_2") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval locked (at -2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 "DQ30") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval locked (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 52 "PMODE_1") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval locked (at -2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 53 "DQ29") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole oval locked (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 54 "PMODE_0") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole oval locked (at -2.54 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 55 "DQ28") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole oval locked (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole oval locked (at -2.54 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 56 "GPIO45") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" thru_hole oval locked (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" thru_hole oval locked (at -2.54 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 57 "DQ27") (pinfunction "Pin_16") (pintype "passive"))
    (pad "17" thru_hole oval locked (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" thru_hole oval locked (at -2.54 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 58 "DQ26") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" thru_hole oval locked (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "B_TXP04") (pinfunction "Pin_19") (pintype "passive"))
    (pad "20" thru_hole oval locked (at -2.54 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 59 "DQ25") (pinfunction "Pin_20") (pintype "passive"))
    (pad "21" thru_hole oval locked (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "B_TXN04") (pinfunction "Pin_21") (pintype "passive"))
    (pad "22" thru_hole oval locked (at -2.54 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 60 "DQ24") (pinfunction "Pin_22") (pintype "passive"))
    (pad "23" thru_hole oval locked (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "B_TXP05") (pinfunction "Pin_23") (pintype "passive"))
    (pad "24" thru_hole oval locked (at -2.54 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 61 "DQ23") (pinfunction "Pin_24") (pintype "passive"))
    (pad "25" thru_hole oval locked (at 0 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_25") (pintype "passive"))
    (pad "26" thru_hole oval locked (at -2.54 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 62 "DQ22") (pinfunction "Pin_26") (pintype "passive"))
    (pad "27" thru_hole oval locked (at 0 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 "B_TXN05") (pinfunction "Pin_27") (pintype "passive"))
    (pad "28" thru_hole oval locked (at -2.54 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 63 "DQ21") (pinfunction "Pin_28") (pintype "passive"))
    (pad "29" thru_hole oval locked (at 0 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_29") (pintype "passive"))
    (pad "30" thru_hole oval locked (at -2.54 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 64 "DQ20") (pinfunction "Pin_30") (pintype "passive"))
    (pad "31" thru_hole oval locked (at 0 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 65 "I2S_WS") (pinfunction "Pin_31") (pintype "passive"))
    (pad "32" thru_hole oval locked (at -2.54 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 66 "DQ19") (pinfunction "Pin_32") (pintype "passive"))
    (pad "33" thru_hole oval locked (at 0 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 67 "I2S_SD") (pinfunction "Pin_33") (pintype "passive"))
    (pad "34" thru_hole oval locked (at -2.54 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 68 "DQ18") (pinfunction "Pin_34") (pintype "passive"))
    (pad "35" thru_hole oval locked (at 0 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 69 "I2S_MCLK") (pinfunction "Pin_35") (pintype "passive"))
    (pad "36" thru_hole oval locked (at -2.54 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 70 "DQ17") (pinfunction "Pin_36") (pintype "passive"))
    (pad "37" thru_hole oval locked (at 0 45.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 71 "I2S_CLK") (pinfunction "Pin_37") (pintype "passive"))
    (pad "38" thru_hole oval locked (at -2.54 45.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 "B_TXP06") (pinfunction "Pin_38") (pintype "passive"))
    (pad "39" thru_hole oval locked (at 0 48.26 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_39") (pintype "passive"))
    (pad "40" thru_hole oval locked (at -2.54 48.26 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_40") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x20_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" locked (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 217.94125 153.76375)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "AdapterBoard.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H5" (at 0 -4.2) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_2x20_P2.54mm_Horizontal" (layer "F.Cu")
    (tedit 5A19A423)
    (at 160.23362 150.27362 90)
    (descr "Through hole angled socket strip, 2x20, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated")
    (tags "Through hole angled socket strip THT 2x20 2.54mm double row")
    (property "Sheetfile" "AdapterBoard.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J6" (at 3.24 -0.68 90) (layer "F.SilkS"))
    (fp_text value "Conn_02x20_Odd_Even" (at -5.65 51.03 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -8.315 24.13) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "DQ8") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at -2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "DQ9") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval locked (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 104 "DQ6") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval locked (at -2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 110 "DQ7") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval locked (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval locked (at -2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval locked (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 101 "DQ4") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval locked (at -2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 99 "DQ5") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval locked (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 108 "DQ2") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval locked (at -2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 103 "DQ3") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole oval locked (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole oval locked (at -2.54 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole oval locked (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 106 "DQ1") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole oval locked (at -2.54 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 88 "unconnected-(J6-Pad14)") (pinfunction "Pin_14") (pintype "passive+no_connect"))
    (pad "15" thru_hole oval locked (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 105 "DQ0") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" thru_hole oval locked (at -2.54 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 89 "unconnected-(J6-Pad16)") (pinfunction "Pin_16") (pintype "passive+no_connect"))
    (pad "17" thru_hole oval locked (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" thru_hole oval locked (at -2.54 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" thru_hole oval locked (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 107 "PCLK") (pinfunction "Pin_19") (pintype "passive"))
    (pad "20" thru_hole oval locked (at -2.54 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 90 "unconnected-(J6-Pad20)") (pinfunction "Pin_20") (pintype "passive+no_connect"))
    (pad "21" thru_hole oval locked (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 109 "CTL0") (pinfunction "Pin_21") (pintype "passive"))
    (pad "22" thru_hole oval locked (at -2.54 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 91 "unconnected-(J6-Pad22)") (pinfunction "Pin_22") (pintype "passive+no_connect"))
    (pad "23" thru_hole oval locked (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_23") (pintype "passive"))
    (pad "24" thru_hole oval locked (at -2.54 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_24") (pintype "passive"))
    (pad "25" thru_hole oval locked (at 0 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 102 "CTL1") (pinfunction "Pin_25") (pintype "passive"))
    (pad "26" thru_hole oval locked (at -2.54 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 92 "unconnected-(J6-Pad26)") (pinfunction "Pin_26") (pintype "passive+no_connect"))
    (pad "27" thru_hole oval locked (at 0 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 100 "CTL2") (pinfunction "Pin_27") (pintype "passive"))
    (pad "28" thru_hole oval locked (at -2.54 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 93 "unconnected-(J6-Pad28)") (pinfunction "Pin_28") (pintype "passive+no_connect"))
    (pad "29" thru_hole oval locked (at 0 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_29") (pintype "passive"))
    (pad "30" thru_hole oval locked (at -2.54 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_30") (pintype "passive"))
    (pad "31" thru_hole oval locked (at 0 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 98 "CTL3") (pinfunction "Pin_31") (pintype "passive"))
    (pad "32" thru_hole oval locked (at -2.54 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 94 "unconnected-(J6-Pad32)") (pinfunction "Pin_32") (pintype "passive+no_connect"))
    (pad "33" thru_hole oval locked (at 0 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "CTL4") (pinfunction "Pin_33") (pintype "passive"))
    (pad "34" thru_hole oval locked (at -2.54 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 95 "unconnected-(J6-Pad34)") (pinfunction "Pin_34") (pintype "passive+no_connect"))
    (pad "35" thru_hole oval locked (at 0 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_35") (pintype "passive"))
    (pad "36" thru_hole oval locked (at -2.54 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_36") (pintype "passive"))
    (pad "37" thru_hole oval locked (at 0 45.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "CTL5") (pinfunction "Pin_37") (pintype "passive"))
    (pad "38" thru_hole oval locked (at -2.54 45.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 96 "unconnected-(J6-Pad38)") (pinfunction "Pin_38") (pintype "passive+no_connect"))
    (pad "39" thru_hole oval locked (at 0 48.26 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "CTL6") (pinfunction "Pin_39") (pintype "passive"))
    (pad "40" thru_hole oval locked (at -2.54 48.26 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 97 "unconnected-(J6-Pad40)") (pinfunction "Pin_40") (pintype "passive+no_connect"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x20_P2.54mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line locked (start 81.52125 156.76375) (end 81.52125 35.15375) (layer "Edge.Cuts") (width 0.15))
  (gr_line locked (start 220.94125 35.15375) (end 220.94125 156.76375) (layer "Edge.Cuts") (width 0.15))
  (gr_line locked (start 220.94125 156.76375) (end 81.52125 156.76375) (layer "Edge.Cuts") (width 0.15))
  (gr_line locked (start 81.52125 35.15375) (end 220.94125 35.15375) (layer "Edge.Cuts") (width 0.15))
  (gr_text "FX3 to T120BGA324 Dev Board Adapter\n\n6/2022" (at 88.28362 142.89362 -270) (layer "F.SilkS"))
  (gr_text "Connect to P2 adapter on Efinix" (at 183.44237 130.29487) (layer "F.SilkS"))
  (gr_text "Connect to P3 adapter on Efinix" (at 131.37237 130.29487) (layer "F.SilkS"))
  (gr_text "FX3" (at 115.49737 78.22487) (layer "F.SilkS"))
  (gr_text "USB" (at 86.36 76.2 90) (layer "F.SilkS"))
  (zone locked (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour allowed) (footprints not_allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 121.82125 71.55375)
        (xy 121.82125 79.17375)
        (xy 175.16125 79.17375)
        (xy 175.16125 71.55375)
      )
    )
  )
  (zone locked (net 1) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 79.536211 32.616882)
        (xy 222.82145 32.61375)
        (xy 222.82145 158.24215)
        (xy 80.01 158.245282)
      )
    )
  )
)
