(kicad_pcb (version 20171130) (host pcbnew "(5.1.6)-1")
  (general
    (thickness 1.6)
    (drawings 63)
    (tracks 397)
    (zones 0)
    (modules 39)
    (nets 42)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (1 In1.Gnd.Cu power hide)
    (2 In2.3v3.Cu power hide)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.2032)
    (user_trace_width 0.2032)
    (user_trace_width 0.4064)
    (trace_clearance 0.2032)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.4064)
    (via_drill 0.3048)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.15)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.7 1.7)
    (pad_drill 1)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /FREE)
  (net 2 /TX)
  (net 3 /RX)
  (net 4 GND)
  (net 5 /AREF)
  (net 6 +3V3)
  (net 7 /~RST)
  (net 8 /SDA)
  (net 9 /SCL)
  (net 10 /VUSB)
  (net 11 /EN)
  (net 12 /VBAT)
  (net 13 +BATT)
  (net 14 "Net-(D1-Pad2)")
  (net 15 /SD_DOut)
  (net 16 /SD_DIn)
  (net 17 /SD_CLK)
  (net 18 /APDS_INT)
  (net 19 /Batt_Meas)
  (net 20 /VUSB_Meas)
  (net 21 /3v3_Reg_En)
  (net 22 /3v3_feather)
  (net 23 /32KHz)
  (net 24 /DS3231_INT)
  (net 25 /DS3231_RST)
  (net 26 /PDM_DATA)
  (net 27 /PDM_CLK)
  (net 28 "Net-(J3-Pad1)")
  (net 29 /SD_CS)
  (net 30 "Net-(J3-Pad8)")
  (net 31 /SD_CD)
  (net 32 "Net-(JP2-Pad2)")
  (net 33 "Net-(JP3-Pad1)")
  (net 34 "Net-(JP5-Pad2)")
  (net 35 "Net-(R3-Pad2)")
  (net 36 "Net-(U1-Pad3)")
  (net 37 "Net-(U4-Pad4)")
  (net 38 /RTC_BATT)
  (net 39 /SHT30_ALERT)
  (net 40 "Net-(J1-Pad9)")
  (net 41 "Net-(J2-Pad7)")
  (net_class Default "This is the default net class."
    (clearance 0.2032)
    (trace_width 0.25)
    (via_dia 0.4064)
    (via_drill 0.3048)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /32KHz)
    (add_net /3v3_Reg_En)
    (add_net /APDS_INT)
    (add_net /AREF)
    (add_net /Batt_Meas)
    (add_net /DS3231_INT)
    (add_net /DS3231_RST)
    (add_net /EN)
    (add_net /FREE)
    (add_net /PDM_CLK)
    (add_net /PDM_DATA)
    (add_net /RTC_BATT)
    (add_net /RX)
    (add_net /SCL)
    (add_net /SDA)
    (add_net /SD_CD)
    (add_net /SD_CLK)
    (add_net /SD_CS)
    (add_net /SD_DIn)
    (add_net /SD_DOut)
    (add_net /SHT30_ALERT)
    (add_net /TX)
    (add_net /VUSB)
    (add_net /VUSB_Meas)
    (add_net /~RST)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(J1-Pad9)")
    (add_net "Net-(J2-Pad7)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J3-Pad8)")
    (add_net "Net-(JP2-Pad2)")
    (add_net "Net-(JP3-Pad1)")
    (add_net "Net-(JP5-Pad2)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U4-Pad4)")
  )
  (net_class Power ""
    (clearance 0.2032)
    (trace_width 0.4064)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +BATT)
    (add_net /3v3_feather)
    (add_net /VBAT)
    (add_net GND)
  )
  (module "My Libraries:MPD_BK-870" (layer B.Cu) (tedit 5EC94DD8)
    (at 36.2458 35.4584 90)
    (fp_text reference BT1 (at 0.0381 6.4262 90) (layer B.SilkS))
    (fp_text value 10mm (at 3.81663 -6.74276 90) (layer B.Fab))
    (fp_text user + (at -12.2065 -0.90048 90) (layer B.SilkS))
    (pad 1 smd rect (at -7.695 0 90) (size 3.2 3.2) (layers B.Cu B.Paste B.Mask)
      (net 13 +BATT))
    (pad 1 smd rect (at 7.695 0 90) (size 3.2 3.2) (layers B.Cu B.Paste B.Mask)
      (net 13 +BATT))
    (pad 2 smd circle (at 0 0 90) (size 8.13 8.13) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
  )
  (module "My Libraries:AMPHENOL_1140084168" (layer F.Cu) (tedit 5EC1940A)
    (at 28.702 36.576 270)
    (fp_text reference J3 (at -3.3274 -10.9474 90) (layer F.SilkS))
    (fp_text value 1140084168 (at 9.891 4.111 90) (layer F.Fab))
    (pad 1 smd rect (at 3.2 0.875 270) (size 0.7 1.75) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(J3-Pad1)"))
    (pad 2 smd rect (at 2.1 0.875 270) (size 0.7 1.75) (layers F.Cu F.Paste F.Mask)
      (net 29 /SD_CS))
    (pad 3 smd rect (at 1 0.875 270) (size 0.7 1.75) (layers F.Cu F.Paste F.Mask)
      (net 16 /SD_DIn))
    (pad 4 smd rect (at -0.1 0.875 270) (size 0.7 1.75) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 5 smd rect (at -1.2 0.875 270) (size 0.7 1.75) (layers F.Cu F.Paste F.Mask)
      (net 17 /SD_CLK))
    (pad 6 smd rect (at -2.3 0.875 270) (size 0.7 1.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 7 smd rect (at -3.4 0.875 270) (size 0.7 1.75) (layers F.Cu F.Paste F.Mask)
      (net 15 /SD_DOut))
    (pad 8 smd rect (at -4.5 0.875 270) (size 0.7 1.75) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(J3-Pad8)"))
    (pad 9 smd rect (at 5.575 -9.925 270) (size 1 1.55) (layers F.Cu F.Paste F.Mask)
      (net 31 /SD_CD))
    (pad 10 smd rect (at -5.625 -8.35 270) (size 1.45 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad S1 smd rect (at 5.65 0.75 270) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad S2 smd rect (at -5.7 0.75 270) (size 1.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad S3 smd rect (at 5.975 -7.5 270) (size 0.8 1.4) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad S4 smd rect (at -5.95 -6.85 270) (size 0.8 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
  )
  (module "My Libraries:DFN250X250X100-9N" (layer F.Cu) (tedit 5EC18B64)
    (at 73.533 36.322 180)
    (fp_text reference U3 (at -1.651 1.778) (layer F.SilkS))
    (fp_text value SHT30-DIS (at 3.384954 1.897078) (layer F.Fab))
    (pad 1 smd rect (at -1.175 -0.75 180) (size 0.55 0.25) (layers F.Cu F.Paste F.Mask)
      (net 8 /SDA))
    (pad 2 smd rect (at -1.175 -0.25 180) (size 0.55 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 3 smd rect (at -1.175 0.25 180) (size 0.55 0.25) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(JP3-Pad1)"))
    (pad 4 smd rect (at -1.175 0.75 180) (size 0.55 0.25) (layers F.Cu F.Paste F.Mask)
      (net 9 /SCL))
    (pad 8 smd rect (at 1.175 -0.75 180) (size 0.55 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 7 smd rect (at 1.175 -0.25 180) (size 0.55 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 6 smd rect (at 1.175 0.25 180) (size 0.55 0.25) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(R3-Pad2)"))
    (pad 5 smd rect (at 1.175 0.75 180) (size 0.55 0.25) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 9 smd rect (at 0 0 180) (size 1 1.7) (layers F.Cu F.Mask)
      (net 4 GND))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x12_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 69.85 26.67 90)
    (descr "Through hole straight pin header, 1x12, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x12 2.54mm single row")
    (fp_text reference J2 (at 0 2.33 90) (layer B.SilkS) hide)
    (fp_text value "feather short" (at 0 -30.27 90) (layer B.Fab) hide)
    (fp_text user %R (at 0 -13.97) (layer B.Fab))
    (pad 12 thru_hole oval (at 0 -27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /VBAT))
    (pad 11 thru_hole oval (at 0 -25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /EN))
    (pad 10 thru_hole oval (at 0 -22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /VUSB))
    (pad 9 thru_hole oval (at 0 -20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /3v3_Reg_En))
    (pad 8 thru_hole oval (at 0 -17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 /SHT30_ALERT))
    (pad 7 thru_hole oval (at 0 -15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 "Net-(J2-Pad7)"))
    (pad 6 thru_hole oval (at 0 -12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /32KHz))
    (pad 5 thru_hole oval (at 0 -10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /PDM_DATA))
    (pad 4 thru_hole oval (at 0 -7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 /DS3231_INT))
    (pad 3 thru_hole oval (at 0 -5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /DS3231_RST))
    (pad 2 thru_hole oval (at 0 -2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /SCL))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /SDA))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x12_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "My Libraries:XDCR_CMM-4737DT-26186-TR" (layer F.Cu) (tedit 5EC9525D)
    (at 73.152 40.894 270)
    (fp_text reference U5 (at -2.54 -2.032 180) (layer F.SilkS))
    (fp_text value CMM-4737DT-26186-TR (at 11.89 3.395 90) (layer F.Fab))
    (pad 1 smd circle (at -1.17 -1.65 270) (size 0.91 0.91) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd circle (at -1.17 0 270) (size 0.91 0.91) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 3 smd circle (at -1.17 1.65 270) (size 0.91 0.91) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 4 smd circle (at 1.17 1.65 270) (size 0.91 0.91) (layers F.Cu F.Paste F.Mask)
      (net 27 /PDM_CLK))
    (pad 5 smd circle (at 1.17 0 270) (size 0.91 0.91) (layers F.Cu F.Paste F.Mask)
      (net 26 /PDM_DATA))
    (pad 6 smd circle (at 1.17 -1.65 270) (size 0.5 0.5) (layers F.Cu)
      (net 6 +3V3))
  )
  (module Jumper:SolderJumper-2_P1.3mm_Bridged_RoundedPad1.0x1.5mm (layer F.Cu) (tedit 5C745284)
    (at 65.024 42.926 180)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, bridged with 1 copper strip")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP7 (at 0 -1.8) (layer F.SilkS) hide)
    (fp_text value SolderJumper_2_Bridged (at 0 1.9) (layer F.Fab))
    (pad 1 smd custom (at -0.65 0 180) (size 1 0.5) (layers F.Cu F.Mask)
      (net 27 /PDM_CLK) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy 0.5 -0.75) (xy 0.5 0.75) (xy 0 0.75)) (width 0))
      ))
    (pad 2 smd custom (at 0.65 0 180) (size 1 0.5) (layers F.Cu F.Mask)
      (net 2 /TX) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy -0.5 -0.75) (xy -0.5 0.75) (xy 0 0.75)) (width 0))
      ))
  )
  (module Diode_SMD:D_SOD-123F (layer F.Cu) (tedit 587F7769)
    (at 41.91 31.496 90)
    (descr D_SOD-123F)
    (tags D_SOD-123F)
    (attr smd)
    (fp_text reference D2 (at -0.127 -1.524 90) (layer F.SilkS))
    (fp_text value MBR120 (at 0 2.1 90) (layer F.Fab))
    (fp_text user %R (at -0.127 -1.905 90) (layer F.Fab))
    (pad 2 smd rect (at 1.4 0 90) (size 1.1 1.1) (layers F.Cu F.Paste F.Mask)
      (net 12 /VBAT))
    (pad 1 smd rect (at -1.4 0 90) (size 1.1 1.1) (layers F.Cu F.Paste F.Mask)
      (net 10 /VUSB))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123F.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Symbol:OSHW-Logo_5.7x6mm_SilkScreen locked (layer B.Cu) (tedit 0)
    (at 72.9361 36.4236 180)
    (descr "Open Source Hardware Logo")
    (tags "Logo OSHW")
    (attr virtual)
    (fp_text reference REF** (at 0 0) (layer B.SilkS) hide)
    (fp_text value OSHW-Logo_5.7x6mm_SilkScreen (at 0.75 0) (layer B.Fab) hide)
  )
  (module Jumper:SolderJumper-3_P1.3mm_Bridged12_RoundedPad1.0x1.5mm (layer B.Cu) (tedit 5ED870A5)
    (at 61.595 38.5064)
    (descr "SMD Solder 3-pad Jumper, 1x1.5mm rounded Pads, 0.3mm gap, pads 1-2 bridged with 1 copper strip")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP6 (at -0.0381 1.5367) (layer B.SilkS))
    (fp_text value "RTC Batt Select" (at -0.0508 -1.5494) (layer B.SilkS))
    (pad 1 smd custom (at -1.3 0) (size 1 0.5) (layers B.Cu B.Mask)
      (net 12 /VBAT) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy 0.55 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.55 -0.75)) (width 0))
      ))
    (pad 2 smd rect (at 0 0) (size 1 1.5) (layers B.Cu B.Mask)
      (net 38 /RTC_BATT))
    (pad 3 smd custom (at 1.3 0) (size 1 0.5) (layers B.Cu B.Mask)
      (net 13 +BATT) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy -0.55 0.75) (xy 0 0.75) (xy 0 -0.75) (xy -0.55 -0.75)) (width 0))
      ))
  )
  (module Package_SO:SOIC-8_3.9x4.9mm_P1.27mm (layer F.Cu) (tedit 5D9F72B1)
    (at 61.5823 32.9946 90)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference U2 (at 0.0254 -3.1115 90) (layer F.SilkS))
    (fp_text value DS3231MZ (at 0 3.4 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 8 smd roundrect (at 2.475 -1.905 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 /SCL))
    (pad 7 smd roundrect (at 2.475 -0.635 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 /SDA))
    (pad 6 smd roundrect (at 2.475 0.635 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 38 /RTC_BATT))
    (pad 5 smd roundrect (at 2.475 1.905 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (pad 4 smd roundrect (at -2.475 1.905 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 /DS3231_RST))
    (pad 3 smd roundrect (at -2.475 0.635 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 /DS3231_INT))
    (pad 2 smd roundrect (at -2.475 -0.635 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 +3V3))
    (pad 1 smd roundrect (at -2.475 -1.905 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 /32KHz))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 5EC951F1)
    (at 50.6222 35.56 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JP2 (at -0.0254 -1.8542 90) (layer F.SilkS))
    (fp_text value M02 (at 0 4.87 270) (layer F.Fab))
    (fp_text user %R (at 0 1.27) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(JP2-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 +3V3))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.5mm locked (layer F.Cu) (tedit 56D1B4CB)
    (at 73.66 27.94)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.7) (layer F.Fab) hide)
    (fp_text value MountingHole_2.5mm (at 0 3.7) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.5mm locked (layer F.Cu) (tedit 56D1B4CB)
    (at 73.66 45.72)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at -0.06604 -1.8415) (layer F.Fab) hide)
    (fp_text value MountingHole_2.5mm (at 0 3.7) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module Package_TO_SOT_SMD:SOT-23-5 (layer F.Cu) (tedit 5A02FF57)
    (at 46.863 31.9024)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U4 (at 0 -2.2606) (layer F.SilkS))
    (fp_text value MIC5504-3.3YM5 (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 5 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(JP2-Pad2)"))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(U4-Pad4)"))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 21 /3v3_Reg_En))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 10 /VUSB))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "My Libraries:APDS-9960" (layer F.Cu) (tedit 5EC184F8)
    (at 73.406 32.258 270)
    (descr "<h3>APDS-9960 Proximity, Light, RGB, Gesture Sensor</h3><p>Specifications:<ul><li>Pin Count: 8</li><li>Dimensions: 3.94 x 2.36 x 1.35 mm</li><li>Pitch: 0.97 mm</li></ul><p>Devices Using:</p><ul><li>APDS-9960</li></ul>")
    (fp_text reference U1 (at -1.778 1.778 180) (layer F.SilkS))
    (fp_text value APDS-9960 (at 0 2.4638 90) (layer F.Fab))
    (pad 1 smd rect (at 0.7 -1.455 270) (size 0.6 0.72) (layers F.Cu F.Paste F.Mask)
      (net 8 /SDA))
    (pad 2 smd rect (at 0.7 -0.485 270) (size 0.6 0.72) (layers F.Cu F.Paste F.Mask)
      (net 18 /APDS_INT))
    (pad 3 smd rect (at 0.7 0.485 270) (size 0.6 0.72) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(U1-Pad3)"))
    (pad 4 smd rect (at 0.7 1.455 270) (size 0.6 0.72) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(U1-Pad3)"))
    (pad 5 smd rect (at -0.7 1.455 270) (size 0.6 0.72) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 6 smd rect (at -0.7 0.485 270) (size 0.6 0.72) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 7 smd rect (at -0.7 -0.485 270) (size 0.6 0.72) (layers F.Cu F.Paste F.Mask)
      (net 9 /SCL))
    (pad 8 smd rect (at -0.7 -1.455 270) (size 0.6 0.72) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 66.802 30.48 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R13 (at 0 -1.4224 90) (layer F.SilkS))
    (fp_text value 4.7K (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 /SCL))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 68.58 30.48 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R12 (at -0.0508 1.4478 90) (layer F.SilkS))
    (fp_text value 4.7K (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 /SDA))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 33.3375 26.924 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R11 (at 2.1209 0.0762 90) (layer F.SilkS))
    (fp_text value 1K (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 "Net-(JP5-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 54.0512 32.766)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R6 (at 2.0828 0.0254 90) (layer F.SilkS))
    (fp_text value 4.7K (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 /VUSB_Meas))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 54.0512 30.861)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at 2.1082 0 90) (layer F.SilkS))
    (fp_text value 4.7K (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 /VUSB_Meas))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 /VUSB))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 46.736 36.83)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at -2.286 0.762) (layer F.SilkS))
    (fp_text value DNP (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 /3v3_Reg_En))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 /VUSB))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 67.056 36.7665 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at 0 -1.3208 90) (layer F.SilkS))
    (fp_text value 4.7K (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 "Net-(R3-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 63.4873 38.5826 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at -2.3368 -0.0127 90) (layer F.SilkS))
    (fp_text value 4.7K (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 /DS3231_INT))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 59.5503 38.5826 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at -2.3368 -0.0381 90) (layer F.SilkS))
    (fp_text value 4.7K (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 /32KHz))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm (layer F.Cu) (tedit 5B391E66)
    (at 33.3375 29.083 180)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP5 (at 1.8923 0.3048 90) (layer F.SilkS) hide)
    (fp_text value "LED En" (at -3.0861 0.381 180) (layer F.SilkS))
    (pad 2 smd custom (at 0.65 0 180) (size 1 0.5) (layers F.Cu F.Mask)
      (net 34 "Net-(JP5-Pad2)") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy -0.5 -0.75) (xy -0.5 0.75) (xy 0 0.75)) (width 0))
      ))
    (pad 1 smd custom (at -0.65 0 180) (size 1 0.5) (layers F.Cu F.Mask)
      (net 6 +3V3) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy 0.5 -0.75) (xy 0.5 0.75) (xy 0 0.75)) (width 0))
      ))
  )
  (module Jumper:SolderJumper-2_P1.3mm_Bridged_RoundedPad1.0x1.5mm (layer F.Cu) (tedit 5C745284)
    (at 50.038 32.0548 270)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, bridged with 1 copper strip")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP4 (at -1.8034 0 180) (layer F.SilkS) hide)
    (fp_text value "Reg En" (at 0 -1.4986 270) (layer F.SilkS))
    (pad 1 smd custom (at -0.65 0 270) (size 1 0.5) (layers F.Cu F.Mask)
      (net 32 "Net-(JP2-Pad2)") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy 0.5 -0.75) (xy 0.5 0.75) (xy 0 0.75)) (width 0))
      ))
    (pad 2 smd custom (at 0.65 0 270) (size 1 0.5) (layers F.Cu F.Mask)
      (net 6 +3V3) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy -0.5 -0.75) (xy -0.5 0.75) (xy 0 0.75)) (width 0))
      ))
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm (layer B.Cu) (tedit 5B391E66)
    (at 66.7258 36.6395 270)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP3 (at -2.4384 -0.0381 270) (layer B.SilkS))
    (fp_text value SHT30-Alert (at 0 -1.9 270) (layer B.SilkS))
    (pad 2 smd custom (at 0.65 0 270) (size 1 0.5) (layers B.Cu B.Mask)
      (net 39 /SHT30_ALERT) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)) (width 0))
      ))
    (pad 1 smd custom (at -0.65 0 270) (size 1 0.5) (layers B.Cu B.Mask)
      (net 33 "Net-(JP3-Pad1)") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy 0 0.75) (xy 0.5 0.75) (xy 0.5 -0.75) (xy 0 -0.75)) (width 0))
      ))
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm (layer F.Cu) (tedit 5B391E66)
    (at 32.639 44.704)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP1 (at 2.2225 0.5969) (layer F.SilkS) hide)
    (fp_text value "3.3V Select" (at 3.937 -0.8255) (layer F.SilkS))
    (pad 2 smd custom (at 0.65 0) (size 1 0.5) (layers F.Cu F.Mask)
      (net 22 /3v3_feather) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy -0.5 -0.75) (xy -0.5 0.75) (xy 0 0.75)) (width 0))
      ))
    (pad 1 smd custom (at -0.65 0) (size 1 0.5) (layers F.Cu F.Mask)
      (net 6 +3V3) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy 0.5 -0.75) (xy 0.5 0.75) (xy 0 0.75)) (width 0))
      ))
  )
  (module LED_SMD:LED_1206_3216Metric (layer F.Cu) (tedit 5B301BBE)
    (at 37.338 26.924 180)
    (descr "LED SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D1 (at -0.0635 0) (layer F.SilkS))
    (fp_text value PWR_LED (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 14 "Net-(D1-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 4 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 41.656 36.8935)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C7 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 46.6344 34.7218 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C6 (at 2.1844 -0.5842) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 43.9674 31.9278 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C5 (at -2.286 0 180) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 /VUSB))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 69.0626 36.6776 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at -1.991102 -0.520734 180) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 67.818 33.274 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at -2.032 0 90) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 61.5188 38.5826 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at 2.3368 0 90) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 69.088 40.894 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 0.762 -1.27 90) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.7mm_M2.5 locked (layer F.Cu) (tedit 56D1B4CB)
    (at 27.94 45.72)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.7) (layer F.Fab) hide)
    (fp_text value MountingHole_2.7mm_M2.5 (at 0 3.7) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.7mm_M2.5 locked (layer F.Cu) (tedit 56D1B4CB)
    (at 27.94 27.94)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.7) (layer F.Fab) hide)
    (fp_text value MountingHole_2.7mm_M2.5 (at 0 3.7) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x16_P2.54mm_Vertical (layer B.Cu) (tedit 5ED2013A)
    (at 69.85 46.99 90)
    (descr "Through hole straight pin header, 1x16, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x16 2.54mm single row")
    (fp_text reference J1 (at 0 2.33 90) (layer B.SilkS) hide)
    (fp_text value "feather long" (at 0 -40.43 90) (layer B.Fab) hide)
    (fp_text user %R (at 0 -19.05) (layer B.Fab))
    (pad 16 thru_hole oval (at 0 -38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /~RST))
    (pad 15 thru_hole oval (at 0 -35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /3v3_feather))
    (pad 14 thru_hole oval (at 0 -33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /AREF))
    (pad 13 thru_hole oval (at 0 -30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 12 thru_hole oval (at 0 -27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 /SD_CD))
    (pad 11 thru_hole oval (at 0 -25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /SD_CS))
    (pad 10 thru_hole oval (at 0 -22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /APDS_INT))
    (pad 9 thru_hole oval (at 0 -20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 "Net-(J1-Pad9)"))
    (pad 8 thru_hole oval (at 0 -17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /Batt_Meas))
    (pad 7 thru_hole oval (at 0 -15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /VUSB_Meas))
    (pad 6 thru_hole oval (at 0 -12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /SD_CLK))
    (pad 5 thru_hole oval (at 0 -10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /SD_DIn))
    (pad 4 thru_hole oval (at 0 -7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /SD_DOut))
    (pad 3 thru_hole oval (at 0 -5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /RX))
    (pad 2 thru_hole oval (at 0 -2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /TX))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /FREE))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x16_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text PDM (at 67.564 43.942) (layer B.SilkS))
  (gr_text PDM (at 67.564 43.942) (layer F.SilkS))
  (gr_text TX (at 62.992 42.926 90) (layer F.SilkS))
  (gr_text "SHLT Sensor Wing\njames@baldengineer.com\nRev2\nHi to everyone who helped on the Twitch Stream!\n(balden3Yay)" (at 58.6232 41.529) (layer B.SilkS))
  (gr_text "SHLT Sensor Wing\nrev 2" (at 50.4825 42.8625) (layer F.SilkS))
  (gr_text SDA (at 69.8119 28.575) (layer B.SilkS))
  (gr_text SCL (at 67.2846 28.5877) (layer B.SilkS))
  (gr_text DSRST (at 64.77 28.5496) (layer B.SilkS))
  (gr_text DSINT (at 62.23 28.5496) (layer B.SilkS))
  (gr_text 32K (at 57.15 28.575) (layer B.SilkS))
  (gr_text "PDM\nCLK" (at 59.69 28.702) (layer B.SilkS))
  (gr_text "SHT\nALERT" (at 52.0573 28.956) (layer B.SilkS))
  (gr_text "3v3\nEn" (at 49.5173 28.9433) (layer B.SilkS))
  (gr_text VUSB (at 46.9646 28.575) (layer B.SilkS))
  (gr_text EN (at 44.45 28.6004) (layer B.SilkS))
  (gr_text VBAT (at 41.8973 28.5623) (layer B.SilkS))
  (gr_text AREF (at 36.83 45.0977) (layer B.SilkS))
  (gr_text GND (at 39.3827 45.0977) (layer B.SilkS))
  (gr_text "SD\nCD" (at 41.91 44.831) (layer B.SilkS))
  (gr_text "SD\nCS" (at 44.4246 44.831) (layer B.SilkS))
  (gr_text "VUSB\nMeas" (at 54.61 44.831) (layer B.SilkS))
  (gr_text "Batt\nMeas" (at 52.1081 44.831) (layer B.SilkS))
  (gr_text "APDS\nINT" (at 46.99 44.831) (layer B.SilkS))
  (gr_text "SD\nCLK" (at 57.1246 44.831) (layer B.SilkS))
  (gr_text MOSI (at 59.69 45.0977) (layer B.SilkS))
  (gr_text MISO (at 62.2554 45.0596) (layer B.SilkS))
  (gr_text RX (at 64.77 45.0596) (layer B.SilkS))
  (gr_text TX (at 67.3862 45.0723) (layer B.SilkS))
  (gr_text 3v3 (at 50.6222 34.1884) (layer F.SilkS))
  (gr_text 3v3 (at 50.6095 34.1884) (layer B.SilkS))
  (gr_text LiPo (at 58.8645 38.5191 90) (layer B.SilkS))
  (gr_text Coin (at 64.3509 38.4683 90) (layer B.SilkS))
  (gr_text 32K (at 57.15 28.575) (layer F.SilkS))
  (gr_text VUSB (at 46.99 28.575) (layer F.SilkS))
  (gr_text VBAT (at 41.91 28.575) (layer F.SilkS))
  (gr_text EN (at 44.45 28.575) (layer F.SilkS))
  (gr_text "3v3\nEn" (at 49.53 28.956) (layer F.SilkS))
  (gr_text "SHT\nALERT" (at 52.07 28.956) (layer F.SilkS))
  (gr_text "PDM\nCLK" (at 59.69 28.702) (layer F.SilkS))
  (gr_text DSINT (at 62.23 28.575) (layer F.SilkS))
  (gr_text DSRST (at 64.77 28.575) (layer F.SilkS))
  (gr_text SCL (at 67.31 28.575) (layer F.SilkS))
  (gr_text SDA (at 69.85 28.575) (layer F.SilkS))
  (gr_text TX (at 67.31 45.085) (layer F.SilkS))
  (gr_text RX (at 64.77 45.085) (layer F.SilkS))
  (gr_text MISO (at 62.23 45.085) (layer F.SilkS))
  (gr_text MOSI (at 59.69 45.085) (layer F.SilkS))
  (gr_text "SD\nCLK" (at 57.15 44.831) (layer F.SilkS))
  (gr_text "APDS\nINT" (at 46.99 44.831) (layer F.SilkS))
  (gr_text "Batt\nMeas" (at 52.07 44.831) (layer F.SilkS))
  (gr_text "VUSB\nMeas" (at 54.61 44.831) (layer F.SilkS))
  (gr_text "SD\nCS" (at 44.45 44.831) (layer F.SilkS))
  (gr_text "SD\nCD" (at 41.91 44.831) (layer F.SilkS))
  (gr_text GND (at 39.37 45.085) (layer F.SilkS))
  (gr_text AREF (at 36.83 45.085) (layer F.SilkS))
  (gr_arc (start 73.66 27.94) (end 76.2 27.94) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 73.66 45.72) (end 73.66 48.26) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 27.94 45.72) (end 25.4 45.72) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 27.94 27.94) (end 27.94 25.4) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 25.4 45.72) (end 25.4 27.94) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 73.66 48.26) (end 27.94 48.26) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 76.2 27.94) (end 76.2 45.72) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 27.94 25.4) (end 73.66 25.4) (layer Edge.Cuts) (width 0.2))
  (zone (net 4) (net_name GND) (layer In1.Gnd.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 76.2 48.26) (xy 25.4 48.26) (xy 25.4 25.4) (xy 76.2 25.4)
      )
    )
  )
  (zone (net 4) (net_name GND) (layer B.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 76.2 48.26) (xy 25.4 48.26) (xy 25.4 25.4) (xy 76.2 25.4)
      )
    )
  )
  (zone (net 6) (net_name +3V3) (layer In2.3v3.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 76.2 48.26) (xy 25.4 48.26) (xy 25.4 25.4) (xy 76.2 25.4)
      )
    )
  )
  (zone (net 4) (net_name GND) (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 76.2 48.26) (xy 25.4 48.26) (xy 25.4 25.4) (xy 76.2 25.4)
      )
    )
  )
  (zone (net 4) (net_name GND) (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.2032))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 77.2 49.26) (xy 26.4 49.26) (xy 26.4 26.4) (xy 77.2 26.4)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 75.946 38.354) (xy 70.866 38.354) (xy 70.866 34.29) (xy 75.946 34.29)
      )
    )
  )
  (zone (net 0) (net_name "") (layers F.Cu In1.Gnd.Cu In2.3v3.Cu B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 75.946 38.354) (xy 70.866 38.354) (xy 70.866 34.29) (xy 75.946 34.29)
      )
    )
  )
)
