(kicad_pcb (version 20171130) (host pcbnew "(5.1.6-0-10_14)")
  (general
    (thickness 1.6)
    (drawings 6)
    (tracks 108)
    (zones 0)
    (modules 8)
    (nets 44)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad12)")
  (net 2 "Net-(J1-Pad11)")
  (net 3 "Net-(J1-Pad10)")
  (net 4 "Net-(J1-Pad9)")
  (net 5 "Net-(J1-Pad8)")
  (net 6 "Net-(J1-Pad7)")
  (net 7 "Net-(J1-Pad6)")
  (net 8 "Net-(J1-Pad5)")
  (net 9 "/74HC595(1)")
  (net 10 "Net-(J1-Pad3)")
  (net 11 "Net-(J1-Pad2)")
  (net 12 "Net-(J1-Pad1)")
  (net 13 "Net-(J2-Pad10)")
  (net 14 "Net-(J2-Pad13)")
  (net 15 "Net-(J2-Pad14)")
  (net 16 "Net-(J2-Pad12)")
  (net 17 "Net-(J2-Pad11)")
  (net 18 "Net-(J2-Pad9)")
  (net 19 "Net-(J3-Pad7)")
  (net 20 "Net-(J3-Pad6)")
  (net 21 "Net-(J3-Pad5)")
  (net 22 "Net-(J3-Pad4)")
  (net 23 "Net-(J3-Pad3)")
  (net 24 "Net-(J3-Pad9)")
  (net 25 "Net-(J4-Pad12)")
  (net 26 "Net-(J4-Pad23)")
  (net 27 "Net-(J4-Pad11)")
  (net 28 "Net-(J4-Pad22)")
  (net 29 "Net-(J4-Pad10)")
  (net 30 "Net-(J4-Pad9)")
  (net 31 "Net-(J4-Pad20)")
  (net 32 "Net-(J4-Pad8)")
  (net 33 "Net-(J4-Pad7)")
  (net 34 "Net-(J4-Pad18)")
  (net 35 "Net-(J4-Pad6)")
  (net 36 "Net-(J4-Pad5)")
  (net 37 "Net-(J4-Pad16)")
  (net 38 "Net-(J4-Pad4)")
  (net 39 "Net-(J4-Pad3)")
  (net 40 "Net-(J4-Pad14)")
  (net 41 "Net-(J4-Pad2)")
  (net 42 "Net-(J4-Pad13)")
  (net 43 "Net-(J4-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "/74HC595(1)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad11)")
    (add_net "Net-(J1-Pad12)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J1-Pad9)")
    (add_net "Net-(J2-Pad10)")
    (add_net "Net-(J2-Pad11)")
    (add_net "Net-(J2-Pad12)")
    (add_net "Net-(J2-Pad13)")
    (add_net "Net-(J2-Pad14)")
    (add_net "Net-(J2-Pad9)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J3-Pad4)")
    (add_net "Net-(J3-Pad5)")
    (add_net "Net-(J3-Pad6)")
    (add_net "Net-(J3-Pad7)")
    (add_net "Net-(J3-Pad9)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(J4-Pad10)")
    (add_net "Net-(J4-Pad11)")
    (add_net "Net-(J4-Pad12)")
    (add_net "Net-(J4-Pad13)")
    (add_net "Net-(J4-Pad14)")
    (add_net "Net-(J4-Pad16)")
    (add_net "Net-(J4-Pad18)")
    (add_net "Net-(J4-Pad2)")
    (add_net "Net-(J4-Pad20)")
    (add_net "Net-(J4-Pad22)")
    (add_net "Net-(J4-Pad23)")
    (add_net "Net-(J4-Pad3)")
    (add_net "Net-(J4-Pad4)")
    (add_net "Net-(J4-Pad5)")
    (add_net "Net-(J4-Pad6)")
    (add_net "Net-(J4-Pad7)")
    (add_net "Net-(J4-Pad8)")
    (add_net "Net-(J4-Pad9)")
  )
  (module MountingHole:MountingHole_2.5mm (layer F.Cu) (tedit 56D1B4CB)
    (at 152.4 102.87)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.5mm (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module Package_DIP:DIP-12_W12.70mm_Socket (layer F.Cu) (tedit 60E33EFD)
    (at 127 67.31 90)
    (descr "12-lead though-hole mounted DIP package, row spacing 12.70 mm (500 mils), Socket")
    (tags "THT DIP DIL PDIP 2.54mm 12.70mm 500mil Socket")
    (fp_text reference "4-DIGIT 7-SEG" (at 7.62 6.35 180) (layer F.SilkS))
    (fp_text value Conn_02x06_Counter_Clockwise (at 7.62 16.51 90) (layer F.Fab))
    (fp_text user %R (at 7.62 6.35 90) (layer F.Fab))
    (pad 12 thru_hole oval (at 15.24 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad12)"))
    (pad 11 thru_hole oval (at 15.24 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad11)"))
    (pad 10 thru_hole oval (at 15.24 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad10)"))
    (pad 9 thru_hole oval (at 15.24 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad9)"))
    (pad 8 thru_hole oval (at 15.24 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad8)"))
    (pad 7 thru_hole oval (at 15.24 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad7)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad6)"))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad5)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "/74HC595(1)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad1)"))
  )
  (module MountingHole:MountingHole_2.5mm (layer F.Cu) (tedit 56D1B4CB)
    (at 152.4 54.61)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.5mm (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.5mm (layer F.Cu) (tedit 56D1B4CB)
    (at 114.3 54.61)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.5mm (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.5mm (layer F.Cu) (tedit 56D1B4CB)
    (at 114.3 102.87)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.5mm (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module Package_DIP:DIP-16_W7.62mm (layer F.Cu) (tedit 5A02E8C5)
    (at 148.59 77.47)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference 74HC595-2 (at 3.81 8.89 90) (layer F.SilkS))
    (fp_text value Conn_02x08_Counter_Clockwise (at 3.81 20.11) (layer F.Fab))
    (fp_text user %R (at 3.81 8.89) (layer F.Fab))
    (pad 16 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(J2-Pad10)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(J2-Pad13)"))
    (pad 15 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad9)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(J3-Pad7)"))
    (pad 14 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(J2-Pad9)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(J3-Pad6)"))
    (pad 13 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(J2-Pad13)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(J3-Pad5)"))
    (pad 12 thru_hole oval (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(J2-Pad12)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(J3-Pad4)"))
    (pad 11 thru_hole oval (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(J2-Pad11)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(J3-Pad3)"))
    (pad 10 thru_hole oval (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(J2-Pad10)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad6)"))
    (pad 9 thru_hole oval (at 7.62 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(J3-Pad9)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad8)"))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-16_W7.62mm (layer F.Cu) (tedit 5A02E8C5)
    (at 110.49 77.47)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference 74HC595-1 (at 3.81 8.89 90) (layer F.SilkS))
    (fp_text value Conn_02x08_Counter_Clockwise (at 3.81 20.11) (layer F.Fab))
    (fp_text user %R (at 3.81 8.89) (layer F.Fab))
    (pad 16 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(J2-Pad10)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(J2-Pad13)"))
    (pad 15 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad11)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad12)"))
    (pad 14 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(J2-Pad14)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad5)"))
    (pad 13 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(J2-Pad13)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad10)"))
    (pad 12 thru_hole oval (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(J2-Pad12)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad1)"))
    (pad 11 thru_hole oval (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(J2-Pad11)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad2)"))
    (pad 10 thru_hole oval (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(J2-Pad10)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "/74HC595(1)"))
    (pad 9 thru_hole oval (at 7.62 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(J2-Pad9)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad7)"))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Particle-Devices:PHOTON (layer F.Cu) (tedit 0)
    (at 143.51 72.39 180)
    (fp_text reference PHOTON (at 10.16 -20.32) (layer F.SilkS))
    (fp_text value Conn_02x12_Counter_Clockwise (at 7.62 30.27) (layer F.Fab))
    (fp_text user %R (at 7.62 13.97) (layer F.Fab))
    (fp_text user 24 (at 16.51 -32.766) (layer F.Fab))
    (fp_text user 13 (at 16.51 -4.826) (layer F.Fab))
    (fp_text user 12 (at 2.794 -4.826) (layer F.Fab))
    (fp_text user 1 (at 2.794 -32.766) (layer F.Fab))
    (fp_text user "GROUND PLANE\nAND SIGNAL KEEP OUT\nRECOMMENDED ON ALL LAYERS" (at 3.302 -1.143) (layer F.Fab))
    (fp_text user 13 (at 19.05 -4.826) (layer F.Fab))
    (pad 24 thru_hole circle (at 19.05 -33.02) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 "Net-(J2-Pad10)") (solder_mask_margin 0.1016))
    (pad 23 thru_hole circle (at 19.05 -30.48) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 "Net-(J4-Pad23)") (solder_mask_margin 0.1016))
    (pad 22 thru_hole circle (at 19.05 -27.94) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 28 "Net-(J4-Pad22)") (solder_mask_margin 0.1016))
    (pad 21 thru_hole circle (at 19.05 -25.4) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 14 "Net-(J2-Pad13)") (solder_mask_margin 0.1016))
    (pad 20 thru_hole circle (at 19.05 -22.86) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 31 "Net-(J4-Pad20)") (solder_mask_margin 0.1016))
    (pad 19 thru_hole circle (at 19.05 -20.32) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 16 "Net-(J2-Pad12)") (solder_mask_margin 0.1016))
    (pad 18 thru_hole circle (at 19.05 -17.78) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 34 "Net-(J4-Pad18)") (solder_mask_margin 0.1016))
    (pad 17 thru_hole circle (at 19.05 -15.24) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 "Net-(J2-Pad11)") (solder_mask_margin 0.1016))
    (pad 16 thru_hole circle (at 19.05 -12.7) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 37 "Net-(J4-Pad16)") (solder_mask_margin 0.1016))
    (pad 15 thru_hole circle (at 19.05 -10.16) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 "Net-(J2-Pad14)") (solder_mask_margin 0.1016))
    (pad 14 thru_hole circle (at 19.05 -7.62) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 40 "Net-(J4-Pad14)") (solder_mask_margin 0.1016))
    (pad 13 thru_hole circle (at 19.05 -5.08) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 42 "Net-(J4-Pad13)") (solder_mask_margin 0.1016))
    (pad 12 thru_hole circle (at 1.27 -5.08 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 25 "Net-(J4-Pad12)") (solder_mask_margin 0.1016))
    (pad 11 thru_hole circle (at 1.27 -7.62 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 27 "Net-(J4-Pad11)") (solder_mask_margin 0.1016))
    (pad 10 thru_hole circle (at 1.27 -10.16 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 29 "Net-(J4-Pad10)") (solder_mask_margin 0.1016))
    (pad 9 thru_hole circle (at 1.27 -12.7 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 30 "Net-(J4-Pad9)") (solder_mask_margin 0.1016))
    (pad 8 thru_hole circle (at 1.27 -15.24 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 32 "Net-(J4-Pad8)") (solder_mask_margin 0.1016))
    (pad 7 thru_hole circle (at 1.27 -17.78 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 33 "Net-(J4-Pad7)") (solder_mask_margin 0.1016))
    (pad 6 thru_hole circle (at 1.27 -20.32 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 35 "Net-(J4-Pad6)") (solder_mask_margin 0.1016))
    (pad 5 thru_hole circle (at 1.27 -22.86 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 36 "Net-(J4-Pad5)") (solder_mask_margin 0.1016))
    (pad 4 thru_hole circle (at 1.27 -25.4 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 38 "Net-(J4-Pad4)") (solder_mask_margin 0.1016))
    (pad 3 thru_hole circle (at 1.27 -27.94 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 39 "Net-(J4-Pad3)") (solder_mask_margin 0.1016))
    (pad 2 thru_hole circle (at 1.27 -30.48 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 41 "Net-(J4-Pad2)") (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at 1.27 -33.02 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 43 "Net-(J4-Pad1)") (solder_mask_margin 0.1016))
  )
  (gr_text "DMack, 07/2021" (at 118.11 69.85) (layer B.SilkS))
  (gr_text "Four Digit Display, Rev1" (at 146.05 69.85) (layer B.SilkS))
  (gr_line (start 158.75 48.26) (end 158.75 109.22) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 107.95 48.26) (end 158.75 48.26) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 107.95 109.22) (end 107.95 48.26) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 158.75 109.22) (end 107.95 109.22) (layer Edge.Cuts) (width 0.1))
)
