(kicad_pcb (version 20171130) (host pcbnew "(5.1.5-0-10_14)")
  (general
    (thickness 1.6)
    (drawings 22)
    (tracks 100)
    (zones 0)
    (modules 13)
    (nets 31)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user hide)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.35)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "./"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(C2-Pad1)")
  (net 3 "Net-(J1-Pad13)")
  (net 4 "Net-(J1-Pad12)")
  (net 5 "Net-(J1-Pad11)")
  (net 6 "Net-(J1-Pad10)")
  (net 7 "Net-(J1-Pad9)")
  (net 8 "Net-(J1-Pad8)")
  (net 9 "Net-(J1-Pad7)")
  (net 10 "Net-(J1-Pad6)")
  (net 11 "Net-(J1-Pad5)")
  (net 12 "Net-(J1-Pad4)")
  (net 13 "Net-(J1-Pad3)")
  (net 14 "Net-(J1-Pad2)")
  (net 15 "Net-(J1-Pad1)")
  (net 16 "Net-(J2-Pad13)")
  (net 17 "Net-(J2-Pad12)")
  (net 18 "Net-(J2-Pad11)")
  (net 19 "Net-(J2-Pad10)")
  (net 20 "Net-(J2-Pad9)")
  (net 21 "Net-(J2-Pad8)")
  (net 22 "Net-(J2-Pad7)")
  (net 23 "Net-(J2-Pad6)")
  (net 24 "Net-(J2-Pad3)")
  (net 25 "Net-(J2-Pad1)")
  (net 26 "Net-(J2-Pad2)")
  (net 27 "Net-(J2-Pad5)")
  (net 28 "Net-(J2-Pad4)")
  (net 29 "Net-(C1-Pad1)")
  (net 30 "Net-(P3-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad11)")
    (add_net "Net-(J1-Pad12)")
    (add_net "Net-(J1-Pad13)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J1-Pad9)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad10)")
    (add_net "Net-(J2-Pad11)")
    (add_net "Net-(J2-Pad12)")
    (add_net "Net-(J2-Pad13)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(J2-Pad6)")
    (add_net "Net-(J2-Pad7)")
    (add_net "Net-(J2-Pad8)")
    (add_net "Net-(J2-Pad9)")
    (add_net "Net-(P3-Pad1)")
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 156.2824 92.7608)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 0 -1.45) (layer F.SilkS))
    (fp_text value R (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J1-Pad5)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(P3-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 146.257 95.25 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 0 -1.45) (layer F.SilkS))
    (fp_text value R (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(J1-Pad3)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 151.9428 96.6508 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 0 -1.45 90) (layer F.SilkS))
    (fp_text value R (at 0 1.55 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(J1-Pad3)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module DMND62D0U:SOT65P210X110-3N (layer F.Cu) (tedit 5E7BCFFD)
    (at 159.2166 102.5548)
    (descr DMN62D0UW-7-1)
    (tags "MOSFET (N-Channel)")
    (attr smd)
    (fp_text reference Q3 (at -0.1364 -1.793) (layer F.SilkS))
    (fp_text value DMN62D0UW-7 (at -3.7432 -0.1928 -90) (layer F.SilkS) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 3 smd rect (at 1 0 90) (size 0.5 1) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at -1 0.65 90) (size 0.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1 -0.65 90) (size 0.5 1) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C2-Pad1)"))
    (model DMN62D0UW-7.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${DMN}/DMN62D0UW-7.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 158.3436 105.791)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference C2 (at 0 -1.7) (layer F.SilkS))
    (fp_text value C (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module myfootprints:MicroD-25-M-upsidedown (layer F.Cu) (tedit 5E7D06EB)
    (at 145.4272 116.2558 270)
    (fp_text reference J2 (at 0.0254 13.398) (layer F.SilkS))
    (fp_text value MicroD-25-M (at -3.81 3.8354) (layer F.Fab))
    (pad 26 thru_hole circle (at 2.54 -8.445 270) (size 2.79 2.79) (drill 2.79) (layers *.Cu *.Mask F.SilkS))
    (pad 0 thru_hole circle (at 2.54 16.065 270) (size 2.79 2.79) (drill 2.79) (layers *.Cu *.Mask F.SilkS))
    (pad 14 thru_hole circle (at 1.27 -3.17 270) (size 0.7112 0.7112) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 15 thru_hole circle (at 1.27 -1.9 270) (size 0.7112 0.7112) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 16 thru_hole circle (at 1.27 -0.63 270) (size 0.7112 0.7112) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 17 thru_hole circle (at 1.27 0.64 270) (size 0.7112 0.7112) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 18 thru_hole circle (at 1.27 1.91 270) (size 0.7112 0.7112) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 19 thru_hole circle (at 1.27 3.18 270) (size 0.7112 0.7112) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 20 thru_hole circle (at 1.27 4.45 270) (size 0.7112 0.7112) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 21 thru_hole circle (at 1.27 5.72 270) (size 0.7112 0.7112) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 22 thru_hole circle (at 1.27 6.99 270) (size 0.7112 0.7112) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 23 thru_hole circle (at 1.27 8.26 270) (size 0.7112 0.7112) (drill 0.7112) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 24 thru_hole circle (at 1.27 9.53 270) (size 0.7112 0.7112) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 25 thru_hole circle (at 1.27 10.8 270) (size 0.7112 0.7112) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.27 -3.81 270) (size 0.715 0.715) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(J2-Pad1)"))
    (pad 2 thru_hole circle (at -1.27 -2.54 270) (size 0.715 0.715) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(J2-Pad2)"))
    (pad 3 thru_hole circle (at -1.27 -1.27 270) (size 0.715 0.715) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(J2-Pad3)"))
    (pad 4 thru_hole circle (at -1.27 0 270) (size 0.715 0.715) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(J2-Pad4)"))
    (pad 5 thru_hole circle (at -1.27 1.27 270) (size 0.715 0.715) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(J2-Pad5)"))
    (pad 6 thru_hole circle (at -1.27 2.54 270) (size 0.715 0.715) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(J2-Pad6)"))
    (pad 7 thru_hole circle (at -1.27 3.81 270) (size 0.715 0.715) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(J2-Pad7)"))
    (pad 8 thru_hole circle (at -1.27 5.08 270) (size 0.715 0.715) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(J2-Pad8)"))
    (pad 9 thru_hole circle (at -1.27 6.35 270) (size 0.715 0.715) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(J2-Pad9)"))
    (pad 10 thru_hole circle (at -1.27 7.62 270) (size 0.715 0.715) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(J2-Pad10)"))
    (pad 11 thru_hole circle (at -1.27 8.89 270) (size 0.715 0.715) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(J2-Pad11)"))
    (pad 12 thru_hole circle (at -1.27 10.16 270) (size 0.715 0.715) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(J2-Pad12)"))
    (pad 13 thru_hole circle (at -1.27 11.43 270) (size 0.71 0.71) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(J2-Pad13)"))
    (model /Users/smb2/Documents/PCB/Kicad/Footprints.pretty/3D/MicroD_381-025-112L565.STEP
      (offset (xyz 7.8486 -3.81 -5.181599999999999))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 90))
    )
  )
  (module myfootprints:MicroD-25-M-upsidedown (layer F.Cu) (tedit 5E7D06EB)
    (at 138.6972 90.2208 90)
    (fp_text reference J1 (at -2.54 19.05) (layer F.SilkS))
    (fp_text value MicroD-25-M (at -3.81 3.8354) (layer F.Fab))
    (pad 26 thru_hole circle (at 2.54 -8.445 90) (size 2.79 2.79) (drill 2.79) (layers *.Cu *.Mask F.SilkS))
    (pad 0 thru_hole circle (at 2.54 16.065 90) (size 2.79 2.79) (drill 2.79) (layers *.Cu *.Mask F.SilkS))
    (pad 14 thru_hole circle (at 1.27 -3.17 90) (size 0.7112 0.7112) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 15 thru_hole circle (at 1.27 -1.9 90) (size 0.7112 0.7112) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 16 thru_hole circle (at 1.27 -0.63 90) (size 0.7112 0.7112) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 17 thru_hole circle (at 1.27 0.64 90) (size 0.7112 0.7112) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 18 thru_hole circle (at 1.27 1.91 90) (size 0.7112 0.7112) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 19 thru_hole circle (at 1.27 3.18 90) (size 0.7112 0.7112) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 20 thru_hole circle (at 1.27 4.45 90) (size 0.7112 0.7112) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 21 thru_hole circle (at 1.27 5.72 90) (size 0.7112 0.7112) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 22 thru_hole circle (at 1.27 6.99 90) (size 0.7112 0.7112) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 23 thru_hole circle (at 1.27 8.26 90) (size 0.7112 0.7112) (drill 0.7112) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 24 thru_hole circle (at 1.27 9.53 90) (size 0.7112 0.7112) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 25 thru_hole circle (at 1.27 10.8 90) (size 0.7112 0.7112) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.27 -3.81 90) (size 0.715 0.715) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(J1-Pad1)"))
    (pad 2 thru_hole circle (at -1.27 -2.54 90) (size 0.715 0.715) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(J1-Pad2)"))
    (pad 3 thru_hole circle (at -1.27 -1.27 90) (size 0.715 0.715) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(J1-Pad3)"))
    (pad 4 thru_hole circle (at -1.27 0 90) (size 0.715 0.715) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(J1-Pad4)"))
    (pad 5 thru_hole circle (at -1.27 1.27 90) (size 0.715 0.715) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(J1-Pad5)"))
    (pad 6 thru_hole circle (at -1.27 2.54 90) (size 0.715 0.715) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(J1-Pad6)"))
    (pad 7 thru_hole circle (at -1.27 3.81 90) (size 0.715 0.715) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(J1-Pad7)"))
    (pad 8 thru_hole circle (at -1.27 5.08 90) (size 0.715 0.715) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(J1-Pad8)"))
    (pad 9 thru_hole circle (at -1.27 6.35 90) (size 0.715 0.715) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(J1-Pad9)"))
    (pad 10 thru_hole circle (at -1.27 7.62 90) (size 0.715 0.715) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(J1-Pad10)"))
    (pad 11 thru_hole circle (at -1.27 8.89 90) (size 0.715 0.715) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(J1-Pad11)"))
    (pad 12 thru_hole circle (at -1.27 10.16 90) (size 0.715 0.715) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(J1-Pad12)"))
    (pad 13 thru_hole circle (at -1.27 11.43 90) (size 0.71 0.71) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(J1-Pad13)"))
    (model /Users/smb2/Documents/PCB/Kicad/Footprints.pretty/3D/MicroD_381-025-112L565.STEP
      (offset (xyz 7.8486 -3.81 -5.181599999999999))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 90))
    )
  )
  (module uD:wirebond-1 (layer F.Cu) (tedit 5E7CC403)
    (at 143.0782 91.4908)
    (attr smd)
    (fp_text reference P3 (at 4.0132 5.7658) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 5.9944 9.6266) (layer F.Fab))
    (pad 1 smd rect (at 6.35 7.62) (size 0.762 1) (layers F.Cu F.Mask)
      (net 30 "Net-(P3-Pad1)"))
  )
  (module uD:wirebond-1 (layer F.Cu) (tedit 5E7CC403)
    (at 128.5748 91.4146)
    (attr smd)
    (fp_text reference P1 (at 3.6068 8.9662) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 5.9944 9.6266) (layer F.Fab))
    (pad 1 smd rect (at 6.35 7.62) (size 0.762 1) (layers F.Cu F.Mask)
      (net 29 "Net-(C1-Pad1)"))
  )
  (module uD:wirebond-12 (layer F.Cu) (tedit 5E7CBB8B)
    (at 128.8923 103.7082)
    (fp_text reference P2 (at 3.81 7.62) (layer F.SilkS))
    (fp_text value CONN_01X12 (at 5.08 5.08) (layer F.Fab))
    (pad 12 smd rect (at 20.32 7.62) (size 0.762 1) (layers F.Cu F.Mask)
      (net 25 "Net-(J2-Pad1)"))
    (pad 11 smd rect (at 19.05 7.62) (size 0.762 1) (layers F.Cu F.Mask)
      (net 26 "Net-(J2-Pad2)"))
    (pad 10 smd rect (at 17.78 7.62) (size 0.762 1) (layers F.Cu F.Mask)
      (net 24 "Net-(J2-Pad3)"))
    (pad 9 smd rect (at 16.51 7.62) (size 0.762 1) (layers F.Cu F.Mask)
      (net 28 "Net-(J2-Pad4)"))
    (pad 8 smd rect (at 15.24 7.62) (size 0.762 1) (layers F.Cu F.Mask)
      (net 27 "Net-(J2-Pad5)"))
    (pad 7 smd rect (at 13.97 7.62) (size 0.762 1) (layers F.Cu F.Mask)
      (net 23 "Net-(J2-Pad6)"))
    (pad 6 smd rect (at 12.7 7.62) (size 0.762 1) (layers F.Cu F.Mask)
      (net 22 "Net-(J2-Pad7)"))
    (pad 5 smd rect (at 11.43 7.62) (size 0.762 1) (layers F.Cu F.Mask)
      (net 21 "Net-(J2-Pad8)"))
    (pad 4 smd rect (at 10.16 7.62) (size 0.762 1) (layers F.Cu F.Mask)
      (net 20 "Net-(J2-Pad9)"))
    (pad 3 smd rect (at 8.89 7.62) (size 0.762 1) (layers F.Cu F.Mask)
      (net 19 "Net-(J2-Pad10)"))
    (pad 2 smd rect (at 7.62 7.62) (size 0.762 1) (layers F.Cu F.Mask)
      (net 18 "Net-(J2-Pad11)"))
    (pad 1 smd rect (at 6.35 7.62) (size 0.762 1) (layers F.Cu F.Mask)
      (net 17 "Net-(J2-Pad12)"))
  )
  (module DMND62D0U:SOT65P210X110-3N (layer F.Cu) (tedit 5E7BCFFD)
    (at 152.2128 102.8446)
    (descr DMN62D0UW-7-1)
    (tags "MOSFET (N-Channel)")
    (attr smd)
    (fp_text reference Q2 (at -2.7338 -0.2286) (layer F.SilkS))
    (fp_text value DMN62D0UW-7 (at 1.0508 2.0828) (layer F.SilkS) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 3 smd rect (at 1 0 90) (size 0.5 1) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at -1 0.65 90) (size 0.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1 -0.65 90) (size 0.5 1) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(P3-Pad1)"))
    (model DMN62D0UW-7.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${DMN}/DMN62D0UW-7.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module DMND62D0U:SOT65P210X110-3N (layer F.Cu) (tedit 5E7BCFFD)
    (at 132.7912 95.7166 90)
    (descr DMN62D0UW-7-1)
    (tags "MOSFET (N-Channel)")
    (attr smd)
    (fp_text reference Q1 (at -1.0066 -2.0066 90) (layer F.SilkS))
    (fp_text value DMN62D0UW-7 (at 0 -2.54 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1 0 180) (size 0.5 1) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J1-Pad5)"))
    (pad 2 smd rect (at -1 0.65 180) (size 0.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1 -0.65 180) (size 0.5 1) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(C1-Pad1)"))
    (model DMN62D0UW-7.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${DMN}/DMN62D0UW-7.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 139.653 95.3516)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference C1 (at -1.3246 -1.397) (layer F.SilkS))
    (fp_text value C (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_circle (center 157.4546 111.8108) (end 158.5976 113.03) (layer Edge.Cuts) (width 0.05))
  (gr_circle (center 157.4546 96.5708) (end 158.5976 97.79) (layer Edge.Cuts) (width 0.05))
  (gr_circle (center 126.9746 96.5708) (end 128.1176 97.79) (layer Edge.Cuts) (width 0.05))
  (gr_circle (center 126.9746 111.8108) (end 128.1176 113.03) (layer Edge.Cuts) (width 0.05))
  (gr_text SPD (at 149.3266 97.1804) (layer F.SilkS))
  (gr_text LED (at 134.4168 100.8888) (layer F.SilkS))
  (gr_text 9 (at 140.5382 113.0808) (layer F.SilkS))
  (gr_text 5 (at 145.6182 113.0808) (layer F.SilkS))
  (gr_text 1 (at 150.6982 113.0808) (layer F.SilkS))
  (gr_text "smb2 kangaroo01 2020-03-25" (at 123.5202 104.775 90) (layer F.SilkS))
  (gr_line (start 136.4996 109.8042) (end 147.8788 109.8042) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 147.8788 109.7534) (end 147.8788 109.8042) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 147.8788 98.3488) (end 147.8788 109.7534) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 136.4996 98.3488) (end 147.8788 98.3488) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 136.4996 109.8042) (end 136.4996 98.3488) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 162.6362 83.7438) (end 162.6362 124.4346) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 121.92 83.7438) (end 162.6362 83.7438) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 121.92 124.4346) (end 121.92 83.7438) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 162.6362 124.4346) (end 121.92 124.4346) (layer Edge.Cuts) (width 0.1))
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.35))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 148.7424 110.6424) (xy 135.7376 110.6424) (xy 135.7376 97.6376) (xy 148.7424 97.6376)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.35))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 155.8798 116.1288) (xy 128.8796 116.1288) (xy 128.8796 102.5652) (xy 155.8798 102.5652)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.35))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 164.1856 127.2032) (xy 120.1674 127.2032) (xy 120.1674 82.5246) (xy 164.1856 82.5246)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.35))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 164.2618 127.254) (xy 118.8212 127.254) (xy 118.8212 82.677) (xy 164.2618 82.677)
      )
    )
  )
)
