(kicad_pcb (version 20171130) (host pcbnew 5.0.2-bee76a0~70~ubuntu18.04.1)
  (general
    (thickness 1.6)
    (drawings 86)
    (tracks 217)
    (zones 0)
    (modules 50)
    (nets 36)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 PhoneLeft)
  (net 3 PhoneRight)
  (net 4 "Net-(C2-Pad1)")
  (net 5 "Net-(C3-Pad1)")
  (net 6 RadioSpk)
  (net 7 HeadsetMic)
  (net 8 "Net-(C4-Pad1)")
  (net 9 GNDS)
  (net 10 VCC)
  (net 11 HeadsetGND)
  (net 12 PhoneMic)
  (net 13 "Net-(C11-Pad2)")
  (net 14 "Net-(C12-Pad1)")
  (net 15 HeadsetLeft)
  (net 16 HeadsetRight)
  (net 17 "Net-(C13-Pad1)")
  (net 18 "Net-(J1-Pad3)")
  (net 19 "Net-(J3-PadR)")
  (net 20 "Net-(J4-PadR2)")
  (net 21 "Net-(J4-PadT)")
  (net 22 RadioPTT)
  (net 23 "Net-(J5-PadR2)")
  (net 24 "Net-(J6-PadR2)")
  (net 25 "Net-(J6-PadR1)")
  (net 26 "Net-(J8-PadR2)")
  (net 27 "Net-(J8-PadR1)")
  (net 28 "Net-(R4-Pad2)")
  (net 29 BusMic)
  (net 30 "Net-(R7-Pad2)")
  (net 31 BusLeft)
  (net 32 BusRight)
  (net 33 "Net-(R8-Pad2)")
  (net 34 "Net-(R10-Pad2)")
  (net 35 "Net-(R11-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net BusLeft)
    (add_net BusMic)
    (add_net BusRight)
    (add_net HeadsetLeft)
    (add_net HeadsetMic)
    (add_net HeadsetRight)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C11-Pad2)")
    (add_net "Net-(C12-Pad1)")
    (add_net "Net-(C13-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(J3-PadR)")
    (add_net "Net-(J4-PadR2)")
    (add_net "Net-(J4-PadT)")
    (add_net "Net-(J5-PadR2)")
    (add_net "Net-(J6-PadR1)")
    (add_net "Net-(J6-PadR2)")
    (add_net "Net-(J8-PadR1)")
    (add_net "Net-(J8-PadR2)")
    (add_net "Net-(R10-Pad2)")
    (add_net "Net-(R11-Pad1)")
    (add_net "Net-(R4-Pad2)")
    (add_net "Net-(R7-Pad2)")
    (add_net "Net-(R8-Pad2)")
    (add_net PhoneLeft)
    (add_net PhoneMic)
    (add_net PhoneRight)
    (add_net RadioPTT)
    (add_net RadioSpk)
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 0.508)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GNDS)
    (add_net HeadsetGND)
    (add_net "Net-(J1-Pad3)")
    (add_net VCC)
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 105.6275 120.65)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C1 (at 0 -46.355) (layer F.SilkS))
    (fp_text value 1uF (at -0.2175 -46.355) (layer F.Fab))
    (fp_text user %R (at 1.0525 -45.72) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 2 PhoneLeft))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 105.6275 126.365)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C2 (at -0.2175 -51.435) (layer F.SilkS))
    (fp_text value 1uF (at -0.2175 -51.435) (layer F.Fab))
    (fp_text user %R (at -0.8525 -51.435) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 3 PhoneRight))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 4 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 105.6275 114.935)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C3 (at -0.8525 -40.64) (layer F.SilkS))
    (fp_text value 1uF (at 0 -40.64) (layer F.Fab))
    (fp_text user %R (at -0.2175 -40.64) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 5 "Net-(C3-Pad1)"))
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 6 RadioSpk))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 63.0825 104.14 180)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C4 (at 0 29.845 180) (layer F.SilkS))
    (fp_text value 1uF (at 2.1225 29.845 180) (layer F.Fab))
    (fp_text user %R (at 0.2175 29.845 180) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 7 HeadsetMic))
    (pad 1 smd roundrect (at -1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 8 "Net-(C4-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D8.0mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 73.66 98.425 180)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=8mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 8mm Electrolytic Capacitor")
    (fp_text reference C5 (at 6.985 24.13 180) (layer F.SilkS))
    (fp_text value 100uF (at 5.08 24.13 180) (layer F.Fab))
    (fp_text user %R (at 1.25 0 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 GNDS))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 VCC))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D8.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D8.0mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 82.51 98.425 180)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=8mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 8mm Electrolytic Capacitor")
    (fp_text reference C6 (at 13.93 24.13 180) (layer F.SilkS))
    (fp_text value 100uF (at 14.565 24.13 180) (layer F.Fab))
    (fp_text user %R (at 1.25 0 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 GNDS))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 HeadsetGND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D8.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBE)
    (at 75.565 115.1525 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C7 (at -8.0375 -45.085 90) (layer B.SilkS))
    (fp_text value 1uF (at -8.0375 -45.085 90) (layer B.Fab))
    (fp_text user %R (at -8.0375 -44.45 90) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 10 VCC))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 9 GNDS))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBE)
    (at 78.105 115.1525 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C8 (at -7.4025 -47.625 90) (layer B.SilkS))
    (fp_text value 1uF (at -8.0375 -46.99 90) (layer B.Fab))
    (fp_text user %R (at -8.6725 -47.625 90) (layer B.Fab))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 11 HeadsetGND))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 9 GNDS))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBE)
    (at 75.565 122.7725 270)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C9 (at 1.6875 45.72 270) (layer B.SilkS))
    (fp_text value .1uF (at 1.0525 45.72 270) (layer B.Fab))
    (fp_text user %R (at 1.6875 45.72 270) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 10 VCC))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 9 GNDS))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBE)
    (at 78.105 122.7725 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C10 (at -1.6875 -48.26 90) (layer B.SilkS))
    (fp_text value .1uF (at -1.0525 -47.625 90) (layer B.Fab))
    (fp_text user %R (at -1.6875 -47.625 90) (layer B.Fab))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 11 HeadsetGND))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 9 GNDS))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 105.8275 109.22 180)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C11 (at 1.0525 34.29 180) (layer F.SilkS))
    (fp_text value 1uF (at 1.0525 34.29 180) (layer F.Fab))
    (fp_text user %R (at 1.6875 34.29 180) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 12 PhoneMic))
    (pad 2 smd roundrect (at 1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 13 "Net-(C11-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D8.0mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 64.095 113.03 180)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=8mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 8mm Electrolytic Capacitor")
    (fp_text reference C12 (at 1.23 39.37 180) (layer F.SilkS))
    (fp_text value 100uF (at 0.595 38.735 180) (layer F.Fab))
    (fp_text user %R (at 1.25 0 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(C12-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 HeadsetLeft))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D8.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D8.0mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 64.135 123.825 180)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=8mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 8mm Electrolytic Capacitor")
    (fp_text reference C13 (at 0 49.53 180) (layer F.SilkS))
    (fp_text value 100uF (at 0 49.53 180) (layer F.Fab))
    (fp_text user %R (at 1.25 0 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 HeadsetRight))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(C13-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D8.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_BarrelJack:BarrelJack_Horizontal (layer F.Cu) (tedit 5A1DBF6A)
    (at 76.2 86.36 270)
    (descr "DC Barrel Jack")
    (tags "Power Jack")
    (fp_text reference J1 (at -6.35 45.72 270) (layer F.SilkS))
    (fp_text value "Power In" (at -6.35 45.72 270) (layer F.Fab))
    (fp_text user %R (at -5.08 45.72 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 3.5 3.5) (drill oval 1 3) (layers *.Cu *.Mask)
      (net 10 VCC))
    (pad 2 thru_hole roundrect (at -6 0 270) (size 3 3.5) (drill oval 1 3) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 11 HeadsetGND))
    (pad 3 thru_hole roundrect (at -3 4.7 270) (size 3.5 3.5) (drill oval 3 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 18 "Net-(J1-Pad3)"))
    (model ${KISYS3DMOD}/Connector_BarrelJack.3dshapes/BarrelJack_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Audio:Jack_3.5mm_PJ320D_Horizontal (layer F.Cu) (tedit 5BF5E15D)
    (at 120.65 116.205 180)
    (descr "Headphones with microphone connector, 3.5mm, 4 pins (http://www.qingpu-electronics.com/en/products/WQP-PJ320D-72.html)")
    (tags "3.5mm jack mic microphone phones headphones 4pins audio plug")
    (attr smd)
    (fp_text reference J2 (at -0.635 41.275 180) (layer F.SilkS))
    (fp_text value iPhone (at 6.35 41.275 180) (layer F.Fab))
    (fp_text user %R (at 0.635 41.91 180) (layer F.Fab))
    (pad "" np_thru_hole circle (at 2.225 0 180) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -4.775 0 180) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
    (pad S smd rect (at -3.175 -3.25 180) (size 1.2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 11 HeadsetGND))
    (pad R1 smd rect (at -0.175 -3.25 180) (size 1.2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 3 PhoneRight))
    (pad T smd rect (at 3.825 -3.25 180) (size 1.2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 PhoneLeft))
    (pad R2 smd rect (at 4.925 3.25 180) (size 1.2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 12 PhoneMic))
    (model ${KISYS3DMOD}/Connector_Audio.3dshapes/Jack_3.5mm_PJ320D_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Smitty:PJ-208 (layer F.Cu) (tedit 5C1494FE)
    (at 127 103.505 180)
    (fp_text reference J3 (at 3.175 29.21 180) (layer F.SilkS))
    (fp_text value "Radio 2.5mm" (at 12.065 28.575 180) (layer F.Fab))
    (pad "" np_thru_hole circle (at 1.5 0 180) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 8.5 0 180) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask))
    (pad R smd rect (at 4.4 -3.4 180) (size 1.5 3.6) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(J3-PadR)"))
    (pad S smd rect (at 1.7 3.4 180) (size 1.5 3.6) (layers F.Cu F.Paste F.Mask)
      (net 11 HeadsetGND))
    (pad T smd rect (at 11.2 0 270) (size 1.5 3.6) (layers F.Cu F.Paste F.Mask)
      (net 6 RadioSpk))
  )
  (module Connector_Audio:Jack_3.5mm_PJ320D_Horizontal (layer F.Cu) (tedit 5BF5E15D)
    (at 120.65 90.805 180)
    (descr "Headphones with microphone connector, 3.5mm, 4 pins (http://www.qingpu-electronics.com/en/products/WQP-PJ320D-72.html)")
    (tags "3.5mm jack mic microphone phones headphones 4pins audio plug")
    (attr smd)
    (fp_text reference J4 (at 1.905 15.875 180) (layer F.SilkS))
    (fp_text value "Radio 3.5mm" (at 3.81 15.875 180) (layer F.Fab))
    (fp_text user %R (at 0 15.875 180) (layer F.Fab))
    (pad R2 smd rect (at 4.925 3.25 180) (size 1.2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(J4-PadR2)"))
    (pad T smd rect (at 3.825 -3.25 180) (size 1.2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(J4-PadT)"))
    (pad R1 smd rect (at -0.175 -3.25 180) (size 1.2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 7 HeadsetMic))
    (pad S smd rect (at -3.175 -3.25 180) (size 1.2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 22 RadioPTT))
    (pad "" np_thru_hole circle (at -4.775 0 180) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 2.225 0 180) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_Audio.3dshapes/Jack_3.5mm_PJ320D_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Audio:Jack_3.5mm_PJ320D_Horizontal (layer F.Cu) (tedit 5BF5E15D)
    (at 38.1 116.205)
    (descr "Headphones with microphone connector, 3.5mm, 4 pins (http://www.qingpu-electronics.com/en/products/WQP-PJ320D-72.html)")
    (tags "3.5mm jack mic microphone phones headphones 4pins audio plug")
    (attr smd)
    (fp_text reference J5 (at 1.27 -41.275) (layer F.SilkS))
    (fp_text value Headphones (at -0.025 -41.275) (layer F.Fab))
    (fp_text user %R (at 0 -41.275) (layer F.Fab))
    (pad "" np_thru_hole circle (at 2.225 0) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -4.775 0) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
    (pad S smd rect (at -3.175 -3.25) (size 1.2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 11 HeadsetGND))
    (pad R1 smd rect (at -0.175 -3.25) (size 1.2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 16 HeadsetRight))
    (pad T smd rect (at 3.825 -3.25) (size 1.2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 15 HeadsetLeft))
    (pad R2 smd rect (at 4.925 3.25) (size 1.2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(J5-PadR2)"))
    (model ${KISYS3DMOD}/Connector_Audio.3dshapes/Jack_3.5mm_PJ320D_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Audio:Jack_3.5mm_PJ320D_Horizontal (layer F.Cu) (tedit 5BF5E15D)
    (at 38.1 103.505)
    (descr "Headphones with microphone connector, 3.5mm, 4 pins (http://www.qingpu-electronics.com/en/products/WQP-PJ320D-72.html)")
    (tags "3.5mm jack mic microphone phones headphones 4pins audio plug")
    (attr smd)
    (fp_text reference J6 (at 0.635 -28.575) (layer F.SilkS))
    (fp_text value Mic (at -1.27 -28.575) (layer F.Fab))
    (fp_text user %R (at 0.635 -28.575) (layer F.Fab))
    (pad R2 smd rect (at 4.925 3.25) (size 1.2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(J6-PadR2)"))
    (pad T smd rect (at 3.825 -3.25) (size 1.2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 7 HeadsetMic))
    (pad R1 smd rect (at -0.175 -3.25) (size 1.2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(J6-PadR1)"))
    (pad S smd rect (at -3.175 -3.25) (size 1.2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 11 HeadsetGND))
    (pad "" np_thru_hole circle (at -4.775 0) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 2.225 0) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_Audio.3dshapes/Jack_3.5mm_PJ320D_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 67.31 86.36 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J7 (at 3.81 12.065 180) (layer F.SilkS))
    (fp_text value "Internal Power" (at 2.54 12.065 180) (layer F.Fab))
    (fp_text user %R (at 36.83 5.08 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 VCC))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J1-Pad3)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Audio:Jack_3.5mm_PJ320D_Horizontal (layer F.Cu) (tedit 5BF5E15D)
    (at 38.1 90.805)
    (descr "Headphones with microphone connector, 3.5mm, 4 pins (http://www.qingpu-electronics.com/en/products/WQP-PJ320D-72.html)")
    (tags "3.5mm jack mic microphone phones headphones 4pins audio plug")
    (attr smd)
    (fp_text reference J8 (at 0 -15.875) (layer F.SilkS))
    (fp_text value PTT (at -0.635 -15.875) (layer F.Fab))
    (fp_text user %R (at -1.195 -15.875) (layer F.Fab))
    (pad R2 smd rect (at 4.925 3.25) (size 1.2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(J8-PadR2)"))
    (pad T smd rect (at 3.825 -3.25) (size 1.2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 22 RadioPTT))
    (pad R1 smd rect (at -0.175 -3.25) (size 1.2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(J8-PadR1)"))
    (pad S smd rect (at -3.175 -3.25) (size 1.2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 11 HeadsetGND))
    (pad "" np_thru_hole circle (at -4.775 0) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 2.225 0) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_Audio.3dshapes/Jack_3.5mm_PJ320D_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 116.205 115.9875 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 6.1325 12.065 90) (layer B.SilkS))
    (fp_text value 100 (at -7.2025 12.7 90) (layer B.Fab))
    (fp_text user %R (at 6.1325 12.065 90) (layer B.Fab))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 11 HeadsetGND))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 2 PhoneLeft))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 120.65 115.9875 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at -7.2025 8.255 90) (layer B.SilkS))
    (fp_text value 100 (at -7.2025 7.62 90) (layer B.Fab))
    (fp_text user %R (at 6.1325 8.255 90) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 3 PhoneRight))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 11 HeadsetGND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 115.57 100.7475 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R3 (at 2.9575 12.7 90) (layer B.SilkS))
    (fp_text value 100 (at 2.3225 12.7 90) (layer B.Fab))
    (fp_text user %R (at 1.0525 12.7 90) (layer B.Fab))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 11 HeadsetGND))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 6 RadioSpk))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 75.565 122.7725 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R4 (at 1.0525 45.085 270) (layer F.SilkS))
    (fp_text value 10k (at 1.6875 45.72 270) (layer F.Fab))
    (fp_text user %R (at 1.6875 44.45 270) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 10 VCC))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 28 "Net-(R4-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 78.105 122.7725 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R5 (at -1.6875 -47.625 90) (layer F.SilkS))
    (fp_text value 10k (at -1.6875 -47.625 90) (layer F.Fab))
    (fp_text user %R (at -1.0525 -48.895 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 11 HeadsetGND))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 28 "Net-(R4-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 75.565 107.0975 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R6 (at -2.7575 -45.085 90) (layer F.SilkS))
    (fp_text value 10k (at -2.7575 -45.085 90) (layer F.Fab))
    (fp_text user %R (at -2.7575 -45.085 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 8 "Net-(C4-Pad1)"))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 29 BusMic))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 88.0475 119.38)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R7 (at 0.2175 -44.45) (layer F.SilkS))
    (fp_text value 10k (at 0 -44.45) (layer F.Fab))
    (fp_text user %R (at 0.2175 -44.45) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 30 "Net-(R7-Pad2)"))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 31 BusLeft))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 88.0475 125.095)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R8 (at -0.4175 -50.165) (layer F.SilkS))
    (fp_text value 10k (at 0 -50.165) (layer F.Fab))
    (fp_text user %R (at -1.0525 -50.165) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 32 BusRight))
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 33 "Net-(R8-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 88.0475 113.665)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R9 (at 0 -38.735) (layer F.SilkS))
    (fp_text value 10k (at -1.6875 -38.735) (layer F.Fab))
    (fp_text user %R (at 0.8525 -38.735) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 31 BusLeft))
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 34 "Net-(R10-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 88.0475 116.205)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R10 (at -1.0525 -41.275) (layer F.SilkS))
    (fp_text value 10k (at 1.4875 -41.91) (layer F.Fab))
    (fp_text user %R (at -1.0525 -41.275) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 34 "Net-(R10-Pad2)"))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 32 BusRight))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 88.0475 110.49)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R11 (at 0.2175 -35.56) (layer F.SilkS))
    (fp_text value 10k (at -0.4175 -35.56) (layer F.Fab))
    (fp_text user %R (at 0.2175 -35.56) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 35 "Net-(R11-Pad1)"))
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 34 "Net-(R10-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 88.0475 107.95 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R12 (at 0 33.02 180) (layer F.SilkS))
    (fp_text value 100 (at -0.8525 33.02 180) (layer F.Fab))
    (fp_text user %R (at -0.2175 33.02 180) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 35 "Net-(R11-Pad1)"))
    (pad 1 smd roundrect (at -1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 9 GNDS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 78.105 107.0975 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R13 (at -2.7575 -47.625 90) (layer F.SilkS))
    (fp_text value 10k (at -2.7575 -47.625 90) (layer F.Fab))
    (fp_text user %R (at -2.7575 -47.625 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 29 BusMic))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 35 "Net-(R11-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 80.645 107.0975 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R14 (at -2.7575 -50.165 90) (layer F.SilkS))
    (fp_text value 10k (at -2.7575 -50.165 90) (layer F.Fab))
    (fp_text user %R (at -2.7575 -50.165 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 31 BusLeft))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 14 "Net-(C12-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 80.645 122.7725 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R15 (at 1.6875 50.165 270) (layer F.SilkS))
    (fp_text value 10k (at 1.0525 50.165 270) (layer F.Fab))
    (fp_text user %R (at 1.6875 50.165 270) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 17 "Net-(C13-Pad1)"))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 32 BusRight))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 73.025 107.0975 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R16 (at -2.7575 -42.545 90) (layer F.SilkS))
    (fp_text value 10k (at -2.7575 -42.545 90) (layer F.Fab))
    (fp_text user %R (at -2.7575 -42.545 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 29 BusMic))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 13 "Net-(C11-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 60.1075 116.205)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R17 (at -8.6725 -41.275) (layer B.SilkS))
    (fp_text value 10k (at -3.5925 -41.275) (layer B.Fab))
    (fp_text user %R (at -5.4975 -41.275) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 11 HeadsetGND))
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 15 HeadsetLeft))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 60.1075 120.65)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R18 (at -4.8625 -45.72) (layer B.SilkS))
    (fp_text value 10k (at -3.5925 -45.72) (layer B.Fab))
    (fp_text user %R (at -4.8625 -45.72) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 11 HeadsetGND))
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 16 HeadsetRight))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 117.2575 107.95 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R19 (at 0.4175 33.02 180) (layer B.SilkS))
    (fp_text value 10k (at -12.2825 1.27 180) (layer B.Fab))
    (fp_text user %R (at -0.2175 33.02 180) (layer B.Fab))
    (pad 2 smd roundrect (at 1.4875 0 180) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 12 PhoneMic))
    (pad 1 smd roundrect (at -1.4875 0 180) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 11 HeadsetGND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 117.2575 110.49 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R20 (at 1.0525 36.195 180) (layer B.SilkS))
    (fp_text value 10k (at -12.2825 2.54 180) (layer B.Fab))
    (fp_text user %R (at 0 36.195 180) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4875 0 180) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 11 HeadsetGND))
    (pad 2 smd roundrect (at 1.4875 0 180) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 12 PhoneMic))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometer_THT:Potentiometer_Bourns_3296W_Vertical (layer F.Cu) (tedit 5A3D4994)
    (at 99.695 120.65)
    (descr "Potentiometer, vertical, Bourns 3296W, https://www.bourns.com/pdfs/3296.pdf")
    (tags "Potentiometer vertical Bourns 3296W")
    (fp_text reference RV1 (at -1.905 -45.72) (layer F.SilkS))
    (fp_text value 10k (at -1.905 -46.355) (layer F.Fab))
    (fp_text user %R (at -4.445 -45.72) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at -2.54 0) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(R7-Pad2)"))
    (pad 3 thru_hole circle (at -5.08 0) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 GNDS))
    (model ${KISYS3DMOD}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_3296W_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometer_THT:Potentiometer_Bourns_3296W_Vertical (layer F.Cu) (tedit 5A3D4994)
    (at 99.695 126.365)
    (descr "Potentiometer, vertical, Bourns 3296W, https://www.bourns.com/pdfs/3296.pdf")
    (tags "Potentiometer vertical Bourns 3296W")
    (fp_text reference RV2 (at -1.905 -51.435) (layer F.SilkS))
    (fp_text value 10k (at -4.445 -51.435) (layer F.Fab))
    (fp_text user %R (at -5.08 -51.435) (layer F.Fab))
    (pad 3 thru_hole circle (at -5.08 0) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 GNDS))
    (pad 2 thru_hole circle (at -2.54 0) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "Net-(R8-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_3296W_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometer_THT:Potentiometer_Bourns_3296W_Vertical (layer F.Cu) (tedit 5A3D4994)
    (at 99.695 114.935)
    (descr "Potentiometer, vertical, Bourns 3296W, https://www.bourns.com/pdfs/3296.pdf")
    (tags "Potentiometer vertical Bourns 3296W")
    (fp_text reference RV3 (at -1.905 -40.005) (layer F.SilkS))
    (fp_text value 10k (at -1.27 -40.005) (layer F.Fab))
    (fp_text user %R (at -3.175 -40.005) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at -2.54 0) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(R10-Pad2)"))
    (pad 3 thru_hole circle (at -5.08 0) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 GNDS))
    (model ${KISYS3DMOD}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_3296W_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_THT:SW_PUSH_6mm (layer F.Cu) (tedit 5A02FE31)
    (at 46.99 93.98 90)
    (descr https://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (tags "tact sw push 6mm")
    (fp_text reference SW1 (at 14.605 -16.51 90) (layer F.SilkS))
    (fp_text value PTT (at 12.7 -16.51 90) (layer F.Fab))
    (fp_text user %R (at 13.335 -16.51 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 4.5 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 22 RadioPTT))
    (pad 1 thru_hole circle (at 0 0 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 11 HeadsetGND))
    (pad 2 thru_hole circle (at 6.5 4.5 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 22 RadioPTT))
    (pad 1 thru_hole circle (at 6.5 0 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 11 HeadsetGND))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_PUSH_6mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-14_3.9x8.7mm_P1.27mm (layer F.Cu) (tedit 5A02F2D3)
    (at 76.835 114.935 90)
    (descr "14-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1 (at -8.255 -46.355 90) (layer F.SilkS))
    (fp_text value TL074 (at -9.525 -46.355 90) (layer F.Fab))
    (fp_text user %R (at -8.89 -46.355 90) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -3.81 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 GNDS))
    (pad 2 smd rect (at -2.7 -2.54 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 GNDS))
    (pad 3 smd rect (at -2.7 -1.27 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(R4-Pad2)"))
    (pad 4 smd rect (at -2.7 0 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 VCC))
    (pad 5 smd rect (at -2.7 1.27 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 GNDS))
    (pad 6 smd rect (at -2.7 2.54 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 32 BusRight))
    (pad 7 smd rect (at -2.7 3.81 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(C13-Pad1)"))
    (pad 8 smd rect (at 2.7 3.81 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C12-Pad1)"))
    (pad 9 smd rect (at 2.7 2.54 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 31 BusLeft))
    (pad 10 smd rect (at 2.7 1.27 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 GNDS))
    (pad 11 smd rect (at 2.7 0 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 11 HeadsetGND))
    (pad 12 smd rect (at 2.7 -1.27 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 29 BusMic))
    (pad 13 smd rect (at 2.7 -2.54 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 GNDS))
    (pad 14 smd rect (at 2.7 -3.81 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C11-Pad2)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-14_3.9x8.7mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 36.195 80.645)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -5.715) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at 3.175 -5.715) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 36.195 127)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 1.27 -52.07) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at 3.175 -52.07) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 122.555 127)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at -0.635 -52.07) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at -5.08 -52.07) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 122.555 80.645)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at -0.635 -6.35) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at -3.81 -5.715) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (gr_text "ALL THE 10k!" (at 78.105 130.175) (layer F.SilkS))
  (gr_text "iPhone Out" (at 104.775 95.885) (layer F.SilkS))
  (gr_text "iPhone In" (at 104.775 89.535) (layer F.SilkS))
  (gr_text "Radio Out" (at 104.775 92.71) (layer F.SilkS))
  (gr_text "Radio In" (at 104.775 86.36) (layer F.SilkS))
  (gr_text Phones (at 90.805 95.25) (layer F.SilkS))
  (gr_text Mic (at 90.805 86.36) (layer F.SilkS))
  (gr_text "We miss you, Cliff. K7RR SK" (at 43.815 80.01) (layer F.Mask))
  (gr_text "We miss you, Cliff. K7RR SK" (at 43.815 80.01) (layer F.Cu))
  (gr_text . (at 94.615 100.33 180) (layer B.Mask))
  (gr_text O (at 95.25 95.885 180) (layer B.Mask))
  (gr_text "o\n" (at 93.345 98.425 180) (layer B.Mask))
  (gr_text ><> (at 92.075 100.965 180) (layer B.Mask))
  (gr_text ><> (at 96.52 102.235) (layer B.Mask))
  (gr_text "Volume:\n- Radio\n- Phone L\n- Phone R" (at 92.71 108.585) (layer F.SilkS))
  (gr_text "Satellite Pass Recorder v1.0\nCC BY-NC-SA 2018\n@SmittyHalibut KR6ZY" (at 81.915 80.645) (layer F.SilkS))
  (gr_text iPhone (at 125.095 111.76) (layer F.SilkS))
  (gr_text "Radio 2.5" (at 123.825 99.695) (layer F.SilkS))
  (gr_text Radio3.5 (at 127 86.36) (layer F.SilkS))
  (gr_text 100 (at 113.03 100.965) (layer B.SilkS))
  (gr_text 100 (at 123.19 116.205) (layer B.SilkS))
  (gr_text 100 (at 113.665 116.205) (layer B.SilkS))
  (gr_text 10k (at 113.03 110.49) (layer B.SilkS))
  (gr_text 10k (at 113.03 107.95) (layer B.SilkS))
  (gr_text 1uF (at 73.025 114.935) (layer B.SilkS))
  (gr_text 1uF (at 80.645 114.935) (layer B.SilkS))
  (gr_text 1uF (at 73.025 122.555) (layer B.SilkS))
  (gr_text 1uF (at 80.645 122.555) (layer B.SilkS))
  (gr_text 10k (at 55.88 116.205) (layer B.SilkS))
  (gr_text 10k (at 55.88 120.65) (layer B.SilkS))
  (gr_text TL074 (at 71.12 114.935 90) (layer F.SilkS))
  (gr_text 10k (at 80.645 103.505) (layer F.SilkS))
  (gr_text 10k (at 78.105 104.775 90) (layer F.SilkS))
  (gr_text 10k (at 75.565 104.775 90) (layer F.SilkS))
  (gr_text 10k (at 73.025 103.505) (layer F.SilkS))
  (gr_text 10k (at 80.645 125.73 90) (layer F.SilkS))
  (gr_text 10k (at 78.105 125.73 90) (layer F.SilkS))
  (gr_text 10k (at 75.565 125.73 90) (layer F.SilkS))
  (gr_text 100 (at 88.265 106.045) (layer F.SilkS))
  (gr_text 10k (at 85.725 125.095) (layer F.SilkS))
  (gr_text 10k (at 85.725 119.38) (layer F.SilkS))
  (gr_text 10k (at 85.725 116.205) (layer F.SilkS))
  (gr_text 10k (at 85.725 113.665) (layer F.SilkS))
  (gr_text 10k (at 85.725 110.49) (layer F.SilkS))
  (gr_text 1uF (at 105.41 124.46) (layer F.SilkS))
  (gr_text 1uF (at 105.41 118.745) (layer F.SilkS))
  (gr_text 1uF (at 105.41 113.03) (layer F.SilkS))
  (gr_text 1uF (at 105.41 107.315) (layer F.SilkS))
  (gr_text 10k (at 97.155 130.175) (layer F.SilkS))
  (gr_text 100uF (at 81.28 93.345) (layer F.SilkS))
  (gr_text 100uF (at 72.39 93.345) (layer F.SilkS))
  (gr_text 100uF (at 62.865 118.745) (layer F.SilkS))
  (gr_text 100uF (at 62.865 107.95) (layer F.SilkS))
  (gr_text 1uF (at 62.865 101.6) (layer F.SilkS))
  (gr_text GND (at 65.405 83.82) (layer F.SilkS))
  (gr_text +9-15v (at 65.405 86.36) (layer F.SilkS))
  (gr_text Phones (at 33.02 120.65) (layer F.SilkS))
  (gr_text Mic (at 34.925 107.95) (layer F.SilkS))
  (gr_text PTT (at 34.925 95.25) (layer F.SilkS))
  (gr_line (start 31.75 131.445) (end 31.75 76.2) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 127 131.445) (end 31.75 131.445) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 127 76.2) (end 127 131.445) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 31.75 76.2) (end 127 76.2) (layer Edge.Cuts) (width 0.15))
  (zone (net 11) (net_name HeadsetGND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 31.75 131.445) (xy 31.75 76.2) (xy 127 76.2) (xy 127 131.445) (xy 106.045 131.445)
        (xy 106.045 92.075) (xy 62.23 92.075) (xy 62.23 131.445)
      )
    )
  )
  (zone (net 9) (net_name GNDS) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 63.5 131.445) (xy 104.775 131.445) (xy 105.41 131.445) (xy 105.41 92.71) (xy 62.865 92.71)
        (xy 62.865 131.445)
      )
    )
  )
)
