(kicad_pcb (version 20171130) (host pcbnew "(5.0.1)-4")
  (general
    (thickness 1.6)
    (drawings 9)
    (tracks 9)
    (zones 0)
    (modules 2)
    (nets 9)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.5)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2 2)
    (pad_drill 1.3)
    (pad_to_mask_clearance 0)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x01000_7fffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Gerber"))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad1)")
  (net 2 "Net-(J1-Pad3)")
  (net 3 "Net-(J1-Pad2)")
  (net 4 "Net-(U1-Pad1)")
  (net 5 "Net-(U1-Pad5)")
  (net 6 "Net-(U1-Pad6)")
  (net 7 "Net-(U1-Pad7)")
  (net 8 "Net-(U1-Pad8)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(U1-Pad8)")
  )
  (module Socket_Strips:Socket_Strip_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 5C0588BD)
    (at 58 33 90)
    (descr "Through hole straight socket strip, 1x03, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x03 2.54mm single row")
    (fp_text reference J1 (at 0 -3 180) (layer F.SilkS) hide)
    (fp_text value Conn_01x03 (at 0 7.41 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 90) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x03_Pitch2.54mm.wrl
      (offset (xyz 0 -2.539999961853027 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module FlySorter:MPXV5050 (layer F.Cu) (tedit 5C0588B6)
    (at 60.65 41.647001)
    (fp_text reference U1 (at 8.35 -5.647001) (layer F.SilkS) hide)
    (fp_text value MPXV5050 (at 0 -5.842) (layer F.Fab))
    (pad 1 smd rect (at -8.38 -3.81) (size 2.54 1.52) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(U1-Pad1)"))
    (pad 2 smd rect (at -8.38 -1.27) (size 2.54 1.52) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 3 smd rect (at -8.38 1.27) (size 2.54 1.52) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (pad 4 smd rect (at -8.38 3.81) (size 2.54 1.52) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad3)"))
    (pad 5 smd rect (at 8.38 3.81) (size 2.54 1.52) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(U1-Pad5)"))
    (pad 6 smd rect (at 8.38 1.27) (size 2.54 1.52) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(U1-Pad6)"))
    (pad 7 smd rect (at 8.38 -1.27) (size 2.54 1.52) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(U1-Pad7)"))
    (pad 8 smd rect (at 8.38 -3.81) (size 2.54 1.52) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(U1-Pad8)"))
  )
  (gr_text "Z0 Z2" (at 61 44) (layer B.SilkS))
  (gr_text P (at 66.25 33) (layer F.Cu))
  (gr_text + (at 55 33) (layer F.Cu))
  (dimension 16 (width 0.3) (layer Dwgs.User)
    (gr_text "16.000 mm" (at 41.9 38 90) (layer Dwgs.User))
    (feature1 (pts (xy 48 30) (xy 43.413579 30)))
    (feature2 (pts (xy 48 46) (xy 43.413579 46)))
    (crossbar (pts (xy 44 46) (xy 44 30)))
    (arrow1a (pts (xy 44 30) (xy 44.586421 31.126504)))
    (arrow1b (pts (xy 44 30) (xy 43.413579 31.126504)))
    (arrow2a (pts (xy 44 46) (xy 44.586421 44.873496)))
    (arrow2b (pts (xy 44 46) (xy 43.413579 44.873496)))
  )
  (dimension 21 (width 0.3) (layer Dwgs.User)
    (gr_text "21.000 mm" (at 60.5 22.9) (layer Dwgs.User))
    (feature1 (pts (xy 71 28) (xy 71 24.413579)))
    (feature2 (pts (xy 50 28) (xy 50 24.413579)))
    (crossbar (pts (xy 50 25) (xy 71 25)))
    (arrow1a (pts (xy 71 25) (xy 69.873496 25.586421)))
    (arrow1b (pts (xy 71 25) (xy 69.873496 24.413579)))
    (arrow2a (pts (xy 50 25) (xy 51.126504 25.586421)))
    (arrow2b (pts (xy 50 25) (xy 51.126504 24.413579)))
  )
  (gr_line (start 50 47) (end 50 30) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 71 47) (end 50 47) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 71 30) (end 71 47) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50 30) (end 71 30) (layer Edge.Cuts) (width 0.1))
)
