(kicad_pcb (version 20171130) (host pcbnew "(5.0.0-3-g5ebb6b6)")
  (general
    (thickness 1.5875)
    (drawings 13)
    (tracks 443)
    (zones 0)
    (modules 268)
    (nets 97)
  )
  (page USLetter)
  (title_block
    (title Smoother)
    (date 2018-09-11)
    (company "Cafe Electric LLC")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal hide)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.0254)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.5 2.5)
    (pad_drill 2.5)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 16.503074 14.985778)
    (grid_origin 22.853074 30.225778)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(C2-Pad1)")
  (net 3 "Net-(D1-Pad2)")
  (net 4 "Net-(U2-Pad17)")
  (net 5 "Net-(U2-Pad18)")
  (net 6 "Net-(U2-Pad19)")
  (net 7 "Net-(U2-Pad20)")
  (net 8 "Net-(U2-Pad16)")
  (net 9 "Net-(U2-Pad15)")
  (net 10 "Net-(U2-Pad14)")
  (net 11 "Net-(U2-Pad21)")
  (net 12 "Net-(U2-Pad22)")
  (net 13 "Net-(U2-Pad23)")
  (net 14 "Net-(U2-Pad24)")
  (net 15 "Net-(U2-Pad27)")
  (net 16 "Net-(U2-Pad28)")
  (net 17 "Net-(U2-Pad29)")
  (net 18 "Net-(U2-Pad30)")
  (net 19 "Net-(U2-Pad31)")
  (net 20 "Net-(U2-Pad32)")
  (net 21 "Net-(U2-Pad33)")
  (net 22 "Net-(U2-Pad36)")
  (net 23 "Net-(U2-Pad37)")
  (net 24 "Net-(U2-Pad9)")
  (net 25 "Net-(U2-Pad8)")
  (net 26 "Net-(U2-Pad7)")
  (net 27 "Net-(U2-Pad6)")
  (net 28 "Net-(U2-Pad5)")
  (net 29 "Net-(U2-Pad4)")
  (net 30 "Net-(U2-Pad3)")
  (net 31 "Net-(U2-Pad2)")
  (net 32 "Net-(U2-Pad38)")
  (net 33 "Net-(U2-Pad41)")
  (net 34 "Net-(U2-Pad42)")
  (net 35 "Net-(U2-Pad43)")
  (net 36 "Net-(U2-Pad44)")
  (net 37 "Net-(U2-Pad47)")
  (net 38 "Net-(U2-Pad48)")
  (net 39 "Net-(U2-Pad49)")
  (net 40 "Net-(U2-Pad50)")
  (net 41 "Net-(U2-Pad54)")
  (net 42 "Net-(U2-Pad55)")
  (net 43 "Net-(U2-Pad56)")
  (net 44 "Net-(U2-Pad57)")
  (net 45 "Net-(U2-Pad63)")
  (net 46 "Net-(U2-Pad64)")
  (net 47 "Net-(U2-Pad65)")
  (net 48 "Net-(U2-Pad66)")
  (net 49 "Net-(U2-Pad67)")
  (net 50 "Net-(U2-Pad68)")
  (net 51 "Net-(U2-Pad69)")
  (net 52 "Net-(U2-Pad70)")
  (net 53 "Net-(U2-Pad71)")
  (net 54 "Net-(U2-Pad72)")
  (net 55 "Net-(U2-Pad73)")
  (net 56 "Net-(U2-Pad75)")
  (net 57 "Net-(U2-Pad76)")
  (net 58 "Net-(U2-Pad77)")
  (net 59 "Net-(U2-Pad78)")
  (net 60 "Net-(U2-Pad79)")
  (net 61 "Net-(U2-Pad80)")
  (net 62 "Net-(U2-Pad81)")
  (net 63 "Net-(U2-Pad82)")
  (net 64 "Net-(U2-Pad83)")
  (net 65 "Net-(U2-Pad84)")
  (net 66 "Net-(U2-Pad85)")
  (net 67 "Net-(U2-Pad86)")
  (net 68 "Net-(U2-Pad59)")
  (net 69 "Net-(U2-Pad60)")
  (net 70 "Net-(U2-Pad62)")
  (net 71 "Net-(U2-Pad74)")
  (net 72 "Net-(U2-Pad61)")
  (net 73 +5V)
  (net 74 "Net-(J2-Pad3)")
  (net 75 "Net-(J2-Pad4)")
  (net 76 "Net-(J3-Pad3)")
  (net 77 "Net-(J3-Pad4)")
  (net 78 "Net-(J3-Pad5)")
  (net 79 "Net-(J3-Pad6)")
  (net 80 +3V3)
  (net 81 "Net-(J3-Pad7)")
  (net 82 CAN2H)
  (net 83 CAN2L)
  (net 84 CAN1L)
  (net 85 CAN1H)
  (net 86 "Net-(U2-Pad58)")
  (net 87 "Net-(BT1-Pad1)")
  (net 88 "Net-(D4-Pad2)")
  (net 89 "Net-(D5-Pad2)")
  (net 90 "Net-(Q1-Pad1)")
  (net 91 "Net-(Q2-Pad1)")
  (net 92 "Net-(J15-Pad1)")
  (net 93 "Net-(J16-Pad1)")
  (net 94 "Net-(J21-Pad1)")
  (net 95 2IO)
  (net 96 6IO)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net +3V3)
    (add_net +5V)
    (add_net 2IO)
    (add_net 6IO)
    (add_net CAN1H)
    (add_net CAN1L)
    (add_net CAN2H)
    (add_net CAN2L)
    (add_net GND)
    (add_net "Net-(BT1-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(J15-Pad1)")
    (add_net "Net-(J16-Pad1)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J21-Pad1)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J3-Pad4)")
    (add_net "Net-(J3-Pad5)")
    (add_net "Net-(J3-Pad6)")
    (add_net "Net-(J3-Pad7)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(Q2-Pad1)")
    (add_net "Net-(U2-Pad14)")
    (add_net "Net-(U2-Pad15)")
    (add_net "Net-(U2-Pad16)")
    (add_net "Net-(U2-Pad17)")
    (add_net "Net-(U2-Pad18)")
    (add_net "Net-(U2-Pad19)")
    (add_net "Net-(U2-Pad2)")
    (add_net "Net-(U2-Pad20)")
    (add_net "Net-(U2-Pad21)")
    (add_net "Net-(U2-Pad22)")
    (add_net "Net-(U2-Pad23)")
    (add_net "Net-(U2-Pad24)")
    (add_net "Net-(U2-Pad27)")
    (add_net "Net-(U2-Pad28)")
    (add_net "Net-(U2-Pad29)")
    (add_net "Net-(U2-Pad3)")
    (add_net "Net-(U2-Pad30)")
    (add_net "Net-(U2-Pad31)")
    (add_net "Net-(U2-Pad32)")
    (add_net "Net-(U2-Pad33)")
    (add_net "Net-(U2-Pad36)")
    (add_net "Net-(U2-Pad37)")
    (add_net "Net-(U2-Pad38)")
    (add_net "Net-(U2-Pad4)")
    (add_net "Net-(U2-Pad41)")
    (add_net "Net-(U2-Pad42)")
    (add_net "Net-(U2-Pad43)")
    (add_net "Net-(U2-Pad44)")
    (add_net "Net-(U2-Pad47)")
    (add_net "Net-(U2-Pad48)")
    (add_net "Net-(U2-Pad49)")
    (add_net "Net-(U2-Pad5)")
    (add_net "Net-(U2-Pad50)")
    (add_net "Net-(U2-Pad54)")
    (add_net "Net-(U2-Pad55)")
    (add_net "Net-(U2-Pad56)")
    (add_net "Net-(U2-Pad57)")
    (add_net "Net-(U2-Pad58)")
    (add_net "Net-(U2-Pad59)")
    (add_net "Net-(U2-Pad6)")
    (add_net "Net-(U2-Pad60)")
    (add_net "Net-(U2-Pad61)")
    (add_net "Net-(U2-Pad62)")
    (add_net "Net-(U2-Pad63)")
    (add_net "Net-(U2-Pad64)")
    (add_net "Net-(U2-Pad65)")
    (add_net "Net-(U2-Pad66)")
    (add_net "Net-(U2-Pad67)")
    (add_net "Net-(U2-Pad68)")
    (add_net "Net-(U2-Pad69)")
    (add_net "Net-(U2-Pad7)")
    (add_net "Net-(U2-Pad70)")
    (add_net "Net-(U2-Pad71)")
    (add_net "Net-(U2-Pad72)")
    (add_net "Net-(U2-Pad73)")
    (add_net "Net-(U2-Pad74)")
    (add_net "Net-(U2-Pad75)")
    (add_net "Net-(U2-Pad76)")
    (add_net "Net-(U2-Pad77)")
    (add_net "Net-(U2-Pad78)")
    (add_net "Net-(U2-Pad79)")
    (add_net "Net-(U2-Pad8)")
    (add_net "Net-(U2-Pad80)")
    (add_net "Net-(U2-Pad81)")
    (add_net "Net-(U2-Pad82)")
    (add_net "Net-(U2-Pad83)")
    (add_net "Net-(U2-Pad84)")
    (add_net "Net-(U2-Pad85)")
    (add_net "Net-(U2-Pad86)")
    (add_net "Net-(U2-Pad9)")
  )
  (net_class GND ""
    (clearance 0.1524)
    (trace_width 0.2032)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
  )
  (module Custom:Single_43_63_PTH (layer F.Cu) (tedit 5B9B2E79)
    (at 50.793074 32.765778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single_43_63_PTH (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.6002 1.6002) (drill 1.0922) (layers *.Cu *.Mask))
  )
  (module Custom:Single_43_63_PTH (layer F.Cu) (tedit 5B9B2E79)
    (at 53.333074 32.765778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single_43_63_PTH (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.6002 1.6002) (drill 1.0922) (layers *.Cu *.Mask))
  )
  (module Custom:Single_43_63_PTH (layer F.Cu) (tedit 5B9B2E79)
    (at 82.543074 27.685778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single_43_63_PTH (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.6002 1.6002) (drill 1.0922) (layers *.Cu *.Mask))
  )
  (module Custom:Single_43_63_PTH (layer F.Cu) (tedit 5B9B2E79)
    (at 92.703074 32.765778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single_43_63_PTH (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.6002 1.6002) (drill 1.0922) (layers *.Cu *.Mask))
  )
  (module Custom:Single_43_63_PTH (layer F.Cu) (tedit 5B9B2E79)
    (at 92.703074 30.225778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single_43_63_PTH (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.6002 1.6002) (drill 1.0922) (layers *.Cu *.Mask))
  )
  (module Custom:Single_43_63_PTH (layer F.Cu) (tedit 5B9B2E79)
    (at 82.543074 51.815778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single_43_63_PTH (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.6002 1.6002) (drill 1.0922) (layers *.Cu *.Mask))
  )
  (module Custom:Single_43_63_PTH (layer F.Cu) (tedit 5B9B2E79)
    (at 58.413074 49.275778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single_43_63_PTH (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.6002 1.6002) (drill 1.0922) (layers *.Cu *.Mask))
  )
  (module Custom:Single_43_63_PTH (layer F.Cu) (tedit 5B9B2E79)
    (at 43.173074 42.925778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single_43_63_PTH (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.6002 1.6002) (drill 1.0922) (layers *.Cu *.Mask))
  )
  (module Custom:Single_43_63_PTH (layer F.Cu) (tedit 5B9B2E79)
    (at 45.713074 30.225778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single_43_63_PTH (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.6002 1.6002) (drill 1.0922) (layers *.Cu *.Mask))
  )
  (module Custom:Single_43_63_PTH (layer F.Cu) (tedit 5B9B2E79)
    (at 43.173074 32.765778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single_43_63_PTH (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.6002 1.6002) (drill 1.0922) (layers *.Cu *.Mask))
  )
  (module Custom:Single_43_63_PTH (layer F.Cu) (tedit 5B9B2E79)
    (at 32.378074 21.970778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single_43_63_PTH (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.6002 1.6002) (drill 1.0922) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 50.793074 42.925778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 53.333074 42.925778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 52.063074 42.925778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 46.983074 42.925778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 49.523074 42.925778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 48.253074 42.925778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 50.793074 41.655778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 53.333074 41.655778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 52.063074 41.655778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 46.983074 41.655778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 49.523074 41.655778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 48.253074 41.655778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 50.793074 40.385778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 53.333074 40.385778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 52.063074 40.385778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 46.983074 40.385778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 49.523074 40.385778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 48.253074 40.385778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module teensy:Teensy35_36 (layer F.Cu) (tedit 5B9B2E19)
    (at 52.063074 37.845778)
    (fp_text reference U2 (at -29.21 5.588) (layer F.SilkS))
    (fp_text value Teensy3.6 (at 0 10.16) (layer F.Fab))
    (pad 17 thru_hole circle (at 11.43 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 4 "Net-(U2-Pad17)"))
    (pad 18 thru_hole circle (at 13.97 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 "Net-(U2-Pad18)"))
    (pad 19 thru_hole circle (at 16.51 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 6 "Net-(U2-Pad19)"))
    (pad 20 thru_hole circle (at 19.05 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 7 "Net-(U2-Pad20)"))
    (pad 16 thru_hole circle (at 8.89 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 8 "Net-(U2-Pad16)"))
    (pad 15 thru_hole circle (at 6.35 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 9 "Net-(U2-Pad15)"))
    (pad 14 thru_hole circle (at 3.81 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 10 "Net-(U2-Pad14)"))
    (pad 21 thru_hole circle (at 21.59 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 11 "Net-(U2-Pad21)"))
    (pad 22 thru_hole circle (at 24.13 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 12 "Net-(U2-Pad22)"))
    (pad 23 thru_hole circle (at 26.67 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 13 "Net-(U2-Pad23)"))
    (pad 24 thru_hole circle (at 29.21 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 14 "Net-(U2-Pad24)"))
    (pad 25 thru_hole circle (at 16.51 5.08) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 87 "Net-(BT1-Pad1)"))
    (pad 26 thru_hole circle (at 16.51 2.54) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 80 +3V3))
    (pad 27 thru_hole circle (at 16.51 0) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 15 "Net-(U2-Pad27)"))
    (pad 28 thru_hole circle (at 16.51 -2.54) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 16 "Net-(U2-Pad28)"))
    (pad 29 thru_hole circle (at 16.51 -5.08) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 17 "Net-(U2-Pad29)"))
    (pad 30 thru_hole circle (at 29.21 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 18 "Net-(U2-Pad30)"))
    (pad 31 thru_hole circle (at 26.67 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 19 "Net-(U2-Pad31)"))
    (pad 32 thru_hole circle (at 24.13 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 20 "Net-(U2-Pad32)"))
    (pad 33 thru_hole circle (at 21.59 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 21 "Net-(U2-Pad33)"))
    (pad 34 thru_hole circle (at 19.05 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 96 6IO))
    (pad 35 thru_hole circle (at 16.51 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 95 2IO))
    (pad 36 thru_hole circle (at 13.97 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 22 "Net-(U2-Pad36)"))
    (pad 37 thru_hole circle (at 11.43 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 23 "Net-(U2-Pad37)"))
    (pad 13 thru_hole circle (at 1.27 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 81 "Net-(J3-Pad7)"))
    (pad 12 thru_hole circle (at -1.27 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 76 "Net-(J3-Pad3)"))
    (pad 11 thru_hole circle (at -3.81 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 77 "Net-(J3-Pad4)"))
    (pad 10 thru_hole circle (at -6.35 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 78 "Net-(J3-Pad5)"))
    (pad 9 thru_hole circle (at -8.89 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 24 "Net-(U2-Pad9)"))
    (pad 8 thru_hole circle (at -11.43 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 25 "Net-(U2-Pad8)"))
    (pad 7 thru_hole circle (at -13.97 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 26 "Net-(U2-Pad7)"))
    (pad 6 thru_hole circle (at -16.51 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 27 "Net-(U2-Pad6)"))
    (pad 5 thru_hole circle (at -19.05 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 28 "Net-(U2-Pad5)"))
    (pad 4 thru_hole circle (at -21.59 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 29 "Net-(U2-Pad4)"))
    (pad 3 thru_hole circle (at -24.13 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 30 "Net-(U2-Pad3)"))
    (pad 2 thru_hole circle (at -26.67 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 31 "Net-(U2-Pad2)"))
    (pad 1 thru_hole rect (at -29.21 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 38 thru_hole circle (at 8.89 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 32 "Net-(U2-Pad38)"))
    (pad 39 thru_hole circle (at 6.35 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 40 thru_hole circle (at 3.81 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 79 "Net-(J3-Pad6)"))
    (pad 41 connect circle (at 1.27 -7.62) (size 1.6 1.6) (layers Dwgs.User)
      (net 33 "Net-(U2-Pad41)"))
    (pad 42 connect circle (at -1.27 -7.62) (size 1.6 1.6) (layers Dwgs.User)
      (net 34 "Net-(U2-Pad42)"))
    (pad 43 connect circle (at -3.81 -7.62) (size 1.6 1.6) (layers Dwgs.User)
      (net 35 "Net-(U2-Pad43)"))
    (pad 44 connect circle (at -6.35 -7.62) (size 1.6 1.6) (layers Dwgs.User)
      (net 36 "Net-(U2-Pad44)"))
    (pad 45 thru_hole circle (at -8.89 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 75 "Net-(J2-Pad4)"))
    (pad 46 thru_hole circle (at -11.43 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 74 "Net-(J2-Pad3)"))
    (pad 47 thru_hole circle (at -13.97 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 37 "Net-(U2-Pad47)"))
    (pad 48 thru_hole circle (at -16.51 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 38 "Net-(U2-Pad48)"))
    (pad 49 thru_hole circle (at -19.05 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 39 "Net-(U2-Pad49)"))
    (pad 50 thru_hole circle (at -21.59 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 40 "Net-(U2-Pad50)"))
    (pad 51 thru_hole circle (at -24.13 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 80 +3V3))
    (pad 52 thru_hole circle (at -26.67 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 53 thru_hole circle (at -29.21 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 73 +5V))
    (pad 54 connect circle (at -26.67 -5.08) (size 1.6 1.6) (layers Dwgs.User)
      (net 41 "Net-(U2-Pad54)"))
    (pad 55 connect circle (at -21.59 -5.08) (size 1.6 1.6) (layers Dwgs.User)
      (net 42 "Net-(U2-Pad55)"))
    (pad 56 connect circle (at -19.05 -5.08) (size 1.6 1.6) (layers Dwgs.User)
      (net 43 "Net-(U2-Pad56)"))
    (pad 57 connect circle (at -16.51 -5.08) (size 1.6 1.6) (layers Dwgs.User)
      (net 44 "Net-(U2-Pad57)"))
    (pad 63 connect circle (at -13.97 0) (size 1.6 1.6) (layers Dwgs.User)
      (net 45 "Net-(U2-Pad63)"))
    (pad 64 connect circle (at -11.43 0) (size 1.6 1.6) (layers Dwgs.User)
      (net 46 "Net-(U2-Pad64)"))
    (pad 65 connect circle (at -8.89 0) (size 1.6 1.6) (layers Dwgs.User)
      (net 47 "Net-(U2-Pad65)"))
    (pad 66 connect circle (at -6.35 0) (size 1.6 1.6) (layers Dwgs.User)
      (net 48 "Net-(U2-Pad66)"))
    (pad 67 connect circle (at 8.89 0) (size 1.6 1.6) (layers Dwgs.User)
      (net 49 "Net-(U2-Pad67)"))
    (pad 68 connect circle (at 11.43 0) (size 1.6 1.6) (layers Dwgs.User)
      (net 50 "Net-(U2-Pad68)"))
    (pad 69 connect circle (at 13.97 0) (size 1.6 1.6) (layers Dwgs.User)
      (net 51 "Net-(U2-Pad69)"))
    (pad 70 connect circle (at 19.05 0) (size 1.6 1.6) (layers Dwgs.User)
      (net 52 "Net-(U2-Pad70)"))
    (pad 71 connect circle (at 21.59 0) (size 1.6 1.6) (layers Dwgs.User)
      (net 53 "Net-(U2-Pad71)"))
    (pad 72 connect circle (at 24.13 0) (size 1.6 1.6) (layers Dwgs.User)
      (net 54 "Net-(U2-Pad72)"))
    (pad 73 connect circle (at 26.67 0) (size 1.6 1.6) (layers Dwgs.User)
      (net 55 "Net-(U2-Pad73)"))
    (pad 74 connect circle (at 29.21 0) (size 1.6 1.6) (layers Dwgs.User)
      (net 71 "Net-(U2-Pad74)"))
    (pad 75 connect circle (at 29.21 -2.54) (size 1.6 1.6) (layers Dwgs.User)
      (net 56 "Net-(U2-Pad75)"))
    (pad 76 connect circle (at 26.67 -2.54) (size 1.6 1.6) (layers Dwgs.User)
      (net 57 "Net-(U2-Pad76)"))
    (pad 77 connect circle (at 24.13 -2.54) (size 1.6 1.6) (layers Dwgs.User)
      (net 58 "Net-(U2-Pad77)"))
    (pad 78 connect circle (at 21.59 -2.54) (size 1.6 1.6) (layers Dwgs.User)
      (net 59 "Net-(U2-Pad78)"))
    (pad 79 connect circle (at 19.05 -2.54) (size 1.6 1.6) (layers Dwgs.User)
      (net 60 "Net-(U2-Pad79)"))
    (pad 80 connect circle (at 13.97 -2.54) (size 1.6 1.6) (layers Dwgs.User)
      (net 61 "Net-(U2-Pad80)"))
    (pad 81 connect circle (at 11.43 -2.54) (size 1.6 1.6) (layers Dwgs.User)
      (net 62 "Net-(U2-Pad81)"))
    (pad 82 connect circle (at 8.89 -2.54) (size 1.6 1.6) (layers Dwgs.User)
      (net 63 "Net-(U2-Pad82)"))
    (pad 83 connect circle (at -6.35 -2.54) (size 1.6 1.6) (layers Dwgs.User)
      (net 64 "Net-(U2-Pad83)"))
    (pad 84 connect circle (at -8.89 -2.54) (size 1.6 1.6) (layers Dwgs.User)
      (net 65 "Net-(U2-Pad84)"))
    (pad 85 connect circle (at -11.43 -2.54) (size 1.6 1.6) (layers Dwgs.User)
      (net 66 "Net-(U2-Pad85)"))
    (pad 86 connect circle (at -13.97 -2.54) (size 1.6 1.6) (layers Dwgs.User)
      (net 67 "Net-(U2-Pad86)"))
    (pad 58 connect circle (at -22.86 4.62) (size 1.6 1.6) (layers Dwgs.User)
      (net 86 "Net-(U2-Pad58)"))
    (pad 59 connect circle (at -20.32 4.62) (size 1.6 1.6) (layers Dwgs.User)
      (net 68 "Net-(U2-Pad59)"))
    (pad 60 connect circle (at -17.78 4.62) (size 1.6 1.6) (layers Dwgs.User)
      (net 69 "Net-(U2-Pad60)"))
    (pad 61 connect circle (at -15.24 4.62) (size 1.6 1.6) (layers Dwgs.User)
      (net 72 "Net-(U2-Pad61)"))
    (pad 62 connect circle (at -12.7 4.62) (size 1.6 1.6) (layers Dwgs.User)
      (net 70 "Net-(U2-Pad62)"))
  )
  (module Package_SO:SOIC-8_3.9x4.9mm_P1.27mm (layer F.Cu) (tedit 5A02F2D3)
    (at 82.703074 23.875778)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U3 (at -4.732 -2.794) (layer F.SilkS))
    (fp_text value CAN_SN65HVD23x (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 8 smd rect (at 2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(U2-Pad32)"))
    (pad 7 smd rect (at 2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 82 CAN2H))
    (pad 6 smd rect (at 2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 83 CAN2L))
    (pad 5 smd rect (at 2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 92 "Net-(J15-Pad1)"))
    (pad 4 smd rect (at -2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(U2-Pad31)"))
    (pad 3 smd rect (at -2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 80 +3V3))
    (pad 2 smd rect (at -2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(U2-Pad30)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 76.828074 24.093278 270)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C3 (at 3.4655 0) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.82 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 80 +3V3))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Custom:Single_43_63_PTH (layer F.Cu) (tedit 5B9B2E79)
    (at 60.953074 50.545778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single_43_63_PTH (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.6002 1.6002) (drill 1.0922) (layers *.Cu *.Mask))
  )
  (module Custom:Single_43_63_PTH (layer F.Cu) (tedit 5B9B2E79)
    (at 60.953074 48.005778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single_43_63_PTH (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.6002 1.6002) (drill 1.0922) (layers *.Cu *.Mask))
  )
  (module Custom:Single_43_63_PTH (layer F.Cu) (tedit 5B9B2E79)
    (at 58.413074 40.385778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single_43_63_PTH (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.6002 1.6002) (drill 1.0922) (layers *.Cu *.Mask))
  )
  (module Custom:Single_43_63_PTH (layer F.Cu) (tedit 5B9B2E79)
    (at 60.953074 37.845778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single_43_63_PTH (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.6002 1.6002) (drill 1.0922) (layers *.Cu *.Mask))
  )
  (module Custom:Single_43_63_PTH (layer F.Cu) (tedit 5B9B2E79)
    (at 60.953074 40.385778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single_43_63_PTH (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.6002 1.6002) (drill 1.0922) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 72.383074 53.085778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 72.383074 51.815778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 72.383074 50.545778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 72.383074 49.275778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single_43_63_PTH (layer F.Cu) (tedit 5B9B2E79)
    (at 27.298074 21.970778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single_43_63_PTH (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.6002 1.6002) (drill 1.0922) (layers *.Cu *.Mask))
  )
  (module Custom:Single_43_63_PTH (layer F.Cu) (tedit 5B9B2E79)
    (at 29.838074 21.970778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single_43_63_PTH (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.6002 1.6002) (drill 1.0922) (layers *.Cu *.Mask))
  )
  (module Custom:Single_43_63_PTH (layer F.Cu) (tedit 5B9B2E79)
    (at 22.218074 21.970778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single_43_63_PTH (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.6002 1.6002) (drill 1.0922) (layers *.Cu *.Mask))
  )
  (module Custom:Single_43_63_PTH (layer F.Cu) (tedit 5B9B2E79)
    (at 24.758074 21.970778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single_43_63_PTH (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.6002 1.6002) (drill 1.0922) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 36.188074 26.415778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 36.188074 27.685778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 38.728074 26.415778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 33.648074 26.415778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 38.728074 27.685778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 34.918074 26.415778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 34.918074 27.685778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 37.458074 27.685778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 39.998074 27.685778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 37.458074 26.415778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 32.378074 27.685778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 32.378074 26.415778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 33.648074 27.685778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 39.998074 26.415778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 27.933074 40.385778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 22.853074 40.385778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 27.933074 41.655778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 24.123074 40.385778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 24.123074 41.655778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 26.663074 41.655778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 29.203074 41.655778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 26.663074 40.385778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 21.583074 41.655778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 21.583074 40.385778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 22.853074 41.655778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 29.203074 40.385778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 27.933074 37.845778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 22.853074 37.845778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 27.933074 39.115778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 24.123074 37.845778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 24.123074 39.115778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 26.663074 39.115778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 29.203074 39.115778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 26.663074 37.845778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 21.583074 39.115778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 21.583074 37.845778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 22.853074 39.115778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 29.203074 37.845778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 27.933074 35.305778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 22.853074 35.305778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 27.933074 36.575778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 24.123074 35.305778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 24.123074 36.575778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 26.663074 36.575778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 29.203074 36.575778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 26.663074 35.305778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 21.583074 36.575778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 21.583074 35.305778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 22.853074 36.575778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 29.203074 35.305778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 27.933074 32.765778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 22.853074 32.765778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 27.933074 34.035778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 24.123074 32.765778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 24.123074 34.035778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 26.663074 34.035778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 29.203074 34.035778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 26.663074 32.765778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 21.583074 34.035778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 21.583074 32.765778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 22.853074 34.035778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 29.203074 32.765778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 35.553074 40.385778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 35.553074 41.655778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 38.093074 40.385778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 33.013074 40.385778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 38.093074 41.655778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 34.283074 40.385778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 34.283074 41.655778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 36.823074 41.655778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 39.363074 41.655778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 36.823074 40.385778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 31.743074 41.655778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 31.743074 40.385778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 33.013074 41.655778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 39.363074 40.385778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 35.553074 37.845778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 35.553074 39.115778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 38.093074 37.845778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 33.013074 37.845778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 38.093074 39.115778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 34.283074 37.845778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 34.283074 39.115778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 36.823074 39.115778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 39.363074 39.115778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 36.823074 37.845778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 31.743074 39.115778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 31.743074 37.845778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 33.013074 39.115778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 39.363074 37.845778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 35.553074 35.305778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 35.553074 36.575778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 38.093074 35.305778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 33.013074 35.305778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 38.093074 36.575778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 34.283074 35.305778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 34.283074 36.575778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 36.823074 36.575778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 39.363074 36.575778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 36.823074 35.305778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 31.743074 36.575778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 31.743074 35.305778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 33.013074 36.575778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 39.363074 35.305778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 35.553074 32.765778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 35.553074 34.035778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 38.093074 32.765778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 33.013074 32.765778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 38.093074 34.035778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 34.283074 32.765778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 34.283074 34.035778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 36.823074 34.035778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 39.363074 34.035778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 36.823074 32.765778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 31.743074 34.035778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 31.743074 32.765778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 33.013074 34.035778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 39.363074 32.765778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 45.078074 23.875778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 45.078074 25.145778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 47.618074 23.875778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 42.538074 23.875778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 47.618074 25.145778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 43.808074 23.875778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 43.808074 25.145778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 46.348074 25.145778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 48.888074 25.145778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 46.348074 23.875778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 41.268074 25.145778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 41.268074 23.875778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 42.538074 25.145778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 48.888074 23.875778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 45.078074 26.415778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 45.078074 27.685778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 47.618074 26.415778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 42.538074 26.415778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 47.618074 27.685778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 43.808074 26.415778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 43.808074 27.685778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 46.348074 27.685778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 48.888074 27.685778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 46.348074 26.415778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 41.268074 27.685778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 41.268074 26.415778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 42.538074 27.685778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 48.888074 26.415778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 71.113074 49.275778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 69.843074 49.275778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 68.573074 49.275778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 67.303074 49.275778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 66.033074 49.275778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 64.763074 49.275778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 63.493074 49.275778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 71.113074 50.545778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 71.113074 51.815778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 71.113074 53.085778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 69.843074 53.085778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 68.573074 53.085778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 67.303074 53.085778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 66.033074 53.085778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 64.763074 53.085778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 63.493074 53.085778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 69.843074 51.815778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 69.843074 50.545778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 68.573074 51.815778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 68.573074 50.545778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 67.303074 51.815778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 67.303074 50.545778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 66.033074 51.815778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 64.763074 51.815778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 63.493074 51.815778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single_43_63_PTH (layer F.Cu) (tedit 5B9B2E79)
    (at 92.703074 51.815778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single_43_63_PTH (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.6002 1.6002) (drill 1.0922) (layers *.Cu *.Mask))
  )
  (module Custom:Single_43_63_PTH (layer F.Cu) (tedit 5B9B2E79)
    (at 92.703074 49.275778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single_43_63_PTH (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.6002 1.6002) (drill 1.0922) (layers *.Cu *.Mask))
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBE)
    (at 62.440574 22.605778)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C1 (at 0 1.82) (layer B.SilkS))
    (fp_text value 0.1uf (at 0 -1.82) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 73 +5V))
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBE)
    (at 62.223074 26.415778 180)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C2 (at -0.127 -1.905 180) (layer B.SilkS))
    (fp_text value 0.1uf (at 0 -1.82 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd roundrect (at 1.4875 0 180) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.4875 0 180) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 2 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SMA-SMB_Universal_Handsoldering (layer B.Cu) (tedit 5864381A)
    (at 71.473074 22.605778)
    (descr "Diode, Universal, SMA (DO-214AC) or SMB (DO-214AA), Handsoldering,")
    (tags "Diode Universal SMA (DO-214AC) SMB (DO-214AA) Handsoldering ")
    (attr smd)
    (fp_text reference D1 (at -6.075 -1.524) (layer B.SilkS))
    (fp_text value D (at 0 -3.1) (layer B.Fab))
    (fp_text user %R (at 0 3) (layer B.Fab))
    (pad 1 smd trapezoid (at -2.9 0) (size 3.6 1.7) (rect_delta 0.6 0 ) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C2-Pad1)"))
    (pad 2 smd trapezoid (at 2.9 0 180) (size 3.6 1.7) (rect_delta 0.6 0 ) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMB.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SMC (layer F.Cu) (tedit 5B9DBF28)
    (at 89.401074 48.992778 270)
    (descr "Diode SMC (DO-214AB)")
    (tags "Diode SMC (DO-214AB)")
    (attr smd)
    (fp_text reference D2 (at -4.2255 -3.4925) (layer F.SilkS))
    (fp_text value Z3SMCxxx (at 0 4.2 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -3.4 0) (size 3.3 2.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 3.4 0) (size 3.3 2.5) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMC.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_Nano-Fit_105310-xx08_2x04_P2.50mm_Vertical (layer B.Cu) (tedit 5A17387E)
    (at 88.893074 42.925778)
    (descr "Molex Nano-Fit Power Connectors, 105310-xx08, 4 Pins per row (http://www.molex.com/pdm_docs/sd/1053101208_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex Nano-Fit side entry")
    (fp_text reference J1 (at 0 3.302) (layer B.SilkS))
    (fp_text value Conn_02x04_Top_Bottom (at 1.25 -10.42) (layer B.Fab))
    (fp_text user %R (at 3.54 -3.75 -90) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 0 -2.5) (size 1.7 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 88 "Net-(D4-Pad2)"))
    (pad 3 thru_hole circle (at 0 -5) (size 1.7 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 85 CAN1H))
    (pad 4 thru_hole circle (at 0 -7.5) (size 1.7 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 82 CAN2H))
    (pad 5 thru_hole circle (at 2.5 0) (size 1.7 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 "Net-(D1-Pad2)"))
    (pad 6 thru_hole circle (at 2.5 -2.5) (size 1.7 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 89 "Net-(D5-Pad2)"))
    (pad 7 thru_hole circle (at 2.5 -5) (size 1.7 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 84 CAN1L))
    (pad 8 thru_hole circle (at 2.5 -7.5) (size 1.7 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 83 CAN2L))
    (pad "" np_thru_hole circle (at -1.34 -3.75) (size 1.3 1.3) (drill 1.3) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_Nano-Fit_105310-xx08_2x04_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-89-3_Handsoldering (layer B.Cu) (tedit 5A02FF57)
    (at 55.163074 23.875778 180)
    (descr "SOT-89-3 Handsoldering")
    (tags "SOT-89-3 Handsoldering")
    (attr smd)
    (fp_text reference U1 (at 0.179 -3.556 180) (layer B.SilkS))
    (fp_text value L78L08_SOT89 (at 0.5 -3.15 180) (layer B.Fab))
    (fp_text user %R (at 0.38 0 90) (layer B.Fab))
    (pad 1 smd rect (at -1.98 1.5 270) (size 1 2.5) (layers B.Cu B.Paste B.Mask)
      (net 73 +5V))
    (pad 2 smd rect (at -1.98 0 270) (size 1 2.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.98 -1.5 270) (size 1 2.5) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 1.98 0 270) (size 2 4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd trapezoid (at -0.37 0 90) (size 1.5 0.75) (rect_delta 0 -0.5 ) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-89-3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 64.545574 32.765778)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C5 (at -0.1635 1.397) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0.635) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 95 2IO))
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_Nano-Fit_105309-xx04_1x04_P2.50mm_Vertical (layer B.Cu) (tedit 5B9D842C)
    (at 22.853074 25.145778 270)
    (descr "Molex Nano-Fit Power Connectors, 105309-xx04, 4 Pins per row (http://www.molex.com/pdm_docs/sd/1053091203_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex Nano-Fit side entry")
    (fp_text reference J2 (at 2.794 0.254) (layer B.SilkS))
    (fp_text value displays_0.96inch_I2C_OLED (at 0 -10.42 270) (layer B.Fab) hide)
    (fp_text user %R (at 1.1 -3.75 180) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.2 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 80 +3V3))
    (pad 2 thru_hole oval (at 0 -2.5 270) (size 2.2 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 -5 270) (size 2.2 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 74 "Net-(J2-Pad3)"))
    (pad 4 thru_hole oval (at 0 -7.5 270) (size 2.2 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 75 "Net-(J2-Pad4)"))
    (pad "" np_thru_hole circle (at -1.34 -3.75 270) (size 1.3 1.3) (drill 1.3) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_Nano-Fit_105309-xx04_1x04_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 28.568074 50.128278 270)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C4 (at -2.3765 1.9685) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.82 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 1 GND))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 80 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 88.763074 28.955778 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 0.3145 1.778 180) (layer F.SilkS))
    (fp_text value R (at 0 1.82 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 82 CAN2H))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 83 CAN2L))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 88.763074 31.495778)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at -0.124 1.905) (layer F.SilkS))
    (fp_text value R (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 84 CAN1L))
    (pad 1 smd roundrect (at -1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 85 CAN1H))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-8_3.9x4.9mm_P1.27mm (layer F.Cu) (tedit 5A02F2D3)
    (at 34.123074 49.910778)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U4 (at -3.2055 3.302) (layer F.SilkS))
    (fp_text value CAN_SN65HVD23x (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(U2-Pad5)"))
    (pad 2 smd rect (at -2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 80 +3V3))
    (pad 4 smd rect (at -2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(U2-Pad6)"))
    (pad 5 smd rect (at 2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 93 "Net-(J16-Pad1)"))
    (pad 6 smd rect (at 2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 84 CAN1L))
    (pad 7 smd rect (at 2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 85 CAN1H))
    (pad 8 smd rect (at 2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(U2-Pad8)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Converter_DCDC:Converter_DCDC_TRACO_TSR-1_THT (layer F.Cu) (tedit 59FE1FB7)
    (at 66.033074 26.415778)
    (descr "DCDC-Converter, TRACO, TSR 1-xxxx")
    (tags "DCDC-Converter TRACO TSR-1")
    (fp_text reference U5 (at -5.207 0.127) (layer F.SilkS))
    (fp_text value traco_TSR_0.5-2450 (at 2.5 3.25) (layer F.Fab))
    (fp_text user %R (at 3 -3) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.5 2.5) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(C2-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.5 2.5) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.5 2.5) (drill 1) (layers *.Cu *.Mask)
      (net 73 +5V))
    (model ${KISYS3DMOD}/Converter_DCDC.3dshapes/Converter_DCDC_TRACO_TSR-1_THT.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_Nano-Fit_105309-xx07_1x07_P2.50mm_Vertical (layer B.Cu) (tedit 5A17387E)
    (at 55.873074 49.275778 90)
    (descr "Molex Nano-Fit Power Connectors, 105309-xx07, 7 Pins per row (http://www.molex.com/pdm_docs/sd/1053091203_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex Nano-Fit side entry")
    (fp_text reference J3 (at 1.905 2.54 180) (layer B.SilkS))
    (fp_text value Conn_01x07 (at 0 -17.92 90) (layer B.Fab))
    (fp_text user %R (at 1.1 -7.5) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.2 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 -2.5 90) (size 2.2 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 80 +3V3))
    (pad 3 thru_hole oval (at 0 -5 90) (size 2.2 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 76 "Net-(J3-Pad3)"))
    (pad 4 thru_hole oval (at 0 -7.5 90) (size 2.2 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 77 "Net-(J3-Pad4)"))
    (pad 5 thru_hole oval (at 0 -10 90) (size 2.2 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 78 "Net-(J3-Pad5)"))
    (pad 6 thru_hole oval (at 0 -12.5 90) (size 2.2 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 79 "Net-(J3-Pad6)"))
    (pad 7 thru_hole oval (at 0 -15 90) (size 2.2 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 81 "Net-(J3-Pad7)"))
    (pad "" np_thru_hole circle (at -1.34 -6.25 90) (size 1.3 1.3) (drill 1.3) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_Nano-Fit_105309-xx07_1x07_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 63.493074 50.545778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 64.763074 50.545778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Single30_40 (layer F.Cu) (tedit 5B9B3C0E)
    (at 66.033074 50.545778)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single30_40 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.016 1.016) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Custom:Keystone_3001_1x12mm-CoinCell (layer B.Cu) (tedit 58972363)
    (at 49.523074 36.575778)
    (descr http://www.keyelco.com/product-pdf.cfm?p=778)
    (tags "Keystone type 3001 coin cell retainer")
    (fp_text reference BT1 (at -7.62 4.445) (layer B.SilkS))
    (fp_text value Battery_Cell (at 0 -7.5) (layer B.Fab))
    (pad 2 smd rect (at 0 0) (size 4 4) (layers B.Cu B.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 6.6 0) (size 3 3) (drill 1.9) (layers *.Cu *.Mask)
      (net 87 "Net-(BT1-Pad1)"))
    (pad 1 thru_hole circle (at -6.6 0) (size 3 3) (drill 1.9) (layers *.Cu *.Mask)
      (net 87 "Net-(BT1-Pad1)"))
    (model Battery_Holders.3dshapes/Keystone_3001_1x12mm-CoinCell.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x08_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 85.083074 34.035778)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference J4 (at -1.524 -2.159) (layer F.SilkS))
    (fp_text value Conn_01x08 (at 0 20.11) (layer F.Fab))
    (fp_text user %R (at 0 8.89 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 82 CAN2H))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 83 CAN2L))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 88 "Net-(D4-Pad2)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 89 "Net-(D5-Pad2)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 85 CAN1H))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 84 CAN1L))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 64.545574 39.115778)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C6 (at -5.6245 -0.635) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 96 6IO))
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57)
    (at 59.368074 33.130778 270)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference D3 (at -0.619 2.733) (layer F.SilkS))
    (fp_text value AZ23C3V0-7-F (at 0 2.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 95 2IO))
    (pad 2 smd rect (at -1 0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 96 6IO))
    (pad 3 smd rect (at 1 0 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SMA (layer B.Cu) (tedit 586432E5)
    (at 78.003074 32.765778 180)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (attr smd)
    (fp_text reference D4 (at -2.762 -2.794 180) (layer B.SilkS))
    (fp_text value B140-E3 (at 0 -2.6 180) (layer B.Fab))
    (fp_text user %R (at 0 2.5 180) (layer B.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2.5 1.8) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(D1-Pad2)"))
    (pad 2 smd rect (at 2 0 180) (size 2.5 1.8) (layers B.Cu B.Paste B.Mask)
      (net 88 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SMA (layer B.Cu) (tedit 586432E5)
    (at 78.003074 42.925778 180)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (attr smd)
    (fp_text reference D5 (at -2.635 2.54 180) (layer B.SilkS))
    (fp_text value B140-E3 (at 0 -2.6 180) (layer B.Fab))
    (fp_text user %R (at 0 2.5 180) (layer B.Fab))
    (pad 2 smd rect (at 2 0 180) (size 2.5 1.8) (layers B.Cu B.Paste B.Mask)
      (net 89 "Net-(D5-Pad2)"))
    (pad 1 smd rect (at -2 0 180) (size 2.5 1.8) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Custom:Single_43_63_PTH (layer F.Cu) (tedit 5B9B2E79)
    (at 60.953074 35.305778)
    (fp_text reference J5 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single_Pin (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.6002 1.6002) (drill 1.0922) (layers *.Cu *.Mask)
      (net 95 2IO))
  )
  (module Custom:Single_43_63_PTH (layer F.Cu) (tedit 5B9B2E79)
    (at 60.953074 42.925778)
    (fp_text reference J6 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single_Pin (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.6002 1.6002) (drill 1.0922) (layers *.Cu *.Mask)
      (net 96 6IO))
  )
  (module digikey-footprints:SOT-23-3 (layer F.Cu) (tedit 59D275F3)
    (at 72.163074 33.080778)
    (fp_text reference Q1 (at 3.141 -0.569) (layer F.SilkS))
    (fp_text value FMMT493TA (at 0.025 3.25) (layer F.Fab))
    (fp_text user %R (at -0.125 0.15) (layer F.Fab))
    (pad 1 smd rect (at -1.05 -0.95) (size 1.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 90 "Net-(Q1-Pad1)") (solder_mask_margin 0.07))
    (pad 2 smd rect (at -1.05 0.95) (size 1.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.07))
    (pad 3 smd rect (at 1.05 0) (size 1.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 88 "Net-(D4-Pad2)") (solder_mask_margin 0.07))
  )
  (module digikey-footprints:SOT-23-3 (layer F.Cu) (tedit 59D275F3)
    (at 72.163074 42.605778)
    (fp_text reference Q2 (at 3.141 0.574) (layer F.SilkS))
    (fp_text value FMMT493TA (at 0.025 3.25) (layer F.Fab))
    (fp_text user %R (at -0.125 0.15) (layer F.Fab))
    (pad 3 smd rect (at 1.05 0) (size 1.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 89 "Net-(D5-Pad2)") (solder_mask_margin 0.07))
    (pad 2 smd rect (at -1.05 0.95) (size 1.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.07))
    (pad 1 smd rect (at -1.05 -0.95) (size 1.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 91 "Net-(Q2-Pad1)") (solder_mask_margin 0.07))
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 72.513074 36.575778)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at 2.41 -1.778) (layer F.SilkS))
    (fp_text value R (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 88 "Net-(D4-Pad2)"))
    (pad 2 smd roundrect (at 1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 95 2IO))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 72.383074 39.115778)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at 2.54 1.905) (layer F.SilkS))
    (fp_text value R (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 95 2IO))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 78.863074 39.115778)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at 0.124 1.905) (layer F.SilkS))
    (fp_text value R (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 96 6IO))
    (pad 1 smd roundrect (at -1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 89 "Net-(D5-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 64.633074 42.290778)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R6 (at 0.003 1.778) (layer F.SilkS))
    (fp_text value R (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 96 6IO))
    (pad 2 smd roundrect (at 1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 64.763074 35.940778 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R7 (at 5.842 -0.127 180) (layer F.SilkS))
    (fp_text value R (at 0 1.82 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 95 2IO))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 90 "Net-(Q1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 78.863074 36.575778)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R8 (at 0 -1.82) (layer F.SilkS))
    (fp_text value R (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 91 "Net-(Q2-Pad1)"))
    (pad 2 smd roundrect (at 1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 96 6IO))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Custom:Single_43_63_PTH (layer F.Cu) (tedit 5B9B2E79)
    (at 41.268074 21.970778)
    (fp_text reference J7 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single_Pin (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.6002 1.6002) (drill 1.0922) (layers *.Cu *.Mask)
      (net 73 +5V))
  )
  (module Custom:Single_43_63_PTH (layer F.Cu) (tedit 5B9B2E79)
    (at 53.333074 52.945878)
    (fp_text reference J8 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single_Pin (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.6002 1.6002) (drill 1.0922) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Custom:Single_43_63_PTH (layer F.Cu) (tedit 5B9B2E79)
    (at 43.808074 21.970778)
    (fp_text reference J9 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single_Pin (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.6002 1.6002) (drill 1.0922) (layers *.Cu *.Mask)
      (net 73 +5V))
  )
  (module Custom:Single_43_63_PTH (layer F.Cu) (tedit 5B9B2E79)
    (at 55.873074 52.945878)
    (fp_text reference J10 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single_Pin (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.6002 1.6002) (drill 1.0922) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Custom:Single_43_63_PTH (layer F.Cu) (tedit 5B9B2E79)
    (at 46.348074 21.970778)
    (fp_text reference J11 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single_Pin (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.6002 1.6002) (drill 1.0922) (layers *.Cu *.Mask)
      (net 73 +5V))
  )
  (module Custom:Single_43_63_PTH (layer F.Cu) (tedit 5B9B2E79)
    (at 58.413074 52.945878)
    (fp_text reference J12 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single_Pin (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.6002 1.6002) (drill 1.0922) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Custom:Single_43_63_PTH (layer F.Cu) (tedit 5B9B2E79)
    (at 48.888074 21.970778)
    (fp_text reference J13 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single_Pin (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.6002 1.6002) (drill 1.0922) (layers *.Cu *.Mask)
      (net 73 +5V))
  )
  (module Custom:Single_43_63_PTH (layer F.Cu) (tedit 5B9B2E79)
    (at 60.953074 52.945878)
    (fp_text reference J14 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single_Pin (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.6002 1.6002) (drill 1.0922) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Custom:Single_43_63_PTH (layer F.Cu) (tedit 5B9B2E79)
    (at 85.083074 27.685778)
    (fp_text reference J15 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single_Pin (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.6002 1.6002) (drill 1.0922) (layers *.Cu *.Mask)
      (net 92 "Net-(J15-Pad1)"))
  )
  (module Custom:Single_43_63_PTH (layer F.Cu) (tedit 5B9B2E79)
    (at 38.728074 52.450778)
    (fp_text reference J16 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single_Pin (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.6002 1.6002) (drill 1.0922) (layers *.Cu *.Mask)
      (net 93 "Net-(J16-Pad1)"))
  )
  (module Custom:Single_43_63_PTH (layer F.Cu) (tedit 5B9B2E79)
    (at 92.703074 27.685778)
    (fp_text reference J17 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single_Pin (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.6002 1.6002) (drill 1.0922) (layers *.Cu *.Mask)
      (net 82 CAN2H))
  )
  (module Custom:Single_43_63_PTH (layer F.Cu) (tedit 5B9B2E79)
    (at 85.083074 30.225778)
    (fp_text reference J18 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single_Pin (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.6002 1.6002) (drill 1.0922) (layers *.Cu *.Mask)
      (net 83 CAN2L))
  )
  (module Custom:Single_43_63_PTH (layer F.Cu) (tedit 5B9B2E79)
    (at 43.808074 52.450778)
    (fp_text reference J19 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single_Pin (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.6002 1.6002) (drill 1.0922) (layers *.Cu *.Mask)
      (net 85 CAN1H))
  )
  (module Custom:Single_43_63_PTH (layer F.Cu) (tedit 5B9B2E79)
    (at 41.268074 52.450778)
    (fp_text reference J20 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single_Pin (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.6002 1.6002) (drill 1.0922) (layers *.Cu *.Mask)
      (net 84 CAN1L))
  )
  (module Custom:Single_43_63_PTH (layer F.Cu) (tedit 5B9B2E79)
    (at 58.413074 42.925778)
    (fp_text reference J21 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single_Pin (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.6002 1.6002) (drill 1.0922) (layers *.Cu *.Mask)
      (net 94 "Net-(J21-Pad1)"))
  )
  (module MountingHole:MountingHole_2.5mm (layer F.Cu) (tedit 5B9D8423)
    (at 37 22.75)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.5mm (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.5mm (layer F.Cu) (tedit 5B9D8448)
    (at 77 51.25)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.5mm (at 0 3.5) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (gr_text "Cafe Electric llc\n“Smoother 1.0” 09/2018\nAutomotive Interface board\nTeensy 3.6 based \nw/2 CAN 2.0" (at 56.063574 23.177278) (layer F.SilkS))
  (gr_arc (start 90.75 23.25) (end 87.5 23.25) (angle -90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 90.75 26.5) (end 94 26.5) (layer Edge.Cuts) (width 0.0254))
  (gr_arc (start 23.25 50.75) (end 26.5 50.75) (angle -90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 23.25 47.5) (end 20 47.5) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 26.5 50.75) (end 26.5 54) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 87.5 23.25) (end 87.5 20) (layer Edge.Cuts) (width 0.0254))
  (gr_arc (start 93 53) (end 93 54) (angle -90) (layer Edge.Cuts) (width 0.0254))
  (gr_arc (start 21 21) (end 21 20) (angle -90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 20 47.5) (end 20 21) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 93 54) (end 26.5 54) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 94 26.5) (end 94 53) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 21 20) (end 87.5 20) (layer Edge.Cuts) (width 0.0254))
)
