(kicad_pcb (version 4) (host pcbnew 4.0.2-stable)
  (general
    (links 0)
    (no_connects 29)
    (area 83.251268 76.532848 121.210157 146.491725)
    (thickness 1.6)
    (drawings 102)
    (tracks 125)
    (zones 0)
    (modules 7)
    (nets 30)
  )
  (page USLetter)
  (title_block
    (title "EME Integration Board")
    (date 2016-08-29)
    (rev 1)
    (company "Battlespace Simulations, Inc")
    (comment 1 "For use w/ Fallon CAVE IZLID and SOFLAM")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.778 1.778)
    (pad_drill 1.016)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /P2)
  (net 2 /P1)
  (net 3 /P3)
  (net 4 /P4)
  (net 5 /P5)
  (net 6 /P6)
  (net 7 /P0)
  (net 8 /P7)
  (net 9 /P8)
  (net 10 /P9)
  (net 11 /P10)
  (net 12 /P11)
  (net 13 GND)
  (net 14 /P14)
  (net 15 /P13)
  (net 16 /P15)
  (net 17 /P16)
  (net 18 /P20)
  (net 19 /P21)
  (net 20 /P12)
  (net 21 /P22)
  (net 22 /P23)
  (net 23 /P24)
  (net 24 /P25)
  (net 25 /P26)
  (net 26 +3V3)
  (net 27 /SCL)
  (net 28 /SDA)
  (net 29 /INT)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net /INT)
    (add_net /P0)
    (add_net /P1)
    (add_net /P10)
    (add_net /P11)
    (add_net /P12)
    (add_net /P13)
    (add_net /P14)
    (add_net /P15)
    (add_net /P16)
    (add_net /P2)
    (add_net /P20)
    (add_net /P21)
    (add_net /P22)
    (add_net /P23)
    (add_net /P24)
    (add_net /P25)
    (add_net /P26)
    (add_net /P3)
    (add_net /P4)
    (add_net /P5)
    (add_net /P6)
    (add_net /P7)
    (add_net /P8)
    (add_net /P9)
    (add_net /SCL)
    (add_net /SDA)
    (add_net GND)
  )
  (module Terminal_Blocks:TerminalBlock_Pheonix_PT-3.5mm_12pol (layer F.Cu) (tedit 0)
    (at 115.57 120.06 90)
    (descr "12-way 3.5mm pitch terminal block, Phoenix PT series")
    (fp_text reference P3 (at 19.25 -4.3 90) (layer F.SilkS))
    (fp_text value CONN_01X12 (at 19.25 6 90) (layer F.Fab))
    (pad 3 thru_hole circle (at 7 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 14 /P14))
    (pad 2 thru_hole circle (at 3.5 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 15 /P13))
    (pad 4 thru_hole circle (at 10.5 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 16 /P15))
    (pad 5 thru_hole circle (at 14 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 17 /P16))
    (pad 6 thru_hole circle (at 17.5 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 18 /P20))
    (pad 7 thru_hole circle (at 21 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 19 /P21))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 20 /P12))
    (pad 8 thru_hole circle (at 24.5 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 21 /P22))
    (pad 9 thru_hole circle (at 28 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 22 /P23))
    (pad 10 thru_hole circle (at 31.5 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 23 /P24))
    (pad 11 thru_hole circle (at 35 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 24 /P25))
    (pad 12 thru_hole circle (at 38.5 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 25 /P26))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_PT-3.5mm_12pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Terminal_Blocks:TerminalBlock_Pheonix_PT-3.5mm_12pol (layer F.Cu) (tedit 0)
    (at 88.9 81.9 270)
    (descr "12-way 3.5mm pitch terminal block, Phoenix PT series")
    (fp_text reference P1 (at 19.25 -4.3 270) (layer F.SilkS))
    (fp_text value CONN_01X12 (at 19.25 6 270) (layer F.Fab))
    (pad 3 thru_hole circle (at 7 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 1 /P2))
    (pad 2 thru_hole circle (at 3.5 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 2 /P1))
    (pad 4 thru_hole circle (at 10.5 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 3 /P3))
    (pad 5 thru_hole circle (at 14 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 4 /P4))
    (pad 6 thru_hole circle (at 17.5 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 5 /P5))
    (pad 7 thru_hole circle (at 21 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 6 /P6))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 7 /P0))
    (pad 8 thru_hole circle (at 24.5 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 8 /P7))
    (pad 9 thru_hole circle (at 28 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 9 /P8))
    (pad 10 thru_hole circle (at 31.5 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 10 /P9))
    (pad 11 thru_hole circle (at 35 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 11 /P10))
    (pad 12 thru_hole circle (at 38.5 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 12 /P11))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_PT-3.5mm_12pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Terminal_Blocks:TerminalBlock_Pheonix_PT-3.5mm_6pol (layer F.Cu) (tedit 0)
    (at 115.57 141.9854 90)
    (descr "6-way 3.5mm pitch terminal block, Phoenix PT series")
    (fp_text reference P2 (at 8.75 -4.3 90) (layer F.SilkS))
    (fp_text value CONN_01X06 (at 8.75 6 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 3.5 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 13 GND))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 13 GND))
    (pad 3 thru_hole circle (at 7 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 13 GND))
    (pad 4 thru_hole circle (at 10.5 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 13 GND))
    (pad 5 thru_hole circle (at 14 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 13 GND))
    (pad 6 thru_hole circle (at 17.5 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 13 GND))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_PT-3.5mm_6pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Terminal_Blocks:TerminalBlock_Pheonix_PT-3.5mm_6pol (layer F.Cu) (tedit 0)
    (at 88.9 124.46 270)
    (descr "6-way 3.5mm pitch terminal block, Phoenix PT series")
    (fp_text reference P4 (at 8.75 -4.3 270) (layer F.SilkS))
    (fp_text value CONN_01X06 (at 8.75 6 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 3.5 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 13 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 13 GND))
    (pad 3 thru_hole circle (at 7 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 13 GND))
    (pad 4 thru_hole circle (at 10.5 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 13 GND))
    (pad 5 thru_hole circle (at 14 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 13 GND))
    (pad 6 thru_hole circle (at 17.5 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 13 GND))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_PT-3.5mm_6pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyFootprints:Teensy_LC (layer F.Cu) (tedit 57E318CE)
    (at 102.230712 96.52)
    (fp_text reference U1 (at 0 -10.16) (layer F.SilkS))
    (fp_text value Teensy_LC (at 0 -12.7) (layer F.Fab))
    (pad 1 thru_hole circle (at -7.62 -15.24) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 GND))
    (pad 2 thru_hole circle (at -7.62 -12.7) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 /P0))
    (pad 3 thru_hole circle (at -7.62 -10.16) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 /P1))
    (pad 4 thru_hole circle (at -7.62 -7.62) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 /P2))
    (pad 5 thru_hole circle (at -7.62 -5.08) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 /P3))
    (pad 6 thru_hole circle (at -7.62 -2.54) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 /P4))
    (pad 7 thru_hole circle (at -7.62 0) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 /P5))
    (pad 8 thru_hole circle (at -7.62 2.54) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 /P6))
    (pad 9 thru_hole circle (at -7.62 5.08) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 /P7))
    (pad 10 thru_hole circle (at -7.62 7.62) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 /P8))
    (pad 11 thru_hole circle (at -7.62 10.16) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 /P9))
    (pad 12 thru_hole circle (at -7.62 12.7) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 /P10))
    (pad 13 thru_hole circle (at -7.62 15.24) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 /P11))
    (pad 15 thru_hole circle (at 7.62 -15.24) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 16 thru_hole circle (at 7.62 -12.7) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 GND))
    (pad 17 thru_hole circle (at 7.62 -10.16) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 +3V3))
    (pad 18 thru_hole circle (at 7.62 -7.62) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 /P23))
    (pad 19 thru_hole circle (at 7.62 -5.08) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 /P22))
    (pad 20 thru_hole circle (at 7.62 -2.54) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 /P21))
    (pad 21 thru_hole circle (at 7.62 0) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 /P20))
    (pad 22 thru_hole circle (at 7.62 2.54) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 /SCL))
    (pad 23 thru_hole circle (at 7.62 5.08) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 /SDA))
    (pad 24 thru_hole circle (at 7.62 7.62) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 /INT))
    (pad 25 thru_hole circle (at 7.62 10.16) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 /P16))
    (pad 26 thru_hole circle (at 7.62 12.7) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 /P15))
    (pad 27 thru_hole circle (at 7.62 15.24) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 /P14))
    (pad 14 thru_hole circle (at -7.62 17.78) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 /P12))
    (pad 28 thru_hole circle (at 7.62 17.78) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 /P13))
    (pad 29 thru_hole circle (at 5.08 -7.62) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 30 thru_hole circle (at 5.08 -5.08) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 /P24))
    (pad 31 thru_hole circle (at 5.08 -2.54) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 /P25))
    (pad 32 thru_hole circle (at -5.08 17.78) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 /P26))
    (pad 33 thru_hole circle (at -2.54 17.78) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 34 thru_hole circle (at 0 17.78) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 GND))
    (pad 35 thru_hole circle (at 2.54 17.78) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 36 thru_hole circle (at 5.08 17.78) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 37 thru_hole circle (at 5.08 -12.7) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  )
  (module MyFootprints:BSI_IMU (layer F.Cu) (tedit 57E31981)
    (at 102.743 134.366)
    (fp_text reference U2 (at 0.635 -10.795) (layer F.SilkS))
    (fp_text value BSI_IMU (at 0 -1.27) (layer F.Fab))
    (fp_text user +3V3 (at 5.715 3.81 90) (layer F.SilkS))
    (fp_text user GND (at 3.175 4.445 90) (layer F.SilkS))
    (fp_text user SDA (at 0.635 4.445 90) (layer F.SilkS))
    (fp_text user SCL (at -1.905 4.445 90) (layer F.SilkS))
    (fp_text user RST (at -4.445 4.445 90) (layer F.SilkS))
    (fp_text user INT (at -6.985 4.445 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -6.985 7.62) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 /INT))
    (pad 2 thru_hole circle (at -4.445 7.62) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 3 thru_hole circle (at -1.905 7.62) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 /SCL))
    (pad 4 thru_hole circle (at 0.635 7.62) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 /SDA))
    (pad 5 thru_hole circle (at 3.175 7.62) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 GND))
    (pad 6 thru_hole circle (at 5.715 7.62) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 +3V3))
  )
  (module Graphics:bsi_logo (layer B.Cu) (tedit 0)
    (at 100.076 124.714 270)
    (fp_text reference G*** (at -24.384 -0.508 270) (layer B.SilkS) hide)
    (fp_text value LOGO (at -31.496 -0.762 270) (layer B.SilkS) hide)
  )
  (gr_text "EME Integration Board\nv1.1\nCopyright 2016\n" (at 101.092 96.52 90) (layer B.SilkS))
  (gr_text 26 (at 118.618 81.788) (layer B.SilkS))
  (gr_text 25 (at 118.618 85.09) (layer B.SilkS))
  (gr_text 24 (at 118.618 88.392) (layer B.SilkS))
  (gr_text 23 (at 118.618 91.948) (layer B.SilkS))
  (gr_text 22 (at 118.618 95.504) (layer B.SilkS))
  (gr_text 21 (at 118.618 99.06) (layer B.SilkS))
  (gr_text 20 (at 118.618 102.87) (layer B.SilkS))
  (gr_text 16 (at 118.618 106.172) (layer B.SilkS))
  (gr_text 15 (at 118.618 109.728) (layer B.SilkS))
  (gr_text 14 (at 118.618 113.03) (layer B.SilkS))
  (gr_text 13 (at 118.618 116.586) (layer B.SilkS))
  (gr_text 12 (at 118.618 120.396) (layer B.SilkS))
  (gr_text G (at 118.11 141.986) (layer B.SilkS))
  (gr_text G (at 118.11 138.684) (layer B.SilkS))
  (gr_text G (at 118.11 135.128) (layer B.SilkS))
  (gr_text G (at 118.11 131.572) (layer B.SilkS))
  (gr_text G (at 118.11 128.016) (layer B.SilkS))
  (gr_text G (at 118.11 124.46) (layer B.SilkS))
  (gr_text G (at 86.36 142.24) (layer B.SilkS))
  (gr_text G (at 86.36 138.684) (layer B.SilkS))
  (gr_text G (at 86.36 135.128) (layer B.SilkS))
  (gr_text G (at 86.36 131.572) (layer B.SilkS))
  (gr_text G (at 86.36 128.016) (layer B.SilkS))
  (gr_text G (at 86.36 124.714) (layer B.SilkS))
  (gr_text 11 (at 85.598 120.396) (layer B.SilkS))
  (gr_text 9 (at 86.36 113.538) (layer B.SilkS))
  (gr_text 10 (at 85.598 116.84) (layer B.SilkS))
  (gr_text 8 (at 86.36 109.982) (layer B.SilkS))
  (gr_text 7 (at 86.36 106.68) (layer B.SilkS))
  (gr_text 6 (at 86.36 103.124) (layer B.SilkS))
  (gr_text 5 (at 86.36 99.568) (layer B.SilkS))
  (gr_text 4 (at 86.36 96.012) (layer B.SilkS))
  (gr_text 3 (at 86.36 92.71) (layer B.SilkS))
  (gr_text 2 (at 86.36 89.154) (layer B.SilkS))
  (gr_text 1 (at 86.36 85.598) (layer B.SilkS))
  (gr_text 0 (at 86.36 82.042) (layer B.SilkS))
  (gr_line (start 121.160156 126.477014) (end 121.160156 133.959374) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 102.230713 76.582849) (end 105.713074 76.582849) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 121.160156 81.58285) (end 121.160156 89.06521) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 120.308496 78.783533) (end 120.768437 79.633005) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 119.698906 78.044099) (end 120.308496 78.783533) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.170292 76.684079) (end 118.11 76.974567) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.160156 76.582849) (end 117.170292 76.684079) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 112.677795 76.582849) (end 116.160156 76.582849) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98.748352 76.582849) (end 102.230713 76.582849) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 88.301269 76.582849) (end 91.78363 76.582849) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 118.959472 77.434511) (end 119.698906 78.044099) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 118.11 76.974567) (end 118.959472 77.434511) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 109.195434 76.582849) (end 112.677795 76.582849) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 121.160156 118.994654) (end 121.160156 126.477014) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 83.692988 143.39158) (end 83.4025 142.451864) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 102.230713 146.441724) (end 98.748352 146.441724) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 87.291133 146.340491) (end 86.351426 146.05) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 121.160156 133.959374) (end 121.160156 141.441734) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 121.160156 89.06521) (end 121.160156 96.54757) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105.713074 76.582849) (end 109.195434 76.582849) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 84.762519 144.980491) (end 84.15293 144.24104) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.78363 146.441724) (end 88.301269 146.441724) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 85.501953 145.590062) (end 84.762519 144.980491) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 86.351426 146.05) (end 85.501953 145.590062) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105.713074 146.441724) (end 102.230713 146.441724) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 88.301269 146.441724) (end 87.291133 146.340491) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 84.15293 144.24104) (end 83.692988 143.39158) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 95.265991 146.441724) (end 91.78363 146.441724) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98.748352 146.441724) (end 95.265991 146.441724) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 121.160156 104.029933) (end 121.160156 111.512294) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 109.195434 146.441724) (end 105.713074 146.441724) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.160156 146.441724) (end 112.677795 146.441724) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.170292 146.340491) (end 116.160156 146.441724) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 118.959472 145.590062) (end 118.11 146.05) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 119.698906 144.980491) (end 118.959472 145.590062) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 120.308496 144.24104) (end 119.698906 144.980491) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 121.058925 142.451864) (end 120.768437 143.39158) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 112.677795 146.441724) (end 109.195434 146.441724) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 120.768437 143.39158) (end 120.308496 144.24104) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 121.160156 141.441734) (end 121.058925 142.451864) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 95.265991 76.582849) (end 98.748352 76.582849) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 83.301269 141.441734) (end 83.301269 133.959374) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 121.160156 96.54757) (end 121.160156 104.029933) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 83.4025 142.451864) (end 83.301269 141.441734) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.78363 76.582849) (end 95.265991 76.582849) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 83.301269 133.959374) (end 83.301269 126.477014) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 83.301269 126.477014) (end 83.301269 118.994654) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 83.301269 111.512294) (end 83.301269 104.029933) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 83.301269 89.06521) (end 83.301269 81.58285) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 121.160156 111.512294) (end 121.160156 118.994654) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 83.301269 118.994654) (end 83.301269 111.512294) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 83.301269 104.029933) (end 83.301269 96.54757) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 83.301269 96.54757) (end 83.301269 89.06521) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 83.301269 81.58285) (end 83.4025 80.572714) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 83.4025 80.572714) (end 83.692988 79.633005) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 84.15293 78.783533) (end 84.762519 78.044099) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 84.762519 78.044099) (end 85.501953 77.434511) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 85.501953 77.434511) (end 86.351426 76.974567) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 86.351426 76.974567) (end 87.291133 76.684079) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 83.692988 79.633005) (end 84.15293 78.783533) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 87.291133 76.684079) (end 88.301269 76.582849) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 88.301269 76.582849) (end 88.301269 76.582849) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 120.768437 79.633005) (end 121.058925 80.572714) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 121.058925 80.572714) (end 121.160156 81.58285) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 118.11 146.05) (end 117.170292 146.340491) (layer Edge.Cuts) (width 0.1))
  (zone (net 13) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 83.82 78.74) (xy 120.904 78.74) (xy 121.158 145.034) (xy 83.82 144.78)
      )
    )
  )
)
