(kicad_pcb (version 20171130) (host pcbnew "(5.1.4)-1")
  (general
    (thickness 1.6)
    (drawings 21)
    (tracks 11)
    (zones 0)
    (modules 3)
    (nets 6)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 neckHot)
  (net 2 ground)
  (net 3 middleHot)
  (net 4 bridgeHot)
  (net 5 switchHot)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net bridgeHot)
    (add_net ground)
    (add_net middleHot)
    (add_net neckHot)
    (add_net switchHot)
  )
  (module digikey-footprints:Term_Block_1x4_P5.08mm (layer F.Cu) (tedit 5D4199D7)
    (at 124.46 87.63 180)
    (descr http://www.on-shore.com/wp-content/uploads/2015/09/osttcxx2162.pdf)
    (fp_text reference J2 (at 7.93 -4.78) (layer F.SilkS) hide)
    (fp_text value Conn_01x04 (at 7.57 5.08) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 neckHot))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 3 middleHot))
    (pad 3 thru_hole circle (at 10.16 0 180) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 4 bridgeHot))
    (pad 4 thru_hole circle (at 15.24 0 180) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 5 switchHot))
  )
  (module digikey-footprints:Term_Block_1x6_P5.08mm (layer F.Cu) (tedit 5D419A03)
    (at 98.025001 79.005001)
    (descr http://www.on-shore.com/wp-content/uploads/2015/09/osttcxx2162.pdf)
    (fp_text reference J1 (at 13.36 -4.81) (layer F.SilkS) hide)
    (fp_text value Conn_01x06 (at 12.94 5.08) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 4 bridgeHot))
    (pad 2 thru_hole circle (at 5.08 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 2 ground))
    (pad 3 thru_hole circle (at 10.16 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 3 middleHot))
    (pad 4 thru_hole circle (at 15.24 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 2 ground))
    (pad 5 thru_hole circle (at 20.32 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 neckHot))
    (pad 6 thru_hole circle (at 25.4 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 2 ground))
  )
  (module digikey-footprints:Term_Block_1x2_P5.08MM (layer F.Cu) (tedit 5D4199A2)
    (at 102.87 87.63 180)
    (descr http://www.on-shore.com/wp-content/uploads/2015/09/osttcxx2162.pdf)
    (fp_text reference J3 (at 2.794 -4.826) (layer F.SilkS) hide)
    (fp_text value Conn_01x02 (at 2.032 5.09) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask)
      (net 5 switchHot))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 2.3 2.3) (drill 1.3) (layers *.Cu *.Mask)
      (net 2 ground))
  )
  (gr_arc (start 125.73 73.66) (end 128.27 73.66) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 125.73 92.71) (end 125.73 95.25) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 95.25 92.71) (end 92.71 92.71) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 95.25 73.66) (end 95.25 71.12) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 92.71 92.71) (end 92.71 73.66) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 125.73 95.25) (end 95.25 95.25) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 128.27 73.66) (end 128.27 92.71) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 95.25 71.12) (end 125.73 71.12) (layer Edge.Cuts) (width 0.05))
  (gr_text OG (at 97.79 92.71 180) (layer F.SilkS))
  (gr_text OH (at 102.87 92.71 180) (layer F.SilkS))
  (gr_text SH (at 109.22 92.71 180) (layer F.SilkS))
  (gr_text BS (at 114.3 92.71 180) (layer F.SilkS))
  (gr_text MS (at 119.38 92.71 180) (layer F.SilkS))
  (gr_text NS (at 124.46 92.71 180) (layer F.SilkS))
  (gr_text NG (at 123.19 73.66) (layer F.SilkS))
  (gr_text NH (at 118.11 73.66) (layer F.SilkS))
  (gr_text MG (at 113.03 73.66) (layer F.SilkS))
  (gr_text MH (at 107.95 73.66) (layer F.SilkS))
  (gr_text BG (at 102.87 73.66) (layer F.SilkS))
  (gr_text BH (at 97.79 73.66) (layer F.SilkS))
  (gr_text "5 way pickup selector\nstoddenguitars.com" (at 110.49 83.185) (layer B.SilkS))
  (zone (net 2) (net_name ground) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 93.98 73.66) (xy 128.27 73.66) (xy 128.27 92.71) (xy 93.98 92.71)
      )
    )
  )
)
