(kicad_pcb (version 20171130) (host pcbnew "(5.1.9)-1")
  (general
    (thickness 1.6)
    (drawings 67)
    (tracks 64)
    (zones 0)
    (modules 3)
    (nets 40)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user hide)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (trace_clearance 0.2032)
    (zone_clearance 0)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.2 1.45)
    (pad_drill 1.2)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 127.508 84.455)
    (grid_origin 127.508 84.455)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin true)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "build/gerbers/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 ACC)
  (net 3 MIC_GND)
  (net 4 "Net-(J1-Pad36)")
  (net 5 "Net-(J1-Pad35)")
  (net 6 "Net-(J1-Pad34)")
  (net 7 IGNITION)
  (net 8 REVERSE)
  (net 9 "Net-(J1-Pad31)")
  (net 10 "Net-(J1-Pad30)")
  (net 11 "Net-(J1-Pad29)")
  (net 12 "Net-(J1-Pad28)")
  (net 13 "Net-(J1-Pad27)")
  (net 14 "Net-(J1-Pad26)")
  (net 15 "Net-(J1-Pad25)")
  (net 16 CAN_L)
  (net 17 "Net-(J1-Pad23)")
  (net 18 "Net-(J1-Pad22)")
  (net 19 "Net-(J1-Pad21)")
  (net 20 BATTERY)
  (net 21 "Net-(J1-Pad19)")
  (net 22 MIC_VCC)
  (net 23 MIC_SIG)
  (net 24 "Net-(J1-Pad16)")
  (net 25 "Net-(J1-Pad15)")
  (net 26 "Net-(J1-Pad14)")
  (net 27 PARK_BRAKE)
  (net 28 SPEED)
  (net 29 "Net-(J1-Pad11)")
  (net 30 "Net-(J1-Pad10)")
  (net 31 "Net-(J1-Pad9)")
  (net 32 "Net-(J1-Pad8)")
  (net 33 "Net-(J1-Pad7)")
  (net 34 "Net-(J1-Pad6)")
  (net 35 CAN_H)
  (net 36 "Net-(J1-Pad4)")
  (net 37 "Net-(J1-Pad3)")
  (net 38 "Net-(J1-Pad2)")
  (net 39 "Net-(J1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2032)
    (trace_width 0.254)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net ACC)
    (add_net BATTERY)
    (add_net CAN_H)
    (add_net CAN_L)
    (add_net GND)
    (add_net IGNITION)
    (add_net MIC_GND)
    (add_net MIC_SIG)
    (add_net MIC_VCC)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad11)")
    (add_net "Net-(J1-Pad14)")
    (add_net "Net-(J1-Pad15)")
    (add_net "Net-(J1-Pad16)")
    (add_net "Net-(J1-Pad19)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad21)")
    (add_net "Net-(J1-Pad22)")
    (add_net "Net-(J1-Pad23)")
    (add_net "Net-(J1-Pad25)")
    (add_net "Net-(J1-Pad26)")
    (add_net "Net-(J1-Pad27)")
    (add_net "Net-(J1-Pad28)")
    (add_net "Net-(J1-Pad29)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad30)")
    (add_net "Net-(J1-Pad31)")
    (add_net "Net-(J1-Pad34)")
    (add_net "Net-(J1-Pad35)")
    (add_net "Net-(J1-Pad36)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J1-Pad9)")
    (add_net PARK_BRAKE)
    (add_net REVERSE)
    (add_net SPEED)
  )
  (module 1318384-2:TE_1318384-2 (layer F.Cu) (tedit 60E9174F)
    (at 152.4635 64.262)
    (clearance 0.254)
    (fp_text reference J1 (at -23.622 0) (layer F.SilkS))
    (fp_text value "2009 Harness Connector" (at -7.5565 -14.9225) (layer F.Fab))
    (fp_text user PCB~EDGE (at -0.0635 -22.1615) (layer F.Fab))
    (pad 1 thru_hole oval (at -20.8788 1.4986 90) (size 2.2 1.45) (drill 1.2) (layers *.Cu *.Mask)
      (net 39 "Net-(J1-Pad1)"))
    (pad 2 thru_hole oval (at -18.6788 1.4986 90) (size 2.2 1.45) (drill 1.2) (layers *.Cu *.Mask)
      (net 38 "Net-(J1-Pad2)"))
    (pad 3 thru_hole oval (at -16.4788 1.4986 90) (size 2.2 1.45) (drill 1.2) (layers *.Cu *.Mask)
      (net 37 "Net-(J1-Pad3)"))
    (pad 4 thru_hole oval (at -14.2788 1.4986 90) (size 2.2 1.45) (drill 1.2) (layers *.Cu *.Mask)
      (net 36 "Net-(J1-Pad4)"))
    (pad 5 thru_hole oval (at -12.0788 1.4986 90) (size 2.2 1.45) (drill 1.2) (layers *.Cu *.Mask)
      (net 35 CAN_H))
    (pad 6 thru_hole oval (at -9.8788 1.4986 90) (size 2.2 1.45) (drill 1.2) (layers *.Cu *.Mask)
      (net 34 "Net-(J1-Pad6)"))
    (pad 7 thru_hole oval (at -7.6788 1.4986 90) (size 2.2 1.45) (drill 1.2) (layers *.Cu *.Mask)
      (net 33 "Net-(J1-Pad7)"))
    (pad 8 thru_hole oval (at -5.4788 1.4986 90) (size 2.2 1.45) (drill 1.2) (layers *.Cu *.Mask)
      (net 32 "Net-(J1-Pad8)"))
    (pad 9 thru_hole oval (at -3.2788 1.4986 90) (size 2.2 1.45) (drill 1.2) (layers *.Cu *.Mask)
      (net 31 "Net-(J1-Pad9)"))
    (pad 10 thru_hole oval (at -1.0788 1.4986 90) (size 2.2 1.45) (drill 1.2) (layers *.Cu *.Mask)
      (net 30 "Net-(J1-Pad10)"))
    (pad 11 thru_hole oval (at 1.1212 1.4986 90) (size 2.2 1.45) (drill 1.2) (layers *.Cu *.Mask)
      (net 29 "Net-(J1-Pad11)"))
    (pad 12 thru_hole oval (at 3.3212 1.4986 90) (size 2.2 1.45) (drill 1.2) (layers *.Cu *.Mask)
      (net 28 SPEED))
    (pad 13 thru_hole oval (at 5.5212 1.4986 90) (size 2.2 1.45) (drill 1.2) (layers *.Cu *.Mask)
      (net 27 PARK_BRAKE))
    (pad 14 thru_hole oval (at 7.7212 1.4986 90) (size 2.2 1.45) (drill 1.2) (layers *.Cu *.Mask)
      (net 26 "Net-(J1-Pad14)"))
    (pad 15 thru_hole oval (at 9.9212 1.4986 90) (size 2.2 1.45) (drill 1.2) (layers *.Cu *.Mask)
      (net 25 "Net-(J1-Pad15)"))
    (pad 16 thru_hole oval (at 12.1212 1.4986 90) (size 2.2 1.45) (drill 1.2) (layers *.Cu *.Mask)
      (net 24 "Net-(J1-Pad16)"))
    (pad 17 thru_hole oval (at 14.3212 1.4986 90) (size 2.2 1.45) (drill 1.2) (layers *.Cu *.Mask)
      (net 23 MIC_SIG))
    (pad 18 thru_hole oval (at 16.5212 1.4986 90) (size 2.2 1.45) (drill 1.2) (layers *.Cu *.Mask)
      (net 22 MIC_VCC))
    (pad 19 thru_hole oval (at 18.7212 1.4986 90) (size 2.2 1.45) (drill 1.2) (layers *.Cu *.Mask)
      (net 21 "Net-(J1-Pad19)"))
    (pad 20 thru_hole oval (at 20.9212 1.4986 90) (size 2.2 1.45) (drill 1.2) (layers *.Cu *.Mask)
      (net 20 BATTERY))
    (pad 21 thru_hole oval (at -20.8788 -1.5014 90) (size 2.2 1.45) (drill 1.2) (layers *.Cu *.Mask)
      (net 19 "Net-(J1-Pad21)"))
    (pad 22 thru_hole oval (at -18.6788 -1.5014 90) (size 2.2 1.45) (drill 1.2) (layers *.Cu *.Mask)
      (net 18 "Net-(J1-Pad22)"))
    (pad 23 thru_hole oval (at -16.4788 -1.5014 90) (size 2.2 1.45) (drill 1.2) (layers *.Cu *.Mask)
      (net 17 "Net-(J1-Pad23)"))
    (pad 24 thru_hole oval (at -14.2788 -1.5014 90) (size 2.2 1.45) (drill 1.2) (layers *.Cu *.Mask)
      (net 16 CAN_L))
    (pad 25 thru_hole oval (at -12.0788 -1.5014 90) (size 2.2 1.45) (drill 1.2) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad25)"))
    (pad 26 thru_hole oval (at -9.8788 -1.5014 90) (size 2.2 1.45) (drill 1.2) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-Pad26)"))
    (pad 27 thru_hole oval (at -7.6788 -1.5014 90) (size 2.2 1.45) (drill 1.2) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-Pad27)"))
    (pad 28 thru_hole oval (at -5.4788 -1.5014 90) (size 2.2 1.45) (drill 1.2) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad28)"))
    (pad 29 thru_hole oval (at -3.2788 -1.5014 90) (size 2.2 1.45) (drill 1.2) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad29)"))
    (pad 30 thru_hole oval (at -1.0788 -1.5014 90) (size 2.2 1.45) (drill 1.2) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad30)"))
    (pad 31 thru_hole oval (at 1.1212 -1.5014 90) (size 2.2 1.45) (drill 1.2) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad31)"))
    (pad 32 thru_hole oval (at 3.3212 -1.5014 90) (size 2.2 1.45) (drill 1.2) (layers *.Cu *.Mask)
      (net 8 REVERSE))
    (pad 33 thru_hole oval (at 5.5212 -1.5014 90) (size 2.2 1.45) (drill 1.2) (layers *.Cu *.Mask)
      (net 7 IGNITION))
    (pad 34 thru_hole oval (at 7.7212 -1.5014 90) (size 2.2 1.45) (drill 1.2) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad34)"))
    (pad 35 thru_hole oval (at 9.9212 -1.5014 90) (size 2.2 1.45) (drill 1.2) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad35)"))
    (pad 36 thru_hole oval (at 12.1212 -1.5014 90) (size 2.2 1.45) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad36)"))
    (pad 37 thru_hole oval (at 14.3212 -1.5014 90) (size 2.2 1.45) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 MIC_GND))
    (pad 38 thru_hole oval (at 16.5212 -1.5014 90) (size 2.2 1.45) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 ACC))
    (pad 39 thru_hole oval (at 18.7212 -1.5014 90) (size 2.2 1.45) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 40 thru_hole oval (at 20.9212 -1.5014 90) (size 2.2 1.45) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad "" np_thru_hole circle (at -20.1788 -7.1014 90) (size 3.500001 3.500001) (drill 3.500001) (layers *.Cu *.Mask)
      (clearance 1.905))
    (pad "" np_thru_hole circle (at 20.2212 -7.1014 90) (size 3.500001 3.500001) (drill 3.500001) (layers *.Cu *.Mask)
      (clearance 1.905))
    (model C:/Users/Ryan/Documents/KiCAD/CustomLibs/3D_CAD/te_connectivity/1318384-2.step
      (offset (xyz 0 22.6568 7.8486))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -180))
    )
  )
  (module _my_molex:Molex_Micro-Fit_3.0_43045-1221_2x06-1MP_DualMount_P3.00mm_Horizontal (layer B.Cu) (tedit 60E9117C)
    (at 150.9395 75.438)
    (descr "Molex Micro-Fit 3.0 Connector System, 43045-1221 (alternative finishes: 43045-122x), 6 Pins per row (https://www.molex.com/pdm_docs/sd/430450221_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex Micro-Fit_3.0 horizontal")
    (fp_text reference J2 (at -4.699 -0.5715) (layer B.SilkS))
    (fp_text value "eZ Universal" (at 7.5 -5.7) (layer B.Fab))
    (fp_text user %R (at 7.5 8.22) (layer B.Fab))
    (fp_text user "CU KEEPOUT" (at 18.1 1.46) (layer Cmts.User))
    (fp_text user "CU KEEPOUT" (at -3.1 1.46) (layer Cmts.User))
    (pad "" np_thru_hole circle (at 12.841 4.318) (size 2.9972 2.9972) (drill 2.9972) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 2.159 4.318) (size 2.9972 2.9972) (drill 2.9972) (layers *.Cu *.Mask))
    (pad 12 thru_hole circle (at 15 -3) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask)
      (net 8 REVERSE))
    (pad 11 thru_hole circle (at 12 -3) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask)
      (net 20 BATTERY))
    (pad 10 thru_hole circle (at 9 -3) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask)
      (net 28 SPEED))
    (pad 9 thru_hole circle (at 6 -3) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask)
      (net 16 CAN_L))
    (pad 8 thru_hole circle (at 3 -3) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask)
      (net 1 GND) (clearance 0.254))
    (pad 7 thru_hole circle (at 0 -3) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask)
      (net 2 ACC))
    (pad 6 thru_hole circle (at 15 0) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask)
      (net 22 MIC_VCC))
    (pad 5 thru_hole circle (at 12 0) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask)
      (net 27 PARK_BRAKE))
    (pad 4 thru_hole circle (at 9 0) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask)
      (net 23 MIC_SIG))
    (pad 3 thru_hole circle (at 6 0) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask)
      (net 35 CAN_H))
    (pad 2 thru_hole circle (at 3 0) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask)
      (net 3 MIC_GND))
    (pad 1 thru_hole roundrect (at 0 0) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask) (roundrect_rratio 0.1666666666666667)
      (net 7 IGNITION))
    (pad MP thru_hole circle (at 17.15 4.32) (size 3.41 3.41) (drill 2.41) (layers *.Cu *.Mask))
    (pad MP thru_hole circle (at -2.15 4.32) (size 3.41 3.41) (drill 2.41) (layers *.Cu *.Mask))
    (model C:/Users/Ryan/Documents/KiCAD/CustomLibs/3D_CAD/molex/430451221.stp
      (offset (xyz 7.493 3.9624 3.937))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 180))
    )
    (model C:/Users/Ryan/Documents/KiCAD/CustomLibs/3D_CAD/molex/430451200.stp
      (offset (xyz 7.493 3.9624 3.937))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 180))
    )
  )
  (module Connector_BarrelJack:BarrelJack_Wuerth_6941xx301002 locked (layer F.Cu) (tedit 5B191DE1)
    (at 183.9976 57.0484 180)
    (descr "Wuerth electronics barrel jack connector (5.5mm outher diameter, inner diameter 2.05mm or 2.55mm depending on exact order number), See: http://katalog.we-online.de/em/datasheet/6941xx301002.pdf")
    (tags "connector barrel jack")
    (fp_text reference J3 (at 0 -2.5) (layer F.SilkS))
    (fp_text value Power (at 0 15.5) (layer F.Fab))
    (fp_text user %R (at 0 7.5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 4.4 1.8) (drill oval 3.4 0.8) (layers *.Cu *.Mask)
      (net 2 ACC))
    (pad 2 thru_hole oval (at 0 5.8 180) (size 4 1.8) (drill oval 3 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 4.8 3 270) (size 4 1.8) (drill oval 3 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model C:/Users/Ryan/Documents/KiCAD/CustomLibs/3D_CAD/RAPC722X--3DModel-STEP-1.STEP
      (offset (xyz 0 -13.7414 6.477))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (gr_text "eZ Universal v2" (at 158.496 70.612) (layer B.SilkS))
  (gr_text M85 (at 176.8475 64.262) (layer F.SilkS))
  (gr_text Mic_Vcc (at 167.767 58.293 90) (layer B.SilkS))
  (gr_text Reverse (at 155.702 58.293 90) (layer B.SilkS))
  (gr_text "Park Brake" (at 156.845 57.023 90) (layer B.SilkS))
  (gr_text GND (at 174.879 62.738 90) (layer B.SilkS))
  (gr_text Battery (at 173.482 67.437 90) (layer B.SilkS))
  (gr_text Mic_Sig (at 165.608 61.341 90) (layer B.SilkS))
  (gr_text Speed (at 154.686 61.214 90) (layer B.SilkS))
  (gr_text MIC_GND (at 166.8145 59.69 90) (layer B.SilkS))
  (gr_text Ignition (at 157.988 59.817 90) (layer B.SilkS))
  (gr_text ACC (at 168.9735 60.579 90) (layer B.SilkS))
  (gr_text CAN-L (at 138.176 60.071 90) (layer B.SilkS))
  (gr_text CAN-H (at 139.319 58.674 90) (layer B.SilkS))
  (gr_text "Park Brake" (at 164.465 71.3105 90) (layer F.SilkS))
  (gr_text Mic_Vcc (at 167.513 71.3105 90) (layer F.SilkS))
  (gr_text Reverse (at 165.9255 71.3105 90) (layer F.SilkS))
  (gr_text Battery (at 162.941 71.3105 90) (layer F.SilkS))
  (gr_text Mic_Sig (at 161.4805 68.3895 90) (layer F.SilkS))
  (gr_text Speed (at 159.9565 68.961 90) (layer F.SilkS))
  (gr_text MIC_GND (at 155.448 69.596 90) (layer F.SilkS))
  (gr_text CAN-H (at 158.496 68.58 90) (layer F.SilkS))
  (gr_text CAN-L (at 156.9085 69.977 90) (layer F.SilkS))
  (gr_text GND (at 153.924 70.485 90) (layer F.SilkS))
  (gr_text ACC (at 150.9395 70.485 90) (layer F.SilkS))
  (gr_text Ignition (at 152.4635 69.85 90) (layer F.SilkS))
  (gr_text - (at 184.8485 64.262) (layer F.SilkS))
  (gr_text + (at 181.8005 64.262) (layer F.SilkS))
  (gr_text "External Test PWR\n12VDC" (at 183.1975 61.976) (layer F.SilkS))
  (gr_text "DISCLAIMER: This is custom harwdare.\n*USE THIS COMPONENT AT YOUR OWN RISK*" (at 153.543 49.7205) (layer B.SilkS))
  (gr_text "HW v1.0a" (at 180.92166 73.42632 45) (layer B.Cu))
  (gr_text "2009 Nissan 370Z (US)\neZ Navi-Delete Adapter" (at 180.594 72.771 46) (layer F.SilkS))
  (gr_line (start 171.3865 84.455) (end 189.0268 66.9036) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 144.78 84.455) (end 171.3865 84.455) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 127.508 66.9036) (end 144.78 84.455) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 128.778 47.625) (end 128.778 46.355) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 187.7568 47.625) (end 189.0268 47.625) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 127.508 66.9036) (end 127.508 47.625) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 189.0268 47.625) (end 189.0268 66.9036) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 128.778 46.355) (end 187.7568 46.355) (layer Edge.Cuts) (width 0.05))
  (zone (net 2) (net_name ACC) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.127)
    (fill yes (arc_segments 32) (thermal_gap 0.2032) (thermal_bridge_width 0.508) (smoothing chamfer) (radius 0.381))
    (polygon
      (pts
        (xy 169.672 59.2963) (xy 169.672 63.437294) (xy 168.3004 63.435707) (xy 168.3004 60.9219) (xy 166.8018 59.3725)
        (xy 150.4061 59.3725) (xy 150.4061 71.6788) (xy 151.4729 71.6788) (xy 151.4729 73.1901) (xy 147.2057 73.1901)
        (xy 143.5608 68.834) (xy 143.5608 60.8076) (xy 147.5994 56.8452) (xy 168.0718 56.8452)
      )
    )
  )
  (zone (net 7) (net_name IGNITION) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0))
    (min_thickness 0.127)
    (fill yes (arc_segments 32) (thermal_gap 0.2032) (thermal_bridge_width 0.635) (smoothing chamfer) (radius 0.381))
    (polygon
      (pts
        (xy 158.6992 63.42634) (xy 157.2768 63.42634) (xy 157.2768 60.2615) (xy 148.209 60.2615) (xy 148.209 74.4855)
        (xy 151.63673 74.4855) (xy 151.63927 76.073) (xy 143.57096 76.073) (xy 143.5608 57.404) (xy 158.6992 57.404)
      )
    )
  )
  (zone (net 3) (net_name MIC_GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.127)
    (fill yes (arc_segments 32) (thermal_gap 0.2032) (thermal_bridge_width 0.508) (smoothing chamfer) (radius 0.889))
    (polygon
      (pts
        (xy 155.7274 61.1505) (xy 154.813 61.1505) (xy 154.813 68.453) (xy 152.3619 68.453) (xy 152.3619 59.7535)
        (xy 155.7274 59.7535)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.381))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.635) (smoothing chamfer) (radius 0.381))
    (polygon
      (pts
        (xy 189.0395 84.455) (xy 127.508 84.455) (xy 127.508 46.355) (xy 189.0395 46.355)
      )
    )
  )
  (zone (net 8) (net_name REVERSE) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0))
    (min_thickness 0.127)
    (fill yes (arc_segments 32) (thermal_gap 0.2032) (thermal_bridge_width 1.524) (smoothing chamfer) (radius 0.254))
    (polygon
      (pts
        (xy 156.4894 64.0588) (xy 159.2072 64.0588) (xy 159.2072 68.72478) (xy 154.559 68.72478) (xy 154.559 64.0588)
        (xy 155.0924 64.0588) (xy 155.0924 62.1665) (xy 156.4894 62.177613)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.2032) (thermal_bridge_width 0.635))
    (polygon
      (pts
        (xy 154.46756 68.96862) (xy 165.6588 68.97878) (xy 165.6588 69.85) (xy 152.07234 69.85) (xy 152.077104 75.438)
        (xy 151.706899 75.438) (xy 151.702135 73.49744) (xy 148.30552 73.49744) (xy 148.30552 61.341) (xy 154.46756 61.341)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.2032) (thermal_bridge_width 0.635))
    (polygon
      (pts
        (xy 169.926 64.389) (xy 173.4185 64.389) (xy 173.4185 68.0085) (xy 159.2072 68.00215) (xy 159.2072 63.11265)
        (xy 169.926 63.119)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.2032) (thermal_bridge_width 0.635) (smoothing chamfer) (radius 0.381))
    (polygon
      (pts
        (xy 174.7012 64.3636) (xy 169.926 64.3636) (xy 169.926 61.0616) (xy 174.7012 61.0616)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.2032) (thermal_bridge_width 0.635) (smoothing chamfer) (radius 0.381))
    (polygon
      (pts
        (xy 177.3936 64.3636) (xy 170.7896 64.3636) (xy 170.7896 61.0616) (xy 177.3936 61.0616)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.2032) (thermal_bridge_width 0.635))
    (polygon
      (pts
        (xy 143.256 67.183) (xy 130.429 67.183) (xy 130.429 61.4045) (xy 143.1925 61.4045)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 149.0599 77.6986) (xy 146.6088 77.6986) (xy 146.6088 76.0984) (xy 149.0599 76.0984)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 170.2562 77.6986) (xy 167.8051 77.6986) (xy 167.8051 76.0984) (xy 170.2562 76.0984)
      )
    )
  )
)
