<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.3.0">
<drawing>
<board>
<plain>
<wire x1="35.56" y1="44.45" x2="35.56" y2="57.15" width="0" layer="20"/>
<wire x1="35.56" y1="57.15" x2="36.83" y2="58.42" width="0" layer="20" curve="-90"/>
<wire x1="36.83" y1="58.42" x2="41.91" y2="58.42" width="0" layer="20"/>
<wire x1="41.91" y1="58.42" x2="43.18" y2="57.15" width="0" layer="20" curve="-90"/>
<wire x1="43.18" y1="57.15" x2="43.18" y2="44.45" width="0" layer="20"/>
<wire x1="43.18" y1="44.45" x2="41.91" y2="43.18" width="0" layer="20" curve="-90"/>
<wire x1="41.91" y1="43.18" x2="36.83" y2="43.18" width="0" layer="20"/>
<wire x1="36.83" y1="43.18" x2="35.56" y2="44.45" width="0" layer="20" curve="-90"/>
<text>gnd</text>
<text>vcc</text>
<text>d4</text>
<text>d3</text>
<text>d2</text>
<text>d1</text>
<text>nodemcu_
i2c_qwiic</text>
<text>d3 d4 vcc gnd</text>
<text>d1 d2 vcc gnd</text>
<text>i2c</text>
<text>nodemcu_i2c_qwiic</text>
<text>gnd</text>
<text>vcc</text>
<text>d4</text>
<text>d3</text>
<text>d2</text>
<text>d1</text>
<text>d1 d2 + 0</text>
<text>d1 d2 vcc gnd</text>
<text>d1 d2 + 0</text>
<text>d3 d4 + 0</text>
<text>nodemcu_
i2c_qwiic</text>
<text>d1</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X06_NO_SILK">
<description>&lt;h3&gt;Plated Through Hole - 6 Pin No Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="0-GBR">
<packages>
<package name="1X04_1MM_RA">
<description>&lt;h3&gt;SMD- 4 Pin Right Angle &lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X04-1MM-G">
<description>gbr-sparkfun 6 pin modified to drop down to 4 pins by deleting last 2 and shifting everything in 1mm
&lt;h3&gt;JST SH Vertical  6-Pin Connector -SMD&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:1mm&lt;/li&gt;
&lt;p&gt;&lt;b&gt;&lt;a href="https://www.sparkfun.com/datasheets/GPS/EM406-SMDConnector-eSH.pdf"&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;li&gt;EM-406&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="SparkFun-Connectors" package="1X06_NO_SILK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J4" library="0-GBR" package="1X04_1MM_RA" value="JST-SH-4S">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J5" library="0-GBR" package="1X04_1MM_RA" value="JST-SH-4S">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="0-GBR" package="1X04-1MM-G" value="JST-SH-4">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="0-GBR" package="1X04-1MM-G" value="JST-SH-4">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="D1">
<contactref element="J1" pad="6"/>
<contactref element="J5" pad="4"/>
<contactref element="J2" pad="4"/>
</signal>
<signal name="D2">
<contactref element="J1" pad="5"/>
<contactref element="J5" pad="3"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="D3">
<contactref element="J1" pad="4"/>
<contactref element="J4" pad="4"/>
<contactref element="J3" pad="4"/>
</signal>
<signal name="D4">
<contactref element="J1" pad="3"/>
<contactref element="J4" pad="3"/>
<contactref element="J3" pad="3"/>
</signal>
<signal name="3V3@1">
<contactref element="J1" pad="2"/>
<contactref element="J5" pad="2"/>
<contactref element="J4" pad="2"/>
<contactref element="J3" pad="2"/>
</signal>
<signal name="GND">
<contactref element="J1" pad="1"/>
<contactref element="J5" pad="1"/>
<contactref element="J4" pad="1"/>
<contactref element="J3" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
