(kicad_pcb (version 4) (host pcbnew 4.0.7-e2-6376~58~ubuntu16.04.1)
  (general
    (links 34)
    (no_connects 0)
    (area 88.824999 111.430999 114.375001 129.107001)
    (thickness 1.6)
    (drawings 15)
    (tracks 105)
    (zones 0)
    (modules 17)
    (nets 14)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.5)
    (user_trace_width 0.75)
    (user_trace_width 1)
    (user_trace_width 2)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VDD)
  (net 2 "Net-(D4-Pad1)")
  (net 3 GND)
  (net 4 VBAT)
  (net 5 "Net-(Q1-Pad1)")
  (net 6 "Net-(D1-Pad1)")
  (net 7 /loadsharing/VSHARED)
  (net 8 /loadsharing/HALF_VDD)
  (net 9 /loadsharing/HALF_VBAT)
  (net 10 "Net-(R5-Pad2)")
  (net 11 "Net-(R6-Pad2)")
  (net 12 "Net-(U2-Pad6)")
  (net 13 "Net-(U2-Pad5)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /loadsharing/HALF_VBAT)
    (add_net /loadsharing/HALF_VDD)
    (add_net /loadsharing/VSHARED)
    (add_net GND)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(R6-Pad2)")
    (add_net "Net-(U2-Pad5)")
    (add_net "Net-(U2-Pad6)")
    (add_net VBAT)
    (add_net VDD)
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57FE93A5)
    (at 92.202 113.03 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D4 (at -0.254 -1.5494 180) (layer F.SilkS))
    (fp_text value LED (at 2.413 -0.1778 450) (layer F.Fab))
    (pad 2 smd rect (at 0.8 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 1 smd rect (at -0.8 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(D4-Pad1)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 90.932 119.888 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J1 (at 0.762 4.572 360) (layer F.SilkS))
    (fp_text value SolarPanel (at -1.3462 7.5946 450) (layer F.Fab))
    (fp_text user %R (at 0 1.27 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 VDD))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5A1BBD33)
    (at 111.8362 119.5832 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J2 (at 0.0762 5.0292 180) (layer F.SilkS))
    (fp_text value "LiFePo4 Battery" (at -3.048 5.334 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 1.27 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 VBAT))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 5A1BBF15)
    (at 101.4382 123.5608 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 2.4798 0.5232 270) (layer F.SilkS))
    (fp_text value DMP1045U7 (at -1.3048 2.5 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D1-Pad1)"))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 /loadsharing/VSHARED))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 91.694 125.718 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at -0.496 1.524 450) (layer F.SilkS))
    (fp_text value 100K (at -0.4438 1.7018 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 /loadsharing/HALF_VDD))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 92.19 128.016)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at -2.02 -0.254 90) (layer F.SilkS))
    (fp_text value 100K (at 0.5722 1.5494) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 /loadsharing/HALF_VDD))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 110.49 126.3008 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 0 -1.45 270) (layer F.SilkS))
    (fp_text value 100K (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 VBAT))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 /loadsharing/HALF_VBAT))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 103.39 127.762 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 0.266 1.524 360) (layer F.SilkS))
    (fp_text value 100K (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 /loadsharing/HALF_VBAT))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 95.516 113.03)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at -0.647 1.5494) (layer F.SilkS))
    (fp_text value 1K (at 2.0962 0.1524 90) (layer F.Fab))
    (fp_text user %R (at 1.5882 0.0508 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(D4-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(R5-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 106.16 112.776 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at 2.02 0 270) (layer F.SilkS))
    (fp_text value 1.15K (at -4.4824 0.0508 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(R6-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-5 (layer F.Cu) (tedit 58CE4E7E)
    (at 106.8402 126.3548)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U1 (at -0.338 -2.352) (layer F.SilkS))
    (fp_text value TS391ILT (at 0.0938 3.6932) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 9 /loadsharing/HALF_VBAT))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 8 /loadsharing/HALF_VDD))
    (pad 5 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 4 VBAT))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module dics-exotic-footprints:DFN10-3x3x0.9-MF (layer F.Cu) (tedit 5A1BAA89)
    (at 101.108 115.544)
    (fp_text reference U2 (at 0.762 4.826) (layer F.SilkS))
    (fp_text value MCP73x23 (at 0.746 -1.778) (layer F.Fab))
    (pad 10 smd rect (at 0 0) (size 0.28 0.63) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(R6-Pad2)"))
    (pad 9 smd rect (at 0.5 0) (size 0.28 0.63) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 8 smd rect (at 1 0) (size 0.28 0.63) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 7 smd rect (at 1.5 0) (size 0.28 0.63) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(R5-Pad2)"))
    (pad 6 smd rect (at 2 0) (size 0.28 0.63) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(U2-Pad6)"))
    (pad 5 smd rect (at 2 3.1) (size 0.28 0.63) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(U2-Pad5)"))
    (pad 4 smd rect (at 1.5 3.1) (size 0.28 0.63) (layers F.Cu F.Paste F.Mask)
      (net 4 VBAT))
    (pad 3 smd rect (at 1 3.1) (size 0.28 0.63) (layers F.Cu F.Paste F.Mask)
      (net 4 VBAT))
    (pad 2 smd rect (at 0.5 3.1) (size 0.28 0.63) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 1 smd rect (at 0 3.1) (size 0.28 0.63) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 11 smd rect (at 1 1.55) (size 2.46 1.53) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
  )
  (module dics-exotic-footprints:SOD-323HE (layer F.Cu) (tedit 5A1BBD1D)
    (at 106.5022 122.4788 270)
    (fp_text reference D1 (at 0.254 2.032 270) (layer F.SilkS))
    (fp_text value D_Schottky (at 0.254 -3.302 270) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0 270) (size 1.1 2) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 0 -1.9 270) (size 1.1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 4 VBAT))
  )
  (module dics-exotic-footprints:SOD-323HE (layer F.Cu) (tedit 5A1BBD25)
    (at 96.9772 123.698 90)
    (fp_text reference D2 (at 1.4732 -0.3302 180) (layer F.SilkS))
    (fp_text value D_Schottky (at 0.254 -3.302 90) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0 90) (size 1.1 2) (layers F.Cu F.Paste F.Mask)
      (net 7 /loadsharing/VSHARED))
    (pad 2 smd rect (at 0 -1.9 90) (size 1.1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
  )
  (module Capacitors_SMD:CP_Elec_4x5.7 (layer F.Cu) (tedit 58AA8612)
    (at 96.6978 118.11 90)
    (descr "SMT capacitor, aluminium electrolytic, 4x5.7")
    (attr smd)
    (fp_text reference C1 (at 3.302 2.1082 180) (layer F.SilkS))
    (fp_text value 4.7uF (at -0.0254 -3.0226 90) (layer F.Fab))
    (fp_text user + (at -1.1 -0.08 90) (layer F.Fab))
    (fp_text user + (at -2.77 2.01 90) (layer F.SilkS))
    (fp_text user %R (at 3.302 2.1082 360) (layer F.Fab))
    (pad 1 smd rect (at -1.8 0 270) (size 2.6 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.8 0 270) (size 2.6 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/CP_Elec_4x5.7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:CP_Elec_4x5.7 (layer F.Cu) (tedit 58AA8612)
    (at 107.0356 117.3734 90)
    (descr "SMT capacitor, aluminium electrolytic, 4x5.7")
    (attr smd)
    (fp_text reference C2 (at 3.1242 2.1844 180) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 -3.54 90) (layer F.Fab))
    (fp_text user + (at -1.1 -0.08 90) (layer F.Fab))
    (fp_text user + (at -2.77 2.01 90) (layer F.SilkS))
    (fp_text user %R (at 4.0894 0.4064 180) (layer F.Fab))
    (pad 1 smd rect (at -1.8 0 270) (size 2.6 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 VBAT))
    (pad 2 smd rect (at 1.8 0 270) (size 2.6 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/CP_Elec_4x5.7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 97.028 127.254 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J3 (at 2.032 0 180) (layer F.SilkS))
    (fp_text value Load (at -2.794 1.27 180) (layer F.Fab))
    (fp_text user %R (at 0 1.27 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /loadsharing/VSHARED))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text + (at 94.996 126.746) (layer B.SilkS))
  (gr_text + (at 94.234 126.238) (layer F.SilkS))
  (gr_text "+\n" (at 90.932 121.666) (layer B.SilkS))
  (gr_text + (at 111.76 121.412) (layer B.SilkS))
  (gr_text "Load\napprox 3.2V" (at 107.696 120.142 90) (layer B.SilkS))
  (gr_text "Solar 6V" (at 93.472 118.872 90) (layer B.SilkS))
  (gr_text + (at 111.76 122.174) (layer F.SilkS))
  (gr_text + (at 90.932 122.428) (layer F.SilkS))
  (gr_line (start 114.3 129.032) (end 114.3 111.506) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 88.9 111.506) (end 88.9 129.032) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 114.046 111.506) (end 114.046 111.506) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 114.3 111.506) (end 114.046 111.506) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 88.9 129.032) (end 114.3 129.032) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 114.046 111.506) (end 114.046 111.506) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 88.9 111.506) (end 114.046 111.506) (layer Edge.Cuts) (width 0.15))
  (zone (net 3) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 88.899338 111.5314) (xy 114.299338 111.5314) (xy 114.3 129.032) (xy 88.9 129.032)
      )
    )
  )
)
