(kicad_pcb (version 4) (host pcbnew 4.0.5+dfsg1-4)
  (general
    (links 55)
    (no_connects 0)
    (area 104.064999 53.264999 144.855001 109.295001)
    (thickness 1.6)
    (drawings 32)
    (tracks 69)
    (zones 0)
    (modules 6)
    (nets 28)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal hide)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user hide)
    (37 F.SilkS user hide)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.762 1.524)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerbers))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(J1-Pad1)")
  (net 3 "Net-(J1-Pad2)")
  (net 4 "Net-(J1-Pad3)")
  (net 5 "Net-(J1-Pad4)")
  (net 6 "Net-(J1-Pad5)")
  (net 7 "Net-(J1-Pad6)")
  (net 8 "Net-(J1-Pad7)")
  (net 9 "Net-(J1-Pad8)")
  (net 10 "Net-(J1-Pad9)")
  (net 11 "Net-(J1-Pad10)")
  (net 12 "Net-(J1-Pad11)")
  (net 13 "Net-(J1-Pad12)")
  (net 14 "Net-(J1-Pad13)")
  (net 15 "Net-(J2-Pad1)")
  (net 16 "Net-(J2-Pad2)")
  (net 17 "Net-(J2-Pad3)")
  (net 18 "Net-(J2-Pad4)")
  (net 19 "Net-(J2-Pad5)")
  (net 20 "Net-(J2-Pad6)")
  (net 21 "Net-(J2-Pad7)")
  (net 22 "Net-(J2-Pad8)")
  (net 23 "Net-(J2-Pad9)")
  (net 24 "Net-(J2-Pad10)")
  (net 25 "Net-(J2-Pad11)")
  (net 26 "Net-(J2-Pad12)")
  (net 27 "Net-(J2-Pad13)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad11)")
    (add_net "Net-(J1-Pad12)")
    (add_net "Net-(J1-Pad13)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J1-Pad9)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad10)")
    (add_net "Net-(J2-Pad11)")
    (add_net "Net-(J2-Pad12)")
    (add_net "Net-(J2-Pad13)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(J2-Pad6)")
    (add_net "Net-(J2-Pad7)")
    (add_net "Net-(J2-Pad8)")
    (add_net "Net-(J2-Pad9)")
  )
  (module footprintlib:microDfootprint (layer F.Cu) (tedit 595EB674)
    (at 116.84 59.69)
    (descr "Connecteur DB15 male droit")
    (tags "CONN DB15")
    (fp_text reference "" (at -12.7 -4.699) (layer F.SilkS))
    (fp_text value "" (at 6.604 -5.461) (layer F.Fab))
    (pad 14 thru_hole circle (at 0.635 -2.54) (size 0.8382 0.8382) (drill 0.7112) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0) (size 0.8382 0.8382) (drill 0.7112) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad1)"))
    (pad 2 thru_hole circle (at 1.27 0) (size 0.8382 0.8382) (drill 0.7112) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (pad 3 thru_hole circle (at 2.54 0) (size 0.8382 0.8382) (drill 0.7112) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad3)"))
    (pad 4 thru_hole circle (at 3.81 0) (size 0.8382 0.8382) (drill 0.7112) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad4)"))
    (pad 5 thru_hole circle (at 5.08 0) (size 0.8382 0.8382) (drill 0.7112) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad5)"))
    (pad 6 thru_hole circle (at 6.35 0) (size 0.8382 0.8382) (drill 0.7112) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad6)"))
    (pad 7 thru_hole circle (at 7.62 0) (size 0.8382 0.8382) (drill 0.7112) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad7)"))
    (pad 8 thru_hole circle (at 8.89 0) (size 0.8382 0.8382) (drill 0.7112) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad8)"))
    (pad 9 thru_hole circle (at 10.16 0) (size 0.8382 0.8382) (drill 0.7112) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad9)"))
    (pad 10 thru_hole circle (at 11.43 0) (size 0.8382 0.8382) (drill 0.7112) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad10)"))
    (pad 11 thru_hole circle (at 12.7 0) (size 0.8382 0.8382) (drill 0.7112) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad11)"))
    (pad 12 thru_hole circle (at 13.97 0) (size 0.8382 0.8382) (drill 0.7112) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-Pad12)"))
    (pad 13 thru_hole circle (at 15.24 0) (size 0.8382 0.8382) (drill 0.7112) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-Pad13)"))
    (pad 15 thru_hole circle (at 1.905 -2.54) (size 0.8382 0.8382) (drill 0.7112) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 16 thru_hole circle (at 3.175 -2.54) (size 0.8382 0.8382) (drill 0.7112) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 17 thru_hole circle (at 4.445 -2.54) (size 0.8382 0.8382) (drill 0.7112) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 18 thru_hole circle (at 5.715 -2.54) (size 0.8382 0.8382) (drill 0.7112) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 19 thru_hole circle (at 6.985 -2.54) (size 0.8382 0.8382) (drill 0.7112) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 20 thru_hole circle (at 8.255 -2.54) (size 0.8382 0.8382) (drill 0.7112) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 21 thru_hole circle (at 9.525 -2.54) (size 0.8382 0.8382) (drill 0.7112) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 22 thru_hole circle (at 10.795 -2.54) (size 0.8382 0.8382) (drill 0.7112) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 23 thru_hole circle (at 12.065 -2.54) (size 0.8382 0.8382) (drill 0.7112) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 24 thru_hole circle (at 13.335 -2.54) (size 0.8382 0.8382) (drill 0.7112) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 25 thru_hole circle (at 14.605 -2.54) (size 0.8382 0.8382) (drill 0.7112) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad "" thru_hole circle (at -4.6355 -3.81) (size 3.048 3.048) (drill 2.794) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad "" thru_hole circle (at 19.8755 -3.81) (size 3.048 3.048) (drill 2.794) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Connect.3dshapes/DB15MD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprintlib:microDfootprint (layer F.Cu) (tedit 595EB695)
    (at 132.08 101.6 180)
    (descr "Connecteur DB15 male droit")
    (tags "CONN DB15")
    (fp_text reference "" (at -12.7 -4.699 180) (layer F.SilkS))
    (fp_text value "" (at 6.604 -5.461 180) (layer F.Fab))
    (pad 14 thru_hole circle (at 0.635 -2.54 180) (size 0.8382 0.8382) (drill 0.7112) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 180) (size 0.8382 0.8382) (drill 0.7112) (layers *.Cu *.Mask)
      (net 15 "Net-(J2-Pad1)"))
    (pad 2 thru_hole circle (at 1.27 0 180) (size 0.8382 0.8382) (drill 0.7112) (layers *.Cu *.Mask)
      (net 16 "Net-(J2-Pad2)"))
    (pad 3 thru_hole circle (at 2.54 0 180) (size 0.8382 0.8382) (drill 0.7112) (layers *.Cu *.Mask)
      (net 17 "Net-(J2-Pad3)"))
    (pad 4 thru_hole circle (at 3.81 0 180) (size 0.8382 0.8382) (drill 0.7112) (layers *.Cu *.Mask)
      (net 18 "Net-(J2-Pad4)"))
    (pad 5 thru_hole circle (at 5.08 0 180) (size 0.8382 0.8382) (drill 0.7112) (layers *.Cu *.Mask)
      (net 19 "Net-(J2-Pad5)"))
    (pad 6 thru_hole circle (at 6.35 0 180) (size 0.8382 0.8382) (drill 0.7112) (layers *.Cu *.Mask)
      (net 20 "Net-(J2-Pad6)"))
    (pad 7 thru_hole circle (at 7.62 0 180) (size 0.8382 0.8382) (drill 0.7112) (layers *.Cu *.Mask)
      (net 21 "Net-(J2-Pad7)"))
    (pad 8 thru_hole circle (at 8.89 0 180) (size 0.8382 0.8382) (drill 0.7112) (layers *.Cu *.Mask)
      (net 22 "Net-(J2-Pad8)"))
    (pad 9 thru_hole circle (at 10.16 0 180) (size 0.8382 0.8382) (drill 0.7112) (layers *.Cu *.Mask)
      (net 23 "Net-(J2-Pad9)"))
    (pad 10 thru_hole circle (at 11.43 0 180) (size 0.8382 0.8382) (drill 0.7112) (layers *.Cu *.Mask)
      (net 24 "Net-(J2-Pad10)"))
    (pad 11 thru_hole circle (at 12.7 0 180) (size 0.8382 0.8382) (drill 0.7112) (layers *.Cu *.Mask)
      (net 25 "Net-(J2-Pad11)"))
    (pad 12 thru_hole circle (at 13.97 0 180) (size 0.8382 0.8382) (drill 0.7112) (layers *.Cu *.Mask)
      (net 26 "Net-(J2-Pad12)"))
    (pad 13 thru_hole circle (at 15.24 0 180) (size 0.8382 0.8382) (drill 0.7112) (layers *.Cu *.Mask)
      (net 27 "Net-(J2-Pad13)"))
    (pad 15 thru_hole circle (at 1.905 -2.54 180) (size 0.8382 0.8382) (drill 0.7112) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 16 thru_hole circle (at 3.175 -2.54 180) (size 0.8382 0.8382) (drill 0.7112) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 17 thru_hole circle (at 4.445 -2.54 180) (size 0.8382 0.8382) (drill 0.7112) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 18 thru_hole circle (at 5.715 -2.54 180) (size 0.8382 0.8382) (drill 0.7112) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 19 thru_hole circle (at 6.985 -2.54 180) (size 0.8382 0.8382) (drill 0.7112) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 20 thru_hole circle (at 8.255 -2.54 180) (size 0.8382 0.8382) (drill 0.7112) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 21 thru_hole circle (at 9.525 -2.54 180) (size 0.8382 0.8382) (drill 0.7112) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 22 thru_hole circle (at 10.795 -2.54 180) (size 0.8382 0.8382) (drill 0.7112) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 23 thru_hole circle (at 12.065 -2.54 180) (size 0.8382 0.8382) (drill 0.7112) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 24 thru_hole circle (at 13.335 -2.54 180) (size 0.8382 0.8382) (drill 0.7112) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 25 thru_hole circle (at 14.605 -2.54 180) (size 0.8382 0.8382) (drill 0.7112) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad "" thru_hole circle (at -4.6355 -3.81 180) (size 3.048 3.048) (drill 2.794) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad "" thru_hole circle (at 19.8755 -3.81 180) (size 3.048 3.048) (drill 2.794) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Connect.3dshapes/DB15MD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprintlib:1cm_pads (layer F.Cu) (tedit 59600532)
    (at 118.745 72.136)
    (fp_text reference "" (at 1.778 -0.508) (layer F.SilkS))
    (fp_text value "" (at -3.937 0.635 90) (layer F.Fab))
    (pad 1 smd rect (at -1.905 0.762) (size 0.762 1.524) (layers F.Cu)
      (net 2 "Net-(J1-Pad1)"))
    (pad 2 smd rect (at -0.635 0.762) (size 0.762 1.524) (layers F.Cu)
      (net 3 "Net-(J1-Pad2)"))
    (pad 3 smd rect (at 0.635 0.762) (size 0.762 1.524) (layers F.Cu)
      (net 4 "Net-(J1-Pad3)"))
    (pad 4 smd rect (at 1.905 0.762) (size 0.762 1.524) (layers F.Cu)
      (net 5 "Net-(J1-Pad4)"))
    (pad 5 smd rect (at 3.175 0.762) (size 0.762 1.524) (layers F.Cu)
      (net 6 "Net-(J1-Pad5)"))
    (pad 6 smd rect (at 4.445 0.762) (size 0.762 1.524) (layers F.Cu)
      (net 7 "Net-(J1-Pad6)"))
    (pad 7 smd rect (at 5.715 0.762) (size 0.762 1.524) (layers F.Cu)
      (net 8 "Net-(J1-Pad7)"))
    (pad 8 smd rect (at 6.985 0.762) (size 0.762 1.524) (layers F.Cu)
      (net 9 "Net-(J1-Pad8)"))
    (pad 9 smd rect (at 8.255 0.762) (size 0.762 1.524) (layers F.Cu)
      (net 10 "Net-(J1-Pad9)"))
    (pad 10 smd rect (at 9.525 0.762) (size 0.762 1.524) (layers F.Cu)
      (net 11 "Net-(J1-Pad10)"))
    (pad 11 smd rect (at 10.795 0.762) (size 0.762 1.524) (layers F.Cu)
      (net 12 "Net-(J1-Pad11)"))
    (pad 12 smd rect (at 12.065 0.762) (size 0.762 1.524) (layers F.Cu)
      (net 13 "Net-(J1-Pad12)"))
  )
  (module footprintlib:1cm_pads (layer F.Cu) (tedit 59600579)
    (at 130.175 90.297 180)
    (fp_text reference "" (at -3.302 -0.508 180) (layer F.SilkS))
    (fp_text value "" (at -3.429 -1.016 180) (layer F.Fab))
    (pad 1 smd rect (at -1.905 0.762 180) (size 0.762 1.524) (layers F.Cu)
      (net 15 "Net-(J2-Pad1)"))
    (pad 2 smd rect (at -0.635 0.762 180) (size 0.762 1.524) (layers F.Cu)
      (net 16 "Net-(J2-Pad2)"))
    (pad 3 smd rect (at 0.635 0.762 180) (size 0.762 1.524) (layers F.Cu)
      (net 17 "Net-(J2-Pad3)"))
    (pad 4 smd rect (at 1.905 0.762 180) (size 0.762 1.524) (layers F.Cu)
      (net 18 "Net-(J2-Pad4)"))
    (pad 5 smd rect (at 3.175 0.762 180) (size 0.762 1.524) (layers F.Cu)
      (net 19 "Net-(J2-Pad5)"))
    (pad 6 smd rect (at 4.445 0.762 180) (size 0.762 1.524) (layers F.Cu)
      (net 20 "Net-(J2-Pad6)"))
    (pad 7 smd rect (at 5.715 0.762 180) (size 0.762 1.524) (layers F.Cu)
      (net 21 "Net-(J2-Pad7)"))
    (pad 8 smd rect (at 6.985 0.762 180) (size 0.762 1.524) (layers F.Cu)
      (net 22 "Net-(J2-Pad8)"))
    (pad 9 smd rect (at 8.255 0.762 180) (size 0.762 1.524) (layers F.Cu)
      (net 23 "Net-(J2-Pad9)"))
    (pad 10 smd rect (at 9.525 0.762 180) (size 0.762 1.524) (layers F.Cu)
      (net 24 "Net-(J2-Pad10)"))
    (pad 11 smd rect (at 10.795 0.762 180) (size 0.762 1.524) (layers F.Cu)
      (net 25 "Net-(J2-Pad11)"))
    (pad 12 smd rect (at 12.065 0.762 180) (size 0.762 1.524) (layers F.Cu)
      (net 26 "Net-(J2-Pad12)"))
  )
  (module footprintlib:mounting_holes (layer F.Cu) (tedit 595EB6A6)
    (at 109.22 66.04)
    (zone_connect 1)
    (fp_text reference "" (at 8.001 -4.191) (layer F.SilkS))
    (fp_text value "" (at 4.191 -5.715) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 8.89 8.89) (drill 7.62) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 1))
    (pad 2 thru_hole circle (at 30.48 0) (size 8.89 8.89) (drill 7.62) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 1))
    (pad 3 thru_hole circle (at 0 30.48) (size 8.89 8.89) (drill 7.62) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 1))
    (pad 4 thru_hole circle (at 30.48 30.48) (size 8.89 8.89) (drill 7.62) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 1))
  )
  (module footprintlib:chip_area (layer F.Cu) (tedit 595EAB8A)
    (at 118.491 75.311)
    (fp_text reference "" (at -6.477 2.667) (layer F.SilkS))
    (fp_text value "" (at -5.461 0.381) (layer F.Fab))
  )
  (gr_text | (at 121.92 91.948) (layer F.SilkS))
  (gr_text | (at 127 91.948) (layer F.SilkS))
  (gr_text | (at 132.08 91.948) (layer F.SilkS))
  (gr_text | (at 126.873 70.485) (layer F.SilkS))
  (gr_text | (at 121.793 70.485) (layer F.SilkS))
  (gr_text | (at 116.713 70.485) (layer F.SilkS))
  (gr_text 9 (at 127 54.991 180) (layer F.SilkS))
  (gr_text 5 (at 121.92 54.991 180) (layer F.SilkS))
  (gr_text 1 (at 116.84 54.991 180) (layer F.SilkS))
  (gr_text 9 (at 121.92 106.68) (layer F.SilkS))
  (gr_text 5 (at 127 106.68) (layer F.SilkS))
  (gr_text 1 (at 132.334 106.807) (layer F.SilkS))
  (gr_arc (start 119.126 86.741) (end 118.999 87.376) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 118.999 75.819) (end 118.491 75.819) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 130.048 75.311) (end 129.921 75.311) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 130.048 75.819) (end 130.048 75.311) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 130.556 86.868) (end 130.556 75.819) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 130.048 86.868) (end 130.556 86.868) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 118.999 75.311) (end 129.921 75.311) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 118.491 86.741) (end 118.491 75.819) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 130.048 87.376) (end 118.872 87.376) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text PCB_Edge (at 106.553 52.451) (layer B.CrtYd))
  (gr_line (start 104.14 109.22) (end 104.14 53.34) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 144.78 109.22) (end 104.14 109.22) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 144.78 53.34) (end 144.78 109.22) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 104.14 53.34) (end 144.78 53.34) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 147.32 111.76) (xy 101.6 111.76) (xy 101.6 50.8) (xy 147.32 50.8)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 147.32 111.76) (xy 101.6 111.76) (xy 101.6 50.8) (xy 147.32 50.8)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 143.637 52.451) (xy 134.493 52.451) (xy 134.493 110.363) (xy 146.431 110.363) (xy 146.431 52.451)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.427 110.109) (xy 102.997 110.109) (xy 102.997 52.324) (xy 114.427 52.324)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 133.223 90.678) (xy 115.824 90.678) (xy 115.824 71.882) (xy 133.223 71.882)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.808 61.214) (xy 114.808 100.076) (xy 134.112 100.076) (xy 134.112 61.087) (xy 114.808 61.087)
      )
    )
  )
)
