(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 12)
    (no_connects 0)
    (area 134 83 166.0074 107.000001)
    (thickness 1.6)
    (drawings 5)
    (tracks 28)
    (zones 0)
    (modules 7)
    (nets 5)
  )
  (page USLetter)
  (title_block
    (title "Light Flicker Sensor")
    (date 2017-11-10)
    (rev 1)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (33 F.Adhes user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (47 F.CrtYd user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.5)
    (user_trace_width 0.25)
    (user_trace_width 0.5)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.05)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.254)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +BATT)
  (net 2 GND)
  (net 3 +5V)
  (net 4 "Net-(P1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net +BATT)
    (add_net GND)
    (add_net "Net-(P1-Pad1)")
  )
  (net_class Pwr ""
    (clearance 0.1524)
    (trace_width 0.5)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module Capacitors_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 597BC7C2)
    (at 145.95 93.3 90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C1 (at 2.45 0.05 180) (layer F.SilkS))
    (fp_text value "100 nF" (at 2.5 2.56 90) (layer F.Fab))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +BATT))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 597BC7C2)
    (at 158.3 91.8 270)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C2 (at 2.45 0 270) (layer F.SilkS))
    (fp_text value "100 nF" (at 2.5 2.56 270) (layer F.Fab))
    (fp_text user %R (at 2.5 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_Tantal_D5.0mm_P5.00mm (layer F.Cu) (tedit 597C781B)
    (at 154.05 95.3 180)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=5.0mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 5.0mm Tantal Electrolytic Capacitor")
    (fp_text reference C3 (at 2.5 -0.05 180) (layer F.SilkS))
    (fp_text value "10 µF" (at 2.5 3.81 180) (layer F.Fab))
    (fp_text user %R (at 2.5 0 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_Tantal_D5.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.00mm (layer F.Cu) (tedit 59650533)
    (at 155 88.75 90)
    (descr "Through hole straight pin header, 1x03, 2.00mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.00mm single row")
    (fp_text reference U1 (at -2.45 0 180) (layer F.SilkS))
    (fp_text value TSL252 (at 0 6.06 90) (layer F.Fab))
    (fp_text user %R (at 0 2 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 3 thru_hole oval (at 0 4 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(P1-Pad1)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Terminal_Blocks:TerminalBlock_bornier-2_P5.08mm (layer F.Cu) (tedit 59FF03AB)
    (at 140 95 90)
    (descr "simple 2-pin terminal block, pitch 5.08mm, revamped version of bornier2")
    (tags "terminal block bornier2")
    (fp_text reference BT1 (at 2.85 -2.55 90) (layer F.SilkS))
    (fp_text value Battery (at 2.54 5.08 90) (layer F.Fab))
    (fp_text user %R (at 2.54 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 1 +BATT))
    (pad 2 thru_hole circle (at 5.08 0 90) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Terminal_Blocks.3dshapes/TerminalBlock_bornier-2_P5.08mm.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Terminal_Blocks:TerminalBlock_bornier-2_P5.08mm (layer F.Cu) (tedit 59FF03AB)
    (at 164.9 89.95 270)
    (descr "simple 2-pin terminal block, pitch 5.08mm, revamped version of bornier2")
    (tags "terminal block bornier2")
    (fp_text reference P1 (at 2.85 -2.55 360) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 2.54 5.08 270) (layer F.Fab))
    (fp_text user %R (at 2.54 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 4 "Net-(P1-Pad1)"))
    (pad 2 thru_hole circle (at 5.08 0 270) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Terminal_Blocks.3dshapes/TerminalBlock_bornier-2_P5.08mm.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Customs:TO-92_Inline_Narrow_Flip (layer F.Cu) (tedit 5A024167)
    (at 150.55 89.3 180)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.6mm (see NXP sot054_po.pdf), flipped")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference U2 (at 0 -1.75 180) (layer F.SilkS))
    (fp_text value LM340LAZ-5.0/NOPB (at 0 2.79 180) (layer F.Fab))
    (fp_text user %R (at 0 -3.56 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 0) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 1.27 0) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 +BATT))
    (pad 3 thru_hole oval (at -1.27 0) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 3 +5V))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Narrow_Oval.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (gr_text V1 (at 146.1 96.25) (layer F.SilkS))
  (gr_line (start 135.56 98.5) (end 135.56 86.75) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 169.5 86.75) (end 169.5 98.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 135.56 86.75) (end 169.5 86.75) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 169.5 98.5) (end 135.56 98.5) (layer Edge.Cuts) (width 0.05))
  (zone (net 1) (net_name +BATT) (layer B.Cu) (hatch edge 0.508)
    (priority 5)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 138.5 92.85) (xy 143.75 92.85) (xy 147.95 88.55) (xy 148.45 88.2) (xy 149.75 88.2)
        (xy 149.75 91.15) (xy 145.1 95.8) (xy 145.1 99.2) (xy 134.85 99.2) (xy 134.85 92.85)
      )
    )
  )
  (zone (net 3) (net_name +5V) (layer B.Cu) (hatch edge 0.508)
    (priority 5)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 151.2 88.5) (xy 151.2 96.5) (xy 155.85 96.5) (xy 159.8 92.35) (xy 159.8 90.95)
        (xy 158 89.5) (xy 158 86.45) (xy 156 86.45) (xy 156 89.65) (xy 153.1 89.65)
        (xy 152.3 88.5)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 133.5 85) (xy 133.5 100) (xy 170.5 100) (xy 170.5 85)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 133.5 85) (xy 133.5 100) (xy 170.5 100) (xy 170.5 85)
      )
    )
  )
)
