(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 0)
    (no_connects 0)
    (area 127.532001 62.324 167.125001 115.899001)
    (thickness 1.6)
    (drawings 14)
    (tracks 119)
    (zones 0)
    (modules 11)
    (nets 1)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (36 B.SilkS user hide)
    (37 F.SilkS user hide)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (44 Edge.Cuts user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.25)
    (user_trace_width 0.5)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 10.75 10.75)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ../))
  )
  (net 0 "")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (net_class power ""
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module oled:OLED0.96 (layer F.Cu) (tedit 590E889B)
    (at 140.208 91.694 90)
    (descr http://www.kamami.pl/dl/wc1602a0.pdf)
    (tags "OLED Alphanumeric 4pin")
    (attr smd)
    (fp_text reference "OLED 0.96''" (at -8.636 2.032 90) (layer F.SilkS))
    (fp_text value "" (at 2.286 3.81 90) (layer F.Fab))
    (pad 1 thru_hole oval (at -3.81 0 90) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -1.27 0 90) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 1.27 0 90) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 3.81 0 90) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask))
  )
  (module Buttons_Switches_THT:SW_PUSH_6mm_h5mm (layer F.Cu) (tedit 590D4A42)
    (at 159.258 113.284 90)
    (descr "tactile push button, 6x6mm e.g. PHAP33xx series, height=5mm")
    (tags "tact sw push 6mm")
    (fp_text reference "" (at 10.16 2.54 180) (layer F.SilkS))
    (fp_text value RIGHT (at 3.1115 2.2225 180) (layer F.SilkS))
    (pad 2 thru_hole circle (at 0 4.5 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 0 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 6.5 4.5 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 6.5 0 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask))
    (model Buttons_Switches_THT.3dshapes/SW_PUSH_6mm_h5mm.wrl
      (at (xyz 0.005 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_THT:SW_PUSH_6mm_h5mm (layer F.Cu) (tedit 590D4A4B)
    (at 141.478 113.284 90)
    (descr "tactile push button, 6x6mm e.g. PHAP33xx series, height=5mm")
    (tags "tact sw push 6mm")
    (fp_text reference "" (at 10.16 2.54 90) (layer F.SilkS))
    (fp_text value LEFT (at 3.175 2.2225 180) (layer F.SilkS))
    (pad 2 thru_hole circle (at 0 4.5 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 0 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 6.5 4.5 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 6.5 0 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask))
    (model Buttons_Switches_THT.3dshapes/SW_PUSH_6mm_h5mm.wrl
      (at (xyz 0.005 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 590D4A20)
    (at 154.94 96.774)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference "" (at 3.81 -2.31) (layer F.SilkS))
    (fp_text value "10k Ω" (at 3.81 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-8_W7.62mm (layer F.Cu) (tedit 590FC8F9)
    (at 143.256 96.012)
    (descr "8-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "DIL DIP PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference "" (at 3.81 -2.39) (layer F.SilkS))
    (fp_text value "" (at 3.81 13.97 90) (layer F.Fab))
    (fp_text user ATTINY85 (at 4.064 3.81 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (model Housings_DIP.3dshapes/DIP-8_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 590D4A28)
    (at 154.94 99.822)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference "" (at 3.81 -2.31) (layer F.SilkS))
    (fp_text value "10k Ω" (at 3.81 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 590D4A2D)
    (at 162.56 103.124 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference "" (at 3.81 -2.31 180) (layer F.SilkS))
    (fp_text value "10k Ω" (at 3.81 0 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_THT:SW_PUSH_6mm_h5mm (layer F.Cu) (tedit 590D4A47)
    (at 150.368 113.284 90)
    (descr "tactile push button, 6x6mm e.g. PHAP33xx series, height=5mm")
    (tags "tact sw push 6mm")
    (fp_text reference "" (at 10.16 2.54 90) (layer F.SilkS))
    (fp_text value MID (at 3.2385 2.159 180) (layer F.SilkS))
    (pad 2 thru_hole circle (at 0 4.5 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 0 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 6.5 4.5 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 6.5 0 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask))
    (model Buttons_Switches_THT.3dshapes/SW_PUSH_6mm_h5mm.wrl
      (at (xyz 0.005 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 590F6680)
    (at 165.1 103.632 180)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference "" (at 0.635 3.937 270) (layer F.SilkS))
    (fp_text value "" (at 0 9.95 180) (layer F.Fab))
    (fp_text user "PROG pins" (at -2.54 3.937 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module oled:pockeTETRIS (layer B.Cu) (tedit 590FC525)
    (at 165.862 83.058 180)
    (fp_text reference pockeTETRIS (at 13.208 -2.54 180) (layer B.SilkS) hide)
    (fp_text value "" (at 0 0 180) (layer B.SilkS))
  )
  (module oled:BAT-HLD-001-THM-OTL (layer F.Cu) (tedit 590FC906)
    (at 152.146 82.296 180)
    (fp_text reference REF** (at 7.112 2.794 180) (layer F.SilkS))
    (fp_text value CR2032 (at -7.112 4.826 180) (layer F.Fab))
    (pad 2 smd circle (at 0 0 180) (size 10.75 10.75) (layers F.Cu F.Mask)
      (solder_mask_margin 4))
    (pad 1 thru_hole circle (at 10.4 -1.5 180) (size 2.3 2.3) (drill 1) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole circle (at 10.4 1.6 180) (size 2.3 2.3) (drill 1) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole circle (at -10.4 1.6 180) (size 2.3 2.3) (drill 1) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole circle (at -10.4 -1.5 180) (size 2.3 2.3) (drill 1) (layers *.Cu *.Mask F.SilkS))
  )
  (gr_text "Dominick Anatala" (at 152.654 109.22) (layer B.SilkS))
  (dimension 29.21 (width 0.3) (layer F.Fab)
    (gr_text "29.210 mm" (at 152.273 63.674) (layer F.Fab))
    (feature1 (pts (xy 166.878 76.454) (xy 166.878 62.324)))
    (feature2 (pts (xy 137.668 76.454) (xy 137.668 62.324)))
    (crossbar (pts (xy 137.668 65.024) (xy 166.878 65.024)))
    (arrow1a (pts (xy 166.878 65.024) (xy 165.751496 65.610421)))
    (arrow1b (pts (xy 166.878 65.024) (xy 165.751496 64.437579)))
    (arrow2a (pts (xy 137.668 65.024) (xy 138.794504 65.610421)))
    (arrow2b (pts (xy 137.668 65.024) (xy 138.794504 64.437579)))
  )
  (gr_text 13 (at 165.608 106.172 270) (layer F.SilkS))
  (gr_text 10 (at 165.1 93.345 270) (layer F.SilkS))
  (gr_text TOP (at 140.208 78.232) (layer F.SilkS))
  (gr_text BOT (at 140.208 78.232) (layer B.SilkS))
  (dimension 39.37 (width 0.3) (layer F.Fab)
    (gr_text "39.370 mm" (at 134.032 96.139 270) (layer F.Fab))
    (feature1 (pts (xy 138.176 115.824) (xy 132.682 115.824)))
    (feature2 (pts (xy 138.176 76.454) (xy 132.682 76.454)))
    (crossbar (pts (xy 135.382 76.454) (xy 135.382 115.824)))
    (arrow1a (pts (xy 135.382 115.824) (xy 134.795579 114.697496)))
    (arrow1b (pts (xy 135.382 115.824) (xy 135.968421 114.697496)))
    (arrow2a (pts (xy 135.382 76.454) (xy 134.795579 77.580504)))
    (arrow2b (pts (xy 135.382 76.454) (xy 135.968421 77.580504)))
  )
  (gr_text "rev 1.0\nMay 2017\n" (at 147.32 99.314 90) (layer B.SilkS))
  (gr_text pockeTETRIS (at 152.527 93.091) (layer F.SilkS))
  (gr_line (start 137.668 115.824) (end 137.668 114.554) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 166.878 115.824) (end 137.668 115.824) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 166.878 76.454) (end 166.878 115.824) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 137.668 76.454) (end 166.878 76.454) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 137.668 114.554) (end 137.668 76.454) (angle 90) (layer Edge.Cuts) (width 0.15))
)
