(kicad_pcb (version 20171130) (host pcbnew "(5.1.2)-2")
  (general
    (thickness 1.6)
    (drawings 9)
    (tracks 14)
    (zones 0)
    (modules 6)
    (nets 82)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3.200001 3.200001)
    (pad_drill 3.200001)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(J1-Pad2)")
  (net 3 5V)
  (net 4 "Net-(U1-Pad17)")
  (net 5 "Net-(U1-Pad18)")
  (net 6 "Net-(U1-Pad19)")
  (net 7 "Net-(U1-Pad20)")
  (net 8 "Net-(U1-Pad16)")
  (net 9 "Net-(U1-Pad15)")
  (net 10 "Net-(U1-Pad14)")
  (net 11 "Net-(U1-Pad21)")
  (net 12 "Net-(U1-Pad22)")
  (net 13 "Net-(U1-Pad23)")
  (net 14 "Net-(U1-Pad24)")
  (net 15 "Net-(U1-Pad25)")
  (net 16 "Net-(U1-Pad26)")
  (net 17 "Net-(U1-Pad28)")
  (net 18 "Net-(U1-Pad29)")
  (net 19 "Net-(U1-Pad30)")
  (net 20 "Net-(U1-Pad31)")
  (net 21 "Net-(U1-Pad32)")
  (net 22 "Net-(U1-Pad33)")
  (net 23 "Net-(U1-Pad34)")
  (net 24 "Net-(U1-Pad35)")
  (net 25 "Net-(U1-Pad36)")
  (net 26 "Net-(U1-Pad37)")
  (net 27 "Net-(U1-Pad13)")
  (net 28 "Net-(U1-Pad12)")
  (net 29 "Net-(U1-Pad11)")
  (net 30 "Net-(U1-Pad10)")
  (net 31 "Net-(U1-Pad9)")
  (net 32 "Net-(U1-Pad8)")
  (net 33 "Net-(U1-Pad7)")
  (net 34 "Net-(U1-Pad6)")
  (net 35 "Net-(U1-Pad5)")
  (net 36 "Net-(U1-Pad4)")
  (net 37 "Net-(U1-Pad3)")
  (net 38 "Net-(U1-Pad38)")
  (net 39 "Net-(U1-Pad40)")
  (net 40 "Net-(U1-Pad41)")
  (net 41 "Net-(U1-Pad42)")
  (net 42 "Net-(U1-Pad43)")
  (net 43 "Net-(U1-Pad44)")
  (net 44 "Net-(U1-Pad45)")
  (net 45 "Net-(U1-Pad46)")
  (net 46 "Net-(U1-Pad47)")
  (net 47 "Net-(U1-Pad48)")
  (net 48 "Net-(U1-Pad49)")
  (net 49 "Net-(U1-Pad50)")
  (net 50 "Net-(U1-Pad51)")
  (net 51 "Net-(U1-Pad52)")
  (net 52 "Net-(U1-Pad53)")
  (net 53 "Net-(U1-Pad54)")
  (net 54 "Net-(U1-Pad55)")
  (net 55 "Net-(U1-Pad56)")
  (net 56 "Net-(U1-Pad57)")
  (net 57 "Net-(U1-Pad63)")
  (net 58 "Net-(U1-Pad64)")
  (net 59 "Net-(U1-Pad65)")
  (net 60 "Net-(U1-Pad66)")
  (net 61 "Net-(U1-Pad67)")
  (net 62 "Net-(U1-Pad68)")
  (net 63 "Net-(U1-Pad69)")
  (net 64 "Net-(U1-Pad70)")
  (net 65 "Net-(U1-Pad71)")
  (net 66 "Net-(U1-Pad72)")
  (net 67 "Net-(U1-Pad73)")
  (net 68 "Net-(U1-Pad75)")
  (net 69 "Net-(U1-Pad76)")
  (net 70 "Net-(U1-Pad77)")
  (net 71 "Net-(U1-Pad78)")
  (net 72 "Net-(U1-Pad79)")
  (net 73 "Net-(U1-Pad80)")
  (net 74 "Net-(U1-Pad81)")
  (net 75 "Net-(U1-Pad82)")
  (net 76 "Net-(U1-Pad83)")
  (net 77 "Net-(U1-Pad84)")
  (net 78 "Net-(U1-Pad85)")
  (net 79 "Net-(U1-Pad86)")
  (net 80 "Net-(U1-Pad2)")
  (net 81 "Net-(J1-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net 5V)
    (add_net GND)
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad11)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U1-Pad13)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U1-Pad15)")
    (add_net "Net-(U1-Pad16)")
    (add_net "Net-(U1-Pad17)")
    (add_net "Net-(U1-Pad18)")
    (add_net "Net-(U1-Pad19)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad20)")
    (add_net "Net-(U1-Pad21)")
    (add_net "Net-(U1-Pad22)")
    (add_net "Net-(U1-Pad23)")
    (add_net "Net-(U1-Pad24)")
    (add_net "Net-(U1-Pad25)")
    (add_net "Net-(U1-Pad26)")
    (add_net "Net-(U1-Pad28)")
    (add_net "Net-(U1-Pad29)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad30)")
    (add_net "Net-(U1-Pad31)")
    (add_net "Net-(U1-Pad32)")
    (add_net "Net-(U1-Pad33)")
    (add_net "Net-(U1-Pad34)")
    (add_net "Net-(U1-Pad35)")
    (add_net "Net-(U1-Pad36)")
    (add_net "Net-(U1-Pad37)")
    (add_net "Net-(U1-Pad38)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U1-Pad40)")
    (add_net "Net-(U1-Pad41)")
    (add_net "Net-(U1-Pad42)")
    (add_net "Net-(U1-Pad43)")
    (add_net "Net-(U1-Pad44)")
    (add_net "Net-(U1-Pad45)")
    (add_net "Net-(U1-Pad46)")
    (add_net "Net-(U1-Pad47)")
    (add_net "Net-(U1-Pad48)")
    (add_net "Net-(U1-Pad49)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad50)")
    (add_net "Net-(U1-Pad51)")
    (add_net "Net-(U1-Pad52)")
    (add_net "Net-(U1-Pad53)")
    (add_net "Net-(U1-Pad54)")
    (add_net "Net-(U1-Pad55)")
    (add_net "Net-(U1-Pad56)")
    (add_net "Net-(U1-Pad57)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U1-Pad63)")
    (add_net "Net-(U1-Pad64)")
    (add_net "Net-(U1-Pad65)")
    (add_net "Net-(U1-Pad66)")
    (add_net "Net-(U1-Pad67)")
    (add_net "Net-(U1-Pad68)")
    (add_net "Net-(U1-Pad69)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(U1-Pad70)")
    (add_net "Net-(U1-Pad71)")
    (add_net "Net-(U1-Pad72)")
    (add_net "Net-(U1-Pad73)")
    (add_net "Net-(U1-Pad75)")
    (add_net "Net-(U1-Pad76)")
    (add_net "Net-(U1-Pad77)")
    (add_net "Net-(U1-Pad78)")
    (add_net "Net-(U1-Pad79)")
    (add_net "Net-(U1-Pad8)")
    (add_net "Net-(U1-Pad80)")
    (add_net "Net-(U1-Pad81)")
    (add_net "Net-(U1-Pad82)")
    (add_net "Net-(U1-Pad83)")
    (add_net "Net-(U1-Pad84)")
    (add_net "Net-(U1-Pad85)")
    (add_net "Net-(U1-Pad86)")
    (add_net "Net-(U1-Pad9)")
  )
  (module teensy:USB_A_Female_UE27AC54100-Modified (layer F.Cu) (tedit 5D21AE05)
    (at 127 33.02 90)
    (fp_text reference J1 (at -0.075 -4.925 90) (layer F.SilkS))
    (fp_text value USB_A (at -0.375 17.925 90) (layer F.Fab))
    (fp_text user %R (at -0.025 0.975 90) (layer F.Fab))
    (pad 4 thru_hole circle (at 3.75 -2.71 90) (size 1.92 1.92) (drill 0.92) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at 1.25 -2.71 90) (size 1.92 1.92) (drill 0.92) (layers *.Cu *.Mask)
      (net 81 "Net-(J1-Pad3)"))
    (pad 2 thru_hole circle (at -1.25 -2.71 90) (size 1.92 1.92) (drill 0.92) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 1 thru_hole circle (at -3.75 -2.71 90) (size 1.92 1.92) (drill 0.92) (layers *.Cu *.Mask)
      (net 3 5V))
    (pad 5 thru_hole circle (at 6.57 0 90) (size 3.3 3.3) (drill 2.3) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole circle (at -6.57 0 90) (size 3.3 3.3) (drill 2.3) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 129.54 20.32)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference SC2 (at 0 3.81) (layer Cmts.User))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 129.54 45.72)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference SC3 (at 0 -4.2) (layer Cmts.User))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 66.04 45.72)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference SC4 (at 0 -4.2) (layer Cmts.User))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 66.04 20.32)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference SC1 (at 0 3.81) (layer Cmts.User))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module teensy:Teensy35_36 (layer F.Cu) (tedit 58E3CF68)
    (at 90.17 33.02)
    (fp_text reference U1 (at 0 -10.16) (layer F.SilkS))
    (fp_text value Teensy3.6 (at 0 10.16) (layer F.Fab))
    (pad 17 thru_hole circle (at 11.43 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 4 "Net-(U1-Pad17)"))
    (pad 18 thru_hole circle (at 13.97 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 "Net-(U1-Pad18)"))
    (pad 19 thru_hole circle (at 16.51 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 6 "Net-(U1-Pad19)"))
    (pad 20 thru_hole circle (at 19.05 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 7 "Net-(U1-Pad20)"))
    (pad 16 thru_hole circle (at 8.89 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 8 "Net-(U1-Pad16)"))
    (pad 15 thru_hole circle (at 6.35 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 9 "Net-(U1-Pad15)"))
    (pad 14 thru_hole circle (at 3.81 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 10 "Net-(U1-Pad14)"))
    (pad 21 thru_hole circle (at 21.59 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 11 "Net-(U1-Pad21)"))
    (pad 22 thru_hole circle (at 24.13 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 12 "Net-(U1-Pad22)"))
    (pad 23 thru_hole circle (at 26.67 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 13 "Net-(U1-Pad23)"))
    (pad 24 thru_hole circle (at 29.21 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 14 "Net-(U1-Pad24)"))
    (pad 25 thru_hole circle (at 16.51 5.08) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 15 "Net-(U1-Pad25)"))
    (pad 26 thru_hole circle (at 16.51 2.54) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 16 "Net-(U1-Pad26)"))
    (pad 27 thru_hole circle (at 16.51 0) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 28 thru_hole circle (at 16.51 -2.54) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 17 "Net-(U1-Pad28)"))
    (pad 29 thru_hole circle (at 16.51 -5.08) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 18 "Net-(U1-Pad29)"))
    (pad 30 thru_hole circle (at 29.21 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 19 "Net-(U1-Pad30)"))
    (pad 31 thru_hole circle (at 26.67 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 20 "Net-(U1-Pad31)"))
    (pad 32 thru_hole circle (at 24.13 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 21 "Net-(U1-Pad32)"))
    (pad 33 thru_hole circle (at 21.59 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 22 "Net-(U1-Pad33)"))
    (pad 34 thru_hole circle (at 19.05 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 23 "Net-(U1-Pad34)"))
    (pad 35 thru_hole circle (at 16.51 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 24 "Net-(U1-Pad35)"))
    (pad 36 thru_hole circle (at 13.97 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 25 "Net-(U1-Pad36)"))
    (pad 37 thru_hole circle (at 11.43 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 26 "Net-(U1-Pad37)"))
    (pad 13 thru_hole circle (at 1.27 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 27 "Net-(U1-Pad13)"))
    (pad 12 thru_hole circle (at -1.27 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 28 "Net-(U1-Pad12)"))
    (pad 11 thru_hole circle (at -3.81 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 29 "Net-(U1-Pad11)"))
    (pad 10 thru_hole circle (at -6.35 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 30 "Net-(U1-Pad10)"))
    (pad 9 thru_hole circle (at -8.89 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 31 "Net-(U1-Pad9)"))
    (pad 8 thru_hole circle (at -11.43 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 32 "Net-(U1-Pad8)"))
    (pad 7 thru_hole circle (at -13.97 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 33 "Net-(U1-Pad7)"))
    (pad 6 thru_hole circle (at -16.51 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 34 "Net-(U1-Pad6)"))
    (pad 5 thru_hole circle (at -19.05 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 35 "Net-(U1-Pad5)"))
    (pad 4 thru_hole circle (at -21.59 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 36 "Net-(U1-Pad4)"))
    (pad 3 thru_hole circle (at -24.13 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 37 "Net-(U1-Pad3)"))
    (pad 2 thru_hole circle (at -26.67 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 80 "Net-(U1-Pad2)"))
    (pad 1 thru_hole rect (at -29.21 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 38 thru_hole circle (at 8.89 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 38 "Net-(U1-Pad38)"))
    (pad 39 thru_hole circle (at 6.35 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 40 thru_hole circle (at 3.81 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 39 "Net-(U1-Pad40)"))
    (pad 41 thru_hole circle (at 1.27 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 40 "Net-(U1-Pad41)"))
    (pad 42 thru_hole circle (at -1.27 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 41 "Net-(U1-Pad42)"))
    (pad 43 thru_hole circle (at -3.81 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 42 "Net-(U1-Pad43)"))
    (pad 44 thru_hole circle (at -6.35 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 43 "Net-(U1-Pad44)"))
    (pad 45 thru_hole circle (at -8.89 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 44 "Net-(U1-Pad45)"))
    (pad 46 thru_hole circle (at -11.43 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 45 "Net-(U1-Pad46)"))
    (pad 47 thru_hole circle (at -13.97 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 46 "Net-(U1-Pad47)"))
    (pad 48 thru_hole circle (at -16.51 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 47 "Net-(U1-Pad48)"))
    (pad 49 thru_hole circle (at -19.05 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 48 "Net-(U1-Pad49)"))
    (pad 50 thru_hole circle (at -21.59 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 49 "Net-(U1-Pad50)"))
    (pad 51 thru_hole circle (at -24.13 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 50 "Net-(U1-Pad51)"))
    (pad 52 thru_hole circle (at -26.67 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 51 "Net-(U1-Pad52)"))
    (pad 53 thru_hole circle (at -29.21 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 52 "Net-(U1-Pad53)"))
    (pad 54 thru_hole circle (at -26.67 -5.08) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 53 "Net-(U1-Pad54)"))
    (pad 55 thru_hole circle (at -21.59 -5.08) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 54 "Net-(U1-Pad55)"))
    (pad 56 thru_hole circle (at -19.05 -5.08) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 55 "Net-(U1-Pad56)"))
    (pad 57 thru_hole circle (at -16.51 -5.08) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 56 "Net-(U1-Pad57)"))
    (pad 63 thru_hole circle (at -13.97 0) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 57 "Net-(U1-Pad63)"))
    (pad 64 thru_hole circle (at -11.43 0) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 58 "Net-(U1-Pad64)"))
    (pad 65 thru_hole circle (at -8.89 0) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 59 "Net-(U1-Pad65)"))
    (pad 66 thru_hole circle (at -6.35 0) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 60 "Net-(U1-Pad66)"))
    (pad 67 thru_hole circle (at 8.89 0) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 61 "Net-(U1-Pad67)"))
    (pad 68 thru_hole circle (at 11.43 0) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 62 "Net-(U1-Pad68)"))
    (pad 69 thru_hole circle (at 13.97 0) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 63 "Net-(U1-Pad69)"))
    (pad 70 thru_hole circle (at 19.05 0) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 64 "Net-(U1-Pad70)"))
    (pad 71 thru_hole circle (at 21.59 0) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 65 "Net-(U1-Pad71)"))
    (pad 72 thru_hole circle (at 24.13 0) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 66 "Net-(U1-Pad72)"))
    (pad 73 thru_hole circle (at 26.67 0) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 67 "Net-(U1-Pad73)"))
    (pad 74 thru_hole circle (at 29.21 0) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 75 thru_hole circle (at 29.21 -2.54) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 68 "Net-(U1-Pad75)"))
    (pad 76 thru_hole circle (at 26.67 -2.54) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 69 "Net-(U1-Pad76)"))
    (pad 77 thru_hole circle (at 24.13 -2.54) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 70 "Net-(U1-Pad77)"))
    (pad 78 thru_hole circle (at 21.59 -2.54) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 71 "Net-(U1-Pad78)"))
    (pad 79 thru_hole circle (at 19.05 -2.54) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 72 "Net-(U1-Pad79)"))
    (pad 80 thru_hole circle (at 13.97 -2.54) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 73 "Net-(U1-Pad80)"))
    (pad 81 thru_hole circle (at 11.43 -2.54) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 74 "Net-(U1-Pad81)"))
    (pad 82 thru_hole circle (at 8.89 -2.54) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 75 "Net-(U1-Pad82)"))
    (pad 83 thru_hole circle (at -6.35 -2.54) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 76 "Net-(U1-Pad83)"))
    (pad 84 thru_hole circle (at -8.89 -2.54) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 77 "Net-(U1-Pad84)"))
    (pad 85 thru_hole circle (at -11.43 -2.54) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 78 "Net-(U1-Pad85)"))
    (pad 86 thru_hole circle (at -13.97 -2.54) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 79 "Net-(U1-Pad86)"))
    (pad 58 thru_hole circle (at -22.86 4.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 5V))
    (pad 59 thru_hole circle (at -20.32 4.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 60 thru_hole circle (at -17.78 4.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 81 "Net-(J1-Pad3)"))
    (pad 61 thru_hole circle (at -15.24 4.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 62 thru_hole circle (at -12.7 4.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (gr_line (start 135.89 16.51) (end 59.69 16.51) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 59.69 49.53) (end 135.89 49.53) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 58.42 17.78) (end 59.69 16.51) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 58.42 48.26) (end 59.69 49.53) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 58.42 48.26) (end 58.42 17.78) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 137.16 48.26) (end 137.16 17.78) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 135.89 49.53) (end 137.16 48.26) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 135.89 16.51) (end 137.16 17.78) (layer Edge.Cuts) (width 0.05))
  (gr_text "t3.6 usb breakout\nmount with 3mm nylon screws\ncurious.jp@gmail.com" (at 71.12 20.32) (layer F.SilkS))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 132.08 25.4) (xy 129.54 22.86) (xy 60.96 22.86) (xy 58.42 25.4) (xy 58.42 40.64)
        (xy 60.96 43.18) (xy 129.54 43.18) (xy 132.08 40.64)
      )
    )
  )
)
