<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.4.1">
<drawing>
<board>
<plain>
<wire x1="2.032" y1="29.464" x2="2.032" y2="5.588" width="0.1524" layer="20"/>
<wire x1="2.032" y1="5.588" x2="20.828" y2="5.588" width="0.1524" layer="20"/>
<wire x1="20.828" y1="5.588" x2="20.828" y2="29.464" width="0.1524" layer="20"/>
<wire x1="2.032" y1="29.464" x2="20.828" y2="29.464" width="0.1524" layer="20"/>
</plain>
<libraries>
<library name="wirepad">
<description>&lt;b&gt;Single Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SMD1,27-2,54">
<description>&lt;b&gt;SMD PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="con-yamaichi">
<description>&lt;b&gt;Yamaichi Connectors&lt;/b&gt;&lt;p&gt;
Mini-DIN, USB, Fire Wire&lt;br&gt;
DIN female/male, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="MDIN09SS">
<description>&lt;b&gt;Mini Din&lt;/b&gt; YAMAICHI CONNECTOR</description>
</package>
</packages>
</library>
<library name="special-drill">
<description>&lt;b&gt;Special drills&lt;/b&gt;&lt;p&gt;
For drills bigger as 0.51602 Inch you must draw a circle in Layer 20 Dimension.&lt;br&gt;
See also HELP HOLE,</description>
<packages>
<package name="PAD_0.1000">
<description>&lt;b&gt;0.1000 Inch&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="B" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RIGHT" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="5V" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LEFT" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CVID" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="G" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="GENESIS2-AVJACK" library="con-yamaichi" package="MDIN09SS" value="">
<attribute name="VALUE"/>
</element>
<element name="GRND2" library="special-drill" package="PAD_0.1000" value="">
<attribute name="VALUE"/>
</element>
<element name="GRND3" library="special-drill" package="PAD_0.1000" value="">
<attribute name="VALUE"/>
</element>
<element name="GRD" library="special-drill" package="PAD_0.1000" value="">
<attribute name="VALUE"/>
</element>
<element name="GRND" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SHIELD" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="S$1">
<contactref element="GENESIS2-AVJACK" pad="6"/>
<contactref element="G" pad="1"/>
</signal>
<signal name="S$2">
<contactref element="GENESIS2-AVJACK" pad="9"/>
<contactref element="R" pad="1"/>
</signal>
<signal name="S$3">
<contactref element="GENESIS2-AVJACK" pad="8"/>
<contactref element="CVID" pad="1"/>
</signal>
<signal name="S$4">
<contactref element="GENESIS2-AVJACK" pad="2"/>
<contactref element="B" pad="1"/>
</signal>
<signal name="S$5">
<contactref element="GENESIS2-AVJACK" pad="1"/>
<contactref element="5V" pad="1"/>
</signal>
<signal name="S$6">
<contactref element="GENESIS2-AVJACK" pad="3"/>
</signal>
<signal name="S$7">
<contactref element="GENESIS2-AVJACK" pad="5"/>
</signal>
<signal name="S$8">
<contactref element="GENESIS2-AVJACK" pad="4"/>
<contactref element="LEFT" pad="1"/>
</signal>
<signal name="S$9">
<contactref element="GENESIS2-AVJACK" pad="7"/>
<contactref element="RIGHT" pad="1"/>
</signal>
<signal name="GRD">
<contactref element="GRND2" pad="1"/>
<contactref element="GRD" pad="1"/>
<contactref element="GRND3" pad="1"/>
<contactref element="GRND" pad="1"/>
<contactref element="SHIELD" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
